
Instructions to Build CCS based Flash Writers from Serial Flash and boot Utilities in CCSv7.

**Software required:**



[Serial flash and boot utilities for OMAPL138](http://processors.wiki.ti.com/index.php/Serial_Boot_and_Flash_Loading_Utility_for_OMAP-L138)


[Compiler CGTools 7.4x](http://software-dl.ti.com/codegen/non-esd/downloads/download.htm) [Flash writers projects are configured to build in COFF binaries and CGTools v8.x only builds ELF]


**Step 1**: Add path to Compiler 7.4.x in the CCS compiler discovery path. Go to Windows->Preferences:





**Step 2: Import the project as Legacy CCSv3.3 project and select compiler 7.4 and the common root as shown below:**


** **


****

****

**** ****

****

****

****