JTAG ID= 0x1b98102f. This is a K2H/K2K device, version variant = 1
DEVSTAT= 0x02060ee1. little endian, no boot or I2C slave boot, boot master is ARM core, PLL configuration implies the input clock for core is 122.88MHz
SmartReflex VID= 46, required core voltage= 0.995V.
Die ID= 0x0c011004, 0x04010235, 0x00000000, 0x60ba0001
DSP speed grade = 1200MHz, ARM speed grade= 1200MHz
Enable IRQ and FIQ.
Enable Exception handling...
Initialize main core clock = 122.88MHz/4x39 = 1198MHz
Initialize ARM clock = 125.00MHz/5x48 = 1200MHz
DDR3A initialization
Initialize DDR data rate = 100.000/1*20/6*4= 1333.3 MTS, bus width = 64 bits.
Ethernet port 0 test setup: no connection  , forced 1000M fullduplex  , SerDes internal loopback
Ethernet port 1 test setup: no connection  , forced 1000M fullduplex  , SGMII loopback          
Ethernet port 2 test setup: no connection  , forced 1000M fullduplex  , SerDes internal loopback
Ethernet port 3 test setup: no connection  , forced 1000M fullduplex  , SGMII loopback          
Initialize PASS PLL clock = 122.88MHz/24x205 = 1049MHz
STATSA.RxGoodFrames     =4
STATSA.RxOctets         =584
STATSA.TxGoodFrames     =2
STATSA.TxOctets         =292
STATSA.Frame128t255     =6
STATSA.NetOctets        =876
STATSB.RxGoodFrames     =2
STATSB.RxOctets         =292
STATSB.TxGoodFrames     =2
STATSB.TxOctets         =292
STATSB.Frame128t255     =4
STATSB.NetOctets        =584
STATSC.TxGoodFrames     =2
STATSC.TxOctets         =292
STATSC.Frame128t255     =2
STATSC.NetOctets        =292
STATSD.RxGoodFrames     =2
STATSD.RxOctets         =292
STATSD.TxGoodFrames     =2
STATSD.TxOctets         =292
STATSD.Frame128t255     =4
STATSD.NetOctets        =584
Ethernet port 0 TX  1 packets x  128 bytes, RX  1 packets,     5686 cycles,   215 Mbps
Ethernet port 1 TX  1 packets x  128 bytes, RX  1 packets,     5842 cycles,   210 Mbps
Ethernet port 2 TX  1 packets x  128 bytes, RX  1 packets,     6143 cycles,   199 Mbps
Ethernet port 3 TX  1 packets x  128 bytes, RX  1 packets,     5631 cycles,   217 Mbps

STATSA.RxGoodFrames     =8
STATSA.RxOctets         =4752
STATSA.TxGoodFrames     =4
STATSA.TxOctets         =2376
STATSA.Frame1024tUp     =6
STATSA.NetOctets        =7128
STATSB.RxGoodFrames     =4
STATSB.RxOctets         =2376
STATSB.TxGoodFrames     =4
STATSB.TxOctets         =2376
STATSB.Frame1024tUp     =4
STATSB.NetOctets        =4752
STATSC.TxGoodFrames     =4
STATSC.TxOctets         =2376
STATSC.Frame1024tUp     =2
STATSC.NetOctets        =2376
STATSD.RxGoodFrames     =4
STATSD.RxOctets         =2376
STATSD.TxGoodFrames     =4
STATSD.TxOctets         =2376
STATSD.Frame1024tUp     =4
STATSD.NetOctets        =4752
Ethernet port 0 TX  1 packets x 1024 bytes, RX  1 packets,    21719 cycles,   451 Mbps
Ethernet port 1 TX  1 packets x 1024 bytes, RX  1 packets,    24036 cycles,   408 Mbps
Ethernet port 2 TX  1 packets x 1024 bytes, RX  1 packets,    26773 cycles,   366 Mbps
Ethernet port 3 TX  1 packets x 1024 bytes, RX  1 packets,    28530 cycles,   344 Mbps

STATSA.RxGoodFrames     =12
STATSA.RxOctets         =37592
STATSA.TxGoodFrames     =6
STATSA.TxOctets         =18796
STATSA.Frame1024tUp     =12
STATSA.NetOctets        =56388
STATSB.RxGoodFrames     =6
STATSB.RxOctets         =18796
STATSB.TxGoodFrames     =6
STATSB.TxOctets         =18796
STATSB.Frame1024tUp     =8
STATSB.NetOctets        =37592
STATSC.TxGoodFrames     =6
STATSC.TxOctets         =18796
STATSC.Frame1024tUp     =4
STATSC.NetOctets        =18796
STATSD.RxGoodFrames     =6
STATSD.RxOctets         =18796
STATSD.TxGoodFrames     =6
STATSD.TxOctets         =18796
STATSD.Frame1024tUp     =8
STATSD.NetOctets        =37592
Ethernet port 0 TX  1 packets x 8192 bytes, RX  1 packets,   145797 cycles,   538 Mbps
Ethernet port 1 TX  1 packets x 8192 bytes, RX  1 packets,   173438 cycles,   452 Mbps
Ethernet port 2 TX  1 packets x 8192 bytes, RX  1 packets,   201269 cycles,   390 Mbps
Ethernet port 3 TX  1 packets x 8192 bytes, RX  1 packets,   227601 cycles,   344 Mbps

STATSA.RxGoodFrames     =28
STATSA.RxOctets         =39928
STATSA.TxGoodFrames     =14
STATSA.TxOctets         =19964
STATSA.Frame128t255     =30
STATSA.NetOctets        =59892
STATSB.RxGoodFrames     =14
STATSB.RxOctets         =19964
STATSB.TxGoodFrames     =14
STATSB.TxOctets         =19964
STATSB.Frame128t255     =20
STATSB.NetOctets        =39928
STATSC.TxGoodFrames     =14
STATSC.TxOctets         =19964
STATSC.Frame128t255     =10
STATSC.NetOctets        =19964
STATSD.RxGoodFrames     =14
STATSD.RxOctets         =19964
STATSD.TxGoodFrames     =14
STATSD.TxOctets         =19964
STATSD.Frame128t255     =20
STATSD.NetOctets        =39928
Ethernet port 0 TX  4 packets x  128 bytes, RX  4 packets,    40530 cycles,   121 Mbps
Ethernet port 1 TX  4 packets x  128 bytes, RX  4 packets,    40055 cycles,   122 Mbps
Ethernet port 2 TX  4 packets x  128 bytes, RX  4 packets,    40823 cycles,   120 Mbps
Ethernet port 3 TX  4 packets x  128 bytes, RX  4 packets,    40291 cycles,   121 Mbps

STATSA.RxGoodFrames     =44
STATSA.RxOctets         =56600
STATSA.TxGoodFrames     =22
STATSA.TxOctets         =28300
STATSA.Frame1024tUp     =36
STATSA.NetOctets        =84900
STATSB.RxGoodFrames     =22
STATSB.RxOctets         =28300
STATSB.TxGoodFrames     =22
STATSB.TxOctets         =28300
STATSB.Frame1024tUp     =24
STATSB.NetOctets        =56600
STATSC.TxGoodFrames     =22
STATSC.TxOctets         =28300
STATSC.Frame1024tUp     =12
STATSC.NetOctets        =28300
STATSD.RxGoodFrames     =22
STATSD.RxOctets         =28300
STATSD.TxGoodFrames     =22
STATSD.TxOctets         =28300
STATSD.Frame1024tUp     =24
STATSD.NetOctets        =56600
Ethernet port 0 TX  4 packets x 1024 bytes, RX  4 packets,    68464 cycles,   573 Mbps
Ethernet port 1 TX  4 packets x 1024 bytes, RX  4 packets,    70960 cycles,   553 Mbps
Ethernet port 2 TX  4 packets x 1024 bytes, RX  4 packets,    74348 cycles,   528 Mbps
Ethernet port 3 TX  4 packets x 1024 bytes, RX  4 packets,    76579 cycles,   512 Mbps

STATSA.RxGoodFrames     =60
STATSA.RxOctets         =187960
STATSA.TxGoodFrames     =30
STATSA.TxOctets         =93980
STATSA.Frame1024tUp     =60
STATSA.NetOctets        =281940
STATSB.RxGoodFrames     =30
STATSB.RxOctets         =93980
STATSB.TxGoodFrames     =30
STATSB.TxOctets         =93980
STATSB.Frame1024tUp     =40
STATSB.NetOctets        =187960
STATSC.TxGoodFrames     =30
STATSC.TxOctets         =93980
STATSC.Frame1024tUp     =20
STATSC.NetOctets        =93980
STATSD.RxGoodFrames     =30
STATSD.RxOctets         =93980
STATSD.TxGoodFrames     =30
STATSD.TxOctets         =93980
STATSD.Frame1024tUp     =40
STATSD.NetOctets        =187960
Ethernet port 0 TX  4 packets x 8192 bytes, RX  4 packets,   489223 cycles,   641 Mbps
Ethernet port 1 TX  4 packets x 8192 bytes, RX  4 packets,   516242 cycles,   608 Mbps
Ethernet port 2 TX  4 packets x 8192 bytes, RX  4 packets,   543167 cycles,   578 Mbps
Ethernet port 3 TX  4 packets x 8192 bytes, RX  4 packets,   570799 cycles,   550 Mbps

STATSA.RxGoodFrames     =124
STATSA.RxOctets         =197304
STATSA.TxGoodFrames     =62
STATSA.TxOctets         =98652
STATSA.Frame128t255     =126
STATSA.NetOctets        =295956
STATSB.RxGoodFrames     =62
STATSB.RxOctets         =98652
STATSB.TxGoodFrames     =62
STATSB.TxOctets         =98652
STATSB.Frame128t255     =84
STATSB.NetOctets        =197304
STATSC.TxGoodFrames     =62
STATSC.TxOctets         =98652
STATSC.Frame128t255     =42
STATSC.NetOctets        =98652
STATSD.RxGoodFrames     =62
STATSD.RxOctets         =98652
STATSD.TxGoodFrames     =62
STATSD.TxOctets         =98652
STATSD.Frame128t255     =84
STATSD.NetOctets        =197304
Ethernet port 0 TX 16 packets x  128 bytes, RX 16 packets,   171301 cycles,   114 Mbps
Ethernet port 1 TX 16 packets x  128 bytes, RX 16 packets,   171207 cycles,   114 Mbps
Ethernet port 2 TX 16 packets x  128 bytes, RX 16 packets,   171984 cycles,   114 Mbps
Ethernet port 3 TX 16 packets x  128 bytes, RX 16 packets,   171410 cycles,   114 Mbps

STATSA.RxGoodFrames     =188
STATSA.RxOctets         =263992
STATSA.TxGoodFrames     =94
STATSA.TxOctets         =131996
STATSA.Frame1024tUp     =156
STATSA.NetOctets        =395988
STATSB.RxGoodFrames     =94
STATSB.RxOctets         =131996
STATSB.TxGoodFrames     =94
STATSB.TxOctets         =131996
STATSB.Frame1024tUp     =104
STATSB.NetOctets        =263992
STATSC.TxGoodFrames     =94
STATSC.TxOctets         =131996
STATSC.Frame1024tUp     =52
STATSC.NetOctets        =131996
STATSD.RxGoodFrames     =94
STATSD.RxOctets         =131996
STATSD.TxGoodFrames     =94
STATSD.TxOctets         =131996
STATSD.Frame1024tUp     =104
STATSD.NetOctets        =263992
Ethernet port 0 TX 16 packets x 1024 bytes, RX 16 packets,   262158 cycles,   599 Mbps
Ethernet port 1 TX 16 packets x 1024 bytes, RX 16 packets,   264539 cycles,   593 Mbps
Ethernet port 2 TX 16 packets x 1024 bytes, RX 16 packets,   267266 cycles,   587 Mbps
Ethernet port 3 TX 16 packets x 1024 bytes, RX 16 packets,   270607 cycles,   580 Mbps

STATSA.RxGoodFrames     =252
STATSA.RxOctets         =789432
STATSA.TxGoodFrames     =126
STATSA.TxOctets         =394716
STATSA.Frame1024tUp     =252
STATSA.NetOctets        =1184148
STATSB.RxGoodFrames     =126
STATSB.RxOctets         =394716
STATSB.TxGoodFrames     =126
STATSB.TxOctets         =394716
STATSB.Frame1024tUp     =168
STATSB.NetOctets        =789432
STATSC.TxGoodFrames     =126
STATSC.TxOctets         =394716
STATSC.Frame1024tUp     =84
STATSC.NetOctets        =394716
STATSD.RxGoodFrames     =126
STATSD.RxOctets         =394716
STATSD.TxGoodFrames     =126
STATSD.TxOctets         =394716
STATSD.Frame1024tUp     =168
STATSD.NetOctets        =789432
Ethernet port 0 TX 16 packets x 8192 bytes, RX 16 packets,  1861705 cycles,   674 Mbps
Ethernet port 1 TX 16 packets x 8192 bytes, RX 16 packets,  1888960 cycles,   665 Mbps
Ethernet port 2 TX 16 packets x 8192 bytes, RX 16 packets,  1916320 cycles,   655 Mbps
Ethernet port 3 TX 16 packets x 8192 bytes, RX 16 packets,  1943294 cycles,   646 Mbps

GE test complete.

