JTAG ID= 0x0b9a602f. This is a K2E device, version variant = 0
DEVSTAT= 0x00000661. little endian, no boot or I2C slave boot, boot master is ARM core, PLL configuration implies the input clock for core is 100MHz
SmartReflex VID= 46, required core voltage= 0.995V.
Die ID= 0x0600c004, 0x0c00ea85, 0x00000000, 0x79900000
DSP speed grade = 800MHz, ARM speed grade= 800MHz
Enable IRQ and FIQ.
Enable Exception handling...
Initialize main core clock = 100.00MHz/1x12 = 1200MHz
DDR3A initialization
Initialize DDR data rate = 100.000/1*16/4*4= 1600.0 MTS, bus width = 64 bits.
DDR PHY status PGSR0=0xb0000fff.
PCIE PHY loopback mode at 5.0GHz.
PCIE link 0 start link training...
PCIE link 0 training is finished.
PCIE memory test passed at address 0x51800000
PCIE memory test passed at address 0x54840000
PCIE memory test passed at address 0x54920000
PCIE MSI8 interrupt generated!
PCIE interrupt latency is 2026 cycles
#########RC starts core access performance test!#########
  211 MB/s, copy  65536 bytes from 0x0c080000( local MSRAM) to 0x54920000(  remote LL2), consumes 371547 cycles
   31 MB/s, copy  65536 bytes from 0x54920000(  remote LL2) to 0x0c080000( local MSRAM), consumes 2535523 cycles
   28 MB/s, copy  65536 bytes from 0x54920000(  remote LL2) to 0x54930000(  remote LL2), consumes 2793327 cycles
  204 MB/s, copy  65536 bytes from 0x0c080000( local MSRAM) to 0x54840000(remote MSRAM), consumes 384619 cycles
   29 MB/s, copy  65536 bytes from 0x54840000(remote MSRAM) to 0x0c080000( local MSRAM), consumes 2650626 cycles
   27 MB/s, copy  65536 bytes from 0x54840000(remote MSRAM) to 0x54850000(remote MSRAM), consumes 2907178 cycles
  202 MB/s, copy  65536 bytes from 0x0c080000( local MSRAM) to 0x51800000(remote DDR3A), consumes 387850 cycles
   28 MB/s, copy  65536 bytes from 0x51800000(remote DDR3A) to 0x0c080000( local MSRAM), consumes 2762992 cycles
   26 MB/s, copy  65536 bytes from 0x51800000(remote DDR3A) to 0x51810000(remote DDR3A), consumes 2999557 cycles
Memory load performance test at 0x54920000(  remote LL2)
Index=   0  Cycles/LDRD= 173.69
Index=   1  Cycles/LDRD= 173.66
Index=   2  Cycles/LDRD= 173.66
Index=   3  Cycles/LDRD= 173.69
Index=   4  Cycles/LDRD= 173.67
Index=   5  Cycles/LDRD= 173.67
Index=   6  Cycles/LDRD= 173.66
Index=   7  Cycles/LDRD= 173.69
Index=   8  Cycles/LDRD= 173.67
Index=  10  Cycles/LDRD= 173.67
Index=  12  Cycles/LDRD= 173.62
Index=  14  Cycles/LDRD= 173.64
Index=  16  Cycles/LDRD= 173.70
Index=  18  Cycles/LDRD= 173.67
Index=  20  Cycles/LDRD= 173.70
Index=  22  Cycles/LDRD= 173.72
Index=  24  Cycles/LDRD= 173.70
Index=  26  Cycles/LDRD= 173.67
Index=  28  Cycles/LDRD= 173.69
Index=  30  Cycles/LDRD= 173.73
Index=  32  Cycles/LDRD= 173.70
Index=  40  Cycles/LDRD= 173.65
Index=  48  Cycles/LDRD= 173.68
Index=  56  Cycles/LDRD= 173.66
Memory store performance test at 0x54920000(  remote LL2)
Index=   0  Cycles/STRD= 93.53
Index=   1  Cycles/STRD= 92.98
Index=   2  Cycles/STRD= 92.89
Index=   3  Cycles/STRD= 92.75
Index=   4  Cycles/STRD= 93.13
Index=   5  Cycles/STRD= 93.23
Index=   6  Cycles/STRD= 92.89
Index=   7  Cycles/STRD= 92.78
Index=   8  Cycles/STRD= 92.89
Index=  10  Cycles/STRD= 92.33
Index=  12  Cycles/STRD= 93.24
Index=  14  Cycles/STRD= 93.72
Index=  16  Cycles/STRD= 93.19
Index=  18  Cycles/STRD= 92.83
Index=  20  Cycles/STRD= 92.98
Index=  22  Cycles/STRD= 93.35
Index=  24  Cycles/STRD= 93.05
Index=  26  Cycles/STRD= 93.28
Index=  28  Cycles/STRD= 93.34
Index=  30  Cycles/STRD= 93.08
Index=  32  Cycles/STRD= 92.92
Index=  40  Cycles/STRD= 93.78
Index=  48  Cycles/STRD= 92.84
Index=  56  Cycles/STRD= 92.32
Memory load performance test at 0x54840000(remote MSRAM)
Index=   0  Cycles/LDRD= 182.24
Index=   1  Cycles/LDRD= 182.32
Index=   2  Cycles/LDRD= 182.68
Index=   3  Cycles/LDRD= 182.30
Index=   4  Cycles/LDRD= 182.46
Index=   5  Cycles/LDRD= 182.30
Index=   6  Cycles/LDRD= 182.50
Index=   7  Cycles/LDRD= 182.25
Index=   8  Cycles/LDRD= 182.29
Index=  10  Cycles/LDRD= 182.50
Index=  12  Cycles/LDRD= 182.79
Index=  14  Cycles/LDRD= 182.46
Index=  16  Cycles/LDRD= 182.00
Index=  18  Cycles/LDRD= 182.72
Index=  20  Cycles/LDRD= 182.70
Index=  22  Cycles/LDRD= 182.63
Index=  24  Cycles/LDRD= 182.10
Index=  26  Cycles/LDRD= 182.67
Index=  28  Cycles/LDRD= 182.69
Index=  30  Cycles/LDRD= 182.51
Index=  32  Cycles/LDRD= 182.23
Index=  40  Cycles/LDRD= 182.14
Index=  48  Cycles/LDRD= 182.35
Index=  56  Cycles/LDRD= 182.43
Index=  64  Cycles/LDRD= 182.51
Index=  96  Cycles/LDRD= 182.47
Index= 128  Cycles/LDRD= 182.75
Index= 192  Cycles/LDRD= 182.83
Memory store performance test at 0x54840000(remote MSRAM)
Index=   0  Cycles/STRD= 93.16
Index=   1  Cycles/STRD= 92.84
Index=   2  Cycles/STRD= 92.91
Index=   3  Cycles/STRD= 92.50
Index=   4  Cycles/STRD= 92.92
Index=   5  Cycles/STRD= 92.83
Index=   6  Cycles/STRD= 93.22
Index=   7  Cycles/STRD= 92.83
Index=   8  Cycles/STRD= 92.83
Index=  10  Cycles/STRD= 93.20
Index=  12  Cycles/STRD= 93.78
Index=  14  Cycles/STRD= 92.85
Index=  16  Cycles/STRD= 93.20
Index=  18  Cycles/STRD= 92.99
Index=  20  Cycles/STRD= 93.49
Index=  22  Cycles/STRD= 93.27
Index=  24  Cycles/STRD= 93.23
Index=  26  Cycles/STRD= 93.24
Index=  28  Cycles/STRD= 93.34
Index=  30  Cycles/STRD= 92.84
Index=  32  Cycles/STRD= 93.15
Index=  40  Cycles/STRD= 93.35
Index=  48  Cycles/STRD= 92.99
Index=  56  Cycles/STRD= 92.92
Index=  64  Cycles/STRD= 93.66
Index=  96  Cycles/STRD= 93.29
Index= 128  Cycles/STRD= 93.24
Index= 192  Cycles/STRD= 92.83
Memory load performance test at 0x51800000(remote DDR3A)
Index=   0  Cycles/LDRD= 195.06
Index=   1  Cycles/LDRD= 194.87
Index=   2  Cycles/LDRD= 194.27
Index=   3  Cycles/LDRD= 194.59
Index=   4  Cycles/LDRD= 195.61
Index=   5  Cycles/LDRD= 194.47
Index=   6  Cycles/LDRD= 195.48
Index=   7  Cycles/LDRD= 195.57
Index=   8  Cycles/LDRD= 194.22
Index=  10  Cycles/LDRD= 195.17
Index=  12  Cycles/LDRD= 195.92
Index=  14  Cycles/LDRD= 195.27
Index=  16  Cycles/LDRD= 194.89
Index=  18  Cycles/LDRD= 195.45
Index=  20  Cycles/LDRD= 194.21
Index=  22  Cycles/LDRD= 194.16
Index=  24  Cycles/LDRD= 194.38
Index=  26  Cycles/LDRD= 196.23
Index=  28  Cycles/LDRD= 195.04
Index=  30  Cycles/LDRD= 194.59
Index=  32  Cycles/LDRD= 196.04
Index=  40  Cycles/LDRD= 194.56
Index=  48  Cycles/LDRD= 194.34
Index=  56  Cycles/LDRD= 194.41
Index=  64  Cycles/LDRD= 195.04
Index=  96  Cycles/LDRD= 195.82
Index= 128  Cycles/LDRD= 195.49
Index= 192  Cycles/LDRD= 194.74
Index= 256  Cycles/LDRD= 194.91
Index= 384  Cycles/LDRD= 195.76
Index= 512  Cycles/LDRD= 197.04
Index= 768  Cycles/LDRD= 196.94
Index=1024  Cycles/LDRD= 197.39
Index=1536  Cycles/LDRD= 197.26
Index=2048  Cycles/LDRD= 197.22
Index=3072  Cycles/LDRD= 198.63
Memory store performance test at 0x51800000(remote DDR3A)
Index=   0  Cycles/STRD= 92.98
Index=   1  Cycles/STRD= 93.02
Index=   2  Cycles/STRD= 93.12
Index=   3  Cycles/STRD= 93.06
Index=   4  Cycles/STRD= 93.32
Index=   5  Cycles/STRD= 92.75
Index=   6  Cycles/STRD= 93.07
Index=   7  Cycles/STRD= 93.33
Index=   8  Cycles/STRD= 93.10
Index=  10  Cycles/STRD= 93.28
Index=  12  Cycles/STRD= 93.33
Index=  14  Cycles/STRD= 93.54
Index=  16  Cycles/STRD= 93.34
Index=  18  Cycles/STRD= 93.32
Index=  20  Cycles/STRD= 92.71
Index=  22  Cycles/STRD= 93.00
Index=  24  Cycles/STRD= 93.42
Index=  26  Cycles/STRD= 92.84
Index=  28  Cycles/STRD= 93.04
Index=  30  Cycles/STRD= 92.92
Index=  32  Cycles/STRD= 93.13
Index=  40  Cycles/STRD= 93.09
Index=  48  Cycles/STRD= 92.94
Index=  56  Cycles/STRD= 92.94
Index=  64  Cycles/STRD= 93.39
Index=  96  Cycles/STRD= 92.88
Index= 128  Cycles/STRD= 92.96
Index= 192  Cycles/STRD= 92.59
Index= 256  Cycles/STRD= 93.27
Index= 384  Cycles/STRD= 93.05
Index= 512  Cycles/STRD= 92.99
Index= 768  Cycles/STRD= 93.27
Index=1024  Cycles/STRD= 93.10
Index=1536  Cycles/STRD= 93.24
Index=2048  Cycles/STRD= 92.97
Index=3072  Cycles/STRD= 92.97
#########RC starts EDMA performance test!#########
Overhead test with EDMA CC0 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    590 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    589 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    500 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1431 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1500 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1611 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    498 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    465 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1406 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1495 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1495 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    605 cycles, achieve throughput    15 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    606 cycles, achieve throughput    15 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1403 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1495 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1604 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1496 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1611 cycles, achieve throughput     5 MB/s
Throughput test with EDMA CC0 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139407 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140073 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139234 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108708 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108761 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110041 cycles, achieve throughput   714 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140007 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139642 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140229 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108705 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108650 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110370 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 139229 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 137539 cycles, achieve throughput   571 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 138894 cycles, achieve throughput   566 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108700 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108753 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110705 cycles, achieve throughput   710 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209271 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207529 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207387 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC0 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    589 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    589 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1589 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1696 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1583 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1590 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC0 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139567 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140111 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140012 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108708 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108757 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110485 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 139787 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139653 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140342 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108705 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108748 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110370 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 139787 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140309 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 139783 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108703 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108748 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110595 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207718 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207538 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207500 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC1 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    485 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1368 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1585 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1364 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1477 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC1 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139679 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 139742 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140233 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108599 cycles, achieve throughput   724 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108637 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110262 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140342 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140338 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 138898 cycles, achieve throughput   566 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108706 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108665 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110261 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140339 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140059 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140004 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108702 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108740 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110705 cycles, achieve throughput   710 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209272 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207528 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207498 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC1 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1367 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1583 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1478 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC1 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139790 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 138868 cycles, achieve throughput   566 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139123 cycles, achieve throughput   565 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108598 cycles, achieve throughput   724 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108729 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110373 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 139674 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139830 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139676 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108701 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108751 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110372 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 138564 cycles, achieve throughput   567 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140093 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 139229 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108703 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108751 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110699 cycles, achieve throughput   710 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209162 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207633 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207389 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC1 TC2
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1584 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1364 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1478 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC1 TC2
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139456 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140216 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140345 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108597 cycles, achieve throughput   724 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108636 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110262 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140453 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139969 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139563 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108705 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108734 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110260 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 139451 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140324 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140337 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108703 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108742 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110594 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209273 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207290 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207389 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC1 TC3
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1585 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1585 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1478 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC1 TC3
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140011 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 139434 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139567 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108709 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108641 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110262 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 139343 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140189 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140009 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108705 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108753 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110370 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140451 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139061 cycles, achieve throughput   565 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140560 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108703 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108748 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110594 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209161 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207433 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207389 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC2 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    485 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1367 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1585 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1364 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1479 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC2 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140677 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 139083 cycles, achieve throughput   565 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139344 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108597 cycles, achieve throughput   724 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108744 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110373 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 139676 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139956 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139898 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108705 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108749 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110261 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 139897 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139742 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 139671 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108703 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108738 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110594 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209271 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207519 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207498 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC2 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1585 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1583 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1477 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC2 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139679 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140302 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139789 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108597 cycles, achieve throughput   724 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108746 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110151 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140231 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140336 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140118 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108706 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108755 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110370 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140450 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140102 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 139118 cycles, achieve throughput   565 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108591 cycles, achieve throughput   724 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108737 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110595 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209383 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207523 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207388 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC2 TC2
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1368 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1585 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1478 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC2 TC2
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140234 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140289 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139900 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108710 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108632 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110262 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140229 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140207 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140120 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108707 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108745 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110148 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140116 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140192 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 139782 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108704 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108747 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110594 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209273 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207560 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207389 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC2 TC3
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1367 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1583 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1364 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1479 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC2 TC3
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139456 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140072 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 138569 cycles, achieve throughput   567 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108599 cycles, achieve throughput   724 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108644 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110264 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140120 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140054 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140341 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108706 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108734 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110372 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 139674 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139635 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 139895 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108704 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108757 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110706 cycles, achieve throughput   710 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209382 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207407 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207387 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC3 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    483 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1585 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1585 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1363 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1479 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC3 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 115923 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 115942 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 115924 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 148447 cycles, achieve throughput   529 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 154044 cycles, achieve throughput   510 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 163653 cycles, achieve throughput   480 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 115921 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 115854 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 115920 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 148445 cycles, achieve throughput   529 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 154158 cycles, achieve throughput   510 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 163541 cycles, achieve throughput   480 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 115922 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 115998 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 116028 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 148442 cycles, achieve throughput   529 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 154159 cycles, achieve throughput   510 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 166982 cycles, achieve throughput   470 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 247457 cycles, achieve throughput   317 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 247496 cycles, achieve throughput   317 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 249457 cycles, achieve throughput   315 MB/s
Overhead test with EDMA CC3 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1367 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1583 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1478 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC3 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 115925 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 115954 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 116034 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 148447 cycles, achieve throughput   529 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 154288 cycles, achieve throughput   509 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 163099 cycles, achieve throughput   482 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 116033 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 115946 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 115922 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 148444 cycles, achieve throughput   529 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 154149 cycles, achieve throughput   510 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 163206 cycles, achieve throughput   481 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 116030 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 116022 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 116140 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 148440 cycles, achieve throughput   529 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 154176 cycles, achieve throughput   510 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 168316 cycles, achieve throughput   467 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 247345 cycles, achieve throughput   317 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 248056 cycles, achieve throughput   317 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 249457 cycles, achieve throughput   315 MB/s
Overhead test with EDMA CC4 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    595 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    590 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1472 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1583 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1590 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC4 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139568 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 139188 cycles, achieve throughput   565 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140454 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108708 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108749 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110484 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 139121 cycles, achieve throughput   565 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139646 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 138233 cycles, achieve throughput   568 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108706 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108736 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110260 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 138674 cycles, achieve throughput   567 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140534 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140450 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108702 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108734 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110594 cycles, achieve throughput   711 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209384 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207720 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207499 cycles, achieve throughput   379 MB/s
Overhead test with EDMA CC4 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    590 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1589 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    584 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1473 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1584 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1588 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC4 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139568 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 139978 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 138901 cycles, achieve throughput   566 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108710 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108758 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110373 cycles, achieve throughput   712 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 139454 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139738 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140119 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108702 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108748 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110261 cycles, achieve throughput   713 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140230 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 138968 cycles, achieve throughput   565 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140448 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108703 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108746 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 110706 cycles, achieve throughput   710 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207717 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207520 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207389 cycles, achieve throughput   379 MB/s
EDMA test complete
PCIE test complete.
