JTAG ID= 0x0b9a702f. This is a K2L device, version variant = 0
DEVSTAT= 0x0e000ee1. little endian, no boot or I2C slave boot, boot master is ARM core, PLL configuration implies the input clock for core is 122.88MHz
SmartReflex VID= 46, required core voltage= 0.995V.
Die ID= 0x0400500a, 0x0c00ea81, 0x00000000, 0x5f260020
DSP speed grade = 1200MHz, ARM speed grade= 1200MHz
Enable IRQ and FIQ.
Enable Exception handling...
Initialize main core clock = 100.00MHz/1x12 = 1200MHz
Initialize ARM clock = 100.00MHz/1x12 = 1200MHz
DDR3A initialization
Initialize DDR data rate = 100.000/1*16/4*4= 1600.0 MTS, bus width = 64 bits.
DDR PHY status PGSR0=0xb0000fff.
   85 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c0a0000(MSRAM(strongly ordered)), consumes 1837757 cycles
  129 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 1211820 cycles
  132 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 1187333 cycles
   79 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes 1974042 cycles
  132 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes 1187517 cycles
  132 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 1189154 cycles
   56 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes 2803775 cycles
  132 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes 1187331 cycles
  132 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes 1187329 cycles
  125 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c080000(MSRAM(strongly ordered)), consumes 1251501 cycles
  154 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c0e0000(MSRAM(normal non-cache)), consumes 1015050 cycles
  154 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 1015039 cycles
  131 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes 1199416 cycles
  154 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes 1015026 cycles
  154 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 1016595 cycles
  131 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes 1199398 cycles
  154 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes 1015026 cycles
  154 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes 1015017 cycles
  666 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c080000(MSRAM(strongly ordered)), consumes 235815 cycles
 3300 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 47651 cycles
 4461 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c120000(MSRAM(RA_WB_WA,  in sh)), consumes 35254 cycles
  674 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes 233124 cycles
 2874 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes 54711 cycles
 4239 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 37104 cycles
  534 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes 294495 cycles
 1760 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes 89339 cycles
 4464 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes 35231 cycles
   49 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c080000(MSRAM(strongly ordered)), consumes 3196725 cycles
   63 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 2481921 cycles
   61 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 2578188 cycles
   35 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes 4384199 cycles
   47 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x80022000(DDR3A(strongly ordered)), consumes 3336596 cycles
   48 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes 3275479 cycles
   59 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 2635925 cycles
   37 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes 4150528 cycles
   63 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes 2482050 cycles
   61 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes 2570036 cycles
   61 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c080000(MSRAM(strongly ordered)), consumes 2557606 cycles
   65 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 2395353 cycles
   65 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 2395905 cycles
   34 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes 4507447 cycles
   52 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes 3007274 cycles
   65 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x88022000(DDR3A(normal non-cache)), consumes 2394822 cycles
   64 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 2448251 cycles
   61 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes 2559362 cycles
   65 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes 2395019 cycles
   65 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes 2394683 cycles
  677 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c080000(MSRAM(strongly ordered)), consumes 232129 cycles
 2980 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 52767 cycles
 3494 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 45010 cycles
  545 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes 288558 cycles
 1402 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes 112177 cycles
 2238 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes 70259 cycles
 2793 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90022000(DDR3A(RA_WB_WA,  in sh)), consumes 56298 cycles
  531 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes 295951 cycles
 1689 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes 93114 cycles
 3467 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes 45364 cycles
   57 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x0c080000(MSRAM(strongly ordered)), consumes 2756912 cycles
   74 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 2115309 cycles
   65 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 2399052 cycles
   54 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes 2903444 cycles
   74 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes 2115733 cycles
   65 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 2399422 cycles
   42 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes 3734676 cycles
   43 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x70022000(OSR (strongly ordered) ), consumes 3641048 cycles
   70 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes 2217932 cycles
   65 MB/s, copy 131072 bytes from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes 2399056 cycles
   73 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x0c080000(MSRAM(strongly ordered)), consumes 2142622 cycles
   78 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 1997278 cycles
   78 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 1997278 cycles
   73 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes 2142571 cycles
   78 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes 1997293 cycles
   78 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 1997284 cycles
   64 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes 2455661 cycles
   78 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes 1997278 cycles
   78 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x70062000(OSR (normal non-cache) ), consumes 1997318 cycles
   78 MB/s, copy 131072 bytes from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes 1997345 cycles
  682 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x0c080000(MSRAM(strongly ordered)), consumes 230621 cycles
 3220 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 48833 cycles
 4043 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 38902 cycles
  673 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes 233455 cycles
 2788 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes 56414 cycles
 3905 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 40271 cycles
  511 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes 307333 cycles
 1732 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes 90806 cycles
 4004 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes 39280 cycles
 3988 MB/s, copy 131072 bytes from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a2000(OSR (RA_WB_WA,  in sh) ), consumes 39437 cycles
Memory load performance test at 0x0c080000(MSRAM(strongly ordered))
Index=   0  Cycles/LDRD= 14.33
Index=   1  Cycles/LDRD= 13.34
Index=   2  Cycles/LDRD= 13.31
Index=   3  Cycles/LDRD= 13.21
Index=   4  Cycles/LDRD= 13.33
Index=   5  Cycles/LDRD= 13.22
Index=   6  Cycles/LDRD= 13.33
Index=   7  Cycles/LDRD= 13.33
Index=   8  Cycles/LDRD= 14.33
Index=  10  Cycles/LDRD= 13.31
Index=  12  Cycles/LDRD= 13.33
Index=  14  Cycles/LDRD= 13.33
Index=  16  Cycles/LDRD= 14.13
Index=  18  Cycles/LDRD= 13.29
Index=  20  Cycles/LDRD= 13.35
Index=  22  Cycles/LDRD= 13.30
Index=  24  Cycles/LDRD= 14.33
Index=  26  Cycles/LDRD= 13.34
Index=  28  Cycles/LDRD= 13.32
Index=  30  Cycles/LDRD= 13.33
Index=  32  Cycles/LDRD= 14.32
Index=  40  Cycles/LDRD= 14.27
Index=  48  Cycles/LDRD= 14.32
Index=  56  Cycles/LDRD= 14.32
Memory store performance test at 0x0c080000(MSRAM(strongly ordered))
Index=   0  Cycles/STRD= 8.26
Index=   1  Cycles/STRD= 8.01
Index=   2  Cycles/STRD= 7.77
Index=   3  Cycles/STRD= 7.51
Index=   4  Cycles/STRD= 7.26
Index=   5  Cycles/STRD= 7.01
Index=   6  Cycles/STRD= 6.77
Index=   7  Cycles/STRD= 6.52
Index=   8  Cycles/STRD= 6.27
Index=  10  Cycles/STRD= 6.27
Index=  12  Cycles/STRD= 6.27
Index=  14  Cycles/STRD= 6.27
Index=  16  Cycles/STRD= 6.27
Index=  18  Cycles/STRD= 6.27
Index=  20  Cycles/STRD= 6.27
Index=  22  Cycles/STRD= 6.27
Index=  24  Cycles/STRD= 6.27
Index=  26  Cycles/STRD= 6.27
Index=  28  Cycles/STRD= 6.27
Index=  30  Cycles/STRD= 6.27
Index=  32  Cycles/STRD= 6.26
Index=  40  Cycles/STRD= 6.27
Index=  48  Cycles/STRD= 6.27
Index=  56  Cycles/STRD= 6.27
Memory load performance test at 0x0c0c0000(MSRAM(normal non-cache))
Index=   0  Cycles/LDRD= 62.23
Index=   1  Cycles/LDRD= 62.24
Index=   2  Cycles/LDRD= 62.26
Index=   3  Cycles/LDRD= 62.26
Index=   4  Cycles/LDRD= 62.26
Index=   5  Cycles/LDRD= 62.25
Index=   6  Cycles/LDRD= 62.25
Index=   7  Cycles/LDRD= 62.25
Index=   8  Cycles/LDRD= 62.25
Index=  10  Cycles/LDRD= 62.26
Index=  12  Cycles/LDRD= 62.26
Index=  14  Cycles/LDRD= 62.25
Index=  16  Cycles/LDRD= 62.25
Index=  18  Cycles/LDRD= 62.26
Index=  20  Cycles/LDRD= 62.26
Index=  22  Cycles/LDRD= 62.25
Index=  24  Cycles/LDRD= 62.25
Index=  26  Cycles/LDRD= 62.26
Index=  28  Cycles/LDRD= 62.26
Index=  30  Cycles/LDRD= 62.25
Index=  32  Cycles/LDRD= 62.25
Index=  40  Cycles/LDRD= 62.25
Index=  48  Cycles/LDRD= 62.25
Index=  56  Cycles/LDRD= 62.25
Memory store performance test at 0x0c0c0000(MSRAM(normal non-cache))
Index=   0  Cycles/STRD= 1.92
Index=   1  Cycles/STRD= 2.74
Index=   2  Cycles/STRD= 5.48
Index=   3  Cycles/STRD= 5.00
Index=   4  Cycles/STRD= 4.64
Index=   5  Cycles/STRD= 4.63
Index=   6  Cycles/STRD= 4.44
Index=   7  Cycles/STRD= 4.43
Index=   8  Cycles/STRD= 4.36
Index=  10  Cycles/STRD= 4.40
Index=  12  Cycles/STRD= 4.40
Index=  14  Cycles/STRD= 4.40
Index=  16  Cycles/STRD= 4.39
Index=  18  Cycles/STRD= 4.40
Index=  20  Cycles/STRD= 4.40
Index=  22  Cycles/STRD= 4.40
Index=  24  Cycles/STRD= 4.36
Index=  26  Cycles/STRD= 4.40
Index=  28  Cycles/STRD= 4.40
Index=  30  Cycles/STRD= 4.40
Index=  32  Cycles/STRD= 4.29
Index=  40  Cycles/STRD= 4.36
Index=  48  Cycles/STRD= 4.39
Index=  56  Cycles/STRD= 4.35
Memory load performance test at 0x0c100000(MSRAM(RA_WB_WA,  in sh))
Index=   0  Cycles/LDRD= 1.26
Index=   1  Cycles/LDRD= 2.38
Index=   2  Cycles/LDRD= 3.08
Index=   3  Cycles/LDRD= 4.37
Index=   4  Cycles/LDRD= 5.74
Index=   5  Cycles/LDRD= 7.26
Index=   6  Cycles/LDRD= 8.21
Index=   7  Cycles/LDRD= 10.16
Index=   8  Cycles/LDRD= 10.75
Index=  10  Cycles/LDRD= 11.41
Index=  12  Cycles/LDRD= 10.83
Index=  14  Cycles/LDRD= 11.39
Index=  16  Cycles/LDRD= 15.16
Index=  18  Cycles/LDRD= 12.04
Index=  20  Cycles/LDRD= 11.56
Index=  22  Cycles/LDRD= 12.42
Index=  24  Cycles/LDRD= 12.08
Index=  26  Cycles/LDRD= 12.24
Index=  28  Cycles/LDRD= 12.17
Index=  30  Cycles/LDRD= 14.07
Index=  32  Cycles/LDRD= 24.99
Index=  40  Cycles/LDRD= 12.35
Index=  48  Cycles/LDRD= 12.97
Index=  56  Cycles/LDRD= 11.53
Memory store performance test at 0x0c100000(MSRAM(RA_WB_WA,  in sh))
Index=   0  Cycles/STRD= 1.24
Index=   1  Cycles/STRD= 1.73
Index=   2  Cycles/STRD= 3.06
Index=   3  Cycles/STRD= 4.20
Index=   4  Cycles/STRD= 5.67
Index=   5  Cycles/STRD= 7.20
Index=   6  Cycles/STRD= 8.08
Index=   7  Cycles/STRD= 9.50
Index=   8  Cycles/STRD= 10.89
Index=  10  Cycles/STRD= 10.35
Index=  12  Cycles/STRD= 11.11
Index=  14  Cycles/STRD= 11.16
Index=  16  Cycles/STRD= 15.43
Index=  18  Cycles/STRD= 11.19
Index=  20  Cycles/STRD= 11.37
Index=  22  Cycles/STRD= 11.95
Index=  24  Cycles/STRD= 11.57
Index=  26  Cycles/STRD= 11.67
Index=  28  Cycles/STRD= 11.58
Index=  30  Cycles/STRD= 11.73
Index=  32  Cycles/STRD= 23.81
Index=  40  Cycles/STRD= 12.42
Index=  48  Cycles/STRD= 13.21
Index=  56  Cycles/STRD= 11.88
Memory load performance test at 0x80000000(DDR3A(strongly ordered))
Index=   0  Cycles/LDRD= 23.97
Index=   1  Cycles/LDRD= 23.95
Index=   2  Cycles/LDRD= 23.95
Index=   3  Cycles/LDRD= 23.97
Index=   4  Cycles/LDRD= 23.90
Index=   5  Cycles/LDRD= 24.26
Index=   6  Cycles/LDRD= 23.95
Index=   7  Cycles/LDRD= 24.01
Index=   8  Cycles/LDRD= 23.98
Index=  10  Cycles/LDRD= 23.99
Index=  12  Cycles/LDRD= 24.04
Index=  14  Cycles/LDRD= 24.11
Index=  16  Cycles/LDRD= 24.08
Index=  18  Cycles/LDRD= 24.13
Index=  20  Cycles/LDRD= 24.13
Index=  22  Cycles/LDRD= 24.15
Index=  24  Cycles/LDRD= 24.35
Index=  26  Cycles/LDRD= 24.17
Index=  28  Cycles/LDRD= 24.48
Index=  30  Cycles/LDRD= 24.18
Index=  32  Cycles/LDRD= 24.47
Index=  40  Cycles/LDRD= 24.59
Index=  48  Cycles/LDRD= 24.60
Index=  56  Cycles/LDRD= 25.36
Index=  64  Cycles/LDRD= 24.69
Index=  96  Cycles/LDRD= 24.75
Index= 128  Cycles/LDRD= 25.62
Index= 192  Cycles/LDRD= 25.99
Index= 256  Cycles/LDRD= 26.86
Index= 384  Cycles/LDRD= 26.94
Index= 512  Cycles/LDRD= 29.99
Index= 768  Cycles/LDRD= 30.05
Index=1024  Cycles/LDRD= 30.37
Index=1536  Cycles/LDRD= 30.71
Index=2048  Cycles/LDRD= 30.41
Index=3072  Cycles/LDRD= 30.30
Index=4096  Cycles/LDRD= 30.95
Index=6144  Cycles/LDRD= 30.33
Index=8192  Cycles/LDRD= 60.41
Index=12288  Cycles/LDRD= 30.95
Index=16384  Cycles/LDRD= 60.41
Index=20480  Cycles/LDRD= 30.45
Index=24576  Cycles/LDRD= 60.41
Index=28672  Cycles/LDRD= 30.90
Memory store performance test at 0x80000000(DDR3A(strongly ordered))
Index=   0  Cycles/STRD= 12.15
Index=   1  Cycles/STRD= 12.16
Index=   2  Cycles/STRD= 12.16
Index=   3  Cycles/STRD= 12.15
Index=   4  Cycles/STRD= 12.16
Index=   5  Cycles/STRD= 12.16
Index=   6  Cycles/STRD= 12.16
Index=   7  Cycles/STRD= 12.16
Index=   8  Cycles/STRD= 12.16
Index=  10  Cycles/STRD= 12.66
Index=  12  Cycles/STRD= 12.16
Index=  14  Cycles/STRD= 12.16
Index=  16  Cycles/STRD= 12.16
Index=  18  Cycles/STRD= 12.15
Index=  20  Cycles/STRD= 12.16
Index=  22  Cycles/STRD= 12.29
Index=  24  Cycles/STRD= 12.15
Index=  26  Cycles/STRD= 12.16
Index=  28  Cycles/STRD= 12.16
Index=  30  Cycles/STRD= 12.16
Index=  32  Cycles/STRD= 12.15
Index=  40  Cycles/STRD= 12.16
Index=  48  Cycles/STRD= 12.16
Index=  56  Cycles/STRD= 12.29
Index=  64  Cycles/STRD= 12.16
Index=  96  Cycles/STRD= 12.16
Index= 128  Cycles/STRD= 12.16
Index= 192  Cycles/STRD= 12.16
Index= 256  Cycles/STRD= 12.47
Index= 384  Cycles/STRD= 12.16
Index= 512  Cycles/STRD= 12.16
Index= 768  Cycles/STRD= 12.16
Index=1024  Cycles/STRD= 13.63
Index=1536  Cycles/STRD= 15.57
Index=2048  Cycles/STRD= 19.48
Index=3072  Cycles/STRD= 13.62
Index=4096  Cycles/STRD= 38.89
Index=6144  Cycles/STRD= 19.49
Index=8192  Cycles/STRD= 79.46
Index=12288  Cycles/STRD= 38.63
Index=16384  Cycles/STRD= 79.46
Index=20480  Cycles/STRD= 38.63
Index=24576  Cycles/STRD= 79.58
Index=28672  Cycles/STRD= 38.73
Memory load performance test at 0x88000000(DDR3A(normal non-cache))
Index=   0  Cycles/LDRD= 140.77
Index=   1  Cycles/LDRD= 143.05
Index=   2  Cycles/LDRD= 143.66
Index=   3  Cycles/LDRD= 144.04
Index=   4  Cycles/LDRD= 143.65
Index=   5  Cycles/LDRD= 143.29
Index=   6  Cycles/LDRD= 143.26
Index=   7  Cycles/LDRD= 143.46
Index=   8  Cycles/LDRD= 141.58
Index=  10  Cycles/LDRD= 143.19
Index=  12  Cycles/LDRD= 144.49
Index=  14  Cycles/LDRD= 143.34
Index=  16  Cycles/LDRD= 141.02
Index=  18  Cycles/LDRD= 144.12
Index=  20  Cycles/LDRD= 144.14
Index=  22  Cycles/LDRD= 143.43
Index=  24  Cycles/LDRD= 141.41
Index=  26  Cycles/LDRD= 144.17
Index=  28  Cycles/LDRD= 143.49
Index=  30  Cycles/LDRD= 144.27
Index=  32  Cycles/LDRD= 142.11
Index=  40  Cycles/LDRD= 141.50
Index=  48  Cycles/LDRD= 142.33
Index=  56  Cycles/LDRD= 142.31
Index=  64  Cycles/LDRD= 141.88
Index=  96  Cycles/LDRD= 143.63
Index= 128  Cycles/LDRD= 144.52
Index= 192  Cycles/LDRD= 146.45
Index= 256  Cycles/LDRD= 148.97
Index= 384  Cycles/LDRD= 153.43
Index= 512  Cycles/LDRD= 157.27
Index= 768  Cycles/LDRD= 167.32
Index=1024  Cycles/LDRD= 176.48
Index=1536  Cycles/LDRD= 175.77
Index=2048  Cycles/LDRD= 178.30
Index=3072  Cycles/LDRD= 176.64
Index=4096  Cycles/LDRD= 178.73
Index=6144  Cycles/LDRD= 178.35
Index=8192  Cycles/LDRD= 178.71
Index=12288  Cycles/LDRD= 178.56
Index=16384  Cycles/LDRD= 178.24
Index=20480  Cycles/LDRD= 178.56
Index=24576  Cycles/LDRD= 178.86
Index=28672  Cycles/LDRD= 178.66
Memory store performance test at 0x88000000(DDR3A(normal non-cache))
Index=   0  Cycles/STRD= 2.10
Index=   1  Cycles/STRD= 3.26
Index=   2  Cycles/STRD= 6.28
Index=   3  Cycles/STRD= 6.21
Index=   4  Cycles/STRD= 6.55
Index=   5  Cycles/STRD= 6.18
Index=   6  Cycles/STRD= 6.18
Index=   7  Cycles/STRD= 6.17
Index=   8  Cycles/STRD= 6.18
Index=  10  Cycles/STRD= 6.18
Index=  12  Cycles/STRD= 6.31
Index=  14  Cycles/STRD= 6.18
Index=  16  Cycles/STRD= 6.18
Index=  18  Cycles/STRD= 6.18
Index=  20  Cycles/STRD= 6.18
Index=  22  Cycles/STRD= 6.18
Index=  24  Cycles/STRD= 6.18
Index=  26  Cycles/STRD= 6.18
Index=  28  Cycles/STRD= 6.18
Index=  30  Cycles/STRD= 6.18
Index=  32  Cycles/STRD= 6.17
Index=  40  Cycles/STRD= 6.17
Index=  48  Cycles/STRD= 6.74
Index=  56  Cycles/STRD= 6.18
Index=  64  Cycles/STRD= 6.18
Index=  96  Cycles/STRD= 6.32
Index= 128  Cycles/STRD= 6.35
Index= 192  Cycles/STRD= 6.47
Index= 256  Cycles/STRD= 6.57
Index= 384  Cycles/STRD= 6.51
Index= 512  Cycles/STRD= 8.26
Index= 768  Cycles/STRD= 10.37
Index=1024  Cycles/STRD= 13.29
Index=1536  Cycles/STRD= 15.99
Index=2048  Cycles/STRD= 20.38
Index=3072  Cycles/STRD= 13.16
Index=4096  Cycles/STRD= 36.08
Index=6144  Cycles/STRD= 20.24
Index=8192  Cycles/STRD= 69.85
Index=12288  Cycles/STRD= 36.00
Index=16384  Cycles/STRD= 72.38
Index=20480  Cycles/STRD= 36.08
Index=24576  Cycles/STRD= 72.31
Index=28672  Cycles/STRD= 36.03
Memory load performance test at 0x90000000(DDR3A(RA_WB_WA,  in sh))
Index=   0  Cycles/LDRD= 1.42
Index=   1  Cycles/LDRD= 3.11
Index=   2  Cycles/LDRD= 4.71
Index=   3  Cycles/LDRD= 6.41
Index=   4  Cycles/LDRD= 8.95
Index=   5  Cycles/LDRD= 11.79
Index=   6  Cycles/LDRD= 12.21
Index=   7  Cycles/LDRD= 14.30
Index=   8  Cycles/LDRD= 15.98
Index=  10  Cycles/LDRD= 16.97
Index=  12  Cycles/LDRD= 17.02
Index=  14  Cycles/LDRD= 17.30
Index=  16  Cycles/LDRD= 18.89
Index=  18  Cycles/LDRD= 17.52
Index=  20  Cycles/LDRD= 17.93
Index=  22  Cycles/LDRD= 18.80
Index=  24  Cycles/LDRD= 18.28
Index=  26  Cycles/LDRD= 19.60
Index=  28  Cycles/LDRD= 19.41
Index=  30  Cycles/LDRD= 20.66
Index=  32  Cycles/LDRD= 28.66
Index=  40  Cycles/LDRD= 19.57
Index=  48  Cycles/LDRD= 23.39
Index=  56  Cycles/LDRD= 24.66
Index=  64  Cycles/LDRD= 25.88
Index=  96  Cycles/LDRD= 25.76
Index= 128  Cycles/LDRD= 26.71
Index= 192  Cycles/LDRD= 26.84
Index= 256  Cycles/LDRD= 28.09
Index= 384  Cycles/LDRD= 28.35
Index= 512  Cycles/LDRD= 38.04
Index= 768  Cycles/LDRD= 30.63
Index=1024  Cycles/LDRD= 58.34
Index=1536  Cycles/LDRD= 38.39
Index=2048  Cycles/LDRD= 105.04
Index=3072  Cycles/LDRD= 58.27
Index=4096  Cycles/LDRD= 105.94
Index=6144  Cycles/LDRD= 105.12
Index=8192  Cycles/LDRD= 104.64
Index=12288  Cycles/LDRD= 100.62
Index=16384  Cycles/LDRD= 104.65
Index=20480  Cycles/LDRD= 104.93
Index=24576  Cycles/LDRD= 104.27
Index=28672  Cycles/LDRD= 116.93
Memory store performance test at 0x90000000(DDR3A(RA_WB_WA,  in sh))
Index=   0  Cycles/STRD= 1.38
Index=   1  Cycles/STRD= 1.86
Index=   2  Cycles/STRD= 4.31
Index=   3  Cycles/STRD= 6.38
Index=   4  Cycles/STRD= 8.45
Index=   5  Cycles/STRD= 11.94
Index=   6  Cycles/STRD= 12.84
Index=   7  Cycles/STRD= 17.26
Index=   8  Cycles/STRD= 17.60
Index=  10  Cycles/STRD= 16.99
Index=  12  Cycles/STRD= 18.05
Index=  14  Cycles/STRD= 17.67
Index=  16  Cycles/STRD= 21.27
Index=  18  Cycles/STRD= 18.81
Index=  20  Cycles/STRD= 19.55
Index=  22  Cycles/STRD= 19.13
Index=  24  Cycles/STRD= 19.04
Index=  26  Cycles/STRD= 20.01
Index=  28  Cycles/STRD= 20.04
Index=  30  Cycles/STRD= 20.55
Index=  32  Cycles/STRD= 28.47
Index=  40  Cycles/STRD= 23.86
Index=  48  Cycles/STRD= 26.62
Index=  56  Cycles/STRD= 26.97
Index=  64  Cycles/STRD= 27.23
Index=  96  Cycles/STRD= 27.36
Index= 128  Cycles/STRD= 28.33
Index= 192  Cycles/STRD= 29.42
Index= 256  Cycles/STRD= 33.61
Index= 384  Cycles/STRD= 32.35
Index= 512  Cycles/STRD= 52.61
Index= 768  Cycles/STRD= 34.35
Index=1024  Cycles/STRD= 87.34
Index=1536  Cycles/STRD= 55.85
Index=2048  Cycles/STRD= 121.29
Index=3072  Cycles/STRD= 88.38
Index=4096  Cycles/STRD= 136.99
Index=6144  Cycles/STRD= 119.90
Index=8192  Cycles/STRD= 160.55
Index=12288  Cycles/STRD= 135.00
Index=16384  Cycles/STRD= 158.23
Index=20480  Cycles/STRD= 134.12
Index=24576  Cycles/STRD= 158.48
Index=28672  Cycles/STRD= 135.69
Memory load performance test at 0x70000000(OSR (strongly ordered) )
Index=   0  Cycles/LDRD= 21.69
Index=   1  Cycles/LDRD= 21.66
Index=   2  Cycles/LDRD= 21.66
Index=   3  Cycles/LDRD= 21.66
Index=   4  Cycles/LDRD= 21.66
Index=   5  Cycles/LDRD= 21.66
Index=   6  Cycles/LDRD= 21.66
Index=   7  Cycles/LDRD= 21.66
Index=   8  Cycles/LDRD= 21.66
Index=  10  Cycles/LDRD= 21.66
Index=  12  Cycles/LDRD= 21.66
Index=  14  Cycles/LDRD= 21.66
Index=  16  Cycles/LDRD= 21.66
Index=  18  Cycles/LDRD= 21.66
Index=  20  Cycles/LDRD= 21.66
Index=  22  Cycles/LDRD= 21.66
Index=  24  Cycles/LDRD= 21.66
Index=  26  Cycles/LDRD= 21.68
Index=  28  Cycles/LDRD= 21.65
Index=  30  Cycles/LDRD= 21.66
Index=  32  Cycles/LDRD= 21.66
Index=  40  Cycles/LDRD= 21.66
Index=  48  Cycles/LDRD= 21.66
Index=  56  Cycles/LDRD= 21.66
Memory store performance test at 0x70000000(OSR (strongly ordered) )
Index=   0  Cycles/STRD= 18.36
Index=   1  Cycles/STRD= 18.36
Index=   2  Cycles/STRD= 18.36
Index=   3  Cycles/STRD= 18.36
Index=   4  Cycles/STRD= 18.36
Index=   5  Cycles/STRD= 18.36
Index=   6  Cycles/STRD= 18.36
Index=   7  Cycles/STRD= 18.36
Index=   8  Cycles/STRD= 18.36
Index=  10  Cycles/STRD= 18.36
Index=  12  Cycles/STRD= 18.36
Index=  14  Cycles/STRD= 18.36
Index=  16  Cycles/STRD= 18.36
Index=  18  Cycles/STRD= 18.36
Index=  20  Cycles/STRD= 18.36
Index=  22  Cycles/STRD= 18.36
Index=  24  Cycles/STRD= 18.36
Index=  26  Cycles/STRD= 18.36
Index=  28  Cycles/STRD= 18.36
Index=  30  Cycles/STRD= 18.36
Index=  32  Cycles/STRD= 18.36
Index=  40  Cycles/STRD= 18.35
Index=  48  Cycles/STRD= 18.36
Index=  56  Cycles/STRD= 18.35
Memory load performance test at 0x70040000(OSR (normal non-cache) )
Index=   0  Cycles/LDRD= 122.23
Index=   1  Cycles/LDRD= 122.25
Index=   2  Cycles/LDRD= 122.25
Index=   3  Cycles/LDRD= 122.25
Index=   4  Cycles/LDRD= 122.25
Index=   5  Cycles/LDRD= 122.25
Index=   6  Cycles/LDRD= 122.25
Index=   7  Cycles/LDRD= 122.25
Index=   8  Cycles/LDRD= 122.25
Index=  10  Cycles/LDRD= 122.25
Index=  12  Cycles/LDRD= 122.25
Index=  14  Cycles/LDRD= 122.25
Index=  16  Cycles/LDRD= 122.25
Index=  18  Cycles/LDRD= 122.25
Index=  20  Cycles/LDRD= 122.25
Index=  22  Cycles/LDRD= 122.25
Index=  24  Cycles/LDRD= 122.25
Index=  26  Cycles/LDRD= 122.25
Index=  28  Cycles/LDRD= 122.25
Index=  30  Cycles/LDRD= 122.25
Index=  32  Cycles/LDRD= 122.25
Index=  40  Cycles/LDRD= 122.25
Index=  48  Cycles/LDRD= 122.25
Index=  56  Cycles/LDRD= 122.25
Memory store performance test at 0x70040000(OSR (normal non-cache) )
Index=   0  Cycles/STRD= 2.83
Index=   1  Cycles/STRD= 5.81
Index=   2  Cycles/STRD= 11.05
Index=   3  Cycles/STRD= 10.47
Index=   4  Cycles/STRD= 9.88
Index=   5  Cycles/STRD= 9.89
Index=   6  Cycles/STRD= 9.88
Index=   7  Cycles/STRD= 9.71
Index=   8  Cycles/STRD= 9.54
Index=  10  Cycles/STRD= 9.55
Index=  12  Cycles/STRD= 9.55
Index=  14  Cycles/STRD= 9.55
Index=  16  Cycles/STRD= 9.56
Index=  18  Cycles/STRD= 9.55
Index=  20  Cycles/STRD= 9.55
Index=  22  Cycles/STRD= 9.54
Index=  24  Cycles/STRD= 9.53
Index=  26  Cycles/STRD= 9.55
Index=  28  Cycles/STRD= 9.54
Index=  30  Cycles/STRD= 9.55
Index=  32  Cycles/STRD= 9.47
Index=  40  Cycles/STRD= 9.55
Index=  48  Cycles/STRD= 9.58
Index=  56  Cycles/STRD= 9.54
Memory load performance test at 0x70080000(OSR (RA_WB_WA,  in sh) )
Index=   0  Cycles/LDRD= 1.36
Index=   1  Cycles/LDRD= 2.82
Index=   2  Cycles/LDRD= 4.41
Index=   3  Cycles/LDRD= 5.92
Index=   4  Cycles/LDRD= 7.97
Index=   5  Cycles/LDRD= 10.71
Index=   6  Cycles/LDRD= 11.27
Index=   7  Cycles/LDRD= 13.18
Index=   8  Cycles/LDRD= 14.62
Index=  10  Cycles/LDRD= 15.42
Index=  12  Cycles/LDRD= 14.96
Index=  14  Cycles/LDRD= 15.62
Index=  16  Cycles/LDRD= 17.95
Index=  18  Cycles/LDRD= 16.30
Index=  20  Cycles/LDRD= 16.06
Index=  22  Cycles/LDRD= 16.76
Index=  24  Cycles/LDRD= 16.45
Index=  26  Cycles/LDRD= 17.42
Index=  28  Cycles/LDRD= 17.55
Index=  30  Cycles/LDRD= 18.61
Index=  32  Cycles/LDRD= 27.12
Index=  40  Cycles/LDRD= 17.50
Index=  48  Cycles/LDRD= 20.57
Index=  56  Cycles/LDRD= 21.39
Memory store performance test at 0x70080000(OSR (RA_WB_WA,  in sh) )
Index=   0  Cycles/STRD= 1.28
Index=   1  Cycles/STRD= 2.04
Index=   2  Cycles/STRD= 4.02
Index=   3  Cycles/STRD= 5.72
Index=   4  Cycles/STRD= 7.93
Index=   5  Cycles/STRD= 9.75
Index=   6  Cycles/STRD= 11.25
Index=   7  Cycles/STRD= 14.38
Index=   8  Cycles/STRD= 14.71
Index=  10  Cycles/STRD= 16.11
Index=  12  Cycles/STRD= 15.17
Index=  14  Cycles/STRD= 15.70
Index=  16  Cycles/STRD= 18.02
Index=  18  Cycles/STRD= 16.02
Index=  20  Cycles/STRD= 16.46
Index=  22  Cycles/STRD= 16.46
Index=  24  Cycles/STRD= 16.50
Index=  26  Cycles/STRD= 16.83
Index=  28  Cycles/STRD= 17.46
Index=  30  Cycles/STRD= 17.54
Index=  32  Cycles/STRD= 26.56
Index=  40  Cycles/STRD= 19.95
Index=  48  Cycles/STRD= 21.86
Index=  56  Cycles/STRD= 21.57
Throughput test with EDMA0 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15686 cycles, achieve throughput 10027 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15640 cycles, achieve throughput 10056 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15639 cycles, achieve throughput 10057 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16399 cycles, achieve throughput  9591 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16318 cycles, achieve throughput  9638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16348 cycles, achieve throughput  9621 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  14893 cycles, achieve throughput 10561 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  14894 cycles, achieve throughput 10560 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  14901 cycles, achieve throughput 10555 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15637 cycles, achieve throughput 10058 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15641 cycles, achieve throughput 10056 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15621 cycles, achieve throughput 10068 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16314 cycles, achieve throughput  9641 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16306 cycles, achieve throughput  9645 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16266 cycles, achieve throughput  9669 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  14893 cycles, achieve throughput 10561 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  14891 cycles, achieve throughput 10562 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  14896 cycles, achieve throughput 10558 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15606 cycles, achieve throughput 10078 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15686 cycles, achieve throughput 10027 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15603 cycles, achieve throughput 10080 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16295 cycles, achieve throughput  9652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16320 cycles, achieve throughput  9637 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16314 cycles, achieve throughput  9641 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  14895 cycles, achieve throughput 10559 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  14894 cycles, achieve throughput 10560 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  14889 cycles, achieve throughput 10563 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  20134 cycles, achieve throughput  7811 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20688 cycles, achieve throughput  7602 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20203 cycles, achieve throughput  7785 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  49008 cycles, achieve throughput  3209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  47858 cycles, achieve throughput  3286 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  48502 cycles, achieve throughput  3242 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  20144 cycles, achieve throughput  7808 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  20094 cycles, achieve throughput  7827 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  20087 cycles, achieve throughput  7830 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  20135 cycles, achieve throughput  7811 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20168 cycles, achieve throughput  7798 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20687 cycles, achieve throughput  7603 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  47937 cycles, achieve throughput  3281 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  48097 cycles, achieve throughput  3270 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  48835 cycles, achieve throughput  3220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  20134 cycles, achieve throughput  7811 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  20214 cycles, achieve throughput  7781 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  20082 cycles, achieve throughput  7832 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  22671 cycles, achieve throughput  6937 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  22739 cycles, achieve throughput  6917 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  22343 cycles, achieve throughput  7039 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  50501 cycles, achieve throughput  3114 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  51001 cycles, achieve throughput  3083 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  51331 cycles, achieve throughput  3064 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  22627 cycles, achieve throughput  6951 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  22724 cycles, achieve throughput  6921 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  22637 cycles, achieve throughput  6948 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  12899 cycles, achieve throughput 12193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  12896 cycles, achieve throughput 12196 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  12899 cycles, achieve throughput 12193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  12894 cycles, achieve throughput 12198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  12874 cycles, achieve throughput 12217 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  12899 cycles, achieve throughput 12193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25011 cycles, achieve throughput  6288 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25006 cycles, achieve throughput  6289 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25061 cycles, achieve throughput  6276 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  12898 cycles, achieve throughput 12194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  12895 cycles, achieve throughput 12197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  12898 cycles, achieve throughput 12194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  12892 cycles, achieve throughput 12200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  12888 cycles, achieve throughput 12204 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  12880 cycles, achieve throughput 12211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25010 cycles, achieve throughput  6288 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25006 cycles, achieve throughput  6289 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25017 cycles, achieve throughput  6287 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  12948 cycles, achieve throughput 12147 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  12900 cycles, achieve throughput 12192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  12895 cycles, achieve throughput 12197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  12948 cycles, achieve throughput 12147 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  12885 cycles, achieve throughput 12206 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  12895 cycles, achieve throughput 12197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25011 cycles, achieve throughput  6288 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25061 cycles, achieve throughput  6276 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25010 cycles, achieve throughput  6288 MB/s
Throughput test with EDMA0 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15559 cycles, achieve throughput 10109 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15570 cycles, achieve throughput 10101 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15649 cycles, achieve throughput 10050 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16233 cycles, achieve throughput  9689 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16299 cycles, achieve throughput  9650 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16295 cycles, achieve throughput  9652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  14949 cycles, achieve throughput 10521 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  14948 cycles, achieve throughput 10522 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  14947 cycles, achieve throughput 10522 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15571 cycles, achieve throughput 10101 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15581 cycles, achieve throughput 10094 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15639 cycles, achieve throughput 10057 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16361 cycles, achieve throughput  9613 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16315 cycles, achieve throughput  9640 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16351 cycles, achieve throughput  9619 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  14895 cycles, achieve throughput 10559 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  14890 cycles, achieve throughput 10563 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  14896 cycles, achieve throughput 10558 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15623 cycles, achieve throughput 10067 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15624 cycles, achieve throughput 10066 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15627 cycles, achieve throughput 10065 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16347 cycles, achieve throughput  9621 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16349 cycles, achieve throughput  9620 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16327 cycles, achieve throughput  9633 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  14901 cycles, achieve throughput 10555 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  14900 cycles, achieve throughput 10556 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  14949 cycles, achieve throughput 10521 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  20694 cycles, achieve throughput  7600 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20131 cycles, achieve throughput  7813 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20175 cycles, achieve throughput  7796 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  48250 cycles, achieve throughput  3259 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  47950 cycles, achieve throughput  3280 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  48444 cycles, achieve throughput  3246 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  20100 cycles, achieve throughput  7825 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  20096 cycles, achieve throughput  7826 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  20094 cycles, achieve throughput  7827 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  20160 cycles, achieve throughput  7801 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20131 cycles, achieve throughput  7813 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20134 cycles, achieve throughput  7811 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  47983 cycles, achieve throughput  3277 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  48074 cycles, achieve throughput  3271 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  48339 cycles, achieve throughput  3253 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  20086 cycles, achieve throughput  7830 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  20442 cycles, achieve throughput  7694 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  20096 cycles, achieve throughput  7826 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  22457 cycles, achieve throughput  7003 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  22699 cycles, achieve throughput  6929 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  22607 cycles, achieve throughput  6957 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  51355 cycles, achieve throughput  3062 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  50908 cycles, achieve throughput  3089 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  51346 cycles, achieve throughput  3063 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  22686 cycles, achieve throughput  6933 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  22416 cycles, achieve throughput  7016 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  22723 cycles, achieve throughput  6921 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  12899 cycles, achieve throughput 12193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  12952 cycles, achieve throughput 12143 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  12953 cycles, achieve throughput 12142 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  12879 cycles, achieve throughput 12212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  12889 cycles, achieve throughput 12203 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  12899 cycles, achieve throughput 12193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25010 cycles, achieve throughput  6288 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25006 cycles, achieve throughput  6289 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25017 cycles, achieve throughput  6287 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  12899 cycles, achieve throughput 12193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  12895 cycles, achieve throughput 12197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  12899 cycles, achieve throughput 12193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  12893 cycles, achieve throughput 12199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  12888 cycles, achieve throughput 12204 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  12901 cycles, achieve throughput 12191 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25011 cycles, achieve throughput  6288 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25005 cycles, achieve throughput  6290 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25012 cycles, achieve throughput  6288 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  12901 cycles, achieve throughput 12191 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  12894 cycles, achieve throughput 12198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  12900 cycles, achieve throughput 12192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  12901 cycles, achieve throughput 12191 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  12888 cycles, achieve throughput 12204 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  12904 cycles, achieve throughput 12188 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25064 cycles, achieve throughput  6275 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25064 cycles, achieve throughput  6275 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25017 cycles, achieve throughput  6287 MB/s
Throughput test with EDMA1 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25315 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25393 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25389 cycles, achieve throughput  6195 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25509 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  25305 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  25305 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25316 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25393 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25401 cycles, achieve throughput  6192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25508 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  25246 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25308 cycles, achieve throughput  6214 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25390 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25395 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25504 cycles, achieve throughput  6167 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  25257 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28036 cycles, achieve throughput  5610 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28030 cycles, achieve throughput  5611 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27728 cycles, achieve throughput  5672 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59416 cycles, achieve throughput  2647 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59328 cycles, achieve throughput  2651 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59731 cycles, achieve throughput  2633 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  28173 cycles, achieve throughput  5582 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  27819 cycles, achieve throughput  5653 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28106 cycles, achieve throughput  5596 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28141 cycles, achieve throughput  5589 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27704 cycles, achieve throughput  5677 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28035 cycles, achieve throughput  5610 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59220 cycles, achieve throughput  2655 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  59568 cycles, achieve throughput  2640 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60026 cycles, achieve throughput  2620 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  28053 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  27713 cycles, achieve throughput  5675 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28061 cycles, achieve throughput  5605 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30370 cycles, achieve throughput  5179 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30482 cycles, achieve throughput  5159 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30478 cycles, achieve throughput  5160 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61209 cycles, achieve throughput  2569 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61895 cycles, achieve throughput  2541 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  61012 cycles, achieve throughput  2577 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  30604 cycles, achieve throughput  5139 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  30838 cycles, achieve throughput  5100 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  30384 cycles, achieve throughput  5176 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25312 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25225 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25217 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25326 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25425 cycles, achieve throughput  6186 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25326 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25228 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25379 cycles, achieve throughput  6197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25321 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25239 cycles, achieve throughput  6231 MB/s
Throughput test with EDMA1 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25393 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25395 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25495 cycles, achieve throughput  6169 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25316 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25498 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25369 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25497 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25252 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25376 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25394 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25397 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25405 cycles, achieve throughput  6191 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  25305 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25252 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28049 cycles, achieve throughput  5607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27688 cycles, achieve throughput  5680 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28265 cycles, achieve throughput  5564 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59347 cycles, achieve throughput  2650 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  58843 cycles, achieve throughput  2672 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59420 cycles, achieve throughput  2647 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  28109 cycles, achieve throughput  5595 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  28108 cycles, achieve throughput  5595 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  27992 cycles, achieve throughput  5618 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27789 cycles, achieve throughput  5660 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28147 cycles, achieve throughput  5588 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27717 cycles, achieve throughput  5674 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59171 cycles, achieve throughput  2658 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  59308 cycles, achieve throughput  2652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59608 cycles, achieve throughput  2638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  28045 cycles, achieve throughput  5608 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  28054 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28063 cycles, achieve throughput  5604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30837 cycles, achieve throughput  5100 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30397 cycles, achieve throughput  5174 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30811 cycles, achieve throughput  5104 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61352 cycles, achieve throughput  2563 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61612 cycles, achieve throughput  2552 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  62539 cycles, achieve throughput  2515 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  30808 cycles, achieve throughput  5105 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  30707 cycles, achieve throughput  5122 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  30379 cycles, achieve throughput  5177 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25215 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25274 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25327 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25427 cycles, achieve throughput  6185 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25332 cycles, achieve throughput  6209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25228 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25219 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25216 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25327 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25322 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25278 cycles, achieve throughput  6222 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25328 cycles, achieve throughput  6209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25333 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25285 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25233 cycles, achieve throughput  6233 MB/s
Throughput test with EDMA1 TC2
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25372 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25315 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25372 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25382 cycles, achieve throughput  6196 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25499 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25501 cycles, achieve throughput  6167 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25252 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25315 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25394 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25439 cycles, achieve throughput  6182 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25397 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  25301 cycles, achieve throughput  6216 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25257 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25321 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25390 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25386 cycles, achieve throughput  6195 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25394 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25252 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28147 cycles, achieve throughput  5588 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28072 cycles, achieve throughput  5602 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28055 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59719 cycles, achieve throughput  2633 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59554 cycles, achieve throughput  2641 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58728 cycles, achieve throughput  2678 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  28047 cycles, achieve throughput  5607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  28059 cycles, achieve throughput  5605 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28214 cycles, achieve throughput  5574 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28166 cycles, achieve throughput  5584 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27815 cycles, achieve throughput  5654 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27976 cycles, achieve throughput  5622 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59514 cycles, achieve throughput  2642 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  59507 cycles, achieve throughput  2643 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59371 cycles, achieve throughput  2649 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  28053 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  28153 cycles, achieve throughput  5586 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28101 cycles, achieve throughput  5597 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30393 cycles, achieve throughput  5175 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30467 cycles, achieve throughput  5162 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30478 cycles, achieve throughput  5160 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61300 cycles, achieve throughput  2565 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61262 cycles, achieve throughput  2567 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  60897 cycles, achieve throughput  2582 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  30398 cycles, achieve throughput  5174 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  30596 cycles, achieve throughput  5140 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  30492 cycles, achieve throughput  5158 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25325 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25322 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25438 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25228 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25216 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25324 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25219 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25225 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25285 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25278 cycles, achieve throughput  6222 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25279 cycles, achieve throughput  6222 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25216 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25333 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25323 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25227 cycles, achieve throughput  6234 MB/s
Throughput test with EDMA1 TC3
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25395 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25394 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25499 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25252 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25372 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25403 cycles, achieve throughput  6191 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25397 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25402 cycles, achieve throughput  6191 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25397 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25394 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25511 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28118 cycles, achieve throughput  5593 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28081 cycles, achieve throughput  5601 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28045 cycles, achieve throughput  5608 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59414 cycles, achieve throughput  2647 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59548 cycles, achieve throughput  2641 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59129 cycles, achieve throughput  2660 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  27778 cycles, achieve throughput  5662 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  28065 cycles, achieve throughput  5604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28068 cycles, achieve throughput  5603 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28059 cycles, achieve throughput  5605 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27818 cycles, achieve throughput  5654 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28048 cycles, achieve throughput  5607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59336 cycles, achieve throughput  2650 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58639 cycles, achieve throughput  2682 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59631 cycles, achieve throughput  2637 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  28158 cycles, achieve throughput  5585 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  28045 cycles, achieve throughput  5608 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28066 cycles, achieve throughput  5604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30377 cycles, achieve throughput  5177 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30814 cycles, achieve throughput  5104 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30821 cycles, achieve throughput  5103 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61756 cycles, achieve throughput  2546 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61791 cycles, achieve throughput  2545 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  62173 cycles, achieve throughput  2529 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  30828 cycles, achieve throughput  5102 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  30728 cycles, achieve throughput  5118 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  30391 cycles, achieve throughput  5175 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25275 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25272 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25275 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25327 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25215 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25329 cycles, achieve throughput  6209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25313 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25324 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25286 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25228 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25239 cycles, achieve throughput  6231 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25215 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25222 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25335 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
Throughput test with EDMA2 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25374 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25451 cycles, achieve throughput  6179 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25398 cycles, achieve throughput  6192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25400 cycles, achieve throughput  6192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25315 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25373 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25395 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25390 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25506 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  25302 cycles, achieve throughput  6216 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25301 cycles, achieve throughput  6216 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25391 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25398 cycles, achieve throughput  6192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25496 cycles, achieve throughput  6169 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  25308 cycles, achieve throughput  6214 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28089 cycles, achieve throughput  5599 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27936 cycles, achieve throughput  5630 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27961 cycles, achieve throughput  5625 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59156 cycles, achieve throughput  2658 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59484 cycles, achieve throughput  2644 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59051 cycles, achieve throughput  2663 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  28050 cycles, achieve throughput  5607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  28054 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28332 cycles, achieve throughput  5551 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28044 cycles, achieve throughput  5608 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28150 cycles, achieve throughput  5587 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28039 cycles, achieve throughput  5609 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  58902 cycles, achieve throughput  2670 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  59575 cycles, achieve throughput  2640 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59651 cycles, achieve throughput  2636 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  28061 cycles, achieve throughput  5605 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  28051 cycles, achieve throughput  5607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28062 cycles, achieve throughput  5604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30386 cycles, achieve throughput  5176 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30377 cycles, achieve throughput  5177 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30401 cycles, achieve throughput  5173 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61603 cycles, achieve throughput  2553 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  62190 cycles, achieve throughput  2529 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  61763 cycles, achieve throughput  2546 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  30387 cycles, achieve throughput  5176 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  30490 cycles, achieve throughput  5158 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  30715 cycles, achieve throughput  5120 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25219 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25215 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25329 cycles, achieve throughput  6209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25311 cycles, achieve throughput  6214 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25427 cycles, achieve throughput  6185 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25215 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25306 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25325 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25215 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25224 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25239 cycles, achieve throughput  6231 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25285 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25227 cycles, achieve throughput  6234 MB/s
Throughput test with EDMA2 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25316 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25400 cycles, achieve throughput  6192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25391 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25510 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25315 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25391 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25391 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25508 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  25303 cycles, achieve throughput  6216 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25373 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25374 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25390 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25500 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25497 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  25304 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  25302 cycles, achieve throughput  6216 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28059 cycles, achieve throughput  5605 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28087 cycles, achieve throughput  5599 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28098 cycles, achieve throughput  5597 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59637 cycles, achieve throughput  2637 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59090 cycles, achieve throughput  2661 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59090 cycles, achieve throughput  2661 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  28113 cycles, achieve throughput  5594 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  28047 cycles, achieve throughput  5607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  27948 cycles, achieve throughput  5627 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28067 cycles, achieve throughput  5603 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28046 cycles, achieve throughput  5608 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28061 cycles, achieve throughput  5605 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59568 cycles, achieve throughput  2640 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58650 cycles, achieve throughput  2681 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59094 cycles, achieve throughput  2661 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  28105 cycles, achieve throughput  5596 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  28046 cycles, achieve throughput  5608 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28106 cycles, achieve throughput  5596 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30702 cycles, achieve throughput  5123 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30896 cycles, achieve throughput  5090 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30807 cycles, achieve throughput  5105 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61290 cycles, achieve throughput  2566 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61825 cycles, achieve throughput  2544 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  62003 cycles, achieve throughput  2536 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  30389 cycles, achieve throughput  5175 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  30772 cycles, achieve throughput  5111 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  30816 cycles, achieve throughput  5104 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25219 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25217 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25325 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25323 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25229 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25217 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25430 cycles, achieve throughput  6185 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25315 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25321 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25215 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25272 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25224 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25326 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25287 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25239 cycles, achieve throughput  6231 MB/s
Throughput test with EDMA2 TC2
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25370 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25454 cycles, achieve throughput  6179 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25385 cycles, achieve throughput  6196 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25508 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  25305 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25308 cycles, achieve throughput  6214 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25316 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25508 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25389 cycles, achieve throughput  6195 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25400 cycles, achieve throughput  6192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  25305 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  25304 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25372 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25499 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25393 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25395 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25258 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28033 cycles, achieve throughput  5610 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28053 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28098 cycles, achieve throughput  5597 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59151 cycles, achieve throughput  2659 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59388 cycles, achieve throughput  2648 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58918 cycles, achieve throughput  2669 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  27945 cycles, achieve throughput  5628 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  28055 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28221 cycles, achieve throughput  5573 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27801 cycles, achieve throughput  5657 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27935 cycles, achieve throughput  5630 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28036 cycles, achieve throughput  5610 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59272 cycles, achieve throughput  2653 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  59363 cycles, achieve throughput  2649 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59389 cycles, achieve throughput  2648 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  28053 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  28051 cycles, achieve throughput  5607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28168 cycles, achieve throughput  5583 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30893 cycles, achieve throughput  5091 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30362 cycles, achieve throughput  5180 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30841 cycles, achieve throughput  5099 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61598 cycles, achieve throughput  2553 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61207 cycles, achieve throughput  2569 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  61812 cycles, achieve throughput  2544 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  30722 cycles, achieve throughput  5119 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  30657 cycles, achieve throughput  5130 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  30842 cycles, achieve throughput  5099 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25381 cycles, achieve throughput  6197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25315 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25229 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25219 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25216 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25326 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25325 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25321 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25229 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25219 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25282 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25241 cycles, achieve throughput  6231 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25240 cycles, achieve throughput  6231 MB/s
Throughput test with EDMA2 TC3
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25394 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25386 cycles, achieve throughput  6195 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25497 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  25246 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25315 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25320 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25400 cycles, achieve throughput  6192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25486 cycles, achieve throughput  6171 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25399 cycles, achieve throughput  6192 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  25246 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25245 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25319 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25314 cycles, achieve throughput  6213 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25318 cycles, achieve throughput  6212 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25385 cycles, achieve throughput  6196 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25393 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25395 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  25251 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  25304 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25257 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27947 cycles, achieve throughput  5628 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27897 cycles, achieve throughput  5638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28040 cycles, achieve throughput  5609 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59508 cycles, achieve throughput  2643 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59140 cycles, achieve throughput  2659 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59267 cycles, achieve throughput  2653 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(OSR (strongly ordered) ), consumes  28062 cycles, achieve throughput  5604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70040000(OSR (normal non-cache) ), consumes  28154 cycles, achieve throughput  5586 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28046 cycles, achieve throughput  5608 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28043 cycles, achieve throughput  5608 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28206 cycles, achieve throughput  5576 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27863 cycles, achieve throughput  5644 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59117 cycles, achieve throughput  2660 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  59351 cycles, achieve throughput  2650 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59284 cycles, achieve throughput  2653 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(OSR (strongly ordered) ), consumes  27823 cycles, achieve throughput  5653 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70040000(OSR (normal non-cache) ), consumes  28062 cycles, achieve throughput  5604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  28221 cycles, achieve throughput  5573 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30720 cycles, achieve throughput  5120 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30807 cycles, achieve throughput  5105 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30723 cycles, achieve throughput  5119 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61676 cycles, achieve throughput  2550 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61681 cycles, achieve throughput  2549 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  61396 cycles, achieve throughput  2561 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(OSR (strongly ordered) ), consumes  30831 cycles, achieve throughput  5101 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70040000(OSR (normal non-cache) ), consumes  30394 cycles, achieve throughput  5174 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  30824 cycles, achieve throughput  5102 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25219 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25215 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25274 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25366 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25373 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25323 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70020000(OSR (strongly ordered) ), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70040000(OSR (normal non-cache) ), consumes  25228 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(OSR (strongly ordered) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25290 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25220 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25216 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25324 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25323 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25325 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70000000(OSR (strongly ordered) ), consumes  25286 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70060000(OSR (normal non-cache) ), consumes  25283 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70040000(OSR (normal non-cache) ) to 0x70080000(OSR (RA_WB_WA,  in sh) ), consumes  25239 cycles, achieve throughput  6231 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c080000(MSRAM(strongly ordered)), consumes  25221 cycles, achieve throughput  6236 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25273 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x80000000(DDR3A(strongly ordered)), consumes  25213 cycles, achieve throughput  6238 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x88000000(DDR3A(normal non-cache)), consumes  25218 cycles, achieve throughput  6237 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25324 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70000000(OSR (strongly ordered) ), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x70040000(OSR (normal non-cache) ), consumes  25227 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70080000(OSR (RA_WB_WA,  in sh) ) to 0x700a0000(OSR (RA_WB_WA,  in sh) ), consumes  25240 cycles, achieve throughput  6231 MB/s
EDMA ACNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput     2 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    582 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput     9 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    11 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    14 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput    16 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    18 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput    20 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    22 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    24 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput    26 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    28 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput    30 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    32 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput    64 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput    96 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput   129 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput   161 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput   193 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   221 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   254 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   285 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   317 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   348 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   380 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   412 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   445 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   476 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   507 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   570 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   634 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   697 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   761 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   825 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   890 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   950 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput  1017 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput  1142 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput  1271 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1394 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput  1525 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput  1650 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1774 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1900 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput  2031 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    719 cycles, achieve throughput  1922 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    695 cycles, achieve throughput  2210 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    706 cycles, achieve throughput  2393 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput  2694 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    840 cycles, achieve throughput  2377 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    826 cycles, achieve throughput  2603 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    806 cycles, achieve throughput  2858 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    803 cycles, achieve throughput  3060 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    798 cycles, achieve throughput  3464 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    926 cycles, achieve throughput  3317 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    930 cycles, achieve throughput  3633 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    908 cycles, achieve throughput  4059 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    921 cycles, achieve throughput  4336 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1053 cycles, achieve throughput  4084 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1057 cycles, achieve throughput  4359 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1030 cycles, achieve throughput  4772 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1134 cycles, achieve throughput  4876 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1173 cycles, achieve throughput  5237 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1190 cycles, achieve throughput  5679 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1261 cycles, achieve throughput  5846 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1384 cycles, achieve throughput  5771 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1514 cycles, achieve throughput  5681 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1494 cycles, achieve throughput  6168 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1604 cycles, achieve throughput  6128 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1833 cycles, achieve throughput  6033 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1833 cycles, achieve throughput  6703 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1924 cycles, achieve throughput  7025 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2037 cycles, achieve throughput  7238 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2142 cycles, achieve throughput  7457 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2258 cycles, achieve throughput  7618 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2372 cycles, achieve throughput  7770 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2596 cycles, achieve throughput  7573 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2701 cycles, achieve throughput  7734 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2816 cycles, achieve throughput  7854 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2924 cycles, achieve throughput  7984 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3046 cycles, achieve throughput  8068 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3150 cycles, achieve throughput  8192 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3257 cycles, achieve throughput  8300 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3372 cycles, achieve throughput  8381 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3483 cycles, achieve throughput  8467 MB/s
EDMA ACNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    581 cycles, achieve throughput     2 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    581 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    584 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    585 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    585 cycles, achieve throughput    10 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    696 cycles, achieve throughput    10 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    585 cycles, achieve throughput    14 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    606 cycles, achieve throughput    17 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    715 cycles, achieve throughput    16 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    583 cycles, achieve throughput    22 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    585 cycles, achieve throughput    24 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    606 cycles, achieve throughput    25 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    604 cycles, achieve throughput    27 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    606 cycles, achieve throughput    29 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    604 cycles, achieve throughput    31 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    606 cycles, achieve throughput    63 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    605 cycles, achieve throughput    95 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    606 cycles, achieve throughput   126 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    704 cycles, achieve throughput   136 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    585 cycles, achieve throughput   196 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    815 cycles, achieve throughput   164 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    584 cycles, achieve throughput   263 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    585 cycles, achieve throughput   295 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    604 cycles, achieve throughput   317 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    606 cycles, achieve throughput   348 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    605 cycles, achieve throughput   380 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    605 cycles, achieve throughput   412 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    606 cycles, achieve throughput   443 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    605 cycles, achieve throughput   476 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    605 cycles, achieve throughput   507 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    849 cycles, achieve throughput   407 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    695 cycles, achieve throughput   552 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    682 cycles, achieve throughput   619 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    682 cycles, achieve throughput   675 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    683 cycles, achieve throughput   730 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    684 cycles, achieve throughput   785 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    815 cycles, achieve throughput   706 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    682 cycles, achieve throughput   900 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    682 cycles, achieve throughput  1013 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    684 cycles, achieve throughput  1122 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    682 cycles, achieve throughput  1238 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    682 cycles, achieve throughput  1351 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    682 cycles, achieve throughput  1463 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    686 cycles, achieve throughput  1567 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    684 cycles, achieve throughput  1684 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    683 cycles, achieve throughput  1799 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    815 cycles, achieve throughput  1696 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    815 cycles, achieve throughput  1884 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    795 cycles, achieve throughput  2125 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    794 cycles, achieve throughput  2321 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    794 cycles, achieve throughput  2514 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    793 cycles, achieve throughput  2711 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    795 cycles, achieve throughput  2898 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    937 cycles, achieve throughput  2622 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    940 cycles, achieve throughput  2941 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1281 cycles, achieve throughput  2398 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    937 cycles, achieve throughput  3606 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1032 cycles, achieve throughput  3572 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1141 cycles, achieve throughput  3500 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1129 cycles, achieve throughput  3809 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1129 cycles, achieve throughput  4081 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1129 cycles, achieve throughput  4353 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1262 cycles, achieve throughput  4381 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1404 cycles, achieve throughput  4376 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1384 cycles, achieve throughput  4883 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1495 cycles, achieve throughput  4931 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1608 cycles, achieve throughput  4967 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1586 cycles, achieve throughput  5423 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1695 cycles, achieve throughput  5437 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1806 cycles, achieve throughput  5443 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1919 cycles, achieve throughput  5763 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2029 cycles, achieve throughput  6056 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2251 cycles, achieve throughput  6004 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2360 cycles, achieve throughput  6248 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2471 cycles, achieve throughput  6464 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2919 cycles, achieve throughput  5893 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2930 cycles, achieve throughput  6290 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2923 cycles, achieve throughput  6726 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3152 cycles, achieve throughput  6627 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3261 cycles, achieve throughput  6782 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3486 cycles, achieve throughput  6697 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3591 cycles, achieve throughput  6843 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3710 cycles, achieve throughput  6955 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3825 cycles, achieve throughput  7067 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   4048 cycles, achieve throughput  6981 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   4158 cycles, achieve throughput  7092 MB/s
EDMA ACNTxBCNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput     2 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput    10 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    11 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    13 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    15 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    17 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    19 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    21 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    23 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    25 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    27 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    29 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    31 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    63 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    95 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   127 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   158 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   190 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   221 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   253 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   285 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   317 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   348 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   380 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   411 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   444 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   476 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   506 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   570 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   634 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   697 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   761 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   825 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   890 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   953 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1013 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput  1144 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput  1271 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput  1396 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1520 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput  1650 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1774 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1900 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput  2034 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    715 cycles, achieve throughput  1933 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    699 cycles, achieve throughput  2197 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    693 cycles, achieve throughput  2438 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput  2694 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    825 cycles, achieve throughput  2420 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    815 cycles, achieve throughput  2638 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    803 cycles, achieve throughput  2869 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    802 cycles, achieve throughput  3064 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    802 cycles, achieve throughput  3447 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    939 cycles, achieve throughput  3271 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    949 cycles, achieve throughput  3560 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    918 cycles, achieve throughput  4015 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    920 cycles, achieve throughput  4340 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    925 cycles, achieve throughput  4649 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1070 cycles, achieve throughput  4306 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1070 cycles, achieve throughput  4593 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1161 cycles, achieve throughput  4762 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1137 cycles, achieve throughput  5403 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1261 cycles, achieve throughput  5359 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1279 cycles, achieve throughput  5764 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1385 cycles, achieve throughput  5766 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1524 cycles, achieve throughput  5644 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1519 cycles, achieve throughput  6067 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1605 cycles, achieve throughput  6124 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1613 cycles, achieve throughput  6856 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1850 cycles, achieve throughput  6642 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1920 cycles, achieve throughput  7040 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2038 cycles, achieve throughput  7235 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2143 cycles, achieve throughput  7454 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2260 cycles, achieve throughput  7612 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2372 cycles, achieve throughput  7770 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2596 cycles, achieve throughput  7573 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2706 cycles, achieve throughput  7719 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2816 cycles, achieve throughput  7854 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2930 cycles, achieve throughput  7968 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3100 cycles, achieve throughput  7927 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3160 cycles, achieve throughput  8166 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3273 cycles, achieve throughput  8259 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3378 cycles, achieve throughput  8366 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3499 cycles, achieve throughput  8428 MB/s
transfer    2 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput     4 MB/s
transfer    2 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput     8 MB/s
transfer    2 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput    12 MB/s
transfer    2 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput    16 MB/s
transfer    2 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput    20 MB/s
transfer    2 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    23 MB/s
transfer    2 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    27 MB/s
transfer    2 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    31 MB/s
transfer    2 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    35 MB/s
transfer    2 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    39 MB/s
transfer    2 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    43 MB/s
transfer    2 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    47 MB/s
transfer    2 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    51 MB/s
transfer    2 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    55 MB/s
transfer    2 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    59 MB/s
transfer    2 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    63 MB/s
transfer    2 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   127 MB/s
transfer    2 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   190 MB/s
transfer    2 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   253 MB/s
transfer    2 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   317 MB/s
transfer    2 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   380 MB/s
transfer    2 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   444 MB/s
transfer    2 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   506 MB/s
transfer    2 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   570 MB/s
transfer    2 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   633 MB/s
transfer    2 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   699 MB/s
transfer    2 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   760 MB/s
transfer    2 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   825 MB/s
transfer    2 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   890 MB/s
transfer    2 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   950 MB/s
transfer    2 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput  1015 MB/s
transfer    2 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput  1144 MB/s
transfer    2 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1267 MB/s
transfer    2 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1394 MB/s
transfer    2 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput  1523 MB/s
transfer    2 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput  1650 MB/s
transfer    2 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput  1774 MB/s
transfer    2 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    715 cycles, achieve throughput  1611 MB/s
transfer    2 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    694 cycles, achieve throughput  1770 MB/s
transfer    2 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    682 cycles, achieve throughput  2026 MB/s
transfer    2 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    686 cycles, achieve throughput  2239 MB/s
transfer    2 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput  2441 MB/s
transfer    2 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  2698 MB/s
transfer    2 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    828 cycles, achieve throughput  2411 MB/s
transfer    2 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    815 cycles, achieve throughput  2638 MB/s
transfer    2 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    803 cycles, achieve throughput  2869 MB/s
transfer    2 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    803 cycles, achieve throughput  3060 MB/s
transfer    2 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    804 cycles, achieve throughput  3438 MB/s
transfer    2 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    945 cycles, achieve throughput  3250 MB/s
transfer    2 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    945 cycles, achieve throughput  3575 MB/s
transfer    2 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    919 cycles, achieve throughput  4011 MB/s
transfer    2 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    922 cycles, achieve throughput  4331 MB/s
transfer    2 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1070 cycles, achieve throughput  4019 MB/s
transfer    2 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1057 cycles, achieve throughput  4359 MB/s
transfer    2 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1031 cycles, achieve throughput  4767 MB/s
transfer    2 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1189 cycles, achieve throughput  4650 MB/s
transfer    2 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1131 cycles, achieve throughput  5432 MB/s
transfer    2 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1274 cycles, achieve throughput  5304 MB/s
transfer    2 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1410 cycles, achieve throughput  5228 MB/s
transfer    2 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1276 cycles, achieve throughput  6259 MB/s
transfer    2 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1495 cycles, achieve throughput  5753 MB/s
transfer    2 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1497 cycles, achieve throughput  6156 MB/s
transfer    2 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1605 cycles, achieve throughput  6124 MB/s
transfer    2 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1714 cycles, achieve throughput  6452 MB/s
transfer    2 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1814 cycles, achieve throughput  6773 MB/s
transfer    2 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1927 cycles, achieve throughput  7014 MB/s
transfer    2 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2041 cycles, achieve throughput  7224 MB/s
transfer    2 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2145 cycles, achieve throughput  7447 MB/s
transfer    2 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2270 cycles, achieve throughput  7578 MB/s
transfer    2 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2411 cycles, achieve throughput  7644 MB/s
transfer    2 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2502 cycles, achieve throughput  7858 MB/s
transfer    2 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2814 cycles, achieve throughput  7860 MB/s
transfer    2 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3049 cycles, achieve throughput  8060 MB/s
transfer    2 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3263 cycles, achieve throughput  8284 MB/s
transfer    2 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3533 cycles, achieve throughput  8347 MB/s
transfer    2 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3824 cycles, achieve throughput  8354 MB/s
transfer    2 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4047 cycles, achieve throughput  8501 MB/s
transfer    2 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4273 cycles, achieve throughput  8627 MB/s
transfer    2 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4520 cycles, achieve throughput  8699 MB/s
transfer    2 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4719 cycles, achieve throughput  8853 MB/s
transfer    2 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4988 cycles, achieve throughput  8868 MB/s
transfer    2 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5275 cycles, achieve throughput  8852 MB/s
transfer    2 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5501 cycles, achieve throughput  8935 MB/s
transfer    2 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5681 cycles, achieve throughput  9084 MB/s
transfer    2 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6063 cycles, achieve throughput  8917 MB/s
transfer    2 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6239 cycles, achieve throughput  9059 MB/s
transfer    2 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6437 cycles, achieve throughput  9163 MB/s
transfer    3 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput     6 MB/s
transfer    3 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput    12 MB/s
transfer    3 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput    18 MB/s
transfer    3 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput    24 MB/s
transfer    3 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    585 cycles, achieve throughput    30 MB/s
transfer    3 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    35 MB/s
transfer    3 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    41 MB/s
transfer    3 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    47 MB/s
transfer    3 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    53 MB/s
transfer    3 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    59 MB/s
transfer    3 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    65 MB/s
transfer    3 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    71 MB/s
transfer    3 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput    77 MB/s
transfer    3 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    83 MB/s
transfer    3 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput    89 MB/s
transfer    3 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput    95 MB/s
transfer    3 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   190 MB/s
transfer    3 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   285 MB/s
transfer    3 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   380 MB/s
transfer    3 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   475 MB/s
transfer    3 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    606 cycles, achieve throughput   570 MB/s
transfer    3 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   666 MB/s
transfer    3 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   762 MB/s
transfer    3 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    717 cycles, achieve throughput   723 MB/s
transfer    3 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput   986 MB/s
transfer    3 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    695 cycles, achieve throughput   911 MB/s
transfer    3 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput  1183 MB/s
transfer    3 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput  1094 MB/s
transfer    3 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  1180 MB/s
transfer    3 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput  1263 MB/s
transfer    3 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    682 cycles, achieve throughput  1351 MB/s
transfer    3 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  1518 MB/s
transfer    3 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    682 cycles, achieve throughput  1689 MB/s
transfer    3 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    814 cycles, achieve throughput  1556 MB/s
transfer    3 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput  2021 MB/s
transfer    3 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  2192 MB/s
transfer    3 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  2361 MB/s
transfer    3 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  2530 MB/s
transfer    3 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput  2694 MB/s
transfer    3 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    815 cycles, achieve throughput  2544 MB/s
transfer    3 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    817 cycles, achieve throughput  2820 MB/s
transfer    3 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    804 cycles, achieve throughput  3152 MB/s
transfer    3 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    802 cycles, achieve throughput  3447 MB/s
transfer    3 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    809 cycles, achieve throughput  3702 MB/s
transfer    3 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    953 cycles, achieve throughput  3384 MB/s
transfer    3 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    953 cycles, achieve throughput  3626 MB/s
transfer    3 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    919 cycles, achieve throughput  4011 MB/s
transfer    3 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    918 cycles, achieve throughput  4517 MB/s
transfer    3 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1074 cycles, achieve throughput  4290 MB/s
transfer    3 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1161 cycles, achieve throughput  4365 MB/s
transfer    3 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1129 cycles, achieve throughput  4897 MB/s
transfer    3 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1137 cycles, achieve throughput  5268 MB/s
transfer    3 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1277 cycles, achieve throughput  5051 MB/s
transfer    3 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1267 cycles, achieve throughput  5455 MB/s
transfer    3 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1394 cycles, achieve throughput  5288 MB/s
transfer    3 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1379 cycles, achieve throughput  6014 MB/s
transfer    3 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1482 cycles, achieve throughput  6218 MB/s
transfer    3 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1622 cycles, achieve throughput  6250 MB/s
transfer    3 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1641 cycles, achieve throughput  6739 MB/s
transfer    3 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1729 cycles, achieve throughput  6929 MB/s
transfer    3 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1831 cycles, achieve throughput  7046 MB/s
transfer    3 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1947 cycles, achieve throughput  7100 MB/s
transfer    3 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2049 cycles, achieve throughput  7196 MB/s
transfer    3 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2166 cycles, achieve throughput  7658 MB/s
transfer    3 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2376 cycles, achieve throughput  7757 MB/s
transfer    3 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2600 cycles, achieve throughput  7798 MB/s
transfer    3 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2724 cycles, achieve throughput  8119 MB/s
transfer    3 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2945 cycles, achieve throughput  8136 MB/s
transfer    3 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3075 cycles, achieve throughput  8391 MB/s
transfer    3 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3301 cycles, achieve throughput  8375 MB/s
transfer    3 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3523 cycles, achieve throughput  8371 MB/s
transfer    3 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3937 cycles, achieve throughput  8427 MB/s
transfer    3 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4274 cycles, achieve throughput  8625 MB/s
transfer    3 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4616 cycles, achieve throughput  8784 MB/s
transfer    3 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4995 cycles, achieve throughput  8856 MB/s
transfer    3 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5358 cycles, achieve throughput  8944 MB/s
transfer    3 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5728 cycles, achieve throughput  9010 MB/s
transfer    3 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6065 cycles, achieve throughput  9117 MB/s
transfer    3 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6509 cycles, achieve throughput  9061 MB/s
transfer    3 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6800 cycles, achieve throughput  9216 MB/s
transfer    3 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7213 cycles, achieve throughput  9199 MB/s
transfer    3 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7583 cycles, achieve throughput  9236 MB/s
transfer    3 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7977 cycles, achieve throughput  9242 MB/s
transfer    3 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8323 cycles, achieve throughput  9301 MB/s
transfer    3 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8681 cycles, achieve throughput  9342 MB/s
transfer    3 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9041 cycles, achieve throughput  9378 MB/s
transfer    3 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9385 cycles, achieve throughput  9427 MB/s
transfer    4 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    581 cycles, achieve throughput     8 MB/s
transfer    4 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput    16 MB/s
transfer    4 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    696 cycles, achieve throughput    20 MB/s
transfer    4 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    583 cycles, achieve throughput    32 MB/s
transfer    4 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    695 cycles, achieve throughput    34 MB/s
transfer    4 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    695 cycles, achieve throughput    41 MB/s
transfer    4 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput    49 MB/s
transfer    4 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput    65 MB/s
transfer    4 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput    63 MB/s
transfer    4 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput    70 MB/s
transfer    4 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput    77 MB/s
transfer    4 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    682 cycles, achieve throughput    84 MB/s
transfer    4 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput    91 MB/s
transfer    4 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput    98 MB/s
transfer    4 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    682 cycles, achieve throughput   105 MB/s
transfer    4 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput   131 MB/s
transfer    4 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    585 cycles, achieve throughput   262 MB/s
transfer    4 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    605 cycles, achieve throughput   380 MB/s
transfer    4 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    604 cycles, achieve throughput   508 MB/s
transfer    4 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    705 cycles, achieve throughput   544 MB/s
transfer    4 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput   674 MB/s
transfer    4 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput   785 MB/s
transfer    4 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput  1052 MB/s
transfer    4 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  1012 MB/s
transfer    4 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  1124 MB/s
transfer    4 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    682 cycles, achieve throughput  1238 MB/s
transfer    4 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    682 cycles, achieve throughput  1351 MB/s
transfer    4 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  1461 MB/s
transfer    4 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    683 cycles, achieve throughput  1574 MB/s
transfer    4 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    685 cycles, achieve throughput  1681 MB/s
transfer    4 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    682 cycles, achieve throughput  1801 MB/s
transfer    4 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput  2021 MB/s
transfer    4 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    684 cycles, achieve throughput  2245 MB/s
transfer    4 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    814 cycles, achieve throughput  2075 MB/s
transfer    4 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    694 cycles, achieve throughput  2655 MB/s
transfer    4 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    816 cycles, achieve throughput  2447 MB/s
transfer    4 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    819 cycles, achieve throughput  2625 MB/s
transfer    4 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    802 cycles, achieve throughput  2872 MB/s
transfer    4 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    798 cycles, achieve throughput  3079 MB/s
transfer    4 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    795 cycles, achieve throughput  3477 MB/s
transfer    4 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    804 cycles, achieve throughput  3820 MB/s
transfer    4 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    950 cycles, achieve throughput  3557 MB/s
transfer    4 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    951 cycles, achieve throughput  3876 MB/s
transfer    4 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    918 cycles, achieve throughput  4350 MB/s
transfer    4 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1060 cycles, achieve throughput  4057 MB/s
transfer    4 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1063 cycles, achieve throughput  4334 MB/s
transfer    4 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1033 cycles, achieve throughput  4758 MB/s
transfer    4 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1053 cycles, achieve throughput  5251 MB/s
transfer    4 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1155 cycles, achieve throughput  5319 MB/s
transfer    4 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1168 cycles, achieve throughput  5786 MB/s
transfer    4 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1273 cycles, achieve throughput  5791 MB/s
transfer    4 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1386 cycles, achieve throughput  5762 MB/s
transfer    4 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1486 cycles, achieve throughput  5788 MB/s
transfer    4 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1595 cycles, achieve throughput  5778 MB/s
transfer    4 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1603 cycles, achieve throughput  6132 MB/s
transfer    4 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1727 cycles, achieve throughput  6403 MB/s
transfer    4 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1834 cycles, achieve throughput  6700 MB/s
transfer    4 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1954 cycles, achieve throughput  6917 MB/s
transfer    4 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2069 cycles, achieve throughput  7126 MB/s
transfer    4 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2167 cycles, achieve throughput  7371 MB/s
transfer    4 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2261 cycles, achieve throughput  7608 MB/s
transfer    4 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2373 cycles, achieve throughput  7767 MB/s
transfer    4 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2506 cycles, achieve throughput  7845 MB/s
transfer    4 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2714 cycles, achieve throughput  8149 MB/s
transfer    4 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3044 cycles, achieve throughput  8073 MB/s
transfer    4 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3276 cycles, achieve throughput  8252 MB/s
transfer    4 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3509 cycles, achieve throughput  8404 MB/s
transfer    4 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3736 cycles, achieve throughput  8551 MB/s
transfer    4 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3961 cycles, achieve throughput  8686 MB/s
transfer    4 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4276 cycles, achieve throughput  8621 MB/s
transfer    4 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4519 cycles, achieve throughput  8701 MB/s
transfer    4 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4946 cycles, achieve throughput  8943 MB/s
transfer    4 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5499 cycles, achieve throughput  8938 MB/s
transfer    4 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5992 cycles, achieve throughput  9023 MB/s
transfer    4 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6483 cycles, achieve throughput  9098 MB/s
transfer    4 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6892 cycles, achieve throughput  9271 MB/s
transfer    4 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7458 cycles, achieve throughput  9226 MB/s
transfer    4 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7928 cycles, achieve throughput  9299 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8493 cycles, achieve throughput  9259 MB/s
transfer    4 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9023 cycles, achieve throughput  9260 MB/s
transfer    4 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9379 cycles, achieve throughput  9433 MB/s
transfer    4 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9916 cycles, achieve throughput  9417 MB/s
transfer    4 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  10384 cycles, achieve throughput  9466 MB/s
transfer    4 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  10937 cycles, achieve throughput  9437 MB/s
transfer    4 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  11393 cycles, achieve throughput  9491 MB/s
transfer    4 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  11866 cycles, achieve throughput  9527 MB/s
transfer    4 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12306 cycles, achieve throughput  9585 MB/s
EDMA Index test with EDMA0 TC0
transfer 1024 *     1 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22118 cycles, achieve throughput    55 MB/s
transfer 1024 *     2 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21895 cycles, achieve throughput   112 MB/s
transfer 1024 *     3 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21674 cycles, achieve throughput   170 MB/s
transfer 1024 *     4 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21673 cycles, achieve throughput   226 MB/s
transfer 1024 *     5 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21674 cycles, achieve throughput   283 MB/s
transfer 1024 *     6 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21674 cycles, achieve throughput   340 MB/s
transfer 1024 *     7 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21673 cycles, achieve throughput   396 MB/s
transfer 1024 *     8 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21563 cycles, achieve throughput   455 MB/s
transfer 1024 *     9 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21672 cycles, achieve throughput   510 MB/s
transfer 1024 *    10 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21563 cycles, achieve throughput   569 MB/s
transfer 1024 *    11 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21672 cycles, achieve throughput   623 MB/s
transfer 1024 *    12 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21561 cycles, achieve throughput   683 MB/s
transfer 1024 *    13 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21562 cycles, achieve throughput   740 MB/s
transfer 1024 *    14 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21563 cycles, achieve throughput   797 MB/s
transfer 1024 *    15 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21561 cycles, achieve throughput   854 MB/s
transfer 1024 *    16 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21562 cycles, achieve throughput   911 MB/s
transfer 1024 *    32 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21563 cycles, achieve throughput  1823 MB/s
transfer 1024 *    48 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21565 cycles, achieve throughput  2735 MB/s
transfer 1024 *    64 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21565 cycles, achieve throughput  3646 MB/s
transfer 1024 *    80 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  27341 cycles, achieve throughput  3595 MB/s
transfer 1024 *    96 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28557 cycles, achieve throughput  4130 MB/s
transfer 1024 *   112 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26615 cycles, achieve throughput  5170 MB/s
transfer 1024 *   128 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  27457 cycles, achieve throughput  5728 MB/s
transfer 1024 *   144 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31961 cycles, achieve throughput  5536 MB/s
transfer 1024 *   160 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32614 cycles, achieve throughput  6028 MB/s
transfer 1024 *   176 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31793 cycles, achieve throughput  6802 MB/s
transfer 1024 *   192 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32619 cycles, achieve throughput  7232 MB/s
transfer 1024 *   208 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33513 cycles, achieve throughput  7626 MB/s
transfer 1024 *   224 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32017 cycles, achieve throughput  8597 MB/s
transfer 1024 *   240 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35008 cycles, achieve throughput  8424 MB/s
transfer 1024 *   256 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35000 cycles, achieve throughput  8987 MB/s
transfer 1024 *   320 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41810 cycles, achieve throughput  9404 MB/s
transfer 1024 *   384 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  48484 cycles, achieve throughput  9732 MB/s
transfer 1024 *   448 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59367 cycles, achieve throughput  9272 MB/s
transfer 1024 *   512 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  66498 cycles, achieve throughput  9461 MB/s
transfer 1024 *   768 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  99462 cycles, achieve throughput  9488 MB/s
transfer 1024 *  1024 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133545 cycles, achieve throughput  9422 MB/s
transfer  682 *  1536 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133086 cycles, achieve throughput  9445 MB/s
transfer  512 *  2048 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132387 cycles, achieve throughput  9504 MB/s
transfer  409 *  2560 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132849 cycles, achieve throughput  9457 MB/s
transfer  341 *  3072 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132704 cycles, achieve throughput  9472 MB/s
transfer  292 *  3584 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132111 cycles, achieve throughput  9505 MB/s
transfer  256 *  4096 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132912 cycles, achieve throughput  9467 MB/s
transfer  227 *  4608 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131600 cycles, achieve throughput  9538 MB/s
transfer  204 *  5120 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132108 cycles, achieve throughput  9487 MB/s
transfer  186 *  5632 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132247 cycles, achieve throughput  9505 MB/s
transfer  170 *  6144 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132083 cycles, achieve throughput  9489 MB/s
transfer  157 *  6656 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132586 cycles, achieve throughput  9457 MB/s
transfer  146 *  7168 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132399 cycles, achieve throughput  9485 MB/s
transfer  136 *  7680 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131874 cycles, achieve throughput  9504 MB/s
transfer  128 *  8192 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132768 cycles, achieve throughput  9477 MB/s
transfer 1024 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    695 cycles, achieve throughput  1768 MB/s
transfer 1024 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    806 cycles, achieve throughput  3049 MB/s
transfer 1024 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22296 cycles, achieve throughput   165 MB/s
transfer 1024 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1028 cycles, achieve throughput  4781 MB/s
transfer 1024 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22294 cycles, achieve throughput   275 MB/s
transfer 1024 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21733 cycles, achieve throughput   339 MB/s
transfer 1024 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23516 cycles, achieve throughput   365 MB/s
transfer 1024 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1497 cycles, achieve throughput  6566 MB/s
transfer 1024 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23959 cycles, achieve throughput   461 MB/s
transfer 1024 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21967 cycles, achieve throughput   559 MB/s
transfer 1024 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22527 cycles, achieve throughput   600 MB/s
transfer 1024 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23942 cycles, achieve throughput   615 MB/s
transfer 1024 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24725 cycles, achieve throughput   646 MB/s
transfer 1024 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23057 cycles, achieve throughput   746 MB/s
transfer 1024 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22847 cycles, achieve throughput   806 MB/s
transfer 1024 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2503 cycles, achieve throughput  7854 MB/s
transfer 1024 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4529 cycles, achieve throughput  8682 MB/s
transfer 1024 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31569 cycles, achieve throughput  1868 MB/s
transfer 1024 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8391 cycles, achieve throughput  9372 MB/s
transfer 1024 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32953 cycles, achieve throughput  2983 MB/s
transfer 1024 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23414 cycles, achieve throughput  5038 MB/s
transfer 1024 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34372 cycles, achieve throughput  4004 MB/s
transfer 1024 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  16179 cycles, achieve throughput  9721 MB/s
transfer 1024 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37600 cycles, achieve throughput  4706 MB/s
transfer 1024 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31304 cycles, achieve throughput  6280 MB/s
transfer 1024 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41243 cycles, achieve throughput  5243 MB/s
transfer 1024 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28383 cycles, achieve throughput  8312 MB/s
transfer 1024 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  46701 cycles, achieve throughput  5472 MB/s
transfer 1024 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42145 cycles, achieve throughput  6531 MB/s
transfer 1024 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  50916 cycles, achieve throughput  5792 MB/s
transfer 1024 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34985 cycles, achieve throughput  8991 MB/s
transfer 1024 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42863 cycles, achieve throughput  9173 MB/s
transfer 1024 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  49761 cycles, achieve throughput  9482 MB/s
transfer 1024 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59187 cycles, achieve throughput  9301 MB/s
transfer 1024 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  66221 cycles, achieve throughput  9500 MB/s
transfer 1024 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  99938 cycles, achieve throughput  9443 MB/s
transfer 1024 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133108 cycles, achieve throughput  9453 MB/s
transfer  682 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132270 cycles, achieve throughput  9503 MB/s
transfer  512 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132686 cycles, achieve throughput  9483 MB/s
transfer  409 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132253 cycles, achieve throughput  9500 MB/s
transfer  341 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132057 cycles, achieve throughput  9519 MB/s
transfer  292 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132385 cycles, achieve throughput  9486 MB/s
transfer  256 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131964 cycles, achieve throughput  9535 MB/s
transfer  227 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131998 cycles, achieve throughput  9509 MB/s
transfer  204 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131584 cycles, achieve throughput  9525 MB/s
transfer  186 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131950 cycles, achieve throughput  9526 MB/s
transfer  170 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131600 cycles, achieve throughput  9524 MB/s
transfer  157 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132005 cycles, achieve throughput  9499 MB/s
transfer  146 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132483 cycles, achieve throughput  9479 MB/s
transfer  136 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131869 cycles, achieve throughput  9504 MB/s
transfer  128 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132475 cycles, achieve throughput  9498 MB/s
transfer 1024 *     1 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22169 cycles, achieve throughput    55 MB/s
transfer 1024 *     2 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21921 cycles, achieve throughput   112 MB/s
transfer 1024 *     3 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21521 cycles, achieve throughput   171 MB/s
transfer 1024 *     4 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21836 cycles, achieve throughput   225 MB/s
transfer 1024 *     5 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21824 cycles, achieve throughput   281 MB/s
transfer 1024 *     6 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22829 cycles, achieve throughput   322 MB/s
transfer 1024 *     7 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21296 cycles, achieve throughput   403 MB/s
transfer 1024 *     8 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23396 cycles, achieve throughput   420 MB/s
transfer 1024 *     9 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22044 cycles, achieve throughput   501 MB/s
transfer 1024 *    10 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22504 cycles, achieve throughput   546 MB/s
transfer 1024 *    11 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24034 cycles, achieve throughput   562 MB/s
transfer 1024 *    12 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24142 cycles, achieve throughput   610 MB/s
transfer 1024 *    13 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23166 cycles, achieve throughput   689 MB/s
transfer 1024 *    14 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22410 cycles, achieve throughput   767 MB/s
transfer 1024 *    15 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21337 cycles, achieve throughput   863 MB/s
transfer 1024 *    16 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22946 cycles, achieve throughput   856 MB/s
transfer 1024 *    32 Bytes with index=   33 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23298 cycles, achieve throughput  1687 MB/s
transfer 1024 *    48 Bytes with index=   49 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32832 cycles, achieve throughput  1796 MB/s
transfer 1024 *    64 Bytes with index=   65 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  40752 cycles, achieve throughput  1929 MB/s
transfer 1024 *    80 Bytes with index=   81 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41435 cycles, achieve throughput  2372 MB/s
transfer 1024 *    96 Bytes with index=   97 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42313 cycles, achieve throughput  2787 MB/s
transfer 1024 *   112 Bytes with index=  113 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42877 cycles, achieve throughput  3209 MB/s
transfer 1024 *   128 Bytes with index=  129 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  44311 cycles, achieve throughput  3549 MB/s
transfer 1024 *   144 Bytes with index=  145 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  44884 cycles, achieve throughput  3942 MB/s
transfer 1024 *   160 Bytes with index=  161 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  45340 cycles, achieve throughput  4336 MB/s
transfer 1024 *   176 Bytes with index=  177 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  46374 cycles, achieve throughput  4663 MB/s
transfer 1024 *   192 Bytes with index=  193 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  48918 cycles, achieve throughput  4822 MB/s
transfer 1024 *   208 Bytes with index=  209 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  54068 cycles, achieve throughput  4727 MB/s
transfer 1024 *   224 Bytes with index=  225 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  54128 cycles, achieve throughput  5085 MB/s
transfer 1024 *   240 Bytes with index=  241 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  58034 cycles, achieve throughput  5081 MB/s
transfer 1024 *   256 Bytes with index=  257 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  55476 cycles, achieve throughput  5670 MB/s
transfer 1024 *   320 Bytes with index=  321 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59745 cycles, achieve throughput  6581 MB/s
transfer 1024 *   384 Bytes with index=  385 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  73516 cycles, achieve throughput  6418 MB/s
transfer 1024 *   448 Bytes with index=  449 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  84995 cycles, achieve throughput  6476 MB/s
transfer 1024 *   512 Bytes with index=  513 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  89781 cycles, achieve throughput  7007 MB/s
transfer 1024 *   768 Bytes with index=  769 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 112681 cycles, achieve throughput  8375 MB/s
transfer 1023 *  1024 Bytes with index= 1025 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 146387 cycles, achieve throughput  8587 MB/s
transfer  682 *  1536 Bytes with index= 1537 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 150528 cycles, achieve throughput  8351 MB/s
transfer  511 *  2048 Bytes with index= 2049 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 150403 cycles, achieve throughput  8349 MB/s
transfer  409 *  2560 Bytes with index= 2561 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 150848 cycles, achieve throughput  8329 MB/s
transfer  341 *  3072 Bytes with index= 3073 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 153372 cycles, achieve throughput  8196 MB/s
transfer  292 *  3584 Bytes with index= 3585 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 154632 cycles, achieve throughput  8121 MB/s
transfer  255 *  4096 Bytes with index= 4097 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 156948 cycles, achieve throughput  7985 MB/s
transfer  227 *  4608 Bytes with index= 4609 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 156229 cycles, achieve throughput  8034 MB/s
transfer  204 *  5120 Bytes with index= 5121 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 157016 cycles, achieve throughput  7982 MB/s
transfer  186 *  5632 Bytes with index= 5633 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 157825 cycles, achieve throughput  7964 MB/s
transfer  170 *  6144 Bytes with index= 6145 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 157787 cycles, achieve throughput  7943 MB/s
transfer  157 *  6656 Bytes with index= 6657 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 158435 cycles, achieve throughput  7914 MB/s
transfer  146 *  7168 Bytes with index= 7169 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 159232 cycles, achieve throughput  7886 MB/s
transfer  136 *  7680 Bytes with index= 7681 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 158566 cycles, achieve throughput  7904 MB/s
transfer  127 *  8192 Bytes with index= 8193 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 160591 cycles, achieve throughput  7774 MB/s
transfer 1024 *     1 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20824 cycles, achieve throughput    59 MB/s
transfer 1024 *     2 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20481 cycles, achieve throughput   119 MB/s
transfer 1024 *     3 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21270 cycles, achieve throughput   173 MB/s
transfer 1024 *     4 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21286 cycles, achieve throughput   230 MB/s
transfer 1024 *     5 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21822 cycles, achieve throughput   281 MB/s
transfer 1024 *     6 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20612 cycles, achieve throughput   357 MB/s
transfer 1024 *     7 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22150 cycles, achieve throughput   388 MB/s
transfer 1024 *     8 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21486 cycles, achieve throughput   457 MB/s
transfer 1024 *     9 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22587 cycles, achieve throughput   489 MB/s
transfer 1024 *    10 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20961 cycles, achieve throughput   586 MB/s
transfer 1024 *    11 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20582 cycles, achieve throughput   656 MB/s
transfer 1024 *    12 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21273 cycles, achieve throughput   693 MB/s
transfer 1024 *    13 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22935 cycles, achieve throughput   696 MB/s
transfer 1024 *    14 Bytes with index=   18 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24054 cycles, achieve throughput   715 MB/s
transfer 1024 *    15 Bytes with index=   19 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  25268 cycles, achieve throughput   729 MB/s
transfer 1024 *    16 Bytes with index=   20 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24159 cycles, achieve throughput   813 MB/s
transfer 1024 *    32 Bytes with index=   36 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24533 cycles, achieve throughput  1602 MB/s
transfer 1024 *    48 Bytes with index=   52 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34279 cycles, achieve throughput  1720 MB/s
transfer 1024 *    64 Bytes with index=   68 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37382 cycles, achieve throughput  2103 MB/s
transfer 1024 *    80 Bytes with index=   84 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  38085 cycles, achieve throughput  2581 MB/s
transfer 1024 *    96 Bytes with index=  100 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  38761 cycles, achieve throughput  3043 MB/s
transfer 1024 *   112 Bytes with index=  116 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  39054 cycles, achieve throughput  3523 MB/s
transfer 1024 *   128 Bytes with index=  132 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  40874 cycles, achieve throughput  3848 MB/s
transfer 1024 *   144 Bytes with index=  148 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42155 cycles, achieve throughput  4197 MB/s
transfer 1024 *   160 Bytes with index=  164 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42933 cycles, achieve throughput  4579 MB/s
transfer 1024 *   176 Bytes with index=  180 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  45098 cycles, achieve throughput  4795 MB/s
transfer 1024 *   192 Bytes with index=  196 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  47067 cycles, achieve throughput  5012 MB/s
transfer 1024 *   208 Bytes with index=  212 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  49744 cycles, achieve throughput  5138 MB/s
transfer 1024 *   224 Bytes with index=  228 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  52043 cycles, achieve throughput  5288 MB/s
transfer 1024 *   240 Bytes with index=  244 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  55423 cycles, achieve throughput  5321 MB/s
transfer 1024 *   256 Bytes with index=  260 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  53506 cycles, achieve throughput  5879 MB/s
transfer 1024 *   320 Bytes with index=  324 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59721 cycles, achieve throughput  6584 MB/s
transfer 1024 *   384 Bytes with index=  388 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  70676 cycles, achieve throughput  6676 MB/s
transfer 1024 *   448 Bytes with index=  452 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  80324 cycles, achieve throughput  6853 MB/s
transfer 1024 *   512 Bytes with index=  516 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  87063 cycles, achieve throughput  7226 MB/s
transfer 1024 *   768 Bytes with index=  772 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 112112 cycles, achieve throughput  8417 MB/s
transfer 1020 *  1024 Bytes with index= 1028 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145937 cycles, achieve throughput  8588 MB/s
transfer  680 *  1536 Bytes with index= 1540 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 147697 cycles, achieve throughput  8486 MB/s
transfer  511 *  2048 Bytes with index= 2052 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 148022 cycles, achieve throughput  8484 MB/s
transfer  408 *  2560 Bytes with index= 2564 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 149155 cycles, achieve throughput  8403 MB/s
transfer  340 *  3072 Bytes with index= 3076 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 150728 cycles, achieve throughput  8315 MB/s
transfer  292 *  3584 Bytes with index= 3588 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 151783 cycles, achieve throughput  8273 MB/s
transfer  255 *  4096 Bytes with index= 4100 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 152902 cycles, achieve throughput  8197 MB/s
transfer  227 *  4608 Bytes with index= 4612 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 153748 cycles, achieve throughput  8164 MB/s
transfer  204 *  5120 Bytes with index= 5124 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 154455 cycles, achieve throughput  8114 MB/s
transfer  186 *  5632 Bytes with index= 5636 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155329 cycles, achieve throughput  8092 MB/s
transfer  170 *  6144 Bytes with index= 6148 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155207 cycles, achieve throughput  8075 MB/s
transfer  157 *  6656 Bytes with index= 6660 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 156194 cycles, achieve throughput  8028 MB/s
transfer  146 *  7168 Bytes with index= 7172 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155714 cycles, achieve throughput  8065 MB/s
transfer  136 *  7680 Bytes with index= 7684 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 156554 cycles, achieve throughput  8006 MB/s
transfer  127 *  8192 Bytes with index= 8196 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 156591 cycles, achieve throughput  7972 MB/s
transfer 1024 *     1 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20594 cycles, achieve throughput    59 MB/s
transfer 1024 *     2 Bytes with index=   18 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19376 cycles, achieve throughput   126 MB/s
transfer 1024 *     3 Bytes with index=   19 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19385 cycles, achieve throughput   190 MB/s
transfer 1024 *     4 Bytes with index=   20 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  17268 cycles, achieve throughput   284 MB/s
transfer 1024 *     5 Bytes with index=   21 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  18503 cycles, achieve throughput   332 MB/s
transfer 1024 *     6 Bytes with index=   22 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  17501 cycles, achieve throughput   421 MB/s
transfer 1024 *     7 Bytes with index=   23 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  17692 cycles, achieve throughput   486 MB/s
transfer 1024 *     8 Bytes with index=   24 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  16949 cycles, achieve throughput   579 MB/s
transfer 1024 *     9 Bytes with index=   25 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  17829 cycles, achieve throughput   620 MB/s
transfer 1024 *    10 Bytes with index=   26 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  18298 cycles, achieve throughput   671 MB/s
transfer 1024 *    11 Bytes with index=   27 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  18838 cycles, achieve throughput   717 MB/s
transfer 1024 *    12 Bytes with index=   28 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19956 cycles, achieve throughput   738 MB/s
transfer 1024 *    13 Bytes with index=   29 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20279 cycles, achieve throughput   787 MB/s
transfer 1024 *    14 Bytes with index=   30 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21071 cycles, achieve throughput   816 MB/s
transfer 1024 *    15 Bytes with index=   31 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21838 cycles, achieve throughput   844 MB/s
transfer 1024 *    16 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21474 cycles, achieve throughput   915 MB/s
transfer 1024 *    32 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21960 cycles, achieve throughput  1790 MB/s
transfer 1024 *    48 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  15968 cycles, achieve throughput  3693 MB/s
transfer 1024 *    64 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23859 cycles, achieve throughput  3296 MB/s
transfer 1024 *    80 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23663 cycles, achieve throughput  4154 MB/s
transfer 1024 *    96 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  27564 cycles, achieve throughput  4279 MB/s
transfer 1024 *   112 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22076 cycles, achieve throughput  6234 MB/s
transfer 1024 *   128 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31077 cycles, achieve throughput  5061 MB/s
transfer 1024 *   144 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33188 cycles, achieve throughput  5331 MB/s
transfer 1024 *   160 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34954 cycles, achieve throughput  5624 MB/s
transfer 1024 *   176 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28528 cycles, achieve throughput  7580 MB/s
transfer 1024 *   192 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  38366 cycles, achieve throughput  6149 MB/s
transfer 1024 *   208 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  39320 cycles, achieve throughput  6500 MB/s
transfer 1024 *   224 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  40473 cycles, achieve throughput  6800 MB/s
transfer 1024 *   240 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35031 cycles, achieve throughput  8418 MB/s
transfer 1024 *   256 Bytes with index=  272 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  44549 cycles, achieve throughput  7061 MB/s
transfer 1024 *   320 Bytes with index=  336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  50646 cycles, achieve throughput  7764 MB/s
transfer 1024 *   384 Bytes with index=  400 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59333 cycles, achieve throughput  7952 MB/s
transfer 1024 *   448 Bytes with index=  464 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  66238 cycles, achieve throughput  8310 MB/s
transfer 1024 *   512 Bytes with index=  528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  74225 cycles, achieve throughput  8476 MB/s
transfer 1024 *   768 Bytes with index=  784 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 108054 cycles, achieve throughput  8733 MB/s
transfer 1008 *  1024 Bytes with index= 1040 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 139365 cycles, achieve throughput  8887 MB/s
transfer  675 *  1536 Bytes with index= 1552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 139159 cycles, achieve throughput  8940 MB/s
transfer  508 *  2048 Bytes with index= 2064 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 140834 cycles, achieve throughput  8864 MB/s
transfer  407 *  2560 Bytes with index= 2576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 141183 cycles, achieve throughput  8855 MB/s
transfer  339 *  3072 Bytes with index= 3088 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 141849 cycles, achieve throughput  8809 MB/s
transfer  291 *  3584 Bytes with index= 3600 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 143057 cycles, achieve throughput  8748 MB/s
transfer  255 *  4096 Bytes with index= 4112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 143986 cycles, achieve throughput  8704 MB/s
transfer  226 *  4608 Bytes with index= 4624 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 143412 cycles, achieve throughput  8713 MB/s
transfer  204 *  5120 Bytes with index= 5136 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144361 cycles, achieve throughput  8682 MB/s
transfer  185 *  5632 Bytes with index= 5648 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144599 cycles, achieve throughput  8646 MB/s
transfer  170 *  6144 Bytes with index= 6160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144985 cycles, achieve throughput  8644 MB/s
transfer  157 *  6656 Bytes with index= 6672 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145490 cycles, achieve throughput  8619 MB/s
transfer  145 *  7168 Bytes with index= 7184 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144757 cycles, achieve throughput  8616 MB/s
transfer  136 *  7680 Bytes with index= 7696 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145987 cycles, achieve throughput  8585 MB/s
transfer  127 *  8192 Bytes with index= 8208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145761 cycles, achieve throughput  8565 MB/s
transfer 1024 *     1 Bytes with index=   65 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13027 cycles, achieve throughput    94 MB/s
transfer 1024 *     2 Bytes with index=   66 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12865 cycles, achieve throughput   191 MB/s
transfer 1024 *     3 Bytes with index=   67 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13112 cycles, achieve throughput   281 MB/s
transfer 1024 *     4 Bytes with index=   68 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12886 cycles, achieve throughput   381 MB/s
transfer 1024 *     5 Bytes with index=   69 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13259 cycles, achieve throughput   463 MB/s
transfer 1024 *     6 Bytes with index=   70 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13205 cycles, achieve throughput   558 MB/s
transfer 1024 *     7 Bytes with index=   71 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13472 cycles, achieve throughput   638 MB/s
transfer 1024 *     8 Bytes with index=   72 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12848 cycles, achieve throughput   765 MB/s
transfer 1024 *     9 Bytes with index=   73 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13669 cycles, achieve throughput   809 MB/s
transfer 1024 *    10 Bytes with index=   74 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13642 cycles, achieve throughput   900 MB/s
transfer 1024 *    11 Bytes with index=   75 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13781 cycles, achieve throughput   980 MB/s
transfer 1024 *    12 Bytes with index=   76 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13671 cycles, achieve throughput  1078 MB/s
transfer 1024 *    13 Bytes with index=   77 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14026 cycles, achieve throughput  1138 MB/s
transfer 1024 *    14 Bytes with index=   78 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14010 cycles, achieve throughput  1227 MB/s
transfer 1024 *    15 Bytes with index=   79 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14228 cycles, achieve throughput  1295 MB/s
transfer 1024 *    16 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12809 cycles, achieve throughput  1534 MB/s
transfer 1024 *    32 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12873 cycles, achieve throughput  3054 MB/s
transfer 1024 *    48 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  15961 cycles, achieve throughput  3695 MB/s
transfer 1024 *    64 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  15909 cycles, achieve throughput  4943 MB/s
transfer 1024 *    80 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19015 cycles, achieve throughput  5169 MB/s
transfer 1024 *    96 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  18995 cycles, achieve throughput  6210 MB/s
transfer 1024 *   112 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22261 cycles, achieve throughput  6182 MB/s
transfer 1024 *   128 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22190 cycles, achieve throughput  7088 MB/s
transfer 1024 *   144 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26865 cycles, achieve throughput  6586 MB/s
transfer 1024 *   160 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  27038 cycles, achieve throughput  7271 MB/s
transfer 1024 *   176 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30780 cycles, achieve throughput  7026 MB/s
transfer 1024 *   192 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28538 cycles, achieve throughput  8267 MB/s
transfer 1024 *   208 Bytes with index=  272 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33823 cycles, achieve throughput  7556 MB/s
transfer 1024 *   224 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35879 cycles, achieve throughput  7671 MB/s
transfer 1024 *   240 Bytes with index=  304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37495 cycles, achieve throughput  7865 MB/s
transfer 1024 *   256 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35109 cycles, achieve throughput  8959 MB/s
transfer 1024 *   320 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42370 cycles, achieve throughput  9280 MB/s
transfer 1024 *   384 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  50799 cycles, achieve throughput  9288 MB/s
transfer 1024 *   448 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59582 cycles, achieve throughput  9239 MB/s
transfer 1024 *   512 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  68066 cycles, achieve throughput  9243 MB/s
transfer 1024 *   768 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 100734 cycles, achieve throughput  9368 MB/s
transfer  963 *  1024 Bytes with index= 1088 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 126669 cycles, achieve throughput  9341 MB/s
transfer  655 *  1536 Bytes with index= 1600 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127998 cycles, achieve throughput  9432 MB/s
transfer  496 *  2048 Bytes with index= 2112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128730 cycles, achieve throughput  9469 MB/s
transfer  399 *  2560 Bytes with index= 2624 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129728 cycles, achieve throughput  9448 MB/s
transfer  334 *  3072 Bytes with index= 3136 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129632 cycles, achieve throughput  9498 MB/s
transfer  287 *  3584 Bytes with index= 3648 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130285 cycles, achieve throughput  9474 MB/s
transfer  252 *  4096 Bytes with index= 4160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130454 cycles, achieve throughput  9494 MB/s
transfer  224 *  4608 Bytes with index= 4672 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130095 cycles, achieve throughput  9520 MB/s
transfer  202 *  5120 Bytes with index= 5184 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130742 cycles, achieve throughput  9492 MB/s
transfer  184 *  5632 Bytes with index= 5696 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130519 cycles, achieve throughput  9527 MB/s
transfer  168 *  6144 Bytes with index= 6208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130445 cycles, achieve throughput  9495 MB/s
transfer  156 *  6656 Bytes with index= 6720 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130932 cycles, achieve throughput  9516 MB/s
transfer  144 *  7168 Bytes with index= 7232 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130526 cycles, achieve throughput  9489 MB/s
transfer  135 *  7680 Bytes with index= 7744 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130908 cycles, achieve throughput  9504 MB/s
transfer  127 *  8192 Bytes with index= 8256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131453 cycles, achieve throughput  9497 MB/s
EDMA test complete
Test complete
