JTAG ID= 0x0b9a602f. This is a K2E device, version variant = 0
DEVSTAT= 0x00000661. little endian, no boot or I2C slave boot, boot master is ARM core, PLL configuration implies the input clock for core is 100MHz
SmartReflex VID= 46, required core voltage= 0.995V.
Die ID= 0x0600c004, 0x0c00ea85, 0x00000000, 0x79900000
DSP speed grade = 800MHz, ARM speed grade= 800MHz
Enable IRQ and FIQ.
Enable Exception handling...
Initialize main core clock = 100.00MHz/1x12 = 1200MHz
DDR3A initialization
Initialize DDR data rate = 100.000/1*16/4*4= 1600.0 MTS, bus width = 64 bits.
DDR PHY status PGSR0=0xb0000fff.
   83 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c0a0000(MSRAM(strongly ordered)), consumes 1876004 cycles
  126 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 1243360 cycles
  129 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 1216972 cycles
   78 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes 2006791 cycles
  128 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes 1220074 cycles
  129 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 1217460 cycles
  123 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c080000(MSRAM(strongly ordered)), consumes 1270900 cycles
  149 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c0e0000(MSRAM(normal non-cache)), consumes 1052022 cycles
  149 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 1053806 cycles
  131 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes 1193906 cycles
  149 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes 1053430 cycles
  149 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 1054324 cycles
  682 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c080000(MSRAM(strongly ordered)), consumes 230288 cycles
 3223 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 48798 cycles
 4264 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c120000(MSRAM(RA_WB_WA,  in sh)), consumes 36887 cycles
  685 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes 229518 cycles
 2883 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes 54552 cycles
 4274 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 36799 cycles
   50 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c080000(MSRAM(strongly ordered)), consumes 3137503 cycles
   63 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 2482680 cycles
   62 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 2510820 cycles
   36 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes 4264098 cycles
   47 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x80022000(DDR3A(strongly ordered)), consumes 3333718 cycles
   42 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes 3741254 cycles
   61 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 2577566 cycles
   62 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c080000(MSRAM(strongly ordered)), consumes 2505883 cycles
   66 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 2362645 cycles
   66 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 2361941 cycles
   35 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes 4390411 cycles
   52 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes 2979448 cycles
   66 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x88022000(DDR3A(normal non-cache)), consumes 2374086 cycles
   64 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 2438799 cycles
  677 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c080000(MSRAM(strongly ordered)), consumes 232226 cycles
 3109 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 50586 cycles
 3614 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 43520 cycles
  563 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes 278956 cycles
 1459 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes 107788 cycles
 2189 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes 71853 cycles
 2789 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90022000(DDR3A(RA_WB_WA,  in sh)), consumes 56392 cycles
Memory load performance test at 0x0c080000(MSRAM(strongly ordered))
Index=   0  Cycles/LDRD= 12.68
Index=   1  Cycles/LDRD= 12.63
Index=   2  Cycles/LDRD= 15.24
Index=   3  Cycles/LDRD= 15.15
Index=   4  Cycles/LDRD= 15.27
Index=   5  Cycles/LDRD= 15.24
Index=   6  Cycles/LDRD= 12.67
Index=   7  Cycles/LDRD= 15.27
Index=   8  Cycles/LDRD= 12.68
Index=  10  Cycles/LDRD= 15.24
Index=  12  Cycles/LDRD= 15.27
Index=  14  Cycles/LDRD= 12.67
Index=  16  Cycles/LDRD= 12.68
Index=  18  Cycles/LDRD= 15.24
Index=  20  Cycles/LDRD= 15.27
Index=  22  Cycles/LDRD= 12.67
Index=  24  Cycles/LDRD= 12.68
Index=  26  Cycles/LDRD= 15.24
Index=  28  Cycles/LDRD= 15.27
Index=  30  Cycles/LDRD= 12.67
Index=  32  Cycles/LDRD= 12.68
Index=  40  Cycles/LDRD= 12.68
Index=  48  Cycles/LDRD= 12.68
Index=  56  Cycles/LDRD= 12.68
Memory store performance test at 0x0c080000(MSRAM(strongly ordered))
Index=   0  Cycles/STRD= 8.27
Index=   1  Cycles/STRD= 8.02
Index=   2  Cycles/STRD= 7.77
Index=   3  Cycles/STRD= 7.52
Index=   4  Cycles/STRD= 7.27
Index=   5  Cycles/STRD= 7.01
Index=   6  Cycles/STRD= 6.77
Index=   7  Cycles/STRD= 6.52
Index=   8  Cycles/STRD= 6.26
Index=  10  Cycles/STRD= 6.26
Index=  12  Cycles/STRD= 6.26
Index=  14  Cycles/STRD= 6.26
Index=  16  Cycles/STRD= 6.26
Index=  18  Cycles/STRD= 6.26
Index=  20  Cycles/STRD= 6.26
Index=  22  Cycles/STRD= 6.26
Index=  24  Cycles/STRD= 6.26
Index=  26  Cycles/STRD= 6.26
Index=  28  Cycles/STRD= 6.26
Index=  30  Cycles/STRD= 6.26
Index=  32  Cycles/STRD= 6.26
Index=  40  Cycles/STRD= 6.27
Index=  48  Cycles/STRD= 6.27
Index=  56  Cycles/STRD= 6.27
Memory load performance test at 0x0c0c0000(MSRAM(normal non-cache))
Index=   0  Cycles/LDRD= 62.26
Index=   1  Cycles/LDRD= 64.51
Index=   2  Cycles/LDRD= 64.74
Index=   3  Cycles/LDRD= 64.86
Index=   4  Cycles/LDRD= 65.42
Index=   5  Cycles/LDRD= 64.87
Index=   6  Cycles/LDRD= 64.04
Index=   7  Cycles/LDRD= 64.53
Index=   8  Cycles/LDRD= 62.26
Index=  10  Cycles/LDRD= 64.74
Index=  12  Cycles/LDRD= 64.97
Index=  14  Cycles/LDRD= 64.13
Index=  16  Cycles/LDRD= 62.30
Index=  18  Cycles/LDRD= 64.66
Index=  20  Cycles/LDRD= 65.38
Index=  22  Cycles/LDRD= 64.07
Index=  24  Cycles/LDRD= 62.24
Index=  26  Cycles/LDRD= 64.74
Index=  28  Cycles/LDRD= 65.24
Index=  30  Cycles/LDRD= 64.02
Index=  32  Cycles/LDRD= 62.24
Index=  40  Cycles/LDRD= 62.24
Index=  48  Cycles/LDRD= 62.24
Index=  56  Cycles/LDRD= 62.24
Memory store performance test at 0x0c0c0000(MSRAM(normal non-cache))
Index=   0  Cycles/STRD= 1.93
Index=   1  Cycles/STRD= 2.86
Index=   2  Cycles/STRD= 5.71
Index=   3  Cycles/STRD= 4.79
Index=   4  Cycles/STRD= 4.71
Index=   5  Cycles/STRD= 4.51
Index=   6  Cycles/STRD= 4.49
Index=   7  Cycles/STRD= 4.49
Index=   8  Cycles/STRD= 4.43
Index=  10  Cycles/STRD= 4.49
Index=  12  Cycles/STRD= 4.49
Index=  14  Cycles/STRD= 4.47
Index=  16  Cycles/STRD= 4.44
Index=  18  Cycles/STRD= 4.49
Index=  20  Cycles/STRD= 4.49
Index=  22  Cycles/STRD= 4.47
Index=  24  Cycles/STRD= 4.43
Index=  26  Cycles/STRD= 4.49
Index=  28  Cycles/STRD= 4.49
Index=  30  Cycles/STRD= 4.47
Index=  32  Cycles/STRD= 4.28
Index=  40  Cycles/STRD= 4.44
Index=  48  Cycles/STRD= 4.45
Index=  56  Cycles/STRD= 4.44
Memory load performance test at 0x0c100000(MSRAM(RA_WB_WA,  in sh))
Index=   0  Cycles/LDRD= 1.33
Index=   1  Cycles/LDRD= 2.53
Index=   2  Cycles/LDRD= 3.25
Index=   3  Cycles/LDRD= 4.26
Index=   4  Cycles/LDRD= 6.25
Index=   5  Cycles/LDRD= 7.96
Index=   6  Cycles/LDRD= 9.17
Index=   7  Cycles/LDRD= 10.18
Index=   8  Cycles/LDRD= 11.17
Index=  10  Cycles/LDRD= 11.55
Index=  12  Cycles/LDRD= 11.67
Index=  14  Cycles/LDRD= 12.22
Index=  16  Cycles/LDRD= 16.17
Index=  18  Cycles/LDRD= 12.93
Index=  20  Cycles/LDRD= 12.57
Index=  22  Cycles/LDRD= 13.41
Index=  24  Cycles/LDRD= 12.86
Index=  26  Cycles/LDRD= 12.68
Index=  28  Cycles/LDRD= 13.16
Index=  30  Cycles/LDRD= 15.02
Index=  32  Cycles/LDRD= 26.72
Index=  40  Cycles/LDRD= 13.05
Index=  48  Cycles/LDRD= 13.63
Index=  56  Cycles/LDRD= 11.72
Memory store performance test at 0x0c100000(MSRAM(RA_WB_WA,  in sh))
Index=   0  Cycles/STRD= 1.28
Index=   1  Cycles/STRD= 1.79
Index=   2  Cycles/STRD= 3.29
Index=   3  Cycles/STRD= 4.45
Index=   4  Cycles/STRD= 6.48
Index=   5  Cycles/STRD= 7.28
Index=   6  Cycles/STRD= 8.48
Index=   7  Cycles/STRD= 10.21
Index=   8  Cycles/STRD= 11.93
Index=  10  Cycles/STRD= 11.90
Index=  12  Cycles/STRD= 11.23
Index=  14  Cycles/STRD= 11.63
Index=  16  Cycles/STRD= 16.93
Index=  18  Cycles/STRD= 12.41
Index=  20  Cycles/STRD= 12.20
Index=  22  Cycles/STRD= 12.35
Index=  24  Cycles/STRD= 12.83
Index=  26  Cycles/STRD= 12.25
Index=  28  Cycles/STRD= 12.22
Index=  30  Cycles/STRD= 12.14
Index=  32  Cycles/STRD= 26.34
Index=  40  Cycles/STRD= 12.45
Index=  48  Cycles/STRD= 13.78
Index=  56  Cycles/STRD= 12.34
Memory load performance test at 0x80000000(DDR3A(strongly ordered))
Index=   0  Cycles/LDRD= 24.75
Index=   1  Cycles/LDRD= 24.51
Index=   2  Cycles/LDRD= 24.47
Index=   3  Cycles/LDRD= 24.60
Index=   4  Cycles/LDRD= 24.51
Index=   5  Cycles/LDRD= 24.52
Index=   6  Cycles/LDRD= 24.55
Index=   7  Cycles/LDRD= 24.52
Index=   8  Cycles/LDRD= 24.62
Index=  10  Cycles/LDRD= 24.56
Index=  12  Cycles/LDRD= 24.72
Index=  14  Cycles/LDRD= 24.62
Index=  16  Cycles/LDRD= 24.60
Index=  18  Cycles/LDRD= 24.62
Index=  20  Cycles/LDRD= 24.54
Index=  22  Cycles/LDRD= 24.56
Index=  24  Cycles/LDRD= 24.71
Index=  26  Cycles/LDRD= 24.57
Index=  28  Cycles/LDRD= 24.91
Index=  30  Cycles/LDRD= 24.74
Index=  32  Cycles/LDRD= 24.71
Index=  40  Cycles/LDRD= 25.00
Index=  48  Cycles/LDRD= 24.79
Index=  56  Cycles/LDRD= 25.60
Index=  64  Cycles/LDRD= 25.05
Index=  96  Cycles/LDRD= 25.11
Index= 128  Cycles/LDRD= 25.93
Index= 192  Cycles/LDRD= 26.03
Index= 256  Cycles/LDRD= 27.33
Index= 384  Cycles/LDRD= 27.40
Index= 512  Cycles/LDRD= 30.37
Index= 768  Cycles/LDRD= 30.43
Index=1024  Cycles/LDRD= 30.49
Index=1536  Cycles/LDRD= 30.49
Index=2048  Cycles/LDRD= 30.45
Index=3072  Cycles/LDRD= 30.38
Index=4096  Cycles/LDRD= 30.54
Index=6144  Cycles/LDRD= 30.55
Index=8192  Cycles/LDRD= 30.82
Index=12288  Cycles/LDRD= 30.47
Index=16384  Cycles/LDRD= 60.60
Index=20480  Cycles/LDRD= 30.47
Index=24576  Cycles/LDRD= 30.80
Index=28672  Cycles/LDRD= 30.65
Memory store performance test at 0x80000000(DDR3A(strongly ordered))
Index=   0  Cycles/STRD= 12.16
Index=   1  Cycles/STRD= 12.29
Index=   2  Cycles/STRD= 12.16
Index=   3  Cycles/STRD= 12.16
Index=   4  Cycles/STRD= 12.16
Index=   5  Cycles/STRD= 12.65
Index=   6  Cycles/STRD= 12.16
Index=   7  Cycles/STRD= 12.29
Index=   8  Cycles/STRD= 12.16
Index=  10  Cycles/STRD= 12.17
Index=  12  Cycles/STRD= 12.16
Index=  14  Cycles/STRD= 12.30
Index=  16  Cycles/STRD= 12.17
Index=  18  Cycles/STRD= 12.18
Index=  20  Cycles/STRD= 12.17
Index=  22  Cycles/STRD= 12.18
Index=  24  Cycles/STRD= 12.31
Index=  26  Cycles/STRD= 12.18
Index=  28  Cycles/STRD= 12.17
Index=  30  Cycles/STRD= 12.31
Index=  32  Cycles/STRD= 12.18
Index=  40  Cycles/STRD= 12.19
Index=  48  Cycles/STRD= 12.33
Index=  56  Cycles/STRD= 12.21
Index=  64  Cycles/STRD= 12.21
Index=  96  Cycles/STRD= 12.25
Index= 128  Cycles/STRD= 12.28
Index= 192  Cycles/STRD= 12.49
Index= 256  Cycles/STRD= 12.42
Index= 384  Cycles/STRD= 12.56
Index= 512  Cycles/STRD= 12.70
Index= 768  Cycles/STRD= 12.99
Index=1024  Cycles/STRD= 13.26
Index=1536  Cycles/STRD= 13.83
Index=2048  Cycles/STRD= 14.36
Index=3072  Cycles/STRD= 15.47
Index=4096  Cycles/STRD= 19.50
Index=6144  Cycles/STRD= 18.78
Index=8192  Cycles/STRD= 38.77
Index=12288  Cycles/STRD= 21.10
Index=16384  Cycles/STRD= 78.60
Index=20480  Cycles/STRD= 19.50
Index=24576  Cycles/STRD= 38.79
Index=28672  Cycles/STRD= 20.99
Memory load performance test at 0x88000000(DDR3A(normal non-cache))
Index=   0  Cycles/LDRD= 141.82
Index=   1  Cycles/LDRD= 143.43
Index=   2  Cycles/LDRD= 143.35
Index=   3  Cycles/LDRD= 143.28
Index=   4  Cycles/LDRD= 143.42
Index=   5  Cycles/LDRD= 143.21
Index=   6  Cycles/LDRD= 143.79
Index=   7  Cycles/LDRD= 143.69
Index=   8  Cycles/LDRD= 142.57
Index=  10  Cycles/LDRD= 144.17
Index=  12  Cycles/LDRD= 143.34
Index=  14  Cycles/LDRD= 143.67
Index=  16  Cycles/LDRD= 142.40
Index=  18  Cycles/LDRD= 144.00
Index=  20  Cycles/LDRD= 144.65
Index=  22  Cycles/LDRD= 143.96
Index=  24  Cycles/LDRD= 142.26
Index=  26  Cycles/LDRD= 145.25
Index=  28  Cycles/LDRD= 144.28
Index=  30  Cycles/LDRD= 144.83
Index=  32  Cycles/LDRD= 142.09
Index=  40  Cycles/LDRD= 142.44
Index=  48  Cycles/LDRD= 143.06
Index=  56  Cycles/LDRD= 143.06
Index=  64  Cycles/LDRD= 142.81
Index=  96  Cycles/LDRD= 143.28
Index= 128  Cycles/LDRD= 145.30
Index= 192  Cycles/LDRD= 145.89
Index= 256  Cycles/LDRD= 146.97
Index= 384  Cycles/LDRD= 151.49
Index= 512  Cycles/LDRD= 155.76
Index= 768  Cycles/LDRD= 163.60
Index=1024  Cycles/LDRD= 173.47
Index=1536  Cycles/LDRD= 173.63
Index=2048  Cycles/LDRD= 176.11
Index=3072  Cycles/LDRD= 173.17
Index=4096  Cycles/LDRD= 177.63
Index=6144  Cycles/LDRD= 176.22
Index=8192  Cycles/LDRD= 178.45
Index=12288  Cycles/LDRD= 177.63
Index=16384  Cycles/LDRD= 178.83
Index=20480  Cycles/LDRD= 177.29
Index=24576  Cycles/LDRD= 178.70
Index=28672  Cycles/LDRD= 177.78
Memory store performance test at 0x88000000(DDR3A(normal non-cache))
Index=   0  Cycles/STRD= 2.11
Index=   1  Cycles/STRD= 3.25
Index=   2  Cycles/STRD= 6.26
Index=   3  Cycles/STRD= 6.18
Index=   4  Cycles/STRD= 6.17
Index=   5  Cycles/STRD= 6.17
Index=   6  Cycles/STRD= 6.17
Index=   7  Cycles/STRD= 6.31
Index=   8  Cycles/STRD= 6.18
Index=  10  Cycles/STRD= 6.17
Index=  12  Cycles/STRD= 6.18
Index=  14  Cycles/STRD= 6.17
Index=  16  Cycles/STRD= 6.17
Index=  18  Cycles/STRD= 6.19
Index=  20  Cycles/STRD= 6.19
Index=  22  Cycles/STRD= 6.19
Index=  24  Cycles/STRD= 6.23
Index=  26  Cycles/STRD= 6.19
Index=  28  Cycles/STRD= 6.19
Index=  30  Cycles/STRD= 6.18
Index=  32  Cycles/STRD= 6.22
Index=  40  Cycles/STRD= 6.21
Index=  48  Cycles/STRD= 6.21
Index=  56  Cycles/STRD= 6.23
Index=  64  Cycles/STRD= 6.33
Index=  96  Cycles/STRD= 6.82
Index= 128  Cycles/STRD= 6.63
Index= 192  Cycles/STRD= 6.56
Index= 256  Cycles/STRD= 6.51
Index= 384  Cycles/STRD= 6.60
Index= 512  Cycles/STRD= 8.26
Index= 768  Cycles/STRD= 9.92
Index=1024  Cycles/STRD= 12.21
Index=1536  Cycles/STRD= 12.87
Index=2048  Cycles/STRD= 13.28
Index=3072  Cycles/STRD= 12.29
Index=4096  Cycles/STRD= 20.02
Index=6144  Cycles/STRD= 13.67
Index=8192  Cycles/STRD= 36.47
Index=12288  Cycles/STRD= 20.61
Index=16384  Cycles/STRD= 71.37
Index=20480  Cycles/STRD= 20.62
Index=24576  Cycles/STRD= 36.30
Index=28672  Cycles/STRD= 20.23
Memory load performance test at 0x90000000(DDR3A(RA_WB_WA,  in sh))
Index=   0  Cycles/LDRD= 1.49
Index=   1  Cycles/LDRD= 3.19
Index=   2  Cycles/LDRD= 4.78
Index=   3  Cycles/LDRD= 6.78
Index=   4  Cycles/LDRD= 8.98
Index=   5  Cycles/LDRD= 12.06
Index=   6  Cycles/LDRD= 12.81
Index=   7  Cycles/LDRD= 15.09
Index=   8  Cycles/LDRD= 16.46
Index=  10  Cycles/LDRD= 17.16
Index=  12  Cycles/LDRD= 17.58
Index=  14  Cycles/LDRD= 17.92
Index=  16  Cycles/LDRD= 19.93
Index=  18  Cycles/LDRD= 17.91
Index=  20  Cycles/LDRD= 18.00
Index=  22  Cycles/LDRD= 19.12
Index=  24  Cycles/LDRD= 18.62
Index=  26  Cycles/LDRD= 20.24
Index=  28  Cycles/LDRD= 19.63
Index=  30  Cycles/LDRD= 21.22
Index=  32  Cycles/LDRD= 30.57
Index=  40  Cycles/LDRD= 20.21
Index=  48  Cycles/LDRD= 23.78
Index=  56  Cycles/LDRD= 25.01
Index=  64  Cycles/LDRD= 26.20
Index=  96  Cycles/LDRD= 26.33
Index= 128  Cycles/LDRD= 27.24
Index= 192  Cycles/LDRD= 27.47
Index= 256  Cycles/LDRD= 28.48
Index= 384  Cycles/LDRD= 28.59
Index= 512  Cycles/LDRD= 39.05
Index= 768  Cycles/LDRD= 31.30
Index=1024  Cycles/LDRD= 59.74
Index=1536  Cycles/LDRD= 39.91
Index=2048  Cycles/LDRD= 95.65
Index=3072  Cycles/LDRD= 58.77
Index=4096  Cycles/LDRD= 95.94
Index=6144  Cycles/LDRD= 99.23
Index=8192  Cycles/LDRD= 102.56
Index=12288  Cycles/LDRD= 103.53
Index=16384  Cycles/LDRD= 104.08
Index=20480  Cycles/LDRD= 96.89
Index=24576  Cycles/LDRD= 102.92
Index=28672  Cycles/LDRD= 103.17
Memory store performance test at 0x90000000(DDR3A(RA_WB_WA,  in sh))
Index=   0  Cycles/STRD= 1.28
Index=   1  Cycles/STRD= 2.11
Index=   2  Cycles/STRD= 5.11
Index=   3  Cycles/STRD= 6.50
Index=   4  Cycles/STRD= 8.54
Index=   5  Cycles/STRD= 12.99
Index=   6  Cycles/STRD= 14.64
Index=   7  Cycles/STRD= 18.74
Index=   8  Cycles/STRD= 17.47
Index=  10  Cycles/STRD= 17.35
Index=  12  Cycles/STRD= 17.67
Index=  14  Cycles/STRD= 19.07
Index=  16  Cycles/STRD= 21.46
Index=  18  Cycles/STRD= 17.96
Index=  20  Cycles/STRD= 19.19
Index=  22  Cycles/STRD= 19.21
Index=  24  Cycles/STRD= 19.94
Index=  26  Cycles/STRD= 20.62
Index=  28  Cycles/STRD= 20.09
Index=  30  Cycles/STRD= 19.95
Index=  32  Cycles/STRD= 29.64
Index=  40  Cycles/STRD= 24.16
Index=  48  Cycles/STRD= 25.84
Index=  56  Cycles/STRD= 25.94
Index=  64  Cycles/STRD= 26.71
Index=  96  Cycles/STRD= 27.32
Index= 128  Cycles/STRD= 28.14
Index= 192  Cycles/STRD= 28.15
Index= 256  Cycles/STRD= 34.40
Index= 384  Cycles/STRD= 29.61
Index= 512  Cycles/STRD= 49.01
Index= 768  Cycles/STRD= 35.47
Index=1024  Cycles/STRD= 59.28
Index=1536  Cycles/STRD= 53.97
Index=2048  Cycles/STRD= 111.84
Index=3072  Cycles/STRD= 75.37
Index=4096  Cycles/STRD= 121.29
Index=6144  Cycles/STRD= 111.59
Index=8192  Cycles/STRD= 133.49
Index=12288  Cycles/STRD= 120.71
Index=16384  Cycles/STRD= 153.79
Index=20480  Cycles/STRD= 119.88
Index=24576  Cycles/STRD= 133.48
Index=28672  Cycles/STRD= 120.55
Throughput test with EDMA0 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15718 cycles, achieve throughput 10006 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15612 cycles, achieve throughput 10074 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15695 cycles, achieve throughput 10021 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16331 cycles, achieve throughput  9631 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16208 cycles, achieve throughput  9704 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16238 cycles, achieve throughput  9686 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15659 cycles, achieve throughput 10044 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15654 cycles, achieve throughput 10047 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15659 cycles, achieve throughput 10044 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16318 cycles, achieve throughput  9638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16346 cycles, achieve throughput  9622 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16324 cycles, achieve throughput  9635 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15663 cycles, achieve throughput 10041 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15653 cycles, achieve throughput 10048 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15653 cycles, achieve throughput 10048 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16317 cycles, achieve throughput  9639 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16298 cycles, achieve throughput  9650 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16346 cycles, achieve throughput  9622 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  20043 cycles, achieve throughput  7847 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  19999 cycles, achieve throughput  7864 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  19995 cycles, achieve throughput  7866 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  52527 cycles, achieve throughput  2994 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  52857 cycles, achieve throughput  2975 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  50805 cycles, achieve throughput  3095 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  20019 cycles, achieve throughput  7856 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20219 cycles, achieve throughput  7779 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  19941 cycles, achieve throughput  7887 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  50623 cycles, achieve throughput  3107 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  51488 cycles, achieve throughput  3054 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  51163 cycles, achieve throughput  3074 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  20722 cycles, achieve throughput  7590 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20776 cycles, achieve throughput  7570 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20998 cycles, achieve throughput  7490 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  51808 cycles, achieve throughput  3035 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  52092 cycles, achieve throughput  3019 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  52385 cycles, achieve throughput  3002 MB/s
Throughput test with EDMA0 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15657 cycles, achieve throughput 10045 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15671 cycles, achieve throughput 10036 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15673 cycles, achieve throughput 10035 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16291 cycles, achieve throughput  9654 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16233 cycles, achieve throughput  9689 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16318 cycles, achieve throughput  9638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15654 cycles, achieve throughput 10047 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15647 cycles, achieve throughput 10052 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15656 cycles, achieve throughput 10046 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16251 cycles, achieve throughput  9678 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16241 cycles, achieve throughput  9684 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16340 cycles, achieve throughput  9625 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15666 cycles, achieve throughput 10039 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15669 cycles, achieve throughput 10038 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15663 cycles, achieve throughput 10041 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16345 cycles, achieve throughput  9622 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16417 cycles, achieve throughput  9580 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16338 cycles, achieve throughput  9627 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  20004 cycles, achieve throughput  7862 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20039 cycles, achieve throughput  7849 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20032 cycles, achieve throughput  7851 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  51837 cycles, achieve throughput  3034 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  51053 cycles, achieve throughput  3080 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  51519 cycles, achieve throughput  3052 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  19928 cycles, achieve throughput  7892 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  19958 cycles, achieve throughput  7880 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20029 cycles, achieve throughput  7852 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  49589 cycles, achieve throughput  3171 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  52933 cycles, achieve throughput  2971 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  52652 cycles, achieve throughput  2987 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  20729 cycles, achieve throughput  7587 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20720 cycles, achieve throughput  7591 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20556 cycles, achieve throughput  7651 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  52493 cycles, achieve throughput  2996 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  52316 cycles, achieve throughput  3006 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  52942 cycles, achieve throughput  2970 MB/s
Throughput test with EDMA1 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25335 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25336 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25246 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25224 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25342 cycles, achieve throughput  6206 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25344 cycles, achieve throughput  6206 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25254 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25225 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25340 cycles, achieve throughput  6207 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25333 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27572 cycles, achieve throughput  5704 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27561 cycles, achieve throughput  5706 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27558 cycles, achieve throughput  5707 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  58829 cycles, achieve throughput  2673 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  58635 cycles, achieve throughput  2682 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59550 cycles, achieve throughput  2641 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27480 cycles, achieve throughput  5723 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27558 cycles, achieve throughput  5707 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27519 cycles, achieve throughput  5715 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  58415 cycles, achieve throughput  2692 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58504 cycles, achieve throughput  2688 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59102 cycles, achieve throughput  2661 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28217 cycles, achieve throughput  5574 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28339 cycles, achieve throughput  5550 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28541 cycles, achieve throughput  5510 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  58700 cycles, achieve throughput  2679 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  59677 cycles, achieve throughput  2635 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  59134 cycles, achieve throughput  2659 MB/s
Throughput test with EDMA1 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25225 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25255 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25336 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27240 cycles, achieve throughput  5774 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27587 cycles, achieve throughput  5701 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27369 cycles, achieve throughput  5746 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  58459 cycles, achieve throughput  2690 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59323 cycles, achieve throughput  2651 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58987 cycles, achieve throughput  2666 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27568 cycles, achieve throughput  5705 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27541 cycles, achieve throughput  5710 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27360 cycles, achieve throughput  5748 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59406 cycles, achieve throughput  2647 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58641 cycles, achieve throughput  2682 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58947 cycles, achieve throughput  2668 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28136 cycles, achieve throughput  5590 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28437 cycles, achieve throughput  5531 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28101 cycles, achieve throughput  5597 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  59567 cycles, achieve throughput  2640 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  59741 cycles, achieve throughput  2632 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  59540 cycles, achieve throughput  2641 MB/s
Throughput test with EDMA1 TC2
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25223 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25326 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25246 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25335 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25333 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25254 cycles, achieve throughput  6228 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27475 cycles, achieve throughput  5724 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27341 cycles, achieve throughput  5752 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27578 cycles, achieve throughput  5703 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59016 cycles, achieve throughput  2665 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  58988 cycles, achieve throughput  2666 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58158 cycles, achieve throughput  2704 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27569 cycles, achieve throughput  5705 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27538 cycles, achieve throughput  5711 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27451 cycles, achieve throughput  5729 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59302 cycles, achieve throughput  2652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58969 cycles, achieve throughput  2667 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58370 cycles, achieve throughput  2694 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28126 cycles, achieve throughput  5592 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28200 cycles, achieve throughput  5577 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28448 cycles, achieve throughput  5528 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  59322 cycles, achieve throughput  2651 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  59069 cycles, achieve throughput  2662 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  59048 cycles, achieve throughput  2663 MB/s
Throughput test with EDMA1 TC3
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25250 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25335 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25337 cycles, achieve throughput  6207 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25235 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25336 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27647 cycles, achieve throughput  5689 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27532 cycles, achieve throughput  5712 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27563 cycles, achieve throughput  5706 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  58274 cycles, achieve throughput  2699 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  58871 cycles, achieve throughput  2671 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58472 cycles, achieve throughput  2689 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27239 cycles, achieve throughput  5774 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27653 cycles, achieve throughput  5687 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27648 cycles, achieve throughput  5688 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59076 cycles, achieve throughput  2662 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58951 cycles, achieve throughput  2668 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58400 cycles, achieve throughput  2693 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28015 cycles, achieve throughput  5614 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28448 cycles, achieve throughput  5528 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28483 cycles, achieve throughput  5522 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  59884 cycles, achieve throughput  2626 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  59414 cycles, achieve throughput  2647 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  59953 cycles, achieve throughput  2623 MB/s
Throughput test with EDMA2 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25225 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25335 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25246 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25337 cycles, achieve throughput  6207 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25223 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25246 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25335 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27587 cycles, achieve throughput  5701 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27631 cycles, achieve throughput  5692 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27495 cycles, achieve throughput  5720 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  58357 cycles, achieve throughput  2695 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  58768 cycles, achieve throughput  2676 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58512 cycles, achieve throughput  2688 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27561 cycles, achieve throughput  5706 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27574 cycles, achieve throughput  5704 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27553 cycles, achieve throughput  5708 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  58739 cycles, achieve throughput  2677 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58678 cycles, achieve throughput  2680 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58807 cycles, achieve throughput  2674 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28432 cycles, achieve throughput  5532 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28363 cycles, achieve throughput  5545 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28218 cycles, achieve throughput  5573 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  58611 cycles, achieve throughput  2683 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  58698 cycles, achieve throughput  2679 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  59413 cycles, achieve throughput  2647 MB/s
Throughput test with EDMA2 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25255 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25240 cycles, achieve throughput  6231 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25336 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25224 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25347 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25334 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27573 cycles, achieve throughput  5704 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27567 cycles, achieve throughput  5705 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27658 cycles, achieve throughput  5686 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59010 cycles, achieve throughput  2665 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  58806 cycles, achieve throughput  2674 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58622 cycles, achieve throughput  2683 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27566 cycles, achieve throughput  5705 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27350 cycles, achieve throughput  5750 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27247 cycles, achieve throughput  5772 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  58929 cycles, achieve throughput  2669 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58321 cycles, achieve throughput  2696 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58602 cycles, achieve throughput  2683 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28401 cycles, achieve throughput  5538 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28476 cycles, achieve throughput  5523 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28311 cycles, achieve throughput  5555 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  59365 cycles, achieve throughput  2649 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  58966 cycles, achieve throughput  2667 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  58688 cycles, achieve throughput  2680 MB/s
Throughput test with EDMA2 TC2
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25223 cycles, achieve throughput  6235 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25342 cycles, achieve throughput  6206 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25240 cycles, achieve throughput  6231 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25335 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25337 cycles, achieve throughput  6207 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25255 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27533 cycles, achieve throughput  5712 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27351 cycles, achieve throughput  5750 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27539 cycles, achieve throughput  5711 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  58814 cycles, achieve throughput  2674 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  58460 cycles, achieve throughput  2690 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58873 cycles, achieve throughput  2671 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27642 cycles, achieve throughput  5690 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27465 cycles, achieve throughput  5726 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27567 cycles, achieve throughput  5705 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  58300 cycles, achieve throughput  2697 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58634 cycles, achieve throughput  2682 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58718 cycles, achieve throughput  2678 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28226 cycles, achieve throughput  5572 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28307 cycles, achieve throughput  5556 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28195 cycles, achieve throughput  5578 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  59784 cycles, achieve throughput  2630 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  59068 cycles, achieve throughput  2662 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  59756 cycles, achieve throughput  2632 MB/s
Throughput test with EDMA2 TC3
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25333 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25336 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25248 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25255 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25247 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25249 cycles, achieve throughput  6229 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25239 cycles, achieve throughput  6231 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25233 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25234 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27528 cycles, achieve throughput  5713 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27560 cycles, achieve throughput  5707 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27412 cycles, achieve throughput  5737 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  58083 cycles, achieve throughput  2707 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59045 cycles, achieve throughput  2663 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  58614 cycles, achieve throughput  2683 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27591 cycles, achieve throughput  5700 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27638 cycles, achieve throughput  5690 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27477 cycles, achieve throughput  5724 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  58776 cycles, achieve throughput  2676 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  58785 cycles, achieve throughput  2675 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59425 cycles, achieve throughput  2646 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28349 cycles, achieve throughput  5548 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28340 cycles, achieve throughput  5549 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28322 cycles, achieve throughput  5553 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  60281 cycles, achieve throughput  2609 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  59687 cycles, achieve throughput  2635 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  58710 cycles, achieve throughput  2679 MB/s
Throughput test with EDMA3 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25213 cycles, achieve throughput  6238 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25230 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25231 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25392 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25281 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25281 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25230 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25232 cycles, achieve throughput  6233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25229 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25272 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25274 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25281 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25230 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25237 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25228 cycles, achieve throughput  6234 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25287 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25281 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25288 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28829 cycles, achieve throughput  5455 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28768 cycles, achieve throughput  5467 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28791 cycles, achieve throughput  5463 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59444 cycles, achieve throughput  2645 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59477 cycles, achieve throughput  2644 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59236 cycles, achieve throughput  2655 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28673 cycles, achieve throughput  5485 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28732 cycles, achieve throughput  5474 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28798 cycles, achieve throughput  5461 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  59572 cycles, achieve throughput  2640 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  59724 cycles, achieve throughput  2633 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59895 cycles, achieve throughput  2626 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  29357 cycles, achieve throughput  5357 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29490 cycles, achieve throughput  5333 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29527 cycles, achieve throughput  5326 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  60350 cycles, achieve throughput  2606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  60144 cycles, achieve throughput  2615 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  60335 cycles, achieve throughput  2606 MB/s
Throughput test with EDMA3 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25237 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25237 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25235 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25346 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25347 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25368 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25236 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25331 cycles, achieve throughput  6209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25235 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25348 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25239 cycles, achieve throughput  6231 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25352 cycles, achieve throughput  6204 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25236 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25243 cycles, achieve throughput  6230 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25237 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25238 cycles, achieve throughput  6232 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25351 cycles, achieve throughput  6204 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25360 cycles, achieve throughput  6202 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28703 cycles, achieve throughput  5479 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28769 cycles, achieve throughput  5467 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28804 cycles, achieve throughput  5460 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  59935 cycles, achieve throughput  2624 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59897 cycles, achieve throughput  2625 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60269 cycles, achieve throughput  2609 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28813 cycles, achieve throughput  5458 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28693 cycles, achieve throughput  5481 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28856 cycles, achieve throughput  5450 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  60415 cycles, achieve throughput  2603 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  59748 cycles, achieve throughput  2632 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  59978 cycles, achieve throughput  2622 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  29542 cycles, achieve throughput  5324 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29706 cycles, achieve throughput  5294 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29526 cycles, achieve throughput  5327 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  60876 cycles, achieve throughput  2583 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  60858 cycles, achieve throughput  2584 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  60655 cycles, achieve throughput  2593 MB/s
Throughput test with EDMA4 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15672 cycles, achieve throughput 10036 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15674 cycles, achieve throughput 10034 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15658 cycles, achieve throughput 10045 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16343 cycles, achieve throughput  9624 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16416 cycles, achieve throughput  9581 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16343 cycles, achieve throughput  9624 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15653 cycles, achieve throughput 10048 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15659 cycles, achieve throughput 10044 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15668 cycles, achieve throughput 10038 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16258 cycles, achieve throughput  9674 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16330 cycles, achieve throughput  9631 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16255 cycles, achieve throughput  9676 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15672 cycles, achieve throughput 10036 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15654 cycles, achieve throughput 10047 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15663 cycles, achieve throughput 10041 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16326 cycles, achieve throughput  9634 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16297 cycles, achieve throughput  9651 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16256 cycles, achieve throughput  9675 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  19968 cycles, achieve throughput  7876 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20005 cycles, achieve throughput  7862 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20014 cycles, achieve throughput  7858 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  51311 cycles, achieve throughput  3065 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  50929 cycles, achieve throughput  3088 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  51698 cycles, achieve throughput  3042 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  20151 cycles, achieve throughput  7805 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20028 cycles, achieve throughput  7853 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20270 cycles, achieve throughput  7759 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  50867 cycles, achieve throughput  3092 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  52347 cycles, achieve throughput  3004 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  51059 cycles, achieve throughput  3080 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  20696 cycles, achieve throughput  7599 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20801 cycles, achieve throughput  7561 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20602 cycles, achieve throughput  7634 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  52644 cycles, achieve throughput  2987 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  54515 cycles, achieve throughput  2885 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  51614 cycles, achieve throughput  3047 MB/s
Throughput test with EDMA4 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15655 cycles, achieve throughput 10047 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15640 cycles, achieve throughput 10056 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15662 cycles, achieve throughput 10042 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16339 cycles, achieve throughput  9626 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16258 cycles, achieve throughput  9674 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16173 cycles, achieve throughput  9725 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15655 cycles, achieve throughput 10047 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15672 cycles, achieve throughput 10036 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15671 cycles, achieve throughput 10036 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16319 cycles, achieve throughput  9638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16235 cycles, achieve throughput  9688 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16209 cycles, achieve throughput  9703 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15657 cycles, achieve throughput 10045 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15654 cycles, achieve throughput 10047 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15653 cycles, achieve throughput 10048 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16345 cycles, achieve throughput  9622 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16319 cycles, achieve throughput  9638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16210 cycles, achieve throughput  9703 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  19911 cycles, achieve throughput  7899 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  19913 cycles, achieve throughput  7898 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  19971 cycles, achieve throughput  7875 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  51026 cycles, achieve throughput  3082 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  50996 cycles, achieve throughput  3084 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  52015 cycles, achieve throughput  3023 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  20106 cycles, achieve throughput  7822 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20021 cycles, achieve throughput  7856 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  19970 cycles, achieve throughput  7876 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  51256 cycles, achieve throughput  3068 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  50853 cycles, achieve throughput  3092 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  51675 cycles, achieve throughput  3043 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  20955 cycles, achieve throughput  7505 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20682 cycles, achieve throughput  7604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20535 cycles, achieve throughput  7659 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  52946 cycles, achieve throughput  2970 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  53350 cycles, achieve throughput  2948 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  52497 cycles, achieve throughput  2996 MB/s
EDMA ACNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    601 cycles, achieve throughput     1 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    584 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    10 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    12 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    14 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    16 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput    18 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput    20 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    585 cycles, achieve throughput    22 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    24 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput    26 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    28 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    30 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    32 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    585 cycles, achieve throughput    65 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    97 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   129 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput   162 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput   196 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput   226 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput   250 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput   281 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    611 cycles, achieve throughput   314 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   357 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput   375 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    610 cycles, achieve throughput   409 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput   437 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput   469 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   506 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    610 cycles, achieve throughput   566 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   632 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   695 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   752 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   815 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   885 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   941 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput  1034 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    608 cycles, achieve throughput  1136 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput  1252 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput  1380 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput  1503 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput  1626 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    611 cycles, achieve throughput  1759 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    617 cycles, achieve throughput  1867 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput  2007 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    723 cycles, achieve throughput  1912 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    714 cycles, achieve throughput  2151 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    693 cycles, achieve throughput  2438 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    693 cycles, achieve throughput  2659 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    808 cycles, achieve throughput  2471 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    809 cycles, achieve throughput  2658 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    828 cycles, achieve throughput  2782 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    823 cycles, achieve throughput  2986 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    805 cycles, achieve throughput  3434 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    808 cycles, achieve throughput  3801 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    952 cycles, achieve throughput  3549 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    951 cycles, achieve throughput  3876 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1034 cycles, achieve throughput  3862 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1031 cycles, achieve throughput  4171 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1033 cycles, achieve throughput  4460 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1048 cycles, achieve throughput  4690 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1141 cycles, achieve throughput  4846 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1141 cycles, achieve throughput  5384 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1273 cycles, achieve throughput  5309 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1307 cycles, achieve throughput  5641 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1424 cycles, achieve throughput  5608 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1418 cycles, achieve throughput  6066 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1516 cycles, achieve throughput  6079 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1488 cycles, achieve throughput  6606 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1714 cycles, achieve throughput  6452 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1824 cycles, achieve throughput  6736 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1940 cycles, achieve throughput  6967 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2047 cycles, achieve throughput  7203 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2162 cycles, achieve throughput  7388 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2269 cycles, achieve throughput  7581 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2385 cycles, achieve throughput  7728 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2499 cycles, achieve throughput  7867 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2612 cycles, achieve throughput  7997 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2718 cycles, achieve throughput  8137 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2939 cycles, achieve throughput  7943 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3063 cycles, achieve throughput  8023 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3166 cycles, achieve throughput  8150 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3292 cycles, achieve throughput  8211 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3390 cycles, achieve throughput  8336 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3443 cycles, achieve throughput  8565 MB/s
EDMA ACNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    592 cycles, achieve throughput     2 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    591 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    593 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    593 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    593 cycles, achieve throughput    10 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    592 cycles, achieve throughput    12 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    614 cycles, achieve throughput    13 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    612 cycles, achieve throughput    15 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    614 cycles, achieve throughput    17 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    612 cycles, achieve throughput    19 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    613 cycles, achieve throughput    21 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    614 cycles, achieve throughput    23 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    613 cycles, achieve throughput    25 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    614 cycles, achieve throughput    27 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    627 cycles, achieve throughput    28 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    613 cycles, achieve throughput    31 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    612 cycles, achieve throughput    62 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    607 cycles, achieve throughput    94 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    608 cycles, achieve throughput   126 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    608 cycles, achieve throughput   157 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    628 cycles, achieve throughput   183 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    613 cycles, achieve throughput   219 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    610 cycles, achieve throughput   251 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    592 cycles, achieve throughput   291 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    614 cycles, achieve throughput   312 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    610 cycles, achieve throughput   346 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    610 cycles, achieve throughput   377 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    614 cycles, achieve throughput   406 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    610 cycles, achieve throughput   440 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    608 cycles, achieve throughput   473 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    612 cycles, achieve throughput   501 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    608 cycles, achieve throughput   568 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    720 cycles, achieve throughput   533 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    700 cycles, achieve throughput   603 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    705 cycles, achieve throughput   653 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    704 cycles, achieve throughput   709 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    708 cycles, achieve throughput   759 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    831 cycles, achieve throughput   693 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    703 cycles, achieve throughput   873 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    686 cycles, achieve throughput  1007 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    692 cycles, achieve throughput  1109 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    688 cycles, achieve throughput  1227 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    696 cycles, achieve throughput  1324 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    690 cycles, achieve throughput  1446 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    693 cycles, achieve throughput  1551 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    694 cycles, achieve throughput  1659 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    709 cycles, achieve throughput  1733 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    845 cycles, achieve throughput  1635 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    826 cycles, achieve throughput  1859 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    811 cycles, achieve throughput  2083 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    813 cycles, achieve throughput  2267 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    806 cycles, achieve throughput  2477 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    805 cycles, achieve throughput  2671 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    809 cycles, achieve throughput  2847 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    827 cycles, achieve throughput  2971 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    941 cycles, achieve throughput  2938 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    970 cycles, achieve throughput  3167 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    957 cycles, achieve throughput  3531 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1042 cycles, achieve throughput  3537 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1040 cycles, achieve throughput  3840 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1176 cycles, achieve throughput  3657 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1299 cycles, achieve throughput  3547 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1324 cycles, achieve throughput  3712 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1292 cycles, achieve throughput  4279 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1290 cycles, achieve throughput  4762 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1407 cycles, achieve throughput  4803 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1498 cycles, achieve throughput  4921 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1609 cycles, achieve throughput  4964 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1607 cycles, achieve throughput  5352 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1700 cycles, achieve throughput  5421 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1721 cycles, achieve throughput  5712 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1920 cycles, achieve throughput  5760 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2053 cycles, achieve throughput  5985 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2172 cycles, achieve throughput  6223 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2370 cycles, achieve throughput  6221 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2507 cycles, achieve throughput  6371 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2622 cycles, achieve throughput  6561 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2848 cycles, achieve throughput  6471 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2957 cycles, achieve throughput  6648 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3153 cycles, achieve throughput  6625 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3259 cycles, achieve throughput  6786 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3489 cycles, achieve throughput  6691 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3595 cycles, achieve throughput  6836 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3746 cycles, achieve throughput  6888 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3822 cycles, achieve throughput  7073 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3973 cycles, achieve throughput  7113 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   4276 cycles, achieve throughput  6896 MB/s
EDMA ACNTxBCNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput     2 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    10 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    12 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput    13 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    18 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    20 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    609 cycles, achieve throughput    21 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput    23 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput    26 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    608 cycles, achieve throughput    27 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    611 cycles, achieve throughput    29 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput    31 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput    63 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput    93 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   125 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    629 cycles, achieve throughput   152 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   188 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    608 cycles, achieve throughput   221 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    608 cycles, achieve throughput   252 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    610 cycles, achieve throughput   283 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    628 cycles, achieve throughput   305 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   347 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   389 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput   407 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   439 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    609 cycles, achieve throughput   472 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   506 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    608 cycles, achieve throughput   568 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput   647 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    609 cycles, achieve throughput   693 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput   750 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    609 cycles, achieve throughput   819 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    610 cycles, achieve throughput   881 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    609 cycles, achieve throughput   945 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput  1000 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput  1138 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput  1254 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    598 cycles, achieve throughput  1412 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput  1505 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput  1626 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    610 cycles, achieve throughput  1762 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    610 cycles, achieve throughput  1888 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    610 cycles, achieve throughput  2014 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    724 cycles, achieve throughput  1909 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    721 cycles, achieve throughput  2130 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput  2400 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput  2663 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    835 cycles, achieve throughput  2391 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    834 cycles, achieve throughput  2578 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    803 cycles, achieve throughput  2869 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    799 cycles, achieve throughput  3075 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    800 cycles, achieve throughput  3456 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    809 cycles, achieve throughput  3797 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    923 cycles, achieve throughput  3661 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    930 cycles, achieve throughput  3963 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    954 cycles, achieve throughput  4186 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    947 cycles, achieve throughput  4541 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1047 cycles, achieve throughput  4401 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1038 cycles, achieve throughput  4735 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1156 cycles, achieve throughput  4783 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1162 cycles, achieve throughput  5287 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1274 cycles, achieve throughput  5304 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1260 cycles, achieve throughput  5851 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1390 cycles, achieve throughput  5746 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1387 cycles, achieve throughput  6201 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1539 cycles, achieve throughput  5988 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1504 cycles, achieve throughput  6536 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1737 cycles, achieve throughput  6366 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1828 cycles, achieve throughput  6722 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1942 cycles, achieve throughput  6960 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2047 cycles, achieve throughput  7203 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2157 cycles, achieve throughput  7405 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2276 cycles, achieve throughput  7558 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2389 cycles, achieve throughput  7715 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2504 cycles, achieve throughput  7851 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2604 cycles, achieve throughput  8022 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2835 cycles, achieve throughput  7801 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2950 cycles, achieve throughput  7914 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3062 cycles, achieve throughput  8026 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3161 cycles, achieve throughput  8163 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3273 cycles, achieve throughput  8259 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3398 cycles, achieve throughput  8317 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3615 cycles, achieve throughput  8158 MB/s
transfer    2 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput     4 MB/s
transfer    2 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput     8 MB/s
transfer    2 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput    12 MB/s
transfer    2 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    16 MB/s
transfer    2 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput    20 MB/s
transfer    2 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput    24 MB/s
transfer    2 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    608 cycles, achieve throughput    27 MB/s
transfer    2 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    608 cycles, achieve throughput    31 MB/s
transfer    2 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    36 MB/s
transfer    2 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput    39 MB/s
transfer    2 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    44 MB/s
transfer    2 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    48 MB/s
transfer    2 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput    50 MB/s
transfer    2 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput    54 MB/s
transfer    2 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput    58 MB/s
transfer    2 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput    62 MB/s
transfer    2 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   125 MB/s
transfer    2 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   188 MB/s
transfer    2 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput   250 MB/s
transfer    2 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    608 cycles, achieve throughput   315 MB/s
transfer    2 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    629 cycles, achieve throughput   366 MB/s
transfer    2 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   442 MB/s
transfer    2 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   518 MB/s
transfer    2 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   569 MB/s
transfer    2 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    611 cycles, achieve throughput   628 MB/s
transfer    2 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   695 MB/s
transfer    2 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    609 cycles, achieve throughput   756 MB/s
transfer    2 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput   815 MB/s
transfer    2 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput   906 MB/s
transfer    2 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   948 MB/s
transfer    2 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput  1037 MB/s
transfer    2 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput  1127 MB/s
transfer    2 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    616 cycles, achieve throughput  1246 MB/s
transfer    2 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput  1378 MB/s
transfer    2 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput  1503 MB/s
transfer    2 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    619 cycles, achieve throughput  1612 MB/s
transfer    2 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    616 cycles, achieve throughput  1745 MB/s
transfer    2 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    714 cycles, achieve throughput  1613 MB/s
transfer    2 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    741 cycles, achieve throughput  1658 MB/s
transfer    2 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput  1966 MB/s
transfer    2 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput  2188 MB/s
transfer    2 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    691 cycles, achieve throughput  2445 MB/s
transfer    2 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    688 cycles, achieve throughput  2679 MB/s
transfer    2 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    839 cycles, achieve throughput  2379 MB/s
transfer    2 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    834 cycles, achieve throughput  2578 MB/s
transfer    2 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    837 cycles, achieve throughput  2752 MB/s
transfer    2 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    800 cycles, achieve throughput  3072 MB/s
transfer    2 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    821 cycles, achieve throughput  3367 MB/s
transfer    2 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    806 cycles, achieve throughput  3811 MB/s
transfer    2 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    956 cycles, achieve throughput  3534 MB/s
transfer    2 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    949 cycles, achieve throughput  3884 MB/s
transfer    2 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    930 cycles, achieve throughput  4294 MB/s
transfer    2 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1062 cycles, achieve throughput  4049 MB/s
transfer    2 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1047 cycles, achieve throughput  4401 MB/s
transfer    2 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1048 cycles, achieve throughput  4690 MB/s
transfer    2 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1064 cycles, achieve throughput  5196 MB/s
transfer    2 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1141 cycles, achieve throughput  5384 MB/s
transfer    2 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1276 cycles, achieve throughput  5296 MB/s
transfer    2 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1275 cycles, achieve throughput  5782 MB/s
transfer    2 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1392 cycles, achieve throughput  5737 MB/s
transfer    2 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1539 cycles, achieve throughput  5589 MB/s
transfer    2 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1507 cycles, achieve throughput  6115 MB/s
transfer    2 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1512 cycles, achieve throughput  6501 MB/s
transfer    2 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1622 cycles, achieve throughput  6818 MB/s
transfer    2 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1735 cycles, achieve throughput  7082 MB/s
transfer    2 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1938 cycles, achieve throughput  6974 MB/s
transfer    2 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2049 cycles, achieve throughput  7196 MB/s
transfer    2 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2160 cycles, achieve throughput  7395 MB/s
transfer    2 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2289 cycles, achieve throughput  7515 MB/s
transfer    2 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2384 cycles, achieve throughput  7731 MB/s
transfer    2 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2533 cycles, achieve throughput  7761 MB/s
transfer    2 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2727 cycles, achieve throughput  8110 MB/s
transfer    2 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2965 cycles, achieve throughput  8288 MB/s
transfer    2 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3204 cycles, achieve throughput  8437 MB/s
transfer    2 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3506 cycles, achieve throughput  8411 MB/s
transfer    2 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3751 cycles, achieve throughput  8517 MB/s
transfer    2 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4070 cycles, achieve throughput  8453 MB/s
transfer    2 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4214 cycles, achieve throughput  8747 MB/s
transfer    2 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4440 cycles, achieve throughput  8856 MB/s
transfer    2 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4775 cycles, achieve throughput  8749 MB/s
transfer    2 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4992 cycles, achieve throughput  8861 MB/s
transfer    2 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5293 cycles, achieve throughput  8821 MB/s
transfer    2 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5471 cycles, achieve throughput  8984 MB/s
transfer    2 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5699 cycles, achieve throughput  9055 MB/s
transfer    2 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5921 cycles, achieve throughput  9131 MB/s
transfer    2 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6325 cycles, achieve throughput  8936 MB/s
transfer    2 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6524 cycles, achieve throughput  9040 MB/s
transfer    3 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput     6 MB/s
transfer    3 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    12 MB/s
transfer    3 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    18 MB/s
transfer    3 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    24 MB/s
transfer    3 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    30 MB/s
transfer    3 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput    35 MB/s
transfer    3 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    613 cycles, achieve throughput    41 MB/s
transfer    3 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput    46 MB/s
transfer    3 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    627 cycles, achieve throughput    51 MB/s
transfer    3 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    611 cycles, achieve throughput    58 MB/s
transfer    3 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput    65 MB/s
transfer    3 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput    70 MB/s
transfer    3 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    611 cycles, achieve throughput    76 MB/s
transfer    3 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput    82 MB/s
transfer    3 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    612 cycles, achieve throughput    88 MB/s
transfer    3 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    614 cycles, achieve throughput    93 MB/s
transfer    3 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    628 cycles, achieve throughput   183 MB/s
transfer    3 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   284 MB/s
transfer    3 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    607 cycles, achieve throughput   379 MB/s
transfer    3 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    723 cycles, achieve throughput   398 MB/s
transfer    3 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    586 cycles, achieve throughput   589 MB/s
transfer    3 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   572 MB/s
transfer    3 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   778 MB/s
transfer    3 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput   749 MB/s
transfer    3 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    600 cycles, achieve throughput   960 MB/s
transfer    3 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    631 cycles, achieve throughput  1004 MB/s
transfer    3 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput  1167 MB/s
transfer    3 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    710 cycles, achieve throughput  1054 MB/s
transfer    3 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    596 cycles, achieve throughput  1353 MB/s
transfer    3 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    742 cycles, achieve throughput  1164 MB/s
transfer    3 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput  1310 MB/s
transfer    3 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    611 cycles, achieve throughput  1696 MB/s
transfer    3 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    695 cycles, achieve throughput  1657 MB/s
transfer    3 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    693 cycles, achieve throughput  1828 MB/s
transfer    3 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    698 cycles, achieve throughput  1980 MB/s
transfer    3 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    743 cycles, achieve throughput  2015 MB/s
transfer    3 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    706 cycles, achieve throughput  2284 MB/s
transfer    3 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  2468 MB/s
transfer    3 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput  2663 MB/s
transfer    3 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    836 cycles, achieve throughput  2480 MB/s
transfer    3 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    840 cycles, achieve throughput  2742 MB/s
transfer    3 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    816 cycles, achieve throughput  3105 MB/s
transfer    3 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    825 cycles, achieve throughput  3351 MB/s
transfer    3 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    806 cycles, achieve throughput  3716 MB/s
transfer    3 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    950 cycles, achieve throughput  3395 MB/s
transfer    3 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    942 cycles, achieve throughput  3668 MB/s
transfer    3 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    949 cycles, achieve throughput  3884 MB/s
transfer    3 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    922 cycles, achieve throughput  4498 MB/s
transfer    3 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1033 cycles, achieve throughput  4460 MB/s
transfer    3 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1049 cycles, achieve throughput  4832 MB/s
transfer    3 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1142 cycles, achieve throughput  4842 MB/s
transfer    3 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1141 cycles, achieve throughput  5250 MB/s
transfer    3 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1143 cycles, achieve throughput  5644 MB/s
transfer    3 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1284 cycles, achieve throughput  5383 MB/s
transfer    3 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1295 cycles, achieve throughput  5693 MB/s
transfer    3 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1374 cycles, achieve throughput  6036 MB/s
transfer    3 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1500 cycles, achieve throughput  6144 MB/s
transfer    3 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1647 cycles, achieve throughput  6155 MB/s
transfer    3 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1668 cycles, achieve throughput  6630 MB/s
transfer    3 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1737 cycles, achieve throughput  6897 MB/s
transfer    3 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1863 cycles, achieve throughput  6925 MB/s
transfer    3 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1946 cycles, achieve throughput  7103 MB/s
transfer    3 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2064 cycles, achieve throughput  7144 MB/s
transfer    3 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2176 cycles, achieve throughput  7623 MB/s
transfer    3 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2377 cycles, achieve throughput  7754 MB/s
transfer    3 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2613 cycles, achieve throughput  7759 MB/s
transfer    3 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2718 cycles, achieve throughput  8137 MB/s
transfer    3 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2961 cycles, achieve throughput  8092 MB/s
transfer    3 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3085 cycles, achieve throughput  8364 MB/s
transfer    3 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3288 cycles, achieve throughput  8408 MB/s
transfer    3 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3538 cycles, achieve throughput  8335 MB/s
transfer    3 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3953 cycles, achieve throughput  8393 MB/s
transfer    3 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4267 cycles, achieve throughput  8639 MB/s
transfer    3 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4653 cycles, achieve throughput  8714 MB/s
transfer    3 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4969 cycles, achieve throughput  8902 MB/s
transfer    3 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5339 cycles, achieve throughput  8976 MB/s
transfer    3 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5707 cycles, achieve throughput  9043 MB/s
transfer    3 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6067 cycles, achieve throughput  9114 MB/s
transfer    3 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6488 cycles, achieve throughput  9090 MB/s
transfer    3 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6845 cycles, achieve throughput  9155 MB/s
transfer    3 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7324 cycles, achieve throughput  9059 MB/s
transfer    3 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7667 cycles, achieve throughput  9135 MB/s
transfer    3 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7873 cycles, achieve throughput  9364 MB/s
transfer    3 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8331 cycles, achieve throughput  9292 MB/s
transfer    3 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8639 cycles, achieve throughput  9387 MB/s
transfer    3 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9051 cycles, achieve throughput  9367 MB/s
transfer    3 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9374 cycles, achieve throughput  9438 MB/s
transfer    4 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput     8 MB/s
transfer    4 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    16 MB/s
transfer    4 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    20 MB/s
transfer    4 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    32 MB/s
transfer    4 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput    34 MB/s
transfer    4 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput    40 MB/s
transfer    4 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    690 cycles, achieve throughput    48 MB/s
transfer    4 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    64 MB/s
transfer    4 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput    62 MB/s
transfer    4 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput    69 MB/s
transfer    4 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    690 cycles, achieve throughput    76 MB/s
transfer    4 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput    83 MB/s
transfer    4 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    690 cycles, achieve throughput    90 MB/s
transfer    4 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    691 cycles, achieve throughput    97 MB/s
transfer    4 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    595 cycles, achieve throughput   121 MB/s
transfer    4 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   129 MB/s
transfer    4 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   259 MB/s
transfer    4 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    707 cycles, achieve throughput   325 MB/s
transfer    4 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   518 MB/s
transfer    4 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    740 cycles, achieve throughput   518 MB/s
transfer    4 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput   656 MB/s
transfer    4 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput   766 MB/s
transfer    4 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput  1037 MB/s
transfer    4 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    690 cycles, achieve throughput  1001 MB/s
transfer    4 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    707 cycles, achieve throughput  1086 MB/s
transfer    4 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    694 cycles, achieve throughput  1217 MB/s
transfer    4 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    693 cycles, achieve throughput  1329 MB/s
transfer    4 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    713 cycles, achieve throughput  1400 MB/s
transfer    4 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    707 cycles, achieve throughput  1520 MB/s
transfer    4 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput  1664 MB/s
transfer    4 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    708 cycles, achieve throughput  1735 MB/s
transfer    4 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    688 cycles, achieve throughput  2009 MB/s
transfer    4 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    690 cycles, achieve throughput  2226 MB/s
transfer    4 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    692 cycles, achieve throughput  2441 MB/s
transfer    4 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    708 cycles, achieve throughput  2603 MB/s
transfer    4 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    836 cycles, achieve throughput  2388 MB/s
transfer    4 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    818 cycles, achieve throughput  2628 MB/s
transfer    4 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    833 cycles, achieve throughput  2765 MB/s
transfer    4 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    816 cycles, achieve throughput  3011 MB/s
transfer    4 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    822 cycles, achieve throughput  3363 MB/s
transfer    4 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    803 cycles, achieve throughput  3825 MB/s
transfer    4 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    915 cycles, achieve throughput  3693 MB/s
transfer    4 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    952 cycles, achieve throughput  3872 MB/s
transfer    4 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    950 cycles, achieve throughput  4203 MB/s
transfer    4 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1026 cycles, achieve throughput  4191 MB/s
transfer    4 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1054 cycles, achieve throughput  4371 MB/s
transfer    4 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1043 cycles, achieve throughput  4712 MB/s
transfer    4 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1176 cycles, achieve throughput  4702 MB/s
transfer    4 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1155 cycles, achieve throughput  5319 MB/s
transfer    4 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1255 cycles, achieve throughput  5385 MB/s
transfer    4 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1389 cycles, achieve throughput  5307 MB/s
transfer    4 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1311 cycles, achieve throughput  6092 MB/s
transfer    4 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1427 cycles, achieve throughput  6027 MB/s
transfer    4 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1507 cycles, achieve throughput  6115 MB/s
transfer    4 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1487 cycles, achieve throughput  6610 MB/s
transfer    4 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1605 cycles, achieve throughput  6890 MB/s
transfer    4 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1732 cycles, achieve throughput  7094 MB/s
transfer    4 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1845 cycles, achieve throughput  7326 MB/s
transfer    4 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2044 cycles, achieve throughput  7214 MB/s
transfer    4 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2173 cycles, achieve throughput  7351 MB/s
transfer    4 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2285 cycles, achieve throughput  7528 MB/s
transfer    4 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2399 cycles, achieve throughput  7683 MB/s
transfer    4 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2507 cycles, achieve throughput  7842 MB/s
transfer    4 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2748 cycles, achieve throughput  8048 MB/s
transfer    4 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2960 cycles, achieve throughput  8302 MB/s
transfer    4 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3296 cycles, achieve throughput  8201 MB/s
transfer    4 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3529 cycles, achieve throughput  8356 MB/s
transfer    4 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3727 cycles, achieve throughput  8572 MB/s
transfer    4 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3964 cycles, achieve throughput  8679 MB/s
transfer    4 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4302 cycles, achieve throughput  8569 MB/s
transfer    4 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4450 cycles, achieve throughput  8836 MB/s
transfer    4 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4986 cycles, achieve throughput  8872 MB/s
transfer    4 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5531 cycles, achieve throughput  8886 MB/s
transfer    4 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5974 cycles, achieve throughput  9050 MB/s
transfer    4 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6453 cycles, achieve throughput  9140 MB/s
transfer    4 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7015 cycles, achieve throughput  9108 MB/s
transfer    4 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7460 cycles, achieve throughput  9224 MB/s
transfer    4 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7851 cycles, achieve throughput  9390 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8410 cycles, achieve throughput  9351 MB/s
transfer    4 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8966 cycles, achieve throughput  9319 MB/s
transfer    4 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9410 cycles, achieve throughput  9402 MB/s
transfer    4 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9967 cycles, achieve throughput  9369 MB/s
transfer    4 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  10413 cycles, achieve throughput  9440 MB/s
transfer    4 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  10962 cycles, achieve throughput  9416 MB/s
transfer    4 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  11310 cycles, achieve throughput  9560 MB/s
transfer    4 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  11855 cycles, achieve throughput  9536 MB/s
transfer    4 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12316 cycles, achieve throughput  9578 MB/s
EDMA Index test with EDMA0 TC0
transfer 1024 *     1 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22125 cycles, achieve throughput    55 MB/s
transfer 1024 *     2 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21793 cycles, achieve throughput   112 MB/s
transfer 1024 *     3 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21681 cycles, achieve throughput   170 MB/s
transfer 1024 *     4 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21677 cycles, achieve throughput   226 MB/s
transfer 1024 *     5 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21589 cycles, achieve throughput   284 MB/s
transfer 1024 *     6 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21588 cycles, achieve throughput   341 MB/s
transfer 1024 *     7 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21589 cycles, achieve throughput   398 MB/s
transfer 1024 *     8 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21587 cycles, achieve throughput   455 MB/s
transfer 1024 *     9 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21587 cycles, achieve throughput   512 MB/s
transfer 1024 *    10 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21588 cycles, achieve throughput   569 MB/s
transfer 1024 *    11 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21589 cycles, achieve throughput   626 MB/s
transfer 1024 *    12 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21587 cycles, achieve throughput   683 MB/s
transfer 1024 *    13 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21588 cycles, achieve throughput   739 MB/s
transfer 1024 *    14 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21587 cycles, achieve throughput   796 MB/s
transfer 1024 *    15 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21589 cycles, achieve throughput   853 MB/s
transfer 1024 *    16 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21478 cycles, achieve throughput   915 MB/s
transfer 1024 *    32 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21587 cycles, achieve throughput  1821 MB/s
transfer 1024 *    48 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21588 cycles, achieve throughput  2732 MB/s
transfer 1024 *    64 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21592 cycles, achieve throughput  3642 MB/s
transfer 1024 *    80 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28055 cycles, achieve throughput  3503 MB/s
transfer 1024 *    96 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  29072 cycles, achieve throughput  4057 MB/s
transfer 1024 *   112 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  27519 cycles, achieve throughput  5001 MB/s
transfer 1024 *   128 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  27069 cycles, achieve throughput  5810 MB/s
transfer 1024 *   144 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31551 cycles, achieve throughput  5608 MB/s
transfer 1024 *   160 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32371 cycles, achieve throughput  6073 MB/s
transfer 1024 *   176 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31532 cycles, achieve throughput  6858 MB/s
transfer 1024 *   192 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32372 cycles, achieve throughput  7288 MB/s
transfer 1024 *   208 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33064 cycles, achieve throughput  7730 MB/s
transfer 1024 *   224 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32407 cycles, achieve throughput  8493 MB/s
transfer 1024 *   240 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34713 cycles, achieve throughput  8495 MB/s
transfer 1024 *   256 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34859 cycles, achieve throughput  9024 MB/s
transfer 1024 *   320 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41106 cycles, achieve throughput  9565 MB/s
transfer 1024 *   384 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  48111 cycles, achieve throughput  9807 MB/s
transfer 1024 *   448 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  58298 cycles, achieve throughput  9442 MB/s
transfer 1024 *   512 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  65640 cycles, achieve throughput  9584 MB/s
transfer 1024 *   768 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  97457 cycles, achieve throughput  9683 MB/s
transfer 1024 *  1024 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130128 cycles, achieve throughput  9669 MB/s
transfer  682 *  1536 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130586 cycles, achieve throughput  9626 MB/s
transfer  512 *  2048 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129361 cycles, achieve throughput  9726 MB/s
transfer  409 *  2560 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129865 cycles, achieve throughput  9675 MB/s
transfer  341 *  3072 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129898 cycles, achieve throughput  9677 MB/s
transfer  292 *  3584 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129511 cycles, achieve throughput  9696 MB/s
transfer  256 *  4096 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129994 cycles, achieve throughput  9679 MB/s
transfer  227 *  4608 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129035 cycles, achieve throughput  9727 MB/s
transfer  204 *  5120 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129192 cycles, achieve throughput  9701 MB/s
transfer  186 *  5632 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129231 cycles, achieve throughput  9727 MB/s
transfer  170 *  6144 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129366 cycles, achieve throughput  9688 MB/s
transfer  157 *  6656 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129253 cycles, achieve throughput  9701 MB/s
transfer  146 *  7168 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129609 cycles, achieve throughput  9689 MB/s
transfer  136 *  7680 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128814 cycles, achieve throughput  9730 MB/s
transfer  128 *  8192 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129814 cycles, achieve throughput  9693 MB/s
transfer 1024 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput  1747 MB/s
transfer 1024 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    822 cycles, achieve throughput  2989 MB/s
transfer 1024 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22314 cycles, achieve throughput   165 MB/s
transfer 1024 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1032 cycles, achieve throughput  4762 MB/s
transfer 1024 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22213 cycles, achieve throughput   276 MB/s
transfer 1024 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21747 cycles, achieve throughput   339 MB/s
transfer 1024 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23325 cycles, achieve throughput   368 MB/s
transfer 1024 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1527 cycles, achieve throughput  6437 MB/s
transfer 1024 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23882 cycles, achieve throughput   463 MB/s
transfer 1024 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21879 cycles, achieve throughput   561 MB/s
transfer 1024 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22546 cycles, achieve throughput   599 MB/s
transfer 1024 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23846 cycles, achieve throughput   618 MB/s
transfer 1024 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24522 cycles, achieve throughput   651 MB/s
transfer 1024 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23108 cycles, achieve throughput   744 MB/s
transfer 1024 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22770 cycles, achieve throughput   809 MB/s
transfer 1024 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2464 cycles, achieve throughput  7979 MB/s
transfer 1024 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4454 cycles, achieve throughput  8828 MB/s
transfer 1024 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31385 cycles, achieve throughput  1879 MB/s
transfer 1024 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8458 cycles, achieve throughput  9298 MB/s
transfer 1024 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32633 cycles, achieve throughput  3012 MB/s
transfer 1024 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23339 cycles, achieve throughput  5054 MB/s
transfer 1024 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34094 cycles, achieve throughput  4036 MB/s
transfer 1024 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  16233 cycles, achieve throughput  9689 MB/s
transfer 1024 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37270 cycles, achieve throughput  4747 MB/s
transfer 1024 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30768 cycles, achieve throughput  6390 MB/s
transfer 1024 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  40628 cycles, achieve throughput  5323 MB/s
transfer 1024 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28263 cycles, achieve throughput  8347 MB/s
transfer 1024 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  45819 cycles, achieve throughput  5578 MB/s
transfer 1024 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41290 cycles, achieve throughput  6666 MB/s
transfer 1024 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  50078 cycles, achieve throughput  5889 MB/s
transfer 1024 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34768 cycles, achieve throughput  9047 MB/s
transfer 1024 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42214 cycles, achieve throughput  9314 MB/s
transfer 1024 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  48556 cycles, achieve throughput  9717 MB/s
transfer 1024 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  58092 cycles, achieve throughput  9476 MB/s
transfer 1024 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  65176 cycles, achieve throughput  9653 MB/s
transfer 1024 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  98049 cycles, achieve throughput  9624 MB/s
transfer 1024 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130223 cycles, achieve throughput  9662 MB/s
transfer  682 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129399 cycles, achieve throughput  9714 MB/s
transfer  512 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129769 cycles, achieve throughput  9696 MB/s
transfer  409 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129334 cycles, achieve throughput  9714 MB/s
transfer  341 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128748 cycles, achieve throughput  9763 MB/s
transfer  292 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129076 cycles, achieve throughput  9729 MB/s
transfer  256 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129157 cycles, achieve throughput  9742 MB/s
transfer  227 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128726 cycles, achieve throughput  9751 MB/s
transfer  204 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128983 cycles, achieve throughput  9717 MB/s
transfer  186 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128876 cycles, achieve throughput  9754 MB/s
transfer  170 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128397 cycles, achieve throughput  9761 MB/s
transfer  157 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129181 cycles, achieve throughput  9707 MB/s
transfer  146 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128844 cycles, achieve throughput  9746 MB/s
transfer  136 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128712 cycles, achieve throughput  9737 MB/s
transfer  128 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129296 cycles, achieve throughput  9731 MB/s
transfer 1024 *     1 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22092 cycles, achieve throughput    55 MB/s
transfer 1024 *     2 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21744 cycles, achieve throughput   113 MB/s
transfer 1024 *     3 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21519 cycles, achieve throughput   171 MB/s
transfer 1024 *     4 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21880 cycles, achieve throughput   224 MB/s
transfer 1024 *     5 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21737 cycles, achieve throughput   282 MB/s
transfer 1024 *     6 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22773 cycles, achieve throughput   323 MB/s
transfer 1024 *     7 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21353 cycles, achieve throughput   402 MB/s
transfer 1024 *     8 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23347 cycles, achieve throughput   421 MB/s
transfer 1024 *     9 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22085 cycles, achieve throughput   500 MB/s
transfer 1024 *    10 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22323 cycles, achieve throughput   550 MB/s
transfer 1024 *    11 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23879 cycles, achieve throughput   566 MB/s
transfer 1024 *    12 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23992 cycles, achieve throughput   614 MB/s
transfer 1024 *    13 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23212 cycles, achieve throughput   688 MB/s
transfer 1024 *    14 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22346 cycles, achieve throughput   769 MB/s
transfer 1024 *    15 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21262 cycles, achieve throughput   866 MB/s
transfer 1024 *    16 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22979 cycles, achieve throughput   855 MB/s
transfer 1024 *    32 Bytes with index=   33 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23251 cycles, achieve throughput  1691 MB/s
transfer 1024 *    48 Bytes with index=   49 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32613 cycles, achieve throughput  1808 MB/s
transfer 1024 *    64 Bytes with index=   65 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  40605 cycles, achieve throughput  1936 MB/s
transfer 1024 *    80 Bytes with index=   81 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41116 cycles, achieve throughput  2390 MB/s
transfer 1024 *    96 Bytes with index=   97 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41535 cycles, achieve throughput  2840 MB/s
transfer 1024 *   112 Bytes with index=  113 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42046 cycles, achieve throughput  3273 MB/s
transfer 1024 *   128 Bytes with index=  129 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  43587 cycles, achieve throughput  3608 MB/s
transfer 1024 *   144 Bytes with index=  145 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  43952 cycles, achieve throughput  4025 MB/s
transfer 1024 *   160 Bytes with index=  161 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  44474 cycles, achieve throughput  4420 MB/s
transfer 1024 *   176 Bytes with index=  177 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  45515 cycles, achieve throughput  4751 MB/s
transfer 1024 *   192 Bytes with index=  193 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  48677 cycles, achieve throughput  4846 MB/s
transfer 1024 *   208 Bytes with index=  209 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  52800 cycles, achieve throughput  4840 MB/s
transfer 1024 *   224 Bytes with index=  225 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  53117 cycles, achieve throughput  5181 MB/s
transfer 1024 *   240 Bytes with index=  241 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  56927 cycles, achieve throughput  5180 MB/s
transfer 1024 *   256 Bytes with index=  257 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  54606 cycles, achieve throughput  5760 MB/s
transfer 1024 *   320 Bytes with index=  321 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  58959 cycles, achieve throughput  6669 MB/s
transfer 1024 *   384 Bytes with index=  385 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  72580 cycles, achieve throughput  6501 MB/s
transfer 1024 *   448 Bytes with index=  449 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  83148 cycles, achieve throughput  6620 MB/s
transfer 1024 *   512 Bytes with index=  513 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  87918 cycles, achieve throughput  7156 MB/s
transfer 1024 *   768 Bytes with index=  769 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 110147 cycles, achieve throughput  8567 MB/s
transfer 1023 *  1024 Bytes with index= 1025 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 143242 cycles, achieve throughput  8775 MB/s
transfer  682 *  1536 Bytes with index= 1537 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 147075 cycles, achieve throughput  8547 MB/s
transfer  511 *  2048 Bytes with index= 2049 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 147504 cycles, achieve throughput  8513 MB/s
transfer  409 *  2560 Bytes with index= 2561 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 147560 cycles, achieve throughput  8514 MB/s
transfer  341 *  3072 Bytes with index= 3073 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 149876 cycles, achieve throughput  8387 MB/s
transfer  292 *  3584 Bytes with index= 3585 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 150925 cycles, achieve throughput  8320 MB/s
transfer  255 *  4096 Bytes with index= 4097 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 153067 cycles, achieve throughput  8188 MB/s
transfer  227 *  4608 Bytes with index= 4609 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 152318 cycles, achieve throughput  8240 MB/s
transfer  204 *  5120 Bytes with index= 5121 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 152839 cycles, achieve throughput  8200 MB/s
transfer  186 *  5632 Bytes with index= 5633 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 154421 cycles, achieve throughput  8140 MB/s
transfer  170 *  6144 Bytes with index= 6145 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 153662 cycles, achieve throughput  8156 MB/s
transfer  157 *  6656 Bytes with index= 6657 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 154621 cycles, achieve throughput  8110 MB/s
transfer  146 *  7168 Bytes with index= 7169 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155592 cycles, achieve throughput  8071 MB/s
transfer  136 *  7680 Bytes with index= 7681 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155266 cycles, achieve throughput  8072 MB/s
transfer  127 *  8192 Bytes with index= 8193 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 157339 cycles, achieve throughput  7934 MB/s
transfer 1024 *     1 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20864 cycles, achieve throughput    58 MB/s
transfer 1024 *     2 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20637 cycles, achieve throughput   119 MB/s
transfer 1024 *     3 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21217 cycles, achieve throughput   173 MB/s
transfer 1024 *     4 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21369 cycles, achieve throughput   230 MB/s
transfer 1024 *     5 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21691 cycles, achieve throughput   283 MB/s
transfer 1024 *     6 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20653 cycles, achieve throughput   356 MB/s
transfer 1024 *     7 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22111 cycles, achieve throughput   389 MB/s
transfer 1024 *     8 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21549 cycles, achieve throughput   456 MB/s
transfer 1024 *     9 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22684 cycles, achieve throughput   487 MB/s
transfer 1024 *    10 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20869 cycles, achieve throughput   588 MB/s
transfer 1024 *    11 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20844 cycles, achieve throughput   648 MB/s
transfer 1024 *    12 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21200 cycles, achieve throughput   695 MB/s
transfer 1024 *    13 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22877 cycles, achieve throughput   698 MB/s
transfer 1024 *    14 Bytes with index=   18 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23984 cycles, achieve throughput   717 MB/s
transfer 1024 *    15 Bytes with index=   19 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  25216 cycles, achieve throughput   730 MB/s
transfer 1024 *    16 Bytes with index=   20 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24095 cycles, achieve throughput   815 MB/s
transfer 1024 *    32 Bytes with index=   36 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24555 cycles, achieve throughput  1601 MB/s
transfer 1024 *    48 Bytes with index=   52 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34125 cycles, achieve throughput  1728 MB/s
transfer 1024 *    64 Bytes with index=   68 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37198 cycles, achieve throughput  2114 MB/s
transfer 1024 *    80 Bytes with index=   84 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37489 cycles, achieve throughput  2622 MB/s
transfer 1024 *    96 Bytes with index=  100 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  38023 cycles, achieve throughput  3102 MB/s
transfer 1024 *   112 Bytes with index=  116 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  38519 cycles, achieve throughput  3572 MB/s
transfer 1024 *   128 Bytes with index=  132 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  40496 cycles, achieve throughput  3883 MB/s
transfer 1024 *   144 Bytes with index=  148 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41663 cycles, achieve throughput  4247 MB/s
transfer 1024 *   160 Bytes with index=  164 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42350 cycles, achieve throughput  4642 MB/s
transfer 1024 *   176 Bytes with index=  180 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  43865 cycles, achieve throughput  4930 MB/s
transfer 1024 *   192 Bytes with index=  196 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  46357 cycles, achieve throughput  5089 MB/s
transfer 1024 *   208 Bytes with index=  212 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  48569 cycles, achieve throughput  5262 MB/s
transfer 1024 *   224 Bytes with index=  228 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  50929 cycles, achieve throughput  5404 MB/s
transfer 1024 *   240 Bytes with index=  244 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  54561 cycles, achieve throughput  5405 MB/s
transfer 1024 *   256 Bytes with index=  260 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  52698 cycles, achieve throughput  5969 MB/s
transfer 1024 *   320 Bytes with index=  324 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  58256 cycles, achieve throughput  6749 MB/s
transfer 1024 *   384 Bytes with index=  388 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  69487 cycles, achieve throughput  6790 MB/s
transfer 1024 *   448 Bytes with index=  452 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  78738 cycles, achieve throughput  6991 MB/s
transfer 1024 *   512 Bytes with index=  516 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  85110 cycles, achieve throughput  7392 MB/s
transfer 1024 *   768 Bytes with index=  772 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 109253 cycles, achieve throughput  8637 MB/s
transfer 1020 *  1024 Bytes with index= 1028 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 142581 cycles, achieve throughput  8790 MB/s
transfer  680 *  1536 Bytes with index= 1540 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144252 cycles, achieve throughput  8688 MB/s
transfer  511 *  2048 Bytes with index= 2052 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144716 cycles, achieve throughput  8677 MB/s
transfer  408 *  2560 Bytes with index= 2564 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145910 cycles, achieve throughput  8590 MB/s
transfer  340 *  3072 Bytes with index= 3076 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 147570 cycles, achieve throughput  8493 MB/s
transfer  292 *  3584 Bytes with index= 3588 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 148486 cycles, achieve throughput  8457 MB/s
transfer  255 *  4096 Bytes with index= 4100 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 149369 cycles, achieve throughput  8391 MB/s
transfer  227 *  4608 Bytes with index= 4612 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 150081 cycles, achieve throughput  8363 MB/s
transfer  204 *  5120 Bytes with index= 5124 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 150282 cycles, achieve throughput  8340 MB/s
transfer  186 *  5632 Bytes with index= 5636 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 151214 cycles, achieve throughput  8313 MB/s
transfer  170 *  6144 Bytes with index= 6148 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 151850 cycles, achieve throughput  8254 MB/s
transfer  157 *  6656 Bytes with index= 6660 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 152030 cycles, achieve throughput  8248 MB/s
transfer  146 *  7168 Bytes with index= 7172 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 152550 cycles, achieve throughput  8232 MB/s
transfer  136 *  7680 Bytes with index= 7684 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 152534 cycles, achieve throughput  8217 MB/s
transfer  127 *  8192 Bytes with index= 8196 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 153388 cycles, achieve throughput  8139 MB/s
transfer 1024 *     1 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20629 cycles, achieve throughput    59 MB/s
transfer 1024 *     2 Bytes with index=   18 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19321 cycles, achieve throughput   127 MB/s
transfer 1024 *     3 Bytes with index=   19 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19400 cycles, achieve throughput   190 MB/s
transfer 1024 *     4 Bytes with index=   20 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  17307 cycles, achieve throughput   284 MB/s
transfer 1024 *     5 Bytes with index=   21 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  18515 cycles, achieve throughput   331 MB/s
transfer 1024 *     6 Bytes with index=   22 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  17525 cycles, achieve throughput   420 MB/s
transfer 1024 *     7 Bytes with index=   23 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  17617 cycles, achieve throughput   488 MB/s
transfer 1024 *     8 Bytes with index=   24 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  16978 cycles, achieve throughput   579 MB/s
transfer 1024 *     9 Bytes with index=   25 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  17921 cycles, achieve throughput   617 MB/s
transfer 1024 *    10 Bytes with index=   26 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  18335 cycles, achieve throughput   670 MB/s
transfer 1024 *    11 Bytes with index=   27 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  18972 cycles, achieve throughput   712 MB/s
transfer 1024 *    12 Bytes with index=   28 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19975 cycles, achieve throughput   738 MB/s
transfer 1024 *    13 Bytes with index=   29 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20134 cycles, achieve throughput   793 MB/s
transfer 1024 *    14 Bytes with index=   30 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  20910 cycles, achieve throughput   822 MB/s
transfer 1024 *    15 Bytes with index=   31 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21780 cycles, achieve throughput   846 MB/s
transfer 1024 *    16 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21317 cycles, achieve throughput   922 MB/s
transfer 1024 *    32 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  21687 cycles, achieve throughput  1813 MB/s
transfer 1024 *    48 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  15875 cycles, achieve throughput  3715 MB/s
transfer 1024 *    64 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23802 cycles, achieve throughput  3304 MB/s
transfer 1024 *    80 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23662 cycles, achieve throughput  4154 MB/s
transfer 1024 *    96 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  27048 cycles, achieve throughput  4361 MB/s
transfer 1024 *   112 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22124 cycles, achieve throughput  6220 MB/s
transfer 1024 *   128 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30920 cycles, achieve throughput  5086 MB/s
transfer 1024 *   144 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32867 cycles, achieve throughput  5383 MB/s
transfer 1024 *   160 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34685 cycles, achieve throughput  5668 MB/s
transfer 1024 *   176 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28393 cycles, achieve throughput  7616 MB/s
transfer 1024 *   192 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37979 cycles, achieve throughput  6212 MB/s
transfer 1024 *   208 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  38870 cycles, achieve throughput  6575 MB/s
transfer 1024 *   224 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  40297 cycles, achieve throughput  6830 MB/s
transfer 1024 *   240 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34700 cycles, achieve throughput  8498 MB/s
transfer 1024 *   256 Bytes with index=  272 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  43825 cycles, achieve throughput  7177 MB/s
transfer 1024 *   320 Bytes with index=  336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  49792 cycles, achieve throughput  7897 MB/s
transfer 1024 *   384 Bytes with index=  400 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  58341 cycles, achieve throughput  8087 MB/s
transfer 1024 *   448 Bytes with index=  464 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  65010 cycles, achieve throughput  8467 MB/s
transfer 1024 *   512 Bytes with index=  528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  72987 cycles, achieve throughput  8619 MB/s
transfer 1024 *   768 Bytes with index=  784 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 105566 cycles, achieve throughput  8939 MB/s
transfer 1008 *  1024 Bytes with index= 1040 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 136513 cycles, achieve throughput  9073 MB/s
transfer  675 *  1536 Bytes with index= 1552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 135789 cycles, achieve throughput  9162 MB/s
transfer  508 *  2048 Bytes with index= 2064 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 137327 cycles, achieve throughput  9091 MB/s
transfer  407 *  2560 Bytes with index= 2576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 138458 cycles, achieve throughput  9030 MB/s
transfer  339 *  3072 Bytes with index= 3088 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 139280 cycles, achieve throughput  8972 MB/s
transfer  291 *  3584 Bytes with index= 3600 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 140155 cycles, achieve throughput  8929 MB/s
transfer  255 *  4096 Bytes with index= 4112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 140540 cycles, achieve throughput  8918 MB/s
transfer  226 *  4608 Bytes with index= 4624 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 140756 cycles, achieve throughput  8878 MB/s
transfer  204 *  5120 Bytes with index= 5136 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 141660 cycles, achieve throughput  8847 MB/s
transfer  185 *  5632 Bytes with index= 5648 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 141581 cycles, achieve throughput  8831 MB/s
transfer  170 *  6144 Bytes with index= 6160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 141858 cycles, achieve throughput  8835 MB/s
transfer  157 *  6656 Bytes with index= 6672 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 142422 cycles, achieve throughput  8804 MB/s
transfer  145 *  7168 Bytes with index= 7184 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 141606 cycles, achieve throughput  8807 MB/s
transfer  136 *  7680 Bytes with index= 7696 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 142465 cycles, achieve throughput  8797 MB/s
transfer  127 *  8192 Bytes with index= 8208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 141892 cycles, achieve throughput  8798 MB/s
transfer 1024 *     1 Bytes with index=   65 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12940 cycles, achieve throughput    94 MB/s
transfer 1024 *     2 Bytes with index=   66 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12844 cycles, achieve throughput   191 MB/s
transfer 1024 *     3 Bytes with index=   67 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13054 cycles, achieve throughput   282 MB/s
transfer 1024 *     4 Bytes with index=   68 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12862 cycles, achieve throughput   382 MB/s
transfer 1024 *     5 Bytes with index=   69 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13215 cycles, achieve throughput   464 MB/s
transfer 1024 *     6 Bytes with index=   70 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13261 cycles, achieve throughput   555 MB/s
transfer 1024 *     7 Bytes with index=   71 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13478 cycles, achieve throughput   638 MB/s
transfer 1024 *     8 Bytes with index=   72 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12811 cycles, achieve throughput   767 MB/s
transfer 1024 *     9 Bytes with index=   73 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13651 cycles, achieve throughput   810 MB/s
transfer 1024 *    10 Bytes with index=   74 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13609 cycles, achieve throughput   902 MB/s
transfer 1024 *    11 Bytes with index=   75 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13851 cycles, achieve throughput   975 MB/s
transfer 1024 *    12 Bytes with index=   76 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13610 cycles, achieve throughput  1083 MB/s
transfer 1024 *    13 Bytes with index=   77 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14058 cycles, achieve throughput  1136 MB/s
transfer 1024 *    14 Bytes with index=   78 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14086 cycles, achieve throughput  1221 MB/s
transfer 1024 *    15 Bytes with index=   79 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14260 cycles, achieve throughput  1292 MB/s
transfer 1024 *    16 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12841 cycles, achieve throughput  1531 MB/s
transfer 1024 *    32 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12818 cycles, achieve throughput  3067 MB/s
transfer 1024 *    48 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  15991 cycles, achieve throughput  3688 MB/s
transfer 1024 *    64 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  15931 cycles, achieve throughput  4936 MB/s
transfer 1024 *    80 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19100 cycles, achieve throughput  5146 MB/s
transfer 1024 *    96 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19037 cycles, achieve throughput  6196 MB/s
transfer 1024 *   112 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22144 cycles, achieve throughput  6215 MB/s
transfer 1024 *   128 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22093 cycles, achieve throughput  7119 MB/s
transfer 1024 *   144 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26815 cycles, achieve throughput  6598 MB/s
transfer 1024 *   160 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26757 cycles, achieve throughput  7347 MB/s
transfer 1024 *   176 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30411 cycles, achieve throughput  7111 MB/s
transfer 1024 *   192 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28336 cycles, achieve throughput  8326 MB/s
transfer 1024 *   208 Bytes with index=  272 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33625 cycles, achieve throughput  7601 MB/s
transfer 1024 *   224 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35082 cycles, achieve throughput  7845 MB/s
transfer 1024 *   240 Bytes with index=  304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37211 cycles, achieve throughput  7925 MB/s
transfer 1024 *   256 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34845 cycles, achieve throughput  9027 MB/s
transfer 1024 *   320 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41616 cycles, achieve throughput  9448 MB/s
transfer 1024 *   384 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  49914 cycles, achieve throughput  9453 MB/s
transfer 1024 *   448 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  58646 cycles, achieve throughput  9386 MB/s
transfer 1024 *   512 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  66440 cycles, achieve throughput  9469 MB/s
transfer 1024 *   768 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  98468 cycles, achieve throughput  9584 MB/s
transfer  963 *  1024 Bytes with index= 1088 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 123908 cycles, achieve throughput  9550 MB/s
transfer  655 *  1536 Bytes with index= 1600 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 125337 cycles, achieve throughput  9632 MB/s
transfer  496 *  2048 Bytes with index= 2112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 126254 cycles, achieve throughput  9654 MB/s
transfer  399 *  2560 Bytes with index= 2624 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 126587 cycles, achieve throughput  9682 MB/s
transfer  334 *  3072 Bytes with index= 3136 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127132 cycles, achieve throughput  9684 MB/s
transfer  287 *  3584 Bytes with index= 3648 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127282 cycles, achieve throughput  9697 MB/s
transfer  252 *  4096 Bytes with index= 4160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127343 cycles, achieve throughput  9726 MB/s
transfer  224 *  4608 Bytes with index= 4672 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127708 cycles, achieve throughput  9698 MB/s
transfer  202 *  5120 Bytes with index= 5184 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127710 cycles, achieve throughput  9718 MB/s
transfer  184 *  5632 Bytes with index= 5696 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127922 cycles, achieve throughput  9721 MB/s
transfer  168 *  6144 Bytes with index= 6208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127561 cycles, achieve throughput  9710 MB/s
transfer  156 *  6656 Bytes with index= 6720 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128403 cycles, achieve throughput  9703 MB/s
transfer  144 *  7168 Bytes with index= 7232 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 127707 cycles, achieve throughput  9699 MB/s
transfer  135 *  7680 Bytes with index= 7744 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128009 cycles, achieve throughput  9719 MB/s
transfer  127 *  8192 Bytes with index= 8256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 128379 cycles, achieve throughput  9724 MB/s
EDMA test complete
Test complete
