JTAG ID= 0x1b98102f. This is a K2H/K2K device, version variant = 1
DEVSTAT= 0x02060ee1. little endian, no boot or I2C slave boot, boot master is ARM core, PLL configuration implies the input clock for core is 122.88MHz
SmartReflex VID= 46, required core voltage= 0.995V.
Die ID= 0x0c011004, 0x04010235, 0x00000000, 0x60ba0001
DSP speed grade = 1200MHz, ARM speed grade= 1200MHz
Enable IRQ and FIQ.
Enable Exception handling...
Initialize main core clock = 122.88MHz/4x39 = 1198MHz
Initialize ARM clock = 125.00MHz/5x48 = 1200MHz
DDR3A initialization
Initialize DDR data rate = 100.000/1*20/6*4= 1333.3 MTS, bus width = 64 bits.
PCIE PHY loopback mode at 5.0GHz.
PCIE link 0 start link training...
PCIE link 0 training is finished.
PCIE memory test passed at address 0x51800000
PCIE memory test passed at address 0x54840000
PCIE memory test passed at address 0x54920000
PCIE MSI8 interrupt generated!
PCIE interrupt latency is 1885 cycles
#########RC starts core access performance test!#########
  204 MB/s, copy  65536 bytes from 0x0c080000( local MSRAM) to 0x54920000(  remote LL2), consumes 385311 cycles
   30 MB/s, copy  65536 bytes from 0x54920000(  remote LL2) to 0x0c080000( local MSRAM), consumes 2569611 cycles
   27 MB/s, copy  65536 bytes from 0x54920000(  remote LL2) to 0x54930000(  remote LL2), consumes 2823768 cycles
  203 MB/s, copy  65536 bytes from 0x0c080000( local MSRAM) to 0x54840000(remote MSRAM), consumes 385799 cycles
   29 MB/s, copy  65536 bytes from 0x54840000(remote MSRAM) to 0x0c080000( local MSRAM), consumes 2678788 cycles
   26 MB/s, copy  65536 bytes from 0x54840000(remote MSRAM) to 0x54850000(remote MSRAM), consumes 2936019 cycles
  203 MB/s, copy  65536 bytes from 0x0c080000( local MSRAM) to 0x51800000(remote DDR3A), consumes 386400 cycles
   27 MB/s, copy  65536 bytes from 0x51800000(remote DDR3A) to 0x0c080000( local MSRAM), consumes 2837688 cycles
   24 MB/s, copy  65536 bytes from 0x51800000(remote DDR3A) to 0x51810000(remote DDR3A), consumes 3170943 cycles
Memory load performance test at 0x54920000(  remote LL2)
Index=   0  Cycles/LDRD= 175.52
Index=   1  Cycles/LDRD= 175.20
Index=   2  Cycles/LDRD= 175.12
Index=   3  Cycles/LDRD= 175.12
Index=   4  Cycles/LDRD= 175.22
Index=   5  Cycles/LDRD= 175.14
Index=   6  Cycles/LDRD= 175.22
Index=   7  Cycles/LDRD= 175.14
Index=   8  Cycles/LDRD= 175.08
Index=  10  Cycles/LDRD= 175.24
Index=  12  Cycles/LDRD= 175.21
Index=  14  Cycles/LDRD= 175.09
Index=  16  Cycles/LDRD= 175.20
Index=  18  Cycles/LDRD= 175.20
Index=  20  Cycles/LDRD= 175.19
Index=  22  Cycles/LDRD= 175.17
Index=  24  Cycles/LDRD= 175.18
Index=  26  Cycles/LDRD= 175.21
Index=  28  Cycles/LDRD= 175.29
Index=  30  Cycles/LDRD= 175.22
Index=  32  Cycles/LDRD= 175.14
Index=  40  Cycles/LDRD= 175.14
Index=  48  Cycles/LDRD= 175.23
Index=  56  Cycles/LDRD= 175.12
Memory store performance test at 0x54920000(  remote LL2)
Index=   0  Cycles/STRD= 92.80
Index=   1  Cycles/STRD= 92.73
Index=   2  Cycles/STRD= 93.20
Index=   3  Cycles/STRD= 92.91
Index=   4  Cycles/STRD= 93.18
Index=   5  Cycles/STRD= 92.85
Index=   6  Cycles/STRD= 92.90
Index=   7  Cycles/STRD= 92.86
Index=   8  Cycles/STRD= 92.86
Index=  10  Cycles/STRD= 93.11
Index=  12  Cycles/STRD= 92.85
Index=  14  Cycles/STRD= 93.64
Index=  16  Cycles/STRD= 93.02
Index=  18  Cycles/STRD= 93.19
Index=  20  Cycles/STRD= 93.31
Index=  22  Cycles/STRD= 93.82
Index=  24  Cycles/STRD= 93.57
Index=  26  Cycles/STRD= 92.87
Index=  28  Cycles/STRD= 92.97
Index=  30  Cycles/STRD= 92.97
Index=  32  Cycles/STRD= 93.07
Index=  40  Cycles/STRD= 92.83
Index=  48  Cycles/STRD= 92.90
Index=  56  Cycles/STRD= 93.06
Memory load performance test at 0x54840000(remote MSRAM)
Index=   0  Cycles/LDRD= 184.42
Index=   1  Cycles/LDRD= 184.53
Index=   2  Cycles/LDRD= 184.57
Index=   3  Cycles/LDRD= 184.50
Index=   4  Cycles/LDRD= 184.86
Index=   5  Cycles/LDRD= 184.43
Index=   6  Cycles/LDRD= 184.59
Index=   7  Cycles/LDRD= 184.44
Index=   8  Cycles/LDRD= 184.28
Index=  10  Cycles/LDRD= 184.54
Index=  12  Cycles/LDRD= 184.60
Index=  14  Cycles/LDRD= 184.50
Index=  16  Cycles/LDRD= 184.24
Index=  18  Cycles/LDRD= 184.48
Index=  20  Cycles/LDRD= 184.72
Index=  22  Cycles/LDRD= 184.58
Index=  24  Cycles/LDRD= 184.27
Index=  26  Cycles/LDRD= 184.62
Index=  28  Cycles/LDRD= 184.68
Index=  30  Cycles/LDRD= 184.55
Index=  32  Cycles/LDRD= 184.39
Index=  40  Cycles/LDRD= 184.54
Index=  48  Cycles/LDRD= 184.48
Index=  56  Cycles/LDRD= 184.50
Index=  64  Cycles/LDRD= 184.61
Index=  96  Cycles/LDRD= 184.73
Index= 128  Cycles/LDRD= 184.95
Index= 192  Cycles/LDRD= 185.07
Memory store performance test at 0x54840000(remote MSRAM)
Index=   0  Cycles/STRD= 93.09
Index=   1  Cycles/STRD= 92.87
Index=   2  Cycles/STRD= 92.95
Index=   3  Cycles/STRD= 93.04
Index=   4  Cycles/STRD= 92.85
Index=   5  Cycles/STRD= 92.96
Index=   6  Cycles/STRD= 92.86
Index=   7  Cycles/STRD= 92.89
Index=   8  Cycles/STRD= 92.95
Index=  10  Cycles/STRD= 92.88
Index=  12  Cycles/STRD= 93.50
Index=  14  Cycles/STRD= 92.76
Index=  16  Cycles/STRD= 93.58
Index=  18  Cycles/STRD= 93.16
Index=  20  Cycles/STRD= 92.88
Index=  22  Cycles/STRD= 93.15
Index=  24  Cycles/STRD= 93.21
Index=  26  Cycles/STRD= 93.42
Index=  28  Cycles/STRD= 93.02
Index=  30  Cycles/STRD= 92.64
Index=  32  Cycles/STRD= 93.21
Index=  40  Cycles/STRD= 92.91
Index=  48  Cycles/STRD= 93.37
Index=  56  Cycles/STRD= 93.58
Index=  64  Cycles/STRD= 93.12
Index=  96  Cycles/STRD= 93.00
Index= 128  Cycles/STRD= 93.16
Index= 192  Cycles/STRD= 93.50
Memory load performance test at 0x51800000(remote DDR3A)
Index=   0  Cycles/LDRD= 196.94
Index=   1  Cycles/LDRD= 198.28
Index=   2  Cycles/LDRD= 201.32
Index=   3  Cycles/LDRD= 199.58
Index=   4  Cycles/LDRD= 198.04
Index=   5  Cycles/LDRD= 195.52
Index=   6  Cycles/LDRD= 196.97
Index=   7  Cycles/LDRD= 200.31
Index=   8  Cycles/LDRD= 197.43
Index=  10  Cycles/LDRD= 195.54
Index=  12  Cycles/LDRD= 199.99
Index=  14  Cycles/LDRD= 198.83
Index=  16  Cycles/LDRD= 198.85
Index=  18  Cycles/LDRD= 196.57
Index=  20  Cycles/LDRD= 200.89
Index=  22  Cycles/LDRD= 196.91
Index=  24  Cycles/LDRD= 197.86
Index=  26  Cycles/LDRD= 198.05
Index=  28  Cycles/LDRD= 199.83
Index=  30  Cycles/LDRD= 197.77
Index=  32  Cycles/LDRD= 198.89
Index=  40  Cycles/LDRD= 199.02
Index=  48  Cycles/LDRD= 198.23
Index=  56  Cycles/LDRD= 199.51
Index=  64  Cycles/LDRD= 199.16
Index=  96  Cycles/LDRD= 196.90
Index= 128  Cycles/LDRD= 202.13
Index= 192  Cycles/LDRD= 197.35
Index= 256  Cycles/LDRD= 202.50
Index= 384  Cycles/LDRD= 199.81
Index= 512  Cycles/LDRD= 204.42
Index= 768  Cycles/LDRD= 206.31
Index=1024  Cycles/LDRD= 204.15
Index=1536  Cycles/LDRD= 203.03
Index=2048  Cycles/LDRD= 205.93
Index=3072  Cycles/LDRD= 203.68
Memory store performance test at 0x51800000(remote DDR3A)
Index=   0  Cycles/STRD= 95.73
Index=   1  Cycles/STRD= 94.45
Index=   2  Cycles/STRD= 93.40
Index=   3  Cycles/STRD= 96.10
Index=   4  Cycles/STRD= 94.83
Index=   5  Cycles/STRD= 95.02
Index=   6  Cycles/STRD= 95.58
Index=   7  Cycles/STRD= 96.42
Index=   8  Cycles/STRD= 94.09
Index=  10  Cycles/STRD= 93.64
Index=  12  Cycles/STRD= 93.44
Index=  14  Cycles/STRD= 95.65
Index=  16  Cycles/STRD= 94.43
Index=  18  Cycles/STRD= 94.56
Index=  20  Cycles/STRD= 96.04
Index=  22  Cycles/STRD= 94.61
Index=  24  Cycles/STRD= 93.72
Index=  26  Cycles/STRD= 94.60
Index=  28  Cycles/STRD= 94.88
Index=  30  Cycles/STRD= 94.27
Index=  32  Cycles/STRD= 96.78
Index=  40  Cycles/STRD= 95.35
Index=  48  Cycles/STRD= 93.34
Index=  56  Cycles/STRD= 95.84
Index=  64  Cycles/STRD= 95.48
Index=  96  Cycles/STRD= 95.31
Index= 128  Cycles/STRD= 97.65
Index= 192  Cycles/STRD= 95.78
Index= 256  Cycles/STRD= 95.03
Index= 384  Cycles/STRD= 94.50
Index= 512  Cycles/STRD= 97.29
Index= 768  Cycles/STRD= 97.30
Index=1024  Cycles/STRD= 94.36
Index=1536  Cycles/STRD= 94.78
Index=2048  Cycles/STRD= 95.40
Index=3072  Cycles/STRD= 94.70
#########RC starts EDMA performance test!#########
Overhead test with EDMA CC0 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    593 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    589 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1702 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1480 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1480 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1589 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC0 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 138685 cycles, achieve throughput   567 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 139824 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140243 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108772 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108796 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 111779 cycles, achieve throughput   703 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140243 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140192 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139572 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108661 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108699 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 112556 cycles, achieve throughput   698 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 139797 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139524 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140795 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108666 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108824 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 112006 cycles, achieve throughput   702 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207732 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207401 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 208057 cycles, achieve throughput   377 MB/s
Overhead test with EDMA CC0 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    589 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1590 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   2032 cycles, achieve throughput     4 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1588 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC0 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 138795 cycles, achieve throughput   566 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140159 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140013 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108672 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108714 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 111994 cycles, achieve throughput   702 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140014 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140514 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 138356 cycles, achieve throughput   568 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108662 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108703 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 112112 cycles, achieve throughput   701 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140901 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140419 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140572 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108666 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108819 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 113002 cycles, achieve throughput   695 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207730 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207394 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 208172 cycles, achieve throughput   377 MB/s
Overhead test with EDMA CC1 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    481 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    474 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1589 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1701 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1586 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC1 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140351 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 138845 cycles, achieve throughput   566 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140028 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108664 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108735 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110994 cycles, achieve throughput   708 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140353 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139966 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140246 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108663 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108722 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 110773 cycles, achieve throughput   709 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140575 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140409 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140572 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108779 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108836 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 112670 cycles, achieve throughput   697 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209284 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207297 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207963 cycles, achieve throughput   378 MB/s
Overhead test with EDMA CC1 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1591 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1592 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1700 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1588 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC1 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140244 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140496 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139469 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108668 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108707 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 111557 cycles, achieve throughput   704 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140478 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139278 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140480 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108690 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108718 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 112664 cycles, achieve throughput   698 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140009 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140004 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140133 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108770 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 109690 cycles, achieve throughput   716 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 113000 cycles, achieve throughput   695 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207613 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207281 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 208065 cycles, achieve throughput   377 MB/s
Overhead test with EDMA CC1 TC2
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    488 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1369 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    474 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1480 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1701 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1367 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1591 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC1 TC2
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140244 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140425 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140476 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108655 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108730 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 111221 cycles, achieve throughput   707 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140685 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140064 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139905 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108668 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108837 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 111989 cycles, achieve throughput   702 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 139797 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139395 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140569 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108675 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108747 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 113336 cycles, achieve throughput   693 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207729 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207265 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 208070 cycles, achieve throughput   377 MB/s
Overhead test with EDMA CC1 TC3
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1368 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    474 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    474 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1697 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    590 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1481 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1700 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1367 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1589 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC1 TC3
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139465 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 139952 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139899 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108659 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108729 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 112329 cycles, achieve throughput   700 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140017 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139745 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139797 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108659 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108694 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 111442 cycles, achieve throughput   705 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140359 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139884 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140573 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108774 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108724 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 113900 cycles, achieve throughput   690 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207730 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207262 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 208171 cycles, achieve throughput   377 MB/s
Overhead test with EDMA CC2 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1701 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1589 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1701 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1587 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC2 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140016 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140318 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140237 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108664 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108727 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 111889 cycles, achieve throughput   702 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140471 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 139743 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140796 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108666 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108818 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 112114 cycles, achieve throughput   701 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140348 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139838 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 139901 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108771 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108841 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 111894 cycles, achieve throughput   702 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207628 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207383 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 208401 cycles, achieve throughput   377 MB/s
Overhead test with EDMA CC2 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    480 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1590 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   2477 cycles, achieve throughput     3 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1364 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1589 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC2 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139689 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 138528 cycles, achieve throughput   567 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140469 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108664 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108706 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 111663 cycles, achieve throughput   704 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140457 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140736 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139455 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108658 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108829 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 111440 cycles, achieve throughput   705 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140463 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139627 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140790 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108667 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108731 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 113235 cycles, achieve throughput   694 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 209179 cycles, achieve throughput   375 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207282 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207852 cycles, achieve throughput   378 MB/s
Overhead test with EDMA CC2 TC2
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    474 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    589 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    593 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   2365 cycles, achieve throughput     4 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1705 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1587 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC2 TC2
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140687 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140068 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140129 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108664 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108739 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 111555 cycles, achieve throughput   704 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140124 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140527 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139794 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108782 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108737 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 111002 cycles, achieve throughput   708 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140908 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 139314 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140241 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108775 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108735 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 113001 cycles, achieve throughput   695 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207620 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207296 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207861 cycles, achieve throughput   378 MB/s
Overhead test with EDMA CC2 TC3
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    482 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    478 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1366 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1590 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1589 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1697 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1364 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1586 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC2 TC3
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140246 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140073 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140463 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108662 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108707 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 112224 cycles, achieve throughput   700 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 140575 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140309 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139347 cycles, achieve throughput   564 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108669 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108729 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 111451 cycles, achieve throughput   705 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140353 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140885 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140350 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108783 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108931 cycles, achieve throughput   721 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 111559 cycles, achieve throughput   704 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207734 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207332 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207953 cycles, achieve throughput   378 MB/s
Overhead test with EDMA CC3 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    479 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    475 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1367 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1589 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    592 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1699 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1365 cycles, achieve throughput     7 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1588 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC3 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 115887 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 116017 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 116107 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 149912 cycles, achieve throughput   524 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 155048 cycles, achieve throughput   507 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 168477 cycles, achieve throughput   466 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 116003 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 115852 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 116669 cycles, achieve throughput   674 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 149914 cycles, achieve throughput   524 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 155178 cycles, achieve throughput   506 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 168257 cycles, achieve throughput   467 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 116115 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 116123 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 117018 cycles, achieve throughput   672 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 150147 cycles, achieve throughput   523 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 155970 cycles, achieve throughput   504 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 174942 cycles, achieve throughput   449 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 247420 cycles, achieve throughput   317 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 247916 cycles, achieve throughput   317 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 250423 cycles, achieve throughput   314 MB/s
Overhead test with EDMA CC3 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    484 cycles, achieve throughput    19 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    476 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    477 cycles, achieve throughput    20 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1589 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1590 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    593 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1699 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1588 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC3 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 115997 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 115906 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 116781 cycles, achieve throughput   673 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 150038 cycles, achieve throughput   524 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 155162 cycles, achieve throughput   506 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 166605 cycles, achieve throughput   472 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 115997 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 115974 cycles, achieve throughput   678 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 116778 cycles, achieve throughput   673 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 150028 cycles, achieve throughput   524 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 155176 cycles, achieve throughput   506 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 170040 cycles, achieve throughput   462 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 116340 cycles, achieve throughput   675 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 116030 cycles, achieve throughput   677 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 116892 cycles, achieve throughput   672 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 150026 cycles, achieve throughput   524 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 155198 cycles, achieve throughput   506 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 173707 cycles, achieve throughput   452 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 247437 cycles, achieve throughput   317 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 247934 cycles, achieve throughput   317 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 251976 cycles, achieve throughput   312 MB/s
Overhead test with EDMA CC4 TC0
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1480 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1586 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    585 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1474 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1705 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1809 cycles, achieve throughput     5 MB/s
Throughput test with EDMA CC4 TC0
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 139794 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 140082 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 140034 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108778 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108712 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110992 cycles, achieve throughput   708 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 139574 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140608 cycles, achieve throughput   559 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 139462 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108660 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108726 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 111440 cycles, achieve throughput   705 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140804 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140304 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 140243 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108671 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108739 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 113333 cycles, achieve throughput   693 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207614 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207297 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 207959 cycles, achieve throughput   378 MB/s
Overhead test with EDMA CC4 TC1
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes    592 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes    587 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes   1477 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes   1587 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes   1479 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes   1588 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes    586 cycles, achieve throughput    16 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes   1475 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes   1478 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes   1697 cycles, achieve throughput     5 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes   1480 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x54800000(remote MSRAM) to 0x54840000(local MSRAM ), consumes   1476 cycles, achieve throughput     6 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes   1593 cycles, achieve throughput     6 MB/s
Throughput test with EDMA CC4 TC1
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54920000(remote LL2  ), consumes 140019 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x54840000(remote MSRAM), consumes 139956 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x10820000(local LL2   ) to 0x51800000(remote DDRA ), consumes 139917 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x10840000(local LL2   ), consumes 108774 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x10840000(local LL2   ), consumes 108718 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x10840000(local LL2   ), consumes 110782 cycles, achieve throughput   709 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54920000(remote LL2  ), consumes 139908 cycles, achieve throughput   562 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x54840000(remote MSRAM), consumes 140275 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(local MSRAM ) to 0x51800000(remote DDRA ), consumes 140241 cycles, achieve throughput   560 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x c0c0000(local MSRAM ), consumes 108664 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x c0c0000(local MSRAM ), consumes 108730 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x c0c0000(local MSRAM ), consumes 111220 cycles, achieve throughput   707 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54920000(remote LL2  ), consumes 140151 cycles, achieve throughput   561 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x54840000(remote MSRAM), consumes 140839 cycles, achieve throughput   558 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x88000000(local DDR   ) to 0x51800000(remote DDRA ), consumes 139574 cycles, achieve throughput   563 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x88100000(local DDR   ), consumes 108664 cycles, achieve throughput   723 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x88100000(local DDR   ), consumes 108821 cycles, achieve throughput   722 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x88100000(local DDR   ), consumes 112111 cycles, achieve throughput   701 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54900000(remote LL2  ) to 0x54920000(remote LL2  ), consumes 207728 cycles, achieve throughput   378 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x54800000(remote MSRAM) to 0x54840000(remote MSRAM), consumes 207386 cycles, achieve throughput   379 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x50800000(remote DDRA ) to 0x51800000(remote DDRA ), consumes 208066 cycles, achieve throughput   377 MB/s
EDMA test complete
PCIE test complete.
