JTAG ID= 0x1b98102f. This is a K2H/K2K device, version variant = 1
DEVSTAT= 0x02060ee1. little endian, no boot or I2C slave boot, boot master is ARM core, PLL configuration implies the input clock for core is 122.88MHz
SmartReflex VID= 46, required core voltage= 0.995V.
Die ID= 0x0c011004, 0x04010235, 0x00000000, 0x60ba0001
DSP speed grade = 1200MHz, ARM speed grade= 1200MHz
Enable IRQ and FIQ.
Enable Exception handling...
Initialize main core clock = 122.88MHz/4x39 = 1198MHz
Initialize ARM clock = 125.00MHz/5x48 = 1200MHz
DDR3A initialization
Initialize DDR data rate = 100.000/1*16/4*4= 1600.0 MTS, bus width = 64 bits.
DDR3B initialization
Initialize DDR data rate = 100.000/1*16/4*4= 1600.0 MTS, bus width = 64 bits.
   83 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c0a0000(MSRAM(strongly ordered)), consumes 1874460 cycles
  126 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 1242536 cycles
  129 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 1218228 cycles
   65 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes 2404038 cycles
  129 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes 1217732 cycles
  129 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 1218981 cycles
   46 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes 3370380 cycles
  129 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes 1218509 cycles
  128 MB/s, copy 131072 bytes from 0x0c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes 1220794 cycles
  127 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c080000(MSRAM(strongly ordered)), consumes 1234564 cycles
  147 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c0e0000(MSRAM(normal non-cache)), consumes 1065807 cycles
  147 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 1067585 cycles
  130 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes 1207890 cycles
  147 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes 1066500 cycles
  147 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 1066126 cycles
  130 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes 1207645 cycles
  147 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes 1065692 cycles
  147 MB/s, copy 131072 bytes from 0x0c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes 1067611 cycles
  682 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c080000(MSRAM(strongly ordered)), consumes 230318 cycles
 3219 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 48847 cycles
 4262 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x0c120000(MSRAM(RA_WB_WA,  in sh)), consumes 36903 cycles
  674 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes 233104 cycles
 1924 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes 81708 cycles
 4180 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 37627 cycles
  649 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes 242304 cycles
 1204 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes 130613 cycles
 3914 MB/s, copy 131072 bytes from 0x0c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes 40180 cycles
   49 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c080000(MSRAM(strongly ordered)), consumes 3193959 cycles
   62 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 2522562 cycles
   61 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 2556216 cycles
   32 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes 4855568 cycles
   43 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x80022000(DDR3A(strongly ordered)), consumes 3622477 cycles
   44 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes 3533558 cycles
   59 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 2623820 cycles
   32 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes 4824953 cycles
   62 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes 2519960 cycles
   61 MB/s, copy 131072 bytes from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes 2557925 cycles
   61 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c080000(MSRAM(strongly ordered)), consumes 2574767 cycles
   64 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 2439442 cycles
   64 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 2433288 cycles
   35 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes 4470039 cycles
   51 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes 3050835 cycles
   64 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x88022000(DDR3A(normal non-cache)), consumes 2437799 cycles
   63 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 2495230 cycles
   61 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes 2565909 cycles
   64 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes 2442518 cycles
   64 MB/s, copy 131072 bytes from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes 2434843 cycles
  681 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c080000(MSRAM(strongly ordered)), consumes 230651 cycles
 3086 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 50965 cycles
 3465 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 45384 cycles
  543 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes 289380 cycles
 1397 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes 112543 cycles
 2435 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes 64586 cycles
 2790 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90022000(DDR3A(RA_WB_WA,  in sh)), consumes 56362 cycles
  645 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes 243695 cycles
 1220 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes 128849 cycles
 3234 MB/s, copy 131072 bytes from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes 48632 cycles
   37 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x0c080000(MSRAM(strongly ordered)), consumes 4205665 cycles
   45 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 3473354 cycles
   44 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 3507460 cycles
   32 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes 4787440 cycles
   45 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes 3469330 cycles
   44 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 3498358 cycles
   23 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes 6835642 cycles
   28 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x60022000(DDR3B(strongly ordered)), consumes 5577071 cycles
   36 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes 4264087 cycles
   44 MB/s, copy 131072 bytes from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes 3567317 cycles
   44 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x0c080000(MSRAM(strongly ordered)), consumes 3560689 cycles
   46 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 3394988 cycles
   46 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 3396277 cycles
   44 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes 3538935 cycles
   46 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes 3386990 cycles
   46 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 3375018 cycles
   30 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes 5223866 cycles
   39 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes 4014746 cycles
   46 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x68022000(DDR3B(normal non-cache)), consumes 3393653 cycles
   45 MB/s, copy 131072 bytes from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes 3446188 cycles
  678 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x0c080000(MSRAM(strongly ordered)), consumes 231891 cycles
 2691 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x0c0c0000(MSRAM(normal non-cache)), consumes 58436 cycles
 2804 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x0c100000(MSRAM(RA_WB_WA,  in sh)), consumes 56076 cycles
  661 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes 237845 cycles
 1884 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes 83472 cycles
 2854 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes 55096 cycles
  524 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes 299847 cycles
  943 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes 166670 cycles
 1992 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes 78920 cycles
 2343 MB/s, copy 131072 bytes from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70022000(DDR3B(RA_WB_WA,  in sh)), consumes 67115 cycles
Memory load performance test at 0x0c080000(MSRAM(strongly ordered))
Index=   0  Cycles/LDRD= 14.55
Index=   1  Cycles/LDRD= 14.97
Index=   2  Cycles/LDRD= 15.30
Index=   3  Cycles/LDRD= 15.10
Index=   4  Cycles/LDRD= 15.28
Index=   5  Cycles/LDRD= 15.29
Index=   6  Cycles/LDRD= 15.30
Index=   7  Cycles/LDRD= 15.25
Index=   8  Cycles/LDRD= 12.68
Index=  10  Cycles/LDRD= 15.30
Index=  12  Cycles/LDRD= 14.92
Index=  14  Cycles/LDRD= 15.24
Index=  16  Cycles/LDRD= 12.70
Index=  18  Cycles/LDRD= 14.47
Index=  20  Cycles/LDRD= 15.28
Index=  22  Cycles/LDRD= 15.30
Index=  24  Cycles/LDRD= 12.70
Index=  26  Cycles/LDRD= 15.30
Index=  28  Cycles/LDRD= 13.90
Index=  30  Cycles/LDRD= 15.30
Index=  32  Cycles/LDRD= 15.30
Index=  40  Cycles/LDRD= 12.65
Index=  48  Cycles/LDRD= 12.69
Index=  56  Cycles/LDRD= 12.70
Memory store performance test at 0x0c080000(MSRAM(strongly ordered))
Index=   0  Cycles/STRD= 8.28
Index=   1  Cycles/STRD= 8.03
Index=   2  Cycles/STRD= 7.80
Index=   3  Cycles/STRD= 7.54
Index=   4  Cycles/STRD= 7.30
Index=   5  Cycles/STRD= 7.04
Index=   6  Cycles/STRD= 6.79
Index=   7  Cycles/STRD= 6.55
Index=   8  Cycles/STRD= 6.30
Index=  10  Cycles/STRD= 6.29
Index=  12  Cycles/STRD= 6.29
Index=  14  Cycles/STRD= 6.28
Index=  16  Cycles/STRD= 6.28
Index=  18  Cycles/STRD= 6.28
Index=  20  Cycles/STRD= 6.28
Index=  22  Cycles/STRD= 6.27
Index=  24  Cycles/STRD= 6.28
Index=  26  Cycles/STRD= 6.28
Index=  28  Cycles/STRD= 6.28
Index=  30  Cycles/STRD= 6.28
Index=  32  Cycles/STRD= 6.28
Index=  40  Cycles/STRD= 6.27
Index=  48  Cycles/STRD= 6.28
Index=  56  Cycles/STRD= 6.28
Memory load performance test at 0x0c0c0000(MSRAM(normal non-cache))
Index=   0  Cycles/LDRD= 64.46
Index=   1  Cycles/LDRD= 65.30
Index=   2  Cycles/LDRD= 65.32
Index=   3  Cycles/LDRD= 65.18
Index=   4  Cycles/LDRD= 65.20
Index=   5  Cycles/LDRD= 65.18
Index=   6  Cycles/LDRD= 65.42
Index=   7  Cycles/LDRD= 65.23
Index=   8  Cycles/LDRD= 64.10
Index=  10  Cycles/LDRD= 65.20
Index=  12  Cycles/LDRD= 65.19
Index=  14  Cycles/LDRD= 65.04
Index=  16  Cycles/LDRD= 64.07
Index=  18  Cycles/LDRD= 65.08
Index=  20  Cycles/LDRD= 65.17
Index=  22  Cycles/LDRD= 65.04
Index=  24  Cycles/LDRD= 63.95
Index=  26  Cycles/LDRD= 65.38
Index=  28  Cycles/LDRD= 65.30
Index=  30  Cycles/LDRD= 65.23
Index=  32  Cycles/LDRD= 64.42
Index=  40  Cycles/LDRD= 64.38
Index=  48  Cycles/LDRD= 64.16
Index=  56  Cycles/LDRD= 64.04
Memory store performance test at 0x0c0c0000(MSRAM(normal non-cache))
Index=   0  Cycles/STRD= 1.94
Index=   1  Cycles/STRD= 2.82
Index=   2  Cycles/STRD= 5.55
Index=   3  Cycles/STRD= 4.95
Index=   4  Cycles/STRD= 4.71
Index=   5  Cycles/STRD= 4.50
Index=   6  Cycles/STRD= 4.55
Index=   7  Cycles/STRD= 4.51
Index=   8  Cycles/STRD= 4.45
Index=  10  Cycles/STRD= 4.48
Index=  12  Cycles/STRD= 4.66
Index=  14  Cycles/STRD= 4.47
Index=  16  Cycles/STRD= 4.44
Index=  18  Cycles/STRD= 4.48
Index=  20  Cycles/STRD= 4.48
Index=  22  Cycles/STRD= 4.63
Index=  24  Cycles/STRD= 4.61
Index=  26  Cycles/STRD= 4.49
Index=  28  Cycles/STRD= 4.49
Index=  30  Cycles/STRD= 4.61
Index=  32  Cycles/STRD= 4.29
Index=  40  Cycles/STRD= 4.44
Index=  48  Cycles/STRD= 4.45
Index=  56  Cycles/STRD= 4.64
Memory load performance test at 0x0c100000(MSRAM(RA_WB_WA,  in sh))
Index=   0  Cycles/LDRD= 1.33
Index=   1  Cycles/LDRD= 2.54
Index=   2  Cycles/LDRD= 3.22
Index=   3  Cycles/LDRD= 4.58
Index=   4  Cycles/LDRD= 5.62
Index=   5  Cycles/LDRD= 7.86
Index=   6  Cycles/LDRD= 9.32
Index=   7  Cycles/LDRD= 10.79
Index=   8  Cycles/LDRD= 11.02
Index=  10  Cycles/LDRD= 11.54
Index=  12  Cycles/LDRD= 11.59
Index=  14  Cycles/LDRD= 12.36
Index=  16  Cycles/LDRD= 16.58
Index=  18  Cycles/LDRD= 12.59
Index=  20  Cycles/LDRD= 12.72
Index=  22  Cycles/LDRD= 13.34
Index=  24  Cycles/LDRD= 13.00
Index=  26  Cycles/LDRD= 13.19
Index=  28  Cycles/LDRD= 13.19
Index=  30  Cycles/LDRD= 14.62
Index=  32  Cycles/LDRD= 26.87
Index=  40  Cycles/LDRD= 13.17
Index=  48  Cycles/LDRD= 14.91
Index=  56  Cycles/LDRD= 11.85
Memory store performance test at 0x0c100000(MSRAM(RA_WB_WA,  in sh))
Index=   0  Cycles/STRD= 1.38
Index=   1  Cycles/STRD= 1.80
Index=   2  Cycles/STRD= 3.36
Index=   3  Cycles/STRD= 4.46
Index=   4  Cycles/STRD= 6.11
Index=   5  Cycles/STRD= 7.34
Index=   6  Cycles/STRD= 8.66
Index=   7  Cycles/STRD= 10.01
Index=   8  Cycles/STRD= 11.49
Index=  10  Cycles/STRD= 11.67
Index=  12  Cycles/STRD= 11.76
Index=  14  Cycles/STRD= 11.52
Index=  16  Cycles/STRD= 17.28
Index=  18  Cycles/STRD= 12.12
Index=  20  Cycles/STRD= 12.22
Index=  22  Cycles/STRD= 12.65
Index=  24  Cycles/STRD= 12.89
Index=  26  Cycles/STRD= 12.46
Index=  28  Cycles/STRD= 12.63
Index=  30  Cycles/STRD= 12.75
Index=  32  Cycles/STRD= 26.18
Index=  40  Cycles/STRD= 12.68
Index=  48  Cycles/STRD= 14.09
Index=  56  Cycles/STRD= 12.40
Memory load performance test at 0x80000000(DDR3A(strongly ordered))
Index=   0  Cycles/LDRD= 24.69
Index=   1  Cycles/LDRD= 24.68
Index=   2  Cycles/LDRD= 24.65
Index=   3  Cycles/LDRD= 26.73
Index=   4  Cycles/LDRD= 26.72
Index=   5  Cycles/LDRD= 24.66
Index=   6  Cycles/LDRD= 24.67
Index=   7  Cycles/LDRD= 24.63
Index=   8  Cycles/LDRD= 26.73
Index=  10  Cycles/LDRD= 24.70
Index=  12  Cycles/LDRD= 24.72
Index=  14  Cycles/LDRD= 24.77
Index=  16  Cycles/LDRD= 25.71
Index=  18  Cycles/LDRD= 24.74
Index=  20  Cycles/LDRD= 24.78
Index=  22  Cycles/LDRD= 24.74
Index=  24  Cycles/LDRD= 25.02
Index=  26  Cycles/LDRD= 24.82
Index=  28  Cycles/LDRD= 25.14
Index=  30  Cycles/LDRD= 24.85
Index=  32  Cycles/LDRD= 25.11
Index=  40  Cycles/LDRD= 25.21
Index=  48  Cycles/LDRD= 25.14
Index=  56  Cycles/LDRD= 25.97
Index=  64  Cycles/LDRD= 25.23
Index=  96  Cycles/LDRD= 25.28
Index= 128  Cycles/LDRD= 26.33
Index= 192  Cycles/LDRD= 26.27
Index= 256  Cycles/LDRD= 27.53
Index= 384  Cycles/LDRD= 27.56
Index= 512  Cycles/LDRD= 30.58
Index= 768  Cycles/LDRD= 30.58
Index=1024  Cycles/LDRD= 30.52
Index=1536  Cycles/LDRD= 31.15
Index=2048  Cycles/LDRD= 30.61
Index=3072  Cycles/LDRD= 33.18
Index=4096  Cycles/LDRD= 31.95
Index=6144  Cycles/LDRD= 30.59
Index=8192  Cycles/LDRD= 63.43
Index=12288  Cycles/LDRD= 31.94
Index=16384  Cycles/LDRD= 65.31
Index=20480  Cycles/LDRD= 31.96
Index=24576  Cycles/LDRD= 63.44
Index=28672  Cycles/LDRD= 31.95
Memory store performance test at 0x80000000(DDR3A(strongly ordered))
Index=   0  Cycles/STRD= 12.34
Index=   1  Cycles/STRD= 14.52
Index=   2  Cycles/STRD= 12.36
Index=   3  Cycles/STRD= 12.36
Index=   4  Cycles/STRD= 12.36
Index=   5  Cycles/STRD= 14.44
Index=   6  Cycles/STRD= 12.35
Index=   7  Cycles/STRD= 12.35
Index=   8  Cycles/STRD= 12.36
Index=  10  Cycles/STRD= 12.35
Index=  12  Cycles/STRD= 12.36
Index=  14  Cycles/STRD= 12.33
Index=  16  Cycles/STRD= 14.51
Index=  18  Cycles/STRD= 12.33
Index=  20  Cycles/STRD= 12.34
Index=  22  Cycles/STRD= 12.34
Index=  24  Cycles/STRD= 12.34
Index=  26  Cycles/STRD= 12.34
Index=  28  Cycles/STRD= 12.34
Index=  30  Cycles/STRD= 12.34
Index=  32  Cycles/STRD= 12.35
Index=  40  Cycles/STRD= 14.42
Index=  48  Cycles/STRD= 12.34
Index=  56  Cycles/STRD= 12.34
Index=  64  Cycles/STRD= 12.34
Index=  96  Cycles/STRD= 12.34
Index= 128  Cycles/STRD= 12.34
Index= 192  Cycles/STRD= 12.33
Index= 256  Cycles/STRD= 14.42
Index= 384  Cycles/STRD= 12.33
Index= 512  Cycles/STRD= 12.70
Index= 768  Cycles/STRD= 14.51
Index=1024  Cycles/STRD= 12.34
Index=1536  Cycles/STRD= 15.33
Index=2048  Cycles/STRD= 19.78
Index=3072  Cycles/STRD= 12.34
Index=4096  Cycles/STRD= 41.26
Index=6144  Cycles/STRD= 19.78
Index=8192  Cycles/STRD= 83.60
Index=12288  Cycles/STRD= 39.24
Index=16384  Cycles/STRD= 79.87
Index=20480  Cycles/STRD= 41.24
Index=24576  Cycles/STRD= 79.74
Index=28672  Cycles/STRD= 41.32
Memory load performance test at 0x88000000(DDR3A(normal non-cache))
Index=   0  Cycles/LDRD= 143.24
Index=   1  Cycles/LDRD= 148.88
Index=   2  Cycles/LDRD= 147.68
Index=   3  Cycles/LDRD= 147.29
Index=   4  Cycles/LDRD= 147.73
Index=   5  Cycles/LDRD= 145.38
Index=   6  Cycles/LDRD= 148.51
Index=   7  Cycles/LDRD= 147.03
Index=   8  Cycles/LDRD= 145.17
Index=  10  Cycles/LDRD= 149.61
Index=  12  Cycles/LDRD= 146.89
Index=  14  Cycles/LDRD= 147.19
Index=  16  Cycles/LDRD= 145.15
Index=  18  Cycles/LDRD= 148.51
Index=  20  Cycles/LDRD= 149.56
Index=  22  Cycles/LDRD= 147.62
Index=  24  Cycles/LDRD= 145.59
Index=  26  Cycles/LDRD= 147.65
Index=  28  Cycles/LDRD= 151.20
Index=  30  Cycles/LDRD= 145.52
Index=  32  Cycles/LDRD= 147.70
Index=  40  Cycles/LDRD= 145.30
Index=  48  Cycles/LDRD= 146.01
Index=  56  Cycles/LDRD= 147.10
Index=  64  Cycles/LDRD= 151.08
Index=  96  Cycles/LDRD= 145.97
Index= 128  Cycles/LDRD= 147.61
Index= 192  Cycles/LDRD= 148.05
Index= 256  Cycles/LDRD= 152.79
Index= 384  Cycles/LDRD= 157.26
Index= 512  Cycles/LDRD= 161.61
Index= 768  Cycles/LDRD= 172.18
Index=1024  Cycles/LDRD= 179.17
Index=1536  Cycles/LDRD= 179.46
Index=2048  Cycles/LDRD= 183.17
Index=3072  Cycles/LDRD= 180.74
Index=4096  Cycles/LDRD= 181.57
Index=6144  Cycles/LDRD= 182.55
Index=8192  Cycles/LDRD= 181.65
Index=12288  Cycles/LDRD= 179.54
Index=16384  Cycles/LDRD= 183.93
Index=20480  Cycles/LDRD= 181.92
Index=24576  Cycles/LDRD= 181.79
Index=28672  Cycles/LDRD= 183.58
Memory store performance test at 0x88000000(DDR3A(normal non-cache))
Index=   0  Cycles/STRD= 2.23
Index=   1  Cycles/STRD= 5.08
Index=   2  Cycles/STRD= 10.13
Index=   3  Cycles/STRD= 9.09
Index=   4  Cycles/STRD= 7.44
Index=   5  Cycles/STRD= 7.65
Index=   6  Cycles/STRD= 7.56
Index=   7  Cycles/STRD= 7.13
Index=   8  Cycles/STRD= 6.95
Index=  10  Cycles/STRD= 6.98
Index=  12  Cycles/STRD= 7.04
Index=  14  Cycles/STRD= 7.05
Index=  16  Cycles/STRD= 7.01
Index=  18  Cycles/STRD= 7.09
Index=  20  Cycles/STRD= 7.16
Index=  22  Cycles/STRD= 7.24
Index=  24  Cycles/STRD= 7.30
Index=  26  Cycles/STRD= 7.35
Index=  28  Cycles/STRD= 9.58
Index=  30  Cycles/STRD= 7.48
Index=  32  Cycles/STRD= 9.31
Index=  40  Cycles/STRD= 7.77
Index=  48  Cycles/STRD= 7.96
Index=  56  Cycles/STRD= 8.17
Index=  64  Cycles/STRD= 8.66
Index=  96  Cycles/STRD= 8.62
Index= 128  Cycles/STRD= 8.80
Index= 192  Cycles/STRD= 9.21
Index= 256  Cycles/STRD= 9.59
Index= 384  Cycles/STRD= 10.12
Index= 512  Cycles/STRD= 9.95
Index= 768  Cycles/STRD= 10.74
Index=1024  Cycles/STRD= 12.11
Index=1536  Cycles/STRD= 17.11
Index=2048  Cycles/STRD= 20.71
Index=3072  Cycles/STRD= 12.32
Index=4096  Cycles/STRD= 37.12
Index=6144  Cycles/STRD= 20.70
Index=8192  Cycles/STRD= 77.58
Index=12288  Cycles/STRD= 37.29
Index=16384  Cycles/STRD= 72.48
Index=20480  Cycles/STRD= 37.30
Index=24576  Cycles/STRD= 76.05
Index=28672  Cycles/STRD= 37.29
Memory load performance test at 0x90000000(DDR3A(RA_WB_WA,  in sh))
Index=   0  Cycles/LDRD= 1.50
Index=   1  Cycles/LDRD= 3.27
Index=   2  Cycles/LDRD= 4.71
Index=   3  Cycles/LDRD= 6.61
Index=   4  Cycles/LDRD= 9.01
Index=   5  Cycles/LDRD= 12.45
Index=   6  Cycles/LDRD= 12.75
Index=   7  Cycles/LDRD= 15.13
Index=   8  Cycles/LDRD= 16.50
Index=  10  Cycles/LDRD= 17.40
Index=  12  Cycles/LDRD= 17.68
Index=  14  Cycles/LDRD= 17.95
Index=  16  Cycles/LDRD= 19.98
Index=  18  Cycles/LDRD= 18.86
Index=  20  Cycles/LDRD= 19.05
Index=  22  Cycles/LDRD= 19.33
Index=  24  Cycles/LDRD= 19.25
Index=  26  Cycles/LDRD= 20.44
Index=  28  Cycles/LDRD= 20.39
Index=  30  Cycles/LDRD= 21.57
Index=  32  Cycles/LDRD= 30.29
Index=  40  Cycles/LDRD= 22.71
Index=  48  Cycles/LDRD= 25.83
Index=  56  Cycles/LDRD= 25.76
Index=  64  Cycles/LDRD= 26.95
Index=  96  Cycles/LDRD= 26.93
Index= 128  Cycles/LDRD= 27.96
Index= 192  Cycles/LDRD= 30.03
Index= 256  Cycles/LDRD= 30.93
Index= 384  Cycles/LDRD= 29.05
Index= 512  Cycles/LDRD= 42.39
Index= 768  Cycles/LDRD= 32.26
Index=1024  Cycles/LDRD= 65.14
Index=1536  Cycles/LDRD= 39.42
Index=2048  Cycles/LDRD= 103.09
Index=3072  Cycles/LDRD= 64.53
Index=4096  Cycles/LDRD= 102.46
Index=6144  Cycles/LDRD= 100.36
Index=8192  Cycles/LDRD= 108.58
Index=12288  Cycles/LDRD= 101.81
Index=16384  Cycles/LDRD= 105.88
Index=20480  Cycles/LDRD= 105.14
Index=24576  Cycles/LDRD= 106.20
Index=28672  Cycles/LDRD= 102.35
Memory store performance test at 0x90000000(DDR3A(RA_WB_WA,  in sh))
Index=   0  Cycles/STRD= 1.38
Index=   1  Cycles/STRD= 1.98
Index=   2  Cycles/STRD= 4.59
Index=   3  Cycles/STRD= 6.70
Index=   4  Cycles/STRD= 8.94
Index=   5  Cycles/STRD= 11.49
Index=   6  Cycles/STRD= 13.71
Index=   7  Cycles/STRD= 18.68
Index=   8  Cycles/STRD= 17.29
Index=  10  Cycles/STRD= 18.14
Index=  12  Cycles/STRD= 17.96
Index=  14  Cycles/STRD= 18.01
Index=  16  Cycles/STRD= 20.94
Index=  18  Cycles/STRD= 18.82
Index=  20  Cycles/STRD= 18.60
Index=  22  Cycles/STRD= 19.82
Index=  24  Cycles/STRD= 21.62
Index=  26  Cycles/STRD= 19.91
Index=  28  Cycles/STRD= 20.52
Index=  30  Cycles/STRD= 21.08
Index=  32  Cycles/STRD= 30.05
Index=  40  Cycles/STRD= 21.56
Index=  48  Cycles/STRD= 26.84
Index=  56  Cycles/STRD= 26.77
Index=  64  Cycles/STRD= 26.75
Index=  96  Cycles/STRD= 29.94
Index= 128  Cycles/STRD= 28.83
Index= 192  Cycles/STRD= 28.60
Index= 256  Cycles/STRD= 34.87
Index= 384  Cycles/STRD= 33.06
Index= 512  Cycles/STRD= 51.13
Index= 768  Cycles/STRD= 35.54
Index=1024  Cycles/STRD= 77.69
Index=1536  Cycles/STRD= 53.35
Index=2048  Cycles/STRD= 116.38
Index=3072  Cycles/STRD= 78.23
Index=4096  Cycles/STRD= 127.70
Index=6144  Cycles/STRD= 116.84
Index=8192  Cycles/STRD= 157.73
Index=12288  Cycles/STRD= 127.04
Index=16384  Cycles/STRD= 160.98
Index=20480  Cycles/STRD= 126.84
Index=24576  Cycles/STRD= 158.75
Index=28672  Cycles/STRD= 128.89
Memory load performance test at 0x60000000(DDR3B(strongly ordered))
Index=   0  Cycles/LDRD= 35.04
Index=   1  Cycles/LDRD= 33.14
Index=   2  Cycles/LDRD= 35.07
Index=   3  Cycles/LDRD= 33.14
Index=   4  Cycles/LDRD= 33.12
Index=   5  Cycles/LDRD= 33.13
Index=   6  Cycles/LDRD= 33.12
Index=   7  Cycles/LDRD= 34.93
Index=   8  Cycles/LDRD= 33.15
Index=  10  Cycles/LDRD= 33.53
Index=  12  Cycles/LDRD= 33.18
Index=  14  Cycles/LDRD= 33.17
Index=  16  Cycles/LDRD= 33.19
Index=  18  Cycles/LDRD= 33.21
Index=  20  Cycles/LDRD= 33.19
Index=  22  Cycles/LDRD= 35.03
Index=  24  Cycles/LDRD= 33.40
Index=  26  Cycles/LDRD= 33.23
Index=  28  Cycles/LDRD= 33.50
Index=  30  Cycles/LDRD= 33.21
Index=  32  Cycles/LDRD= 33.38
Index=  40  Cycles/LDRD= 33.42
Index=  48  Cycles/LDRD= 33.52
Index=  56  Cycles/LDRD= 34.27
Index=  64  Cycles/LDRD= 34.26
Index=  96  Cycles/LDRD= 33.78
Index= 128  Cycles/LDRD= 34.51
Index= 192  Cycles/LDRD= 34.55
Index= 256  Cycles/LDRD= 35.96
Index= 384  Cycles/LDRD= 36.04
Index= 512  Cycles/LDRD= 39.59
Index= 768  Cycles/LDRD= 39.04
Index=1024  Cycles/LDRD= 39.12
Index=1536  Cycles/LDRD= 39.17
Index=2048  Cycles/LDRD= 39.15
Index=3072  Cycles/LDRD= 39.12
Index=4096  Cycles/LDRD= 39.80
Index=6144  Cycles/LDRD= 39.11
Index=8192  Cycles/LDRD= 60.54
Index=12288  Cycles/LDRD= 39.17
Index=16384  Cycles/LDRD= 62.85
Index=20480  Cycles/LDRD= 39.19
Index=24576  Cycles/LDRD= 62.40
Index=28672  Cycles/LDRD= 39.17
Memory store performance test at 0x60000000(DDR3B(strongly ordered))
Index=   0  Cycles/STRD= 12.87
Index=   1  Cycles/STRD= 12.90
Index=   2  Cycles/STRD= 12.90
Index=   3  Cycles/STRD= 12.95
Index=   4  Cycles/STRD= 12.96
Index=   5  Cycles/STRD= 12.98
Index=   6  Cycles/STRD= 12.94
Index=   7  Cycles/STRD= 12.99
Index=   8  Cycles/STRD= 14.88
Index=  10  Cycles/STRD= 13.01
Index=  12  Cycles/STRD= 13.45
Index=  14  Cycles/STRD= 13.09
Index=  16  Cycles/STRD= 13.11
Index=  18  Cycles/STRD= 13.20
Index=  20  Cycles/STRD= 13.24
Index=  22  Cycles/STRD= 13.27
Index=  24  Cycles/STRD= 13.38
Index=  26  Cycles/STRD= 13.42
Index=  28  Cycles/STRD= 13.52
Index=  30  Cycles/STRD= 15.11
Index=  32  Cycles/STRD= 13.59
Index=  40  Cycles/STRD= 13.95
Index=  48  Cycles/STRD= 14.16
Index=  56  Cycles/STRD= 14.48
Index=  64  Cycles/STRD= 14.61
Index=  96  Cycles/STRD= 16.20
Index= 128  Cycles/STRD= 16.68
Index= 192  Cycles/STRD= 16.22
Index= 256  Cycles/STRD= 16.78
Index= 384  Cycles/STRD= 16.63
Index= 512  Cycles/STRD= 16.86
Index= 768  Cycles/STRD= 17.09
Index=1024  Cycles/STRD= 17.25
Index=1536  Cycles/STRD= 17.28
Index=2048  Cycles/STRD= 19.88
Index=3072  Cycles/STRD= 17.82
Index=4096  Cycles/STRD= 39.34
Index=6144  Cycles/STRD= 19.89
Index=8192  Cycles/STRD= 82.61
Index=12288  Cycles/STRD= 39.34
Index=16384  Cycles/STRD= 82.70
Index=20480  Cycles/STRD= 39.33
Index=24576  Cycles/STRD= 82.59
Index=28672  Cycles/STRD= 39.34
Memory load performance test at 0x68000000(DDR3B(normal non-cache))
Index=   0  Cycles/LDRD= 206.33
Index=   1  Cycles/LDRD= 205.70
Index=   2  Cycles/LDRD= 207.21
Index=   3  Cycles/LDRD= 205.49
Index=   4  Cycles/LDRD= 204.80
Index=   5  Cycles/LDRD= 204.95
Index=   6  Cycles/LDRD= 205.26
Index=   7  Cycles/LDRD= 205.51
Index=   8  Cycles/LDRD= 204.04
Index=  10  Cycles/LDRD= 206.24
Index=  12  Cycles/LDRD= 205.62
Index=  14  Cycles/LDRD= 210.10
Index=  16  Cycles/LDRD= 204.35
Index=  18  Cycles/LDRD= 205.73
Index=  20  Cycles/LDRD= 204.56
Index=  22  Cycles/LDRD= 207.85
Index=  24  Cycles/LDRD= 204.41
Index=  26  Cycles/LDRD= 207.62
Index=  28  Cycles/LDRD= 201.63
Index=  30  Cycles/LDRD= 205.31
Index=  32  Cycles/LDRD= 204.72
Index=  40  Cycles/LDRD= 204.86
Index=  48  Cycles/LDRD= 205.47
Index=  56  Cycles/LDRD= 204.92
Index=  64  Cycles/LDRD= 204.83
Index=  96  Cycles/LDRD= 205.26
Index= 128  Cycles/LDRD= 209.40
Index= 192  Cycles/LDRD= 210.34
Index= 256  Cycles/LDRD= 211.56
Index= 384  Cycles/LDRD= 215.35
Index= 512  Cycles/LDRD= 219.61
Index= 768  Cycles/LDRD= 229.88
Index=1024  Cycles/LDRD= 236.61
Index=1536  Cycles/LDRD= 236.68
Index=2048  Cycles/LDRD= 241.51
Index=3072  Cycles/LDRD= 236.57
Index=4096  Cycles/LDRD= 244.21
Index=6144  Cycles/LDRD= 239.96
Index=8192  Cycles/LDRD= 241.73
Index=12288  Cycles/LDRD= 241.02
Index=16384  Cycles/LDRD= 243.92
Index=20480  Cycles/LDRD= 241.16
Index=24576  Cycles/LDRD= 241.88
Index=28672  Cycles/LDRD= 243.14
Memory store performance test at 0x68000000(DDR3B(normal non-cache))
Index=   0  Cycles/STRD= 3.42
Index=   1  Cycles/STRD= 7.97
Index=   2  Cycles/STRD= 15.21
Index=   3  Cycles/STRD= 14.58
Index=   4  Cycles/STRD= 12.33
Index=   5  Cycles/STRD= 12.46
Index=   6  Cycles/STRD= 12.12
Index=   7  Cycles/STRD= 11.82
Index=   8  Cycles/STRD= 11.43
Index=  10  Cycles/STRD= 11.40
Index=  12  Cycles/STRD= 11.38
Index=  14  Cycles/STRD= 11.39
Index=  16  Cycles/STRD= 11.39
Index=  18  Cycles/STRD= 12.03
Index=  20  Cycles/STRD= 11.77
Index=  22  Cycles/STRD= 12.14
Index=  24  Cycles/STRD= 11.46
Index=  26  Cycles/STRD= 11.55
Index=  28  Cycles/STRD= 11.62
Index=  30  Cycles/STRD= 11.88
Index=  32  Cycles/STRD= 11.86
Index=  40  Cycles/STRD= 11.88
Index=  48  Cycles/STRD= 11.69
Index=  56  Cycles/STRD= 11.86
Index=  64  Cycles/STRD= 12.19
Index=  96  Cycles/STRD= 12.92
Index= 128  Cycles/STRD= 12.51
Index= 192  Cycles/STRD= 13.39
Index= 256  Cycles/STRD= 13.78
Index= 384  Cycles/STRD= 14.07
Index= 512  Cycles/STRD= 14.20
Index= 768  Cycles/STRD= 15.28
Index=1024  Cycles/STRD= 16.04
Index=1536  Cycles/STRD= 16.92
Index=2048  Cycles/STRD= 21.68
Index=3072  Cycles/STRD= 15.86
Index=4096  Cycles/STRD= 37.61
Index=6144  Cycles/STRD= 21.39
Index=8192  Cycles/STRD= 76.62
Index=12288  Cycles/STRD= 37.60
Index=16384  Cycles/STRD= 74.78
Index=20480  Cycles/STRD= 37.61
Index=24576  Cycles/STRD= 76.62
Index=28672  Cycles/STRD= 37.61
Memory load performance test at 0x70000000(DDR3B(RA_WB_WA,  in sh))
Index=   0  Cycles/LDRD= 1.60
Index=   1  Cycles/LDRD= 4.17
Index=   2  Cycles/LDRD= 6.61
Index=   3  Cycles/LDRD= 8.48
Index=   4  Cycles/LDRD= 11.43
Index=   5  Cycles/LDRD= 14.13
Index=   6  Cycles/LDRD= 15.86
Index=   7  Cycles/LDRD= 18.57
Index=   8  Cycles/LDRD= 21.39
Index=  10  Cycles/LDRD= 21.68
Index=  12  Cycles/LDRD= 22.00
Index=  14  Cycles/LDRD= 22.00
Index=  16  Cycles/LDRD= 24.01
Index=  18  Cycles/LDRD= 23.62
Index=  20  Cycles/LDRD= 23.38
Index=  22  Cycles/LDRD= 24.40
Index=  24  Cycles/LDRD= 24.77
Index=  26  Cycles/LDRD= 25.00
Index=  28  Cycles/LDRD= 25.81
Index=  30  Cycles/LDRD= 26.63
Index=  32  Cycles/LDRD= 33.29
Index=  40  Cycles/LDRD= 25.89
Index=  48  Cycles/LDRD= 35.77
Index=  56  Cycles/LDRD= 34.31
Index=  64  Cycles/LDRD= 36.89
Index=  96  Cycles/LDRD= 34.92
Index= 128  Cycles/LDRD= 35.88
Index= 192  Cycles/LDRD= 35.83
Index= 256  Cycles/LDRD= 37.41
Index= 384  Cycles/LDRD= 37.22
Index= 512  Cycles/LDRD= 50.39
Index= 768  Cycles/LDRD= 42.31
Index=1024  Cycles/LDRD= 86.96
Index=1536  Cycles/LDRD= 48.90
Index=2048  Cycles/LDRD= 149.81
Index=3072  Cycles/LDRD= 74.38
Index=4096  Cycles/LDRD= 143.08
Index=6144  Cycles/LDRD= 138.92
Index=8192  Cycles/LDRD= 136.53
Index=12288  Cycles/LDRD= 130.95
Index=16384  Cycles/LDRD= 138.65
Index=20480  Cycles/LDRD= 129.29
Index=24576  Cycles/LDRD= 138.25
Index=28672  Cycles/LDRD= 132.63
Memory store performance test at 0x70000000(DDR3B(RA_WB_WA,  in sh))
Index=   0  Cycles/STRD= 1.42
Index=   1  Cycles/STRD= 2.62
Index=   2  Cycles/STRD= 5.88
Index=   3  Cycles/STRD= 8.37
Index=   4  Cycles/STRD= 11.80
Index=   5  Cycles/STRD= 18.28
Index=   6  Cycles/STRD= 17.93
Index=   7  Cycles/STRD= 23.42
Index=   8  Cycles/STRD= 25.15
Index=  10  Cycles/STRD= 23.26
Index=  12  Cycles/STRD= 23.99
Index=  14  Cycles/STRD= 23.28
Index=  16  Cycles/STRD= 25.99
Index=  18  Cycles/STRD= 25.17
Index=  20  Cycles/STRD= 24.63
Index=  22  Cycles/STRD= 25.86
Index=  24  Cycles/STRD= 25.53
Index=  26  Cycles/STRD= 25.94
Index=  28  Cycles/STRD= 26.88
Index=  30  Cycles/STRD= 27.20
Index=  32  Cycles/STRD= 33.65
Index=  40  Cycles/STRD= 31.65
Index=  48  Cycles/STRD= 35.87
Index=  56  Cycles/STRD= 35.24
Index=  64  Cycles/STRD= 37.27
Index=  96  Cycles/STRD= 36.79
Index= 128  Cycles/STRD= 37.89
Index= 192  Cycles/STRD= 38.84
Index= 256  Cycles/STRD= 43.38
Index= 384  Cycles/STRD= 39.72
Index= 512  Cycles/STRD= 63.36
Index= 768  Cycles/STRD= 47.27
Index=1024  Cycles/STRD= 92.12
Index=1536  Cycles/STRD= 65.47
Index=2048  Cycles/STRD= 145.49
Index=3072  Cycles/STRD= 69.01
Index=4096  Cycles/STRD= 162.90
Index=6144  Cycles/STRD= 148.59
Index=8192  Cycles/STRD= 189.63
Index=12288  Cycles/STRD= 162.78
Index=16384  Cycles/STRD= 184.51
Index=20480  Cycles/STRD= 157.30
Index=24576  Cycles/STRD= 181.39
Index=28672  Cycles/STRD= 161.93
Throughput test with EDMA0 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15831 cycles, achieve throughput  9935 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15762 cycles, achieve throughput  9978 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15776 cycles, achieve throughput  9969 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16334 cycles, achieve throughput  9629 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  17437 cycles, achieve throughput  9020 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  17338 cycles, achieve throughput  9071 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  14918 cycles, achieve throughput 10543 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  14815 cycles, achieve throughput 10616 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14936 cycles, achieve throughput 10530 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15675 cycles, achieve throughput 10034 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15660 cycles, achieve throughput 10043 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15699 cycles, achieve throughput 10018 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16387 cycles, achieve throughput  9598 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16338 cycles, achieve throughput  9627 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  17372 cycles, achieve throughput  9054 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  14805 cycles, achieve throughput 10623 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  14932 cycles, achieve throughput 10533 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14933 cycles, achieve throughput 10532 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15704 cycles, achieve throughput 10015 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15709 cycles, achieve throughput 10012 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15800 cycles, achieve throughput  9954 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16445 cycles, achieve throughput  9564 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  17398 cycles, achieve throughput  9040 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16469 cycles, achieve throughput  9550 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  14923 cycles, achieve throughput 10539 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  14922 cycles, achieve throughput 10540 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14919 cycles, achieve throughput 10542 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  20564 cycles, achieve throughput  7648 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20573 cycles, achieve throughput  7645 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20514 cycles, achieve throughput  7667 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  48540 cycles, achieve throughput  3240 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  48015 cycles, achieve throughput  3275 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  46847 cycles, achieve throughput  3357 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  20803 cycles, achieve throughput  7560 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  20804 cycles, achieve throughput  7560 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  21936 cycles, achieve throughput  7170 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  20762 cycles, achieve throughput  7575 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20546 cycles, achieve throughput  7655 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20520 cycles, achieve throughput  7665 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  47244 cycles, achieve throughput  3329 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  47234 cycles, achieve throughput  3329 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  47249 cycles, achieve throughput  3328 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  20918 cycles, achieve throughput  7519 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  21679 cycles, achieve throughput  7255 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  20678 cycles, achieve throughput  7606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  20973 cycles, achieve throughput  7499 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  21208 cycles, achieve throughput  7416 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  21332 cycles, achieve throughput  7373 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  48998 cycles, achieve throughput  3210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  47632 cycles, achieve throughput  3302 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  48785 cycles, achieve throughput  3224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  21150 cycles, achieve throughput  7436 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  22561 cycles, achieve throughput  6971 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  21358 cycles, achieve throughput  7364 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  18818 cycles, achieve throughput  8358 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  18843 cycles, achieve throughput  8347 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  18793 cycles, achieve throughput  8369 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  18820 cycles, achieve throughput  8357 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  18904 cycles, achieve throughput  8320 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  19734 cycles, achieve throughput  7970 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  41512 cycles, achieve throughput  3788 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  42627 cycles, achieve throughput  3689 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  41509 cycles, achieve throughput  3789 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  18785 cycles, achieve throughput  8372 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  18828 cycles, achieve throughput  8353 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  18802 cycles, achieve throughput  8365 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  18836 cycles, achieve throughput  8350 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  18826 cycles, achieve throughput  8354 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  19672 cycles, achieve throughput  7995 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  41514 cycles, achieve throughput  3788 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  41738 cycles, achieve throughput  3768 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  41508 cycles, achieve throughput  3789 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  20334 cycles, achieve throughput  7735 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  19968 cycles, achieve throughput  7876 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20064 cycles, achieve throughput  7839 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  20313 cycles, achieve throughput  7743 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  20122 cycles, achieve throughput  7816 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  20586 cycles, achieve throughput  7640 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  42402 cycles, achieve throughput  3709 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  42064 cycles, achieve throughput  3739 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  42067 cycles, achieve throughput  3738 MB/s
Throughput test with EDMA0 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15705 cycles, achieve throughput 10015 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15734 cycles, achieve throughput  9996 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15705 cycles, achieve throughput 10015 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16416 cycles, achieve throughput  9581 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16353 cycles, achieve throughput  9618 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16466 cycles, achieve throughput  9552 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  14816 cycles, achieve throughput 10615 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  14932 cycles, achieve throughput 10533 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14755 cycles, achieve throughput 10659 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15701 cycles, achieve throughput 10017 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15650 cycles, achieve throughput 10050 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15672 cycles, achieve throughput 10036 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  17476 cycles, achieve throughput  9000 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16287 cycles, achieve throughput  9657 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16400 cycles, achieve throughput  9590 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  14825 cycles, achieve throughput 10609 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  14932 cycles, achieve throughput 10533 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14928 cycles, achieve throughput 10536 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15692 cycles, achieve throughput 10023 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15678 cycles, achieve throughput 10032 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15696 cycles, achieve throughput 10020 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16517 cycles, achieve throughput  9522 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16374 cycles, achieve throughput  9605 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16381 cycles, achieve throughput  9601 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  14921 cycles, achieve throughput 10541 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  14813 cycles, achieve throughput 10618 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14923 cycles, achieve throughput 10539 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  22031 cycles, achieve throughput  7139 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  21780 cycles, achieve throughput  7221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20521 cycles, achieve throughput  7664 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  46786 cycles, achieve throughput  3361 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  48328 cycles, achieve throughput  3254 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  48545 cycles, achieve throughput  3240 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  21012 cycles, achieve throughput  7485 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  21930 cycles, achieve throughput  7172 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  20477 cycles, achieve throughput  7681 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  20757 cycles, achieve throughput  7577 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20659 cycles, achieve throughput  7613 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20794 cycles, achieve throughput  7564 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  48013 cycles, achieve throughput  3275 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  48175 cycles, achieve throughput  3264 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  47964 cycles, achieve throughput  3279 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  22249 cycles, achieve throughput  7069 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  20488 cycles, achieve throughput  7677 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  20806 cycles, achieve throughput  7559 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  21387 cycles, achieve throughput  7354 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  21239 cycles, achieve throughput  7405 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  21383 cycles, achieve throughput  7355 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  49005 cycles, achieve throughput  3209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  47842 cycles, achieve throughput  3287 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  47847 cycles, achieve throughput  3287 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  22022 cycles, achieve throughput  7142 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  22339 cycles, achieve throughput  7040 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  22690 cycles, achieve throughput  6931 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  18793 cycles, achieve throughput  8369 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  18878 cycles, achieve throughput  8331 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  18837 cycles, achieve throughput  8349 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  18900 cycles, achieve throughput  8322 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  18813 cycles, achieve throughput  8360 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  18784 cycles, achieve throughput  8373 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  42623 cycles, achieve throughput  3690 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  42400 cycles, achieve throughput  3709 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  41515 cycles, achieve throughput  3788 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  18800 cycles, achieve throughput  8366 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  18851 cycles, achieve throughput  8343 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  19162 cycles, achieve throughput  8208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  18858 cycles, achieve throughput  8340 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  20066 cycles, achieve throughput  7838 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  18926 cycles, achieve throughput  8310 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  41065 cycles, achieve throughput  3830 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  40953 cycles, achieve throughput  3840 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  42285 cycles, achieve throughput  3719 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  20299 cycles, achieve throughput  7748 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20000 cycles, achieve throughput  7864 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20289 cycles, achieve throughput  7752 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  21257 cycles, achieve throughput  7399 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  20100 cycles, achieve throughput  7825 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  19914 cycles, achieve throughput  7898 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  43066 cycles, achieve throughput  3652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  42399 cycles, achieve throughput  3709 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  42404 cycles, achieve throughput  3709 MB/s
Throughput test with EDMA1 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25270 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25267 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25353 cycles, achieve throughput  6203 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25375 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25346 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25435 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25510 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25519 cycles, achieve throughput  6163 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25363 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25363 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25370 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  26141 cycles, achieve throughput  6016 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25377 cycles, achieve throughput  6197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25512 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25441 cycles, achieve throughput  6182 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25653 cycles, achieve throughput  6131 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25270 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25271 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25374 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  26145 cycles, achieve throughput  6015 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26256 cycles, achieve throughput  5990 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25438 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25432 cycles, achieve throughput  6184 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25436 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  29439 cycles, achieve throughput  5342 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29448 cycles, achieve throughput  5341 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29540 cycles, achieve throughput  5324 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  62125 cycles, achieve throughput  2531 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  61035 cycles, achieve throughput  2576 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60076 cycles, achieve throughput  2618 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  29907 cycles, achieve throughput  5259 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  28689 cycles, achieve throughput  5482 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28569 cycles, achieve throughput  5505 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  29463 cycles, achieve throughput  5338 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28440 cycles, achieve throughput  5530 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28350 cycles, achieve throughput  5548 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  60831 cycles, achieve throughput  2585 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  61338 cycles, achieve throughput  2564 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61210 cycles, achieve throughput  2569 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  29785 cycles, achieve throughput  5280 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  28776 cycles, achieve throughput  5465 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28796 cycles, achieve throughput  5462 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  31129 cycles, achieve throughput  5052 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29103 cycles, achieve throughput  5404 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29142 cycles, achieve throughput  5397 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  62002 cycles, achieve throughput  2536 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61579 cycles, achieve throughput  2554 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  61562 cycles, achieve throughput  2554 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  29366 cycles, achieve throughput  5356 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  29250 cycles, achieve throughput  5377 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29604 cycles, achieve throughput  5313 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  26516 cycles, achieve throughput  5931 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26487 cycles, achieve throughput  5938 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26599 cycles, achieve throughput  5913 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  26709 cycles, achieve throughput  5888 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26817 cycles, achieve throughput  5865 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27670 cycles, achieve throughput  5684 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  52188 cycles, achieve throughput  3013 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  53074 cycles, achieve throughput  2963 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  53515 cycles, achieve throughput  2939 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  26566 cycles, achieve throughput  5920 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26836 cycles, achieve throughput  5861 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26889 cycles, achieve throughput  5849 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  27716 cycles, achieve throughput  5674 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  26913 cycles, achieve throughput  5844 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27497 cycles, achieve throughput  5720 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  51851 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  51962 cycles, achieve throughput  3026 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51847 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28176 cycles, achieve throughput  5582 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28166 cycles, achieve throughput  5584 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27824 cycles, achieve throughput  5652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  28928 cycles, achieve throughput  5437 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  28607 cycles, achieve throughput  5498 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  28164 cycles, achieve throughput  5584 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  52960 cycles, achieve throughput  2969 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  52958 cycles, achieve throughput  2970 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  54182 cycles, achieve throughput  2902 MB/s
Throughput test with EDMA1 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25363 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25603 cycles, achieve throughput  6143 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25366 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25339 cycles, achieve throughput  6207 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25539 cycles, achieve throughput  6158 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25430 cycles, achieve throughput  6185 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25628 cycles, achieve throughput  6137 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25288 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25373 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25389 cycles, achieve throughput  6195 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26139 cycles, achieve throughput  6017 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25434 cycles, achieve throughput  6184 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25438 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25437 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25267 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25363 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25367 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26128 cycles, achieve throughput  6019 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25441 cycles, achieve throughput  6182 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25515 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25514 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  29424 cycles, achieve throughput  5345 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28382 cycles, achieve throughput  5541 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28380 cycles, achieve throughput  5542 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  61144 cycles, achieve throughput  2572 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  60403 cycles, achieve throughput  2603 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60051 cycles, achieve throughput  2619 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  29898 cycles, achieve throughput  5260 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  28669 cycles, achieve throughput  5486 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28682 cycles, achieve throughput  5483 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  29457 cycles, achieve throughput  5339 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28318 cycles, achieve throughput  5554 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28331 cycles, achieve throughput  5551 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  60349 cycles, achieve throughput  2606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  60924 cycles, achieve throughput  2581 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61380 cycles, achieve throughput  2562 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  28587 cycles, achieve throughput  5502 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  28650 cycles, achieve throughput  5489 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29783 cycles, achieve throughput  5281 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30119 cycles, achieve throughput  5222 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30096 cycles, achieve throughput  5226 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29123 cycles, achieve throughput  5400 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61873 cycles, achieve throughput  2542 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  60860 cycles, achieve throughput  2584 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  61695 cycles, achieve throughput  2549 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  30765 cycles, achieve throughput  5112 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  30127 cycles, achieve throughput  5220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29468 cycles, achieve throughput  5337 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  26480 cycles, achieve throughput  5939 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26763 cycles, achieve throughput  5877 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26862 cycles, achieve throughput  5855 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  26921 cycles, achieve throughput  5842 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  27687 cycles, achieve throughput  5680 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27731 cycles, achieve throughput  5671 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  51848 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  51959 cycles, achieve throughput  3027 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51852 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  26833 cycles, achieve throughput  5861 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26912 cycles, achieve throughput  5844 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26853 cycles, achieve throughput  5857 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  27386 cycles, achieve throughput  5743 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  27458 cycles, achieve throughput  5728 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26561 cycles, achieve throughput  5921 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  52184 cycles, achieve throughput  3014 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  53296 cycles, achieve throughput  2951 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51962 cycles, achieve throughput  3026 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  27848 cycles, achieve throughput  5648 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27847 cycles, achieve throughput  5648 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28055 cycles, achieve throughput  5606 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  27821 cycles, achieve throughput  5653 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  29152 cycles, achieve throughput  5395 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27833 cycles, achieve throughput  5651 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  52855 cycles, achieve throughput  2975 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  53415 cycles, achieve throughput  2944 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  53302 cycles, achieve throughput  2950 MB/s
Throughput test with EDMA1 TC2
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25322 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25371 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25345 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25385 cycles, achieve throughput  6196 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25515 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25438 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25632 cycles, achieve throughput  6136 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25290 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25289 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25366 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25357 cycles, achieve throughput  6202 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  26241 cycles, achieve throughput  5993 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25393 cycles, achieve throughput  6194 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25518 cycles, achieve throughput  6163 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25511 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25524 cycles, achieve throughput  6162 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25270 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25275 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25346 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  26130 cycles, achieve throughput  6019 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25331 cycles, achieve throughput  6209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25436 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25505 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25434 cycles, achieve throughput  6184 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28372 cycles, achieve throughput  5543 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28317 cycles, achieve throughput  5554 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28353 cycles, achieve throughput  5547 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  61214 cycles, achieve throughput  2569 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  61128 cycles, achieve throughput  2573 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61115 cycles, achieve throughput  2573 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  30898 cycles, achieve throughput  5090 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  28576 cycles, achieve throughput  5504 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28570 cycles, achieve throughput  5505 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  29443 cycles, achieve throughput  5342 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28358 cycles, achieve throughput  5546 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28348 cycles, achieve throughput  5548 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  61210 cycles, achieve throughput  2569 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  60579 cycles, achieve throughput  2596 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60663 cycles, achieve throughput  2592 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  28458 cycles, achieve throughput  5526 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  28439 cycles, achieve throughput  5530 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28781 cycles, achieve throughput  5464 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  29121 cycles, achieve throughput  5401 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29128 cycles, achieve throughput  5399 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28882 cycles, achieve throughput  5445 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  60681 cycles, achieve throughput  2592 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61535 cycles, achieve throughput  2556 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  60478 cycles, achieve throughput  2600 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  30129 cycles, achieve throughput  5220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  30714 cycles, achieve throughput  5121 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29351 cycles, achieve throughput  5358 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  26919 cycles, achieve throughput  5842 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26558 cycles, achieve throughput  5922 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26841 cycles, achieve throughput  5859 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  26714 cycles, achieve throughput  5887 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26591 cycles, achieve throughput  5915 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26605 cycles, achieve throughput  5911 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  51961 cycles, achieve throughput  3027 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  51849 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51853 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  26857 cycles, achieve throughput  5856 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26803 cycles, achieve throughput  5868 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26583 cycles, achieve throughput  5916 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  26837 cycles, achieve throughput  5860 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  26778 cycles, achieve throughput  5873 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27709 cycles, achieve throughput  5676 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  53075 cycles, achieve throughput  2963 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  52861 cycles, achieve throughput  2975 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  53296 cycles, achieve throughput  2951 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28156 cycles, achieve throughput  5586 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28156 cycles, achieve throughput  5586 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28131 cycles, achieve throughput  5591 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  28126 cycles, achieve throughput  5592 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  27809 cycles, achieve throughput  5655 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27826 cycles, achieve throughput  5652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  53738 cycles, achieve throughput  2926 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  52976 cycles, achieve throughput  2969 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  53298 cycles, achieve throughput  2951 MB/s
Throughput test with EDMA1 TC3
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25267 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25306 cycles, achieve throughput  6215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25380 cycles, achieve throughput  6197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25367 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26124 cycles, achieve throughput  6020 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25435 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25507 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25440 cycles, achieve throughput  6182 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25290 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25360 cycles, achieve throughput  6202 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25374 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25368 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25515 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25517 cycles, achieve throughput  6163 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25876 cycles, achieve throughput  6078 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25366 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25365 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25372 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26247 cycles, achieve throughput  5992 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25439 cycles, achieve throughput  6182 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25737 cycles, achieve throughput  6111 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25656 cycles, achieve throughput  6130 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28338 cycles, achieve throughput  5550 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29443 cycles, achieve throughput  5342 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28374 cycles, achieve throughput  5543 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  60782 cycles, achieve throughput  2587 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  60120 cycles, achieve throughput  2616 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61456 cycles, achieve throughput  2559 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  29359 cycles, achieve throughput  5357 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  28565 cycles, achieve throughput  5506 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28670 cycles, achieve throughput  5486 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28097 cycles, achieve throughput  5597 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28336 cycles, achieve throughput  5550 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28365 cycles, achieve throughput  5545 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  61088 cycles, achieve throughput  2574 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  60575 cycles, achieve throughput  2596 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61418 cycles, achieve throughput  2560 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  28897 cycles, achieve throughput  5443 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  29663 cycles, achieve throughput  5302 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28664 cycles, achieve throughput  5487 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  29887 cycles, achieve throughput  5262 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29127 cycles, achieve throughput  5400 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30270 cycles, achieve throughput  5196 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  60895 cycles, achieve throughput  2582 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  62033 cycles, achieve throughput  2535 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  61537 cycles, achieve throughput  2555 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  29361 cycles, achieve throughput  5356 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  30678 cycles, achieve throughput  5127 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29557 cycles, achieve throughput  5321 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  26843 cycles, achieve throughput  5859 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26578 cycles, achieve throughput  5917 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26814 cycles, achieve throughput  5865 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  27356 cycles, achieve throughput  5749 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26566 cycles, achieve throughput  5920 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26827 cycles, achieve throughput  5862 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  52301 cycles, achieve throughput  3007 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  51959 cycles, achieve throughput  3027 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51858 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  26843 cycles, achieve throughput  5859 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26502 cycles, achieve throughput  5934 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26831 cycles, achieve throughput  5862 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  27695 cycles, achieve throughput  5679 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  26815 cycles, achieve throughput  5865 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26600 cycles, achieve throughput  5913 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  52292 cycles, achieve throughput  3007 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  52853 cycles, achieve throughput  2975 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  52295 cycles, achieve throughput  3007 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28179 cycles, achieve throughput  5581 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28162 cycles, achieve throughput  5585 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27845 cycles, achieve throughput  5648 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  29701 cycles, achieve throughput  5295 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  28040 cycles, achieve throughput  5609 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  28143 cycles, achieve throughput  5588 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  53525 cycles, achieve throughput  2938 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  53075 cycles, achieve throughput  2963 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  52966 cycles, achieve throughput  2969 MB/s
Throughput test with EDMA2 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25290 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25346 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  26162 cycles, achieve throughput  6012 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26131 cycles, achieve throughput  6019 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25377 cycles, achieve throughput  6197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25518 cycles, achieve throughput  6163 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25434 cycles, achieve throughput  6184 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25650 cycles, achieve throughput  6132 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25374 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25341 cycles, achieve throughput  6206 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25354 cycles, achieve throughput  6203 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25433 cycles, achieve throughput  6184 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  26431 cycles, achieve throughput  5950 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25638 cycles, achieve throughput  6134 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25272 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25271 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25283 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25337 cycles, achieve throughput  6207 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25346 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25365 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25631 cycles, achieve throughput  6136 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25516 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25432 cycles, achieve throughput  6184 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  29460 cycles, achieve throughput  5338 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29469 cycles, achieve throughput  5337 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28349 cycles, achieve throughput  5548 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  60982 cycles, achieve throughput  2579 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  60771 cycles, achieve throughput  2588 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61555 cycles, achieve throughput  2555 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  28453 cycles, achieve throughput  5527 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  28484 cycles, achieve throughput  5521 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28564 cycles, achieve throughput  5506 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28120 cycles, achieve throughput  5593 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28194 cycles, achieve throughput  5578 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28366 cycles, achieve throughput  5544 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  62448 cycles, achieve throughput  2518 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  60384 cycles, achieve throughput  2604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60861 cycles, achieve throughput  2584 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  28670 cycles, achieve throughput  5486 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  28674 cycles, achieve throughput  5485 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28571 cycles, achieve throughput  5505 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  29245 cycles, achieve throughput  5378 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29136 cycles, achieve throughput  5398 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30017 cycles, achieve throughput  5239 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  60644 cycles, achieve throughput  2593 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61245 cycles, achieve throughput  2568 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  62338 cycles, achieve throughput  2523 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  29568 cycles, achieve throughput  5319 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  29432 cycles, achieve throughput  5344 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29795 cycles, achieve throughput  5278 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  26502 cycles, achieve throughput  5934 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26838 cycles, achieve throughput  5860 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26837 cycles, achieve throughput  5860 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  27703 cycles, achieve throughput  5677 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  27700 cycles, achieve throughput  5678 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27727 cycles, achieve throughput  5672 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  51960 cycles, achieve throughput  3027 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  51849 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51867 cycles, achieve throughput  3032 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  26482 cycles, achieve throughput  5939 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26591 cycles, achieve throughput  5915 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26912 cycles, achieve throughput  5844 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  26610 cycles, achieve throughput  5910 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  27362 cycles, achieve throughput  5748 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26890 cycles, achieve throughput  5849 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  52412 cycles, achieve throughput  3000 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  51854 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51856 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  27824 cycles, achieve throughput  5652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28137 cycles, achieve throughput  5590 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28147 cycles, achieve throughput  5588 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  29164 cycles, achieve throughput  5393 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  28150 cycles, achieve throughput  5587 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  28144 cycles, achieve throughput  5588 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  53296 cycles, achieve throughput  2951 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  53188 cycles, achieve throughput  2957 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  53407 cycles, achieve throughput  2945 MB/s
Throughput test with EDMA2 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25322 cycles, achieve throughput  6211 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25363 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25394 cycles, achieve throughput  6193 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25385 cycles, achieve throughput  6196 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25375 cycles, achieve throughput  6198 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25511 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25519 cycles, achieve throughput  6163 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25464 cycles, achieve throughput  6176 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25271 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25363 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25267 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  26123 cycles, achieve throughput  6020 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25348 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25366 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25510 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25513 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25645 cycles, achieve throughput  6133 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25342 cycles, achieve throughput  6206 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25342 cycles, achieve throughput  6206 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25345 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25438 cycles, achieve throughput  6183 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25325 cycles, achieve throughput  6210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25660 cycles, achieve throughput  6129 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28323 cycles, achieve throughput  5553 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28356 cycles, achieve throughput  5546 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29450 cycles, achieve throughput  5340 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  60446 cycles, achieve throughput  2602 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  60132 cycles, achieve throughput  2615 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60320 cycles, achieve throughput  2607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  28579 cycles, achieve throughput  5503 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  28682 cycles, achieve throughput  5483 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29689 cycles, achieve throughput  5297 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28338 cycles, achieve throughput  5550 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29660 cycles, achieve throughput  5302 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29364 cycles, achieve throughput  5356 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  61090 cycles, achieve throughput  2574 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  60252 cycles, achieve throughput  2610 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60170 cycles, achieve throughput  2614 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  28658 cycles, achieve throughput  5488 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  28581 cycles, achieve throughput  5503 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28775 cycles, achieve throughput  5466 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  29116 cycles, achieve throughput  5402 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30210 cycles, achieve throughput  5206 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29134 cycles, achieve throughput  5398 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  60596 cycles, achieve throughput  2595 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  62354 cycles, achieve throughput  2522 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  60877 cycles, achieve throughput  2583 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  29453 cycles, achieve throughput  5340 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  29353 cycles, achieve throughput  5358 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29552 cycles, achieve throughput  5322 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  26510 cycles, achieve throughput  5933 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26833 cycles, achieve throughput  5861 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26584 cycles, achieve throughput  5916 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  26580 cycles, achieve throughput  5917 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26924 cycles, achieve throughput  5841 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26952 cycles, achieve throughput  5835 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  51744 cycles, achieve throughput  3039 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  52409 cycles, achieve throughput  3001 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51852 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  26498 cycles, achieve throughput  5935 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26920 cycles, achieve throughput  5842 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26512 cycles, achieve throughput  5932 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  27605 cycles, achieve throughput  5697 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  26915 cycles, achieve throughput  5843 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26564 cycles, achieve throughput  5921 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  52858 cycles, achieve throughput  2975 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  52183 cycles, achieve throughput  3014 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  52072 cycles, achieve throughput  3020 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28149 cycles, achieve throughput  5587 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27826 cycles, achieve throughput  5652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28149 cycles, achieve throughput  5587 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  28064 cycles, achieve throughput  5604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  27466 cycles, achieve throughput  5726 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  29029 cycles, achieve throughput  5418 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  52741 cycles, achieve throughput  2982 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  52628 cycles, achieve throughput  2988 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  53295 cycles, achieve throughput  2951 MB/s
Throughput test with EDMA2 TC2
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25267 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25290 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25363 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26146 cycles, achieve throughput  6015 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26259 cycles, achieve throughput  5989 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25520 cycles, achieve throughput  6163 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25521 cycles, achieve throughput  6163 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25621 cycles, achieve throughput  6138 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25267 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  26126 cycles, achieve throughput  6020 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  26129 cycles, achieve throughput  6019 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25500 cycles, achieve throughput  6168 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25729 cycles, achieve throughput  6113 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25533 cycles, achieve throughput  6160 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  26411 cycles, achieve throughput  5955 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25297 cycles, achieve throughput  6217 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25356 cycles, achieve throughput  6203 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  26122 cycles, achieve throughput  6021 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25380 cycles, achieve throughput  6197 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25519 cycles, achieve throughput  6163 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25628 cycles, achieve throughput  6137 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25656 cycles, achieve throughput  6130 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  29438 cycles, achieve throughput  5342 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28252 cycles, achieve throughput  5567 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28355 cycles, achieve throughput  5547 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  62013 cycles, achieve throughput  2536 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  60827 cycles, achieve throughput  2585 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61099 cycles, achieve throughput  2574 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  28676 cycles, achieve throughput  5484 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  28561 cycles, achieve throughput  5507 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28601 cycles, achieve throughput  5499 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  28108 cycles, achieve throughput  5595 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28417 cycles, achieve throughput  5534 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28394 cycles, achieve throughput  5539 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  61795 cycles, achieve throughput  2545 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  61357 cycles, achieve throughput  2563 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  60246 cycles, achieve throughput  2610 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  28680 cycles, achieve throughput  5484 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  29894 cycles, achieve throughput  5261 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  28676 cycles, achieve throughput  5484 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  29115 cycles, achieve throughput  5402 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29111 cycles, achieve throughput  5402 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29195 cycles, achieve throughput  5387 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  60993 cycles, achieve throughput  2578 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  62237 cycles, achieve throughput  2527 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  62772 cycles, achieve throughput  2505 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  29344 cycles, achieve throughput  5360 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  30232 cycles, achieve throughput  5202 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29584 cycles, achieve throughput  5316 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  26740 cycles, achieve throughput  5882 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26831 cycles, achieve throughput  5862 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26509 cycles, achieve throughput  5933 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  26591 cycles, achieve throughput  5915 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26573 cycles, achieve throughput  5919 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26589 cycles, achieve throughput  5915 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  51632 cycles, achieve throughput  3046 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  51629 cycles, achieve throughput  3046 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  53418 cycles, achieve throughput  2944 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  26581 cycles, achieve throughput  5917 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26591 cycles, achieve throughput  5915 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26733 cycles, achieve throughput  5883 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  26711 cycles, achieve throughput  5888 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  27376 cycles, achieve throughput  5745 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26556 cycles, achieve throughput  5922 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  51970 cycles, achieve throughput  3026 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  52301 cycles, achieve throughput  3007 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  52303 cycles, achieve throughput  3007 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28162 cycles, achieve throughput  5585 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28145 cycles, achieve throughput  5588 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28178 cycles, achieve throughput  5581 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  28146 cycles, achieve throughput  5588 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  28137 cycles, achieve throughput  5590 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27818 cycles, achieve throughput  5654 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  53415 cycles, achieve throughput  2944 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  52965 cycles, achieve throughput  2969 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  53085 cycles, achieve throughput  2962 MB/s
Throughput test with EDMA2 TC3
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25267 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25290 cycles, achieve throughput  6219 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26041 cycles, achieve throughput  6039 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25364 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25294 cycles, achieve throughput  6218 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25635 cycles, achieve throughput  6135 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25648 cycles, achieve throughput  6132 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25269 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25370 cycles, achieve throughput  6199 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25363 cycles, achieve throughput  6201 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27035 cycles, achieve throughput  5817 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25516 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25431 cycles, achieve throughput  6184 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25515 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25268 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25270 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25348 cycles, achieve throughput  6205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25368 cycles, achieve throughput  6200 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25328 cycles, achieve throughput  6209 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26245 cycles, achieve throughput  5993 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25511 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25441 cycles, achieve throughput  6182 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25516 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  28371 cycles, achieve throughput  5543 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28378 cycles, achieve throughput  5542 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28327 cycles, achieve throughput  5552 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  61335 cycles, achieve throughput  2564 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  59660 cycles, achieve throughput  2636 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61071 cycles, achieve throughput  2575 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  28581 cycles, achieve throughput  5503 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  29676 cycles, achieve throughput  5300 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29799 cycles, achieve throughput  5278 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  29564 cycles, achieve throughput  5320 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28366 cycles, achieve throughput  5544 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29422 cycles, achieve throughput  5345 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  60099 cycles, achieve throughput  2617 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  61324 cycles, achieve throughput  2564 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61354 cycles, achieve throughput  2563 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  28674 cycles, achieve throughput  5485 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  29702 cycles, achieve throughput  5295 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29906 cycles, achieve throughput  5259 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30018 cycles, achieve throughput  5239 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28885 cycles, achieve throughput  5445 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29802 cycles, achieve throughput  5277 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61715 cycles, achieve throughput  2548 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61595 cycles, achieve throughput  2553 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  62232 cycles, achieve throughput  2527 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  30338 cycles, achieve throughput  5184 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  30269 cycles, achieve throughput  5196 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  29355 cycles, achieve throughput  5358 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  26826 cycles, achieve throughput  5863 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26525 cycles, achieve throughput  5929 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26553 cycles, achieve throughput  5923 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  26597 cycles, achieve throughput  5913 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26606 cycles, achieve throughput  5911 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26903 cycles, achieve throughput  5846 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  52741 cycles, achieve throughput  2982 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  51848 cycles, achieve throughput  3033 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  52070 cycles, achieve throughput  3020 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  26853 cycles, achieve throughput  5857 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  26915 cycles, achieve throughput  5843 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  26918 cycles, achieve throughput  5843 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  26602 cycles, achieve throughput  5912 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  27698 cycles, achieve throughput  5678 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26572 cycles, achieve throughput  5919 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  52410 cycles, achieve throughput  3001 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  51738 cycles, achieve throughput  3040 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51861 cycles, achieve throughput  3032 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28160 cycles, achieve throughput  5585 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28137 cycles, achieve throughput  5590 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27810 cycles, achieve throughput  5655 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  28138 cycles, achieve throughput  5589 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  29178 cycles, achieve throughput  5390 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27804 cycles, achieve throughput  5656 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  53076 cycles, achieve throughput  2963 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  53074 cycles, achieve throughput  2963 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  53302 cycles, achieve throughput  2950 MB/s
Throughput test with EDMA3 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25275 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25311 cycles, achieve throughput  6214 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25275 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  25504 cycles, achieve throughput  6167 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  25729 cycles, achieve throughput  6113 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25509 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25572 cycles, achieve throughput  6150 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25562 cycles, achieve throughput  6153 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25896 cycles, achieve throughput  6073 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25258 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25274 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25280 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25505 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  25507 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26766 cycles, achieve throughput  5876 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25568 cycles, achieve throughput  6151 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25568 cycles, achieve throughput  6151 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25912 cycles, achieve throughput  6070 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25255 cycles, achieve throughput  6227 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25274 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25275 cycles, achieve throughput  6223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25545 cycles, achieve throughput  6157 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  25540 cycles, achieve throughput  6158 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  26742 cycles, achieve throughput  5881 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25569 cycles, achieve throughput  6151 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25569 cycles, achieve throughput  6151 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25570 cycles, achieve throughput  6151 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  29938 cycles, achieve throughput  5253 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29913 cycles, achieve throughput  5258 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  29940 cycles, achieve throughput  5253 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  62020 cycles, achieve throughput  2536 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  62279 cycles, achieve throughput  2525 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  62044 cycles, achieve throughput  2535 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  30407 cycles, achieve throughput  5172 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  31863 cycles, achieve throughput  4936 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  31645 cycles, achieve throughput  4970 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  29915 cycles, achieve throughput  5257 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30119 cycles, achieve throughput  5222 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30929 cycles, achieve throughput  5085 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  60969 cycles, achieve throughput  2579 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  60845 cycles, achieve throughput  2585 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  61260 cycles, achieve throughput  2567 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  31610 cycles, achieve throughput  4975 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  30656 cycles, achieve throughput  5130 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  31609 cycles, achieve throughput  4976 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30570 cycles, achieve throughput  5145 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30468 cycles, achieve throughput  5162 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30547 cycles, achieve throughput  5148 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  62751 cycles, achieve throughput  2506 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  62962 cycles, achieve throughput  2498 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  62454 cycles, achieve throughput  2518 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  31305 cycles, achieve throughput  5024 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  31304 cycles, achieve throughput  5024 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  31165 cycles, achieve throughput  5046 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27183 cycles, achieve throughput  5786 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27544 cycles, achieve throughput  5710 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27328 cycles, achieve throughput  5755 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  28766 cycles, achieve throughput  5467 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  28729 cycles, achieve throughput  5474 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27512 cycles, achieve throughput  5717 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  51295 cycles, achieve throughput  3066 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  51522 cycles, achieve throughput  3052 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51185 cycles, achieve throughput  3072 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27224 cycles, achieve throughput  5777 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27468 cycles, achieve throughput  5726 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27244 cycles, achieve throughput  5773 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  28872 cycles, achieve throughput  5447 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  27825 cycles, achieve throughput  5652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27885 cycles, achieve throughput  5640 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  51187 cycles, achieve throughput  3072 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  51403 cycles, achieve throughput  3059 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51513 cycles, achieve throughput  3053 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28770 cycles, achieve throughput  5467 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28746 cycles, achieve throughput  5471 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28401 cycles, achieve throughput  5538 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  30051 cycles, achieve throughput  5233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  29086 cycles, achieve throughput  5407 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  28944 cycles, achieve throughput  5434 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  53519 cycles, achieve throughput  2938 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  52294 cycles, achieve throughput  3007 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  53518 cycles, achieve throughput  2938 MB/s
Throughput test with EDMA3 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  25281 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25286 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25281 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  26754 cycles, achieve throughput  5878 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  26607 cycles, achieve throughput  5911 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25746 cycles, achieve throughput  6109 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  25666 cycles, achieve throughput  6128 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  25335 cycles, achieve throughput  6208 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25677 cycles, achieve throughput  6125 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  25284 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  25270 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  25287 cycles, achieve throughput  6220 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  25513 cycles, achieve throughput  6164 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  26654 cycles, achieve throughput  5901 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25510 cycles, achieve throughput  6165 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  25663 cycles, achieve throughput  6128 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  25669 cycles, achieve throughput  6127 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25903 cycles, achieve throughput  6072 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  25282 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  25270 cycles, achieve throughput  6224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  25280 cycles, achieve throughput  6221 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  25505 cycles, achieve throughput  6166 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  26514 cycles, achieve throughput  5932 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  25743 cycles, achieve throughput  6109 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  25670 cycles, achieve throughput  6127 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  25784 cycles, achieve throughput  6100 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  25664 cycles, achieve throughput  6128 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  31254 cycles, achieve throughput  5032 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  29873 cycles, achieve throughput  5265 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  31154 cycles, achieve throughput  5048 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  62254 cycles, achieve throughput  2526 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  61142 cycles, achieve throughput  2572 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  62424 cycles, achieve throughput  2519 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  30625 cycles, achieve throughput  5135 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  30494 cycles, achieve throughput  5157 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  30635 cycles, achieve throughput  5134 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  31001 cycles, achieve throughput  5073 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30969 cycles, achieve throughput  5078 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  30156 cycles, achieve throughput  5215 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  62580 cycles, achieve throughput  2513 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  61107 cycles, achieve throughput  2573 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  62779 cycles, achieve throughput  2505 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  31830 cycles, achieve throughput  4941 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  30406 cycles, achieve throughput  5172 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  30746 cycles, achieve throughput  5115 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  30654 cycles, achieve throughput  5131 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  30385 cycles, achieve throughput  5176 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  31810 cycles, achieve throughput  4944 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  61614 cycles, achieve throughput  2552 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  61868 cycles, achieve throughput  2542 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  64839 cycles, achieve throughput  2425 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  31393 cycles, achieve throughput  5010 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  31086 cycles, achieve throughput  5059 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  31308 cycles, achieve throughput  5023 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  27495 cycles, achieve throughput  5720 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27534 cycles, achieve throughput  5712 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27298 cycles, achieve throughput  5761 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  29150 cycles, achieve throughput  5395 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  27545 cycles, achieve throughput  5710 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  28536 cycles, achieve throughput  5511 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  52522 cycles, achieve throughput  2994 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  51182 cycles, achieve throughput  3073 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  52417 cycles, achieve throughput  3000 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  27337 cycles, achieve throughput  5753 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  27525 cycles, achieve throughput  5714 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  27184 cycles, achieve throughput  5785 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  27859 cycles, achieve throughput  5645 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  27847 cycles, achieve throughput  5648 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  27846 cycles, achieve throughput  5648 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  52190 cycles, achieve throughput  3013 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  51189 cycles, achieve throughput  3072 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  51410 cycles, achieve throughput  3059 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  28748 cycles, achieve throughput  5471 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  28394 cycles, achieve throughput  5539 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  28447 cycles, achieve throughput  5529 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  29105 cycles, achieve throughput  5404 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  29107 cycles, achieve throughput  5403 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  30313 cycles, achieve throughput  5188 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  52420 cycles, achieve throughput  3000 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  54078 cycles, achieve throughput  2908 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  53739 cycles, achieve throughput  2926 MB/s
Throughput test with EDMA4 TC0
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15673 cycles, achieve throughput 10035 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15735 cycles, achieve throughput  9995 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15645 cycles, achieve throughput 10053 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16291 cycles, achieve throughput  9654 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16337 cycles, achieve throughput  9627 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  17306 cycles, achieve throughput  9088 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  14915 cycles, achieve throughput 10545 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  14928 cycles, achieve throughput 10536 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14812 cycles, achieve throughput 10618 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15657 cycles, achieve throughput 10045 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15668 cycles, achieve throughput 10038 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15744 cycles, achieve throughput  9990 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16372 cycles, achieve throughput  9607 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16446 cycles, achieve throughput  9563 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  17395 cycles, achieve throughput  9042 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  14916 cycles, achieve throughput 10544 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  14915 cycles, achieve throughput 10545 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14917 cycles, achieve throughput 10544 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15692 cycles, achieve throughput 10023 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15659 cycles, achieve throughput 10044 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15759 cycles, achieve throughput  9980 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  16450 cycles, achieve throughput  9561 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16464 cycles, achieve throughput  9553 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16388 cycles, achieve throughput  9597 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  14917 cycles, achieve throughput 10544 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  14934 cycles, achieve throughput 10532 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14822 cycles, achieve throughput 10611 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  20546 cycles, achieve throughput  7655 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20551 cycles, achieve throughput  7653 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20977 cycles, achieve throughput  7498 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  46984 cycles, achieve throughput  3347 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  47155 cycles, achieve throughput  3335 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  47092 cycles, achieve throughput  3339 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  20797 cycles, achieve throughput  7562 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  20480 cycles, achieve throughput  7680 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  20623 cycles, achieve throughput  7626 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  21570 cycles, achieve throughput  7291 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20779 cycles, achieve throughput  7569 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20559 cycles, achieve throughput  7650 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  48112 cycles, achieve throughput  3269 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  48220 cycles, achieve throughput  3261 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  48649 cycles, achieve throughput  3233 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  20816 cycles, achieve throughput  7556 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  20683 cycles, achieve throughput  7604 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  20693 cycles, achieve throughput  7600 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  21121 cycles, achieve throughput  7446 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  21203 cycles, achieve throughput  7418 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  21137 cycles, achieve throughput  7441 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  48995 cycles, achieve throughput  3210 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  49301 cycles, achieve throughput  3190 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  48773 cycles, achieve throughput  3224 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  21146 cycles, achieve throughput  7438 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  22155 cycles, achieve throughput  7099 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  21463 cycles, achieve throughput  7328 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  18884 cycles, achieve throughput  8329 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  18811 cycles, achieve throughput  8361 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  18838 cycles, achieve throughput  8349 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  18802 cycles, achieve throughput  8365 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  18815 cycles, achieve throughput  8359 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  19046 cycles, achieve throughput  8258 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  42177 cycles, achieve throughput  3729 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  40957 cycles, achieve throughput  3840 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  41516 cycles, achieve throughput  3788 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  18885 cycles, achieve throughput  8328 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  18850 cycles, achieve throughput  8344 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  18883 cycles, achieve throughput  8329 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  18913 cycles, achieve throughput  8316 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  18877 cycles, achieve throughput  8332 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  18999 cycles, achieve throughput  8278 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  41735 cycles, achieve throughput  3768 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  41294 cycles, achieve throughput  3808 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  41285 cycles, achieve throughput  3809 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  19930 cycles, achieve throughput  7891 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20286 cycles, achieve throughput  7753 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20015 cycles, achieve throughput  7858 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  19716 cycles, achieve throughput  7977 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  20956 cycles, achieve throughput  7505 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  19783 cycles, achieve throughput  7950 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  42627 cycles, achieve throughput  3689 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  42407 cycles, achieve throughput  3708 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  42063 cycles, achieve throughput  3739 MB/s
Throughput test with EDMA4 TC1
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0a0000(MSRAM(strongly ordered)), consumes  15740 cycles, achieve throughput  9992 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15769 cycles, achieve throughput  9974 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15699 cycles, achieve throughput 10018 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  16368 cycles, achieve throughput  9609 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  16478 cycles, achieve throughput  9545 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16366 cycles, achieve throughput  9610 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  14933 cycles, achieve throughput 10532 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  14930 cycles, achieve throughput 10534 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c080000(MSRAM(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14915 cycles, achieve throughput 10545 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  15634 cycles, achieve throughput 10060 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c0e0000(MSRAM(normal non-cache)), consumes  15716 cycles, achieve throughput 10008 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  15742 cycles, achieve throughput  9991 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  16462 cycles, achieve throughput  9554 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  16319 cycles, achieve throughput  9638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  17374 cycles, achieve throughput  9052 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  14926 cycles, achieve throughput 10537 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  14930 cycles, achieve throughput 10534 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c0c0000(MSRAM(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14920 cycles, achieve throughput 10541 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  15785 cycles, achieve throughput  9964 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  15695 cycles, achieve throughput 10021 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x c120000(MSRAM(RA_WB_WA,  in sh)), consumes  15633 cycles, achieve throughput 10061 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  17415 cycles, achieve throughput  9031 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  16481 cycles, achieve throughput  9543 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  16695 cycles, achieve throughput  9421 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  14808 cycles, achieve throughput 10621 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  14818 cycles, achieve throughput 10614 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x c100000(MSRAM(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  14913 cycles, achieve throughput 10546 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  20553 cycles, achieve throughput  7652 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  21694 cycles, achieve throughput  7250 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20869 cycles, achieve throughput  7536 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x80020000(DDR3A(strongly ordered)), consumes  47087 cycles, achieve throughput  3340 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  46907 cycles, achieve throughput  3353 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  48796 cycles, achieve throughput  3223 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x60000000(DDR3B(strongly ordered)), consumes  20687 cycles, achieve throughput  7603 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  20705 cycles, achieve throughput  7596 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x80000000(DDR3A(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  20694 cycles, achieve throughput  7600 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  21675 cycles, achieve throughput  7256 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  20654 cycles, achieve throughput  7615 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20766 cycles, achieve throughput  7574 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  49378 cycles, achieve throughput  3185 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x88020000(DDR3A(normal non-cache)), consumes  48868 cycles, achieve throughput  3218 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  47221 cycles, achieve throughput  3330 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  21694 cycles, achieve throughput  7250 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x68000000(DDR3B(normal non-cache)), consumes  20592 cycles, achieve throughput  7638 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x88000000(DDR3A(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  20584 cycles, achieve throughput  7641 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  21322 cycles, achieve throughput  7376 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  21251 cycles, achieve throughput  7401 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  20928 cycles, achieve throughput  7515 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  48188 cycles, achieve throughput  3264 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  47713 cycles, achieve throughput  3296 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x90020000(DDR3A(RA_WB_WA,  in sh)), consumes  49073 cycles, achieve throughput  3205 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  21131 cycles, achieve throughput  7443 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  21372 cycles, achieve throughput  7359 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x90000000(DDR3A(RA_WB_WA,  in sh)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  21369 cycles, achieve throughput  7360 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c080000(MSRAM(strongly ordered)), consumes  18844 cycles, achieve throughput  8346 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  18820 cycles, achieve throughput  8357 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  18791 cycles, achieve throughput  8370 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x80000000(DDR3A(strongly ordered)), consumes  18996 cycles, achieve throughput  8279 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x88000000(DDR3A(normal non-cache)), consumes  19006 cycles, achieve throughput  8275 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  18820 cycles, achieve throughput  8357 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x60020000(DDR3B(strongly ordered)), consumes  40957 cycles, achieve throughput  3840 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x68000000(DDR3B(normal non-cache)), consumes  41404 cycles, achieve throughput  3798 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x60000000(DDR3B(strongly ordered)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  41621 cycles, achieve throughput  3779 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c080000(MSRAM(strongly ordered)), consumes  18823 cycles, achieve throughput  8356 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  18794 cycles, achieve throughput  8368 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  19036 cycles, achieve throughput  8262 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x80000000(DDR3A(strongly ordered)), consumes  18845 cycles, achieve throughput  8346 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x88000000(DDR3A(normal non-cache)), consumes  19681 cycles, achieve throughput  7991 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  18790 cycles, achieve throughput  8370 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x60000000(DDR3B(strongly ordered)), consumes  41067 cycles, achieve throughput  3829 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x68020000(DDR3B(normal non-cache)), consumes  42406 cycles, achieve throughput  3709 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x68000000(DDR3B(normal non-cache)) to 0x70000000(DDR3B(RA_WB_WA,  in sh)), consumes  41738 cycles, achieve throughput  3768 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c080000(MSRAM(strongly ordered)), consumes  20017 cycles, achieve throughput  7857 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c0c0000(MSRAM(normal non-cache)), consumes  19662 cycles, achieve throughput  7999 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x c100000(MSRAM(RA_WB_WA,  in sh)), consumes  19969 cycles, achieve throughput  7876 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x80000000(DDR3A(strongly ordered)), consumes  21054 cycles, achieve throughput  7470 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x88000000(DDR3A(normal non-cache)), consumes  19708 cycles, achieve throughput  7980 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x90000000(DDR3A(RA_WB_WA,  in sh)), consumes  20429 cycles, achieve throughput  7699 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x60000000(DDR3B(strongly ordered)), consumes  43520 cycles, achieve throughput  3614 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x68000000(DDR3B(normal non-cache)), consumes  42624 cycles, achieve throughput  3690 MB/s
transfer    8 * 16384 Bytes with index=16384 from 0x70000000(DDR3B(RA_WB_WA,  in sh)) to 0x70020000(DDR3B(RA_WB_WA,  in sh)), consumes  42625 cycles, achieve throughput  3690 MB/s
EDMA ACNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    602 cycles, achieve throughput     1 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    595 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    10 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    12 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    14 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    16 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    18 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    20 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    22 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    24 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    26 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    814 cycles, achieve throughput    20 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    30 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    32 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    64 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    97 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput   129 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput   163 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput   194 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   227 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput   258 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   292 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput   323 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput   355 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   389 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   422 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   454 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput   489 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput   521 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   584 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput   650 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   713 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   778 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   843 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput   906 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput   969 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput  1041 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput   983 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  1097 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1205 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput  1312 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1424 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1533 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  1645 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput  1750 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput  1966 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    706 cycles, achieve throughput  2175 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    705 cycles, achieve throughput  2396 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    811 cycles, achieve throughput  2272 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    809 cycles, achieve throughput  2468 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  2645 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  2833 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    817 cycles, achieve throughput  3008 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    811 cycles, achieve throughput  3409 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    930 cycles, achieve throughput  3303 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    927 cycles, achieve throughput  3645 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    925 cycles, achieve throughput  3985 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    924 cycles, achieve throughput  4322 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1037 cycles, achieve throughput  4147 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1037 cycles, achieve throughput  4443 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1049 cycles, achieve throughput  4685 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1157 cycles, achieve throughput  4779 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1163 cycles, achieve throughput  5282 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1269 cycles, achieve throughput  5325 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1273 cycles, achieve throughput  5791 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1390 cycles, achieve throughput  5746 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1392 cycles, achieve throughput  6179 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1509 cycles, achieve throughput  6107 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1512 cycles, achieve throughput  6501 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1727 cycles, achieve throughput  6403 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1853 cycles, achieve throughput  6631 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1952 cycles, achieve throughput  6924 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2069 cycles, achieve throughput  7126 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2190 cycles, achieve throughput  7294 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2303 cycles, achieve throughput  7469 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2354 cycles, achieve throughput  7830 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2518 cycles, achieve throughput  7808 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2642 cycles, achieve throughput  7906 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2747 cycles, achieve throughput  8051 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2860 cycles, achieve throughput  8163 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2987 cycles, achieve throughput  8227 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3131 cycles, achieve throughput  8241 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3312 cycles, achieve throughput  8162 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3355 cycles, achieve throughput  8423 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3540 cycles, achieve throughput  8330 MB/s
EDMA ACNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    591 cycles, achieve throughput     2 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    590 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    591 cycles, achieve throughput    10 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    590 cycles, achieve throughput    12 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    594 cycles, achieve throughput    14 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    591 cycles, achieve throughput    16 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    588 cycles, achieve throughput    18 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput    20 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput    22 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    592 cycles, achieve throughput    24 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    591 cycles, achieve throughput    26 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    591 cycles, achieve throughput    28 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    590 cycles, achieve throughput    30 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    590 cycles, achieve throughput    32 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    592 cycles, achieve throughput    64 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput    97 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    591 cycles, achieve throughput   129 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    597 cycles, achieve throughput   160 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    590 cycles, achieve throughput   195 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    593 cycles, achieve throughput   226 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput   260 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    590 cycles, achieve throughput   292 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput   325 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput   358 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    589 cycles, achieve throughput   391 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    593 cycles, achieve throughput   420 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    592 cycles, achieve throughput   454 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    590 cycles, achieve throughput   488 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    703 cycles, achieve throughput   436 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    593 cycles, achieve throughput   582 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    704 cycles, achieve throughput   545 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    701 cycles, achieve throughput   602 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    702 cycles, achieve throughput   656 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    701 cycles, achieve throughput   712 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    701 cycles, achieve throughput   766 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    703 cycles, achieve throughput   819 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    704 cycles, achieve throughput   872 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    702 cycles, achieve throughput   984 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    700 cycles, achieve throughput  1097 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    702 cycles, achieve throughput  1203 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    699 cycles, achieve throughput  1318 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    702 cycles, achieve throughput  1422 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    701 cycles, achieve throughput  1533 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    702 cycles, achieve throughput  1641 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    700 cycles, achieve throughput  1755 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    813 cycles, achieve throughput  1700 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    812 cycles, achieve throughput  1891 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    811 cycles, achieve throughput  2083 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    812 cycles, achieve throughput  2269 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    811 cycles, achieve throughput  2462 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    813 cycles, achieve throughput  2645 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    816 cycles, achieve throughput  2823 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    925 cycles, achieve throughput  2656 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    922 cycles, achieve throughput  2998 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes    928 cycles, achieve throughput  3310 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1036 cycles, achieve throughput  3261 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1041 cycles, achieve throughput  3541 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1148 cycles, achieve throughput  3478 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1150 cycles, achieve throughput  3739 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1152 cycles, achieve throughput  4000 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1150 cycles, achieve throughput  4274 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1263 cycles, achieve throughput  4378 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1368 cycles, achieve throughput  4491 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1485 cycles, achieve throughput  4551 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1481 cycles, achieve throughput  4978 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1727 cycles, achieve throughput  4624 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1596 cycles, achieve throughput  5389 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1710 cycles, achieve throughput  5389 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1821 cycles, achieve throughput  5398 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   1929 cycles, achieve throughput  5733 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2152 cycles, achieve throughput  5710 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2268 cycles, achieve throughput  5959 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2384 cycles, achieve throughput  6185 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2611 cycles, achieve throughput  6118 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2721 cycles, achieve throughput  6322 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   2831 cycles, achieve throughput  6510 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3067 cycles, achieve throughput  6410 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3155 cycles, achieve throughput  6621 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3381 cycles, achieve throughput  6541 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3498 cycles, achieve throughput  6674 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3606 cycles, achieve throughput  6815 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   4850 cycles, achieve throughput  5320 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   3948 cycles, achieve throughput  6847 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   4067 cycles, achieve throughput  6949 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x80000000(DDR3A) to 0x c080000(MSMC RAM), consumes   4303 cycles, achieve throughput  6853 MB/s
EDMA ACNTxBCNT test with EDMA0 TC0
transfer    1 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput     2 MB/s
transfer    1 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput     4 MB/s
transfer    1 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput     6 MB/s
transfer    1 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput     8 MB/s
transfer    1 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    10 MB/s
transfer    1 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    12 MB/s
transfer    1 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    14 MB/s
transfer    1 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput    16 MB/s
transfer    1 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    18 MB/s
transfer    1 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    20 MB/s
transfer    1 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    22 MB/s
transfer    1 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    24 MB/s
transfer    1 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    26 MB/s
transfer    1 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    28 MB/s
transfer    1 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput    30 MB/s
transfer    1 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    32 MB/s
transfer    1 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    64 MB/s
transfer    1 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    97 MB/s
transfer    1 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   129 MB/s
transfer    1 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput   162 MB/s
transfer    1 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput   195 MB/s
transfer    1 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput   226 MB/s
transfer    1 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   259 MB/s
transfer    1 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput   293 MB/s
transfer    1 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput   325 MB/s
transfer    1 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput   259 MB/s
transfer    1 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   389 MB/s
transfer    1 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput   423 MB/s
transfer    1 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   454 MB/s
transfer    1 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput   489 MB/s
transfer    1 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   519 MB/s
transfer    1 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput   585 MB/s
transfer    1 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   649 MB/s
transfer    1 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   713 MB/s
transfer    1 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   779 MB/s
transfer    1 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   843 MB/s
transfer    1 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   909 MB/s
transfer    1 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput   976 MB/s
transfer    1 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput  1039 MB/s
transfer    1 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   981 MB/s
transfer    1 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1095 MB/s
transfer    1 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    705 cycles, achieve throughput  1198 MB/s
transfer    1 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput  1309 MB/s
transfer    1 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  1426 MB/s
transfer    1 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1533 MB/s
transfer    1 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  1645 MB/s
transfer    1 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1752 MB/s
transfer    1 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    708 cycles, achieve throughput  1952 MB/s
transfer    1 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  2194 MB/s
transfer    1 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput  2406 MB/s
transfer    1 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    811 cycles, achieve throughput  2272 MB/s
transfer    1 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  2456 MB/s
transfer    1 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    812 cycles, achieve throughput  2648 MB/s
transfer    1 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    812 cycles, achieve throughput  2837 MB/s
transfer    1 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  3022 MB/s
transfer    1 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  3400 MB/s
transfer    1 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    930 cycles, achieve throughput  3303 MB/s
transfer    1 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    929 cycles, achieve throughput  3637 MB/s
transfer    1 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    925 cycles, achieve throughput  3985 MB/s
transfer    1 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    929 cycles, achieve throughput  4298 MB/s
transfer    1 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1036 cycles, achieve throughput  4151 MB/s
transfer    1 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1046 cycles, achieve throughput  4405 MB/s
transfer    1 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1045 cycles, achieve throughput  4703 MB/s
transfer    1 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1158 cycles, achieve throughput  4775 MB/s
transfer    1 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1263 cycles, achieve throughput  4864 MB/s
transfer    1 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1269 cycles, achieve throughput  5325 MB/s
transfer    1 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1271 cycles, achieve throughput  5800 MB/s
transfer    1 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1385 cycles, achieve throughput  5766 MB/s
transfer    1 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1384 cycles, achieve throughput  6215 MB/s
transfer    1 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1504 cycles, achieve throughput  6127 MB/s
transfer    1 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1515 cycles, achieve throughput  6488 MB/s
transfer    1 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1632 cycles, achieve throughput  6776 MB/s
transfer    1 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1835 cycles, achieve throughput  6696 MB/s
transfer    1 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1942 cycles, achieve throughput  6960 MB/s
transfer    1 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2093 cycles, achieve throughput  7045 MB/s
transfer    1 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2189 cycles, achieve throughput  7297 MB/s
transfer    1 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2308 cycles, achieve throughput  7453 MB/s
transfer    1 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2430 cycles, achieve throughput  7585 MB/s
transfer    1 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2515 cycles, achieve throughput  7817 MB/s
transfer    1 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2652 cycles, achieve throughput  7876 MB/s
transfer    1 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2794 cycles, achieve throughput  7916 MB/s
transfer    1 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2969 cycles, achieve throughput  7863 MB/s
transfer    1 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2989 cycles, achieve throughput  8222 MB/s
transfer    1 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3124 cycles, achieve throughput  8260 MB/s
transfer    1 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3328 cycles, achieve throughput  8123 MB/s
transfer    1 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3408 cycles, achieve throughput  8292 MB/s
transfer    1 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3551 cycles, achieve throughput  8305 MB/s
transfer    2 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput     4 MB/s
transfer    2 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput     8 MB/s
transfer    2 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    12 MB/s
transfer    2 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput    16 MB/s
transfer    2 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    20 MB/s
transfer    2 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    24 MB/s
transfer    2 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    28 MB/s
transfer    2 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    32 MB/s
transfer    2 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    36 MB/s
transfer    2 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput    40 MB/s
transfer    2 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput    44 MB/s
transfer    2 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    594 cycles, achieve throughput    48 MB/s
transfer    2 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    52 MB/s
transfer    2 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    56 MB/s
transfer    2 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    61 MB/s
transfer    2 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    588 cycles, achieve throughput    65 MB/s
transfer    2 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput   109 MB/s
transfer    2 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   194 MB/s
transfer    2 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   259 MB/s
transfer    2 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    597 cycles, achieve throughput   321 MB/s
transfer    2 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput   328 MB/s
transfer    2 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    699 cycles, achieve throughput   384 MB/s
transfer    2 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   518 MB/s
transfer    2 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput   492 MB/s
transfer    2 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput   546 MB/s
transfer    2 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   600 MB/s
transfer    2 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   779 MB/s
transfer    2 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput   710 MB/s
transfer    2 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    705 cycles, achieve throughput   762 MB/s
transfer    2 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput   820 MB/s
transfer    2 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput  1041 MB/s
transfer    2 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput   984 MB/s
transfer    2 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput  1094 MB/s
transfer    2 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput  1201 MB/s
transfer    2 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1314 MB/s
transfer    2 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1424 MB/s
transfer    2 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput  1527 MB/s
transfer    2 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    706 cycles, achieve throughput  1631 MB/s
transfer    2 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput  1750 MB/s
transfer    2 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput  1966 MB/s
transfer    2 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput  2188 MB/s
transfer    2 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput  2400 MB/s
transfer    2 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  2629 MB/s
transfer    2 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    815 cycles, achieve throughput  2450 MB/s
transfer    2 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  2645 MB/s
transfer    2 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    814 cycles, achieve throughput  2830 MB/s
transfer    2 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  3022 MB/s
transfer    2 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  3400 MB/s
transfer    2 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    928 cycles, achieve throughput  3310 MB/s
transfer    2 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    929 cycles, achieve throughput  3637 MB/s
transfer    2 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1035 cycles, achieve throughput  3561 MB/s
transfer    2 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    934 cycles, achieve throughput  4275 MB/s
transfer    2 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1034 cycles, achieve throughput  4159 MB/s
transfer    2 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1034 cycles, achieve throughput  4456 MB/s
transfer    2 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1033 cycles, achieve throughput  4758 MB/s
transfer    2 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1148 cycles, achieve throughput  4816 MB/s
transfer    2 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1817 cycles, achieve throughput  3381 MB/s
transfer    2 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1265 cycles, achieve throughput  5342 MB/s
transfer    2 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1373 cycles, achieve throughput  5369 MB/s
transfer    2 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1374 cycles, achieve throughput  5813 MB/s
transfer    2 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1388 cycles, achieve throughput  6197 MB/s
transfer    2 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1484 cycles, achieve throughput  6210 MB/s
transfer    2 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1606 cycles, achieve throughput  6121 MB/s
transfer    2 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1716 cycles, achieve throughput  6444 MB/s
transfer    2 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1832 cycles, achieve throughput  6707 MB/s
transfer    2 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1938 cycles, achieve throughput  6974 MB/s
transfer    2 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2076 cycles, achieve throughput  7102 MB/s
transfer    2 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2167 cycles, achieve throughput  7371 MB/s
transfer    2 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2413 cycles, achieve throughput  7129 MB/s
transfer    2 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2389 cycles, achieve throughput  7715 MB/s
transfer    2 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2618 cycles, achieve throughput  7509 MB/s
transfer    2 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2764 cycles, achieve throughput  8002 MB/s
transfer    2 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3092 cycles, achieve throughput  7948 MB/s
transfer    2 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3338 cycles, achieve throughput  8098 MB/s
transfer    2 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3454 cycles, achieve throughput  8538 MB/s
transfer    2 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3780 cycles, achieve throughput  8452 MB/s
transfer    2 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4093 cycles, achieve throughput  8406 MB/s
transfer    2 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4321 cycles, achieve throughput  8531 MB/s
transfer    2 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4523 cycles, achieve throughput  8693 MB/s
transfer    2 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4721 cycles, achieve throughput  8849 MB/s
transfer    2 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5037 cycles, achieve throughput  8782 MB/s
transfer    2 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5284 cycles, achieve throughput  8836 MB/s
transfer    2 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5502 cycles, achieve throughput  8933 MB/s
transfer    2 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5802 cycles, achieve throughput  8895 MB/s
transfer    2 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6048 cycles, achieve throughput  8939 MB/s
transfer    2 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6188 cycles, achieve throughput  9134 MB/s
transfer    2 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6519 cycles, achieve throughput  9047 MB/s
transfer    3 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput     6 MB/s
transfer    3 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    10 MB/s
transfer    3 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    15 MB/s
transfer    3 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    24 MB/s
transfer    3 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput    25 MB/s
transfer    3 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    30 MB/s
transfer    3 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput    35 MB/s
transfer    3 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput    48 MB/s
transfer    3 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput    46 MB/s
transfer    3 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    51 MB/s
transfer    3 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    56 MB/s
transfer    3 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    811 cycles, achieve throughput    53 MB/s
transfer    3 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput    66 MB/s
transfer    3 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    697 cycles, achieve throughput    72 MB/s
transfer    3 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput    77 MB/s
transfer    3 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput    97 MB/s
transfer    3 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput   195 MB/s
transfer    3 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   245 MB/s
transfer    3 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    590 cycles, achieve throughput   390 MB/s
transfer    3 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput   410 MB/s
transfer    3 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput   493 MB/s
transfer    3 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput   575 MB/s
transfer    3 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    592 cycles, achieve throughput   778 MB/s
transfer    3 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   736 MB/s
transfer    3 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput   821 MB/s
transfer    3 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput   901 MB/s
transfer    3 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput   984 MB/s
transfer    3 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  1069 MB/s
transfer    3 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1150 MB/s
transfer    3 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput  1227 MB/s
transfer    3 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1314 MB/s
transfer    3 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput  1474 MB/s
transfer    3 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  1645 MB/s
transfer    3 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput  1800 MB/s
transfer    3 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  1972 MB/s
transfer    3 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    816 cycles, achieve throughput  1835 MB/s
transfer    3 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  2304 MB/s
transfer    3 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    931 cycles, achieve throughput  1856 MB/s
transfer    3 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    812 cycles, achieve throughput  2269 MB/s
transfer    3 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    814 cycles, achieve throughput  2547 MB/s
transfer    3 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    815 cycles, achieve throughput  2826 MB/s
transfer    3 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  3117 MB/s
transfer    3 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    812 cycles, achieve throughput  3404 MB/s
transfer    3 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    928 cycles, achieve throughput  3227 MB/s
transfer    3 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    926 cycles, achieve throughput  3483 MB/s
transfer    3 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1034 cycles, achieve throughput  3342 MB/s
transfer    3 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    929 cycles, achieve throughput  3968 MB/s
transfer    3 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1041 cycles, achieve throughput  3983 MB/s
transfer    3 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1037 cycles, achieve throughput  4443 MB/s
transfer    3 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1156 cycles, achieve throughput  4384 MB/s
transfer    3 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1153 cycles, achieve throughput  4795 MB/s
transfer    3 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1150 cycles, achieve throughput  5209 MB/s
transfer    3 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1264 cycles, achieve throughput  5103 MB/s
transfer    3 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1260 cycles, achieve throughput  5485 MB/s
transfer    3 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1370 cycles, achieve throughput  5381 MB/s
transfer    3 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1486 cycles, achieve throughput  5581 MB/s
transfer    3 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1500 cycles, achieve throughput  6144 MB/s
transfer    3 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1599 cycles, achieve throughput  6339 MB/s
transfer    3 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1716 cycles, achieve throughput  6444 MB/s
transfer    3 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1833 cycles, achieve throughput  6536 MB/s
transfer    3 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1839 cycles, achieve throughput  7015 MB/s
transfer    3 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1942 cycles, achieve throughput  7118 MB/s
transfer    3 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2066 cycles, achieve throughput  7137 MB/s
transfer    3 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2281 cycles, achieve throughput  7272 MB/s
transfer    3 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2398 cycles, achieve throughput  7686 MB/s
transfer    3 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2630 cycles, achieve throughput  7709 MB/s
transfer    3 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2844 cycles, achieve throughput  7777 MB/s
transfer    3 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2975 cycles, achieve throughput  8054 MB/s
transfer    3 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3193 cycles, achieve throughput  8081 MB/s
transfer    3 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3348 cycles, achieve throughput  8258 MB/s
transfer    3 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3471 cycles, achieve throughput  8496 MB/s
transfer    3 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3890 cycles, achieve throughput  8528 MB/s
transfer    3 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4261 cycles, achieve throughput  8651 MB/s
transfer    3 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5672 cycles, achieve throughput  7149 MB/s
transfer    3 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5046 cycles, achieve throughput  8766 MB/s
transfer    3 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5367 cycles, achieve throughput  8929 MB/s
transfer    3 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5758 cycles, achieve throughput  8963 MB/s
transfer    3 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6084 cycles, achieve throughput  9088 MB/s
transfer    3 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6485 cycles, achieve throughput  9095 MB/s
transfer    3 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6823 cycles, achieve throughput  9184 MB/s
transfer    3 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7235 cycles, achieve throughput  9171 MB/s
transfer    3 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8614 cycles, achieve throughput  8131 MB/s
transfer    3 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7973 cycles, achieve throughput  9247 MB/s
transfer    3 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8391 cycles, achieve throughput  9225 MB/s
transfer    3 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8672 cycles, achieve throughput  9352 MB/s
transfer    3 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  10160 cycles, achieve throughput  8345 MB/s
transfer    3 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9517 cycles, achieve throughput  9296 MB/s
transfer    4 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput     8 MB/s
transfer    4 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    16 MB/s
transfer    4 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput    20 MB/s
transfer    4 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1148 cycles, achieve throughput    16 MB/s
transfer    4 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput    34 MB/s
transfer    4 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    41 MB/s
transfer    4 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    47 MB/s
transfer    4 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    593 cycles, achieve throughput    64 MB/s
transfer    4 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    61 MB/s
transfer    4 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    699 cycles, achieve throughput    68 MB/s
transfer    4 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput    75 MB/s
transfer    4 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    705 cycles, achieve throughput    81 MB/s
transfer    4 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    699 cycles, achieve throughput    89 MB/s
transfer    4 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput    95 MB/s
transfer    4 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   102 MB/s
transfer    4 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    589 cycles, achieve throughput   130 MB/s
transfer    4 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   259 MB/s
transfer    4 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   327 MB/s
transfer    4 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    591 cycles, achieve throughput   519 MB/s
transfer    4 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   545 MB/s
transfer    4 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput   658 MB/s
transfer    4 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput   765 MB/s
transfer    4 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput   872 MB/s
transfer    4 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    811 cycles, achieve throughput   852 MB/s
transfer    4 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    704 cycles, achieve throughput  1090 MB/s
transfer    4 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    817 cycles, achieve throughput  1034 MB/s
transfer    4 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    702 cycles, achieve throughput  1312 MB/s
transfer    4 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    814 cycles, achieve throughput  1226 MB/s
transfer    4 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    815 cycles, achieve throughput  1319 MB/s
transfer    4 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    815 cycles, achieve throughput  1413 MB/s
transfer    4 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    700 cycles, achieve throughput  1755 MB/s
transfer    4 *   288 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    816 cycles, achieve throughput  1694 MB/s
transfer    4 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    703 cycles, achieve throughput  2184 MB/s
transfer    4 *   352 Bytes with index=  352 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    820 cycles, achieve throughput  2060 MB/s
transfer    4 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    701 cycles, achieve throughput  2629 MB/s
transfer    4 *   416 Bytes with index=  416 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    824 cycles, achieve throughput  2423 MB/s
transfer    4 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  2645 MB/s
transfer    4 *   480 Bytes with index=  480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    932 cycles, achieve throughput  2472 MB/s
transfer    4 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    812 cycles, achieve throughput  3026 MB/s
transfer    4 *   576 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    811 cycles, achieve throughput  3409 MB/s
transfer    4 *   640 Bytes with index=  640 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    923 cycles, achieve throughput  3328 MB/s
transfer    4 *   704 Bytes with index=  704 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1040 cycles, achieve throughput  3249 MB/s
transfer    4 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    931 cycles, achieve throughput  3959 MB/s
transfer    4 *   832 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    933 cycles, achieve throughput  4280 MB/s
transfer    4 *   896 Bytes with index=  896 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1034 cycles, achieve throughput  4159 MB/s
transfer    4 *   960 Bytes with index=  960 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1034 cycles, achieve throughput  4456 MB/s
transfer    4 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1035 cycles, achieve throughput  4748 MB/s
transfer    4 *  1152 Bytes with index= 1152 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1152 cycles, achieve throughput  4800 MB/s
transfer    4 *  1280 Bytes with index= 1280 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1157 cycles, achieve throughput  5310 MB/s
transfer    4 *  1408 Bytes with index= 1408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1261 cycles, achieve throughput  5359 MB/s
transfer    4 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1375 cycles, achieve throughput  5362 MB/s
transfer    4 *  1664 Bytes with index= 1664 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1388 cycles, achieve throughput  5754 MB/s
transfer    4 *  1792 Bytes with index= 1792 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1487 cycles, achieve throughput  5784 MB/s
transfer    4 *  1920 Bytes with index= 1920 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1486 cycles, achieve throughput  6201 MB/s
transfer    4 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1603 cycles, achieve throughput  6132 MB/s
transfer    4 *  2304 Bytes with index= 2304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1709 cycles, achieve throughput  6471 MB/s
transfer    4 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1833 cycles, achieve throughput  6703 MB/s
transfer    4 *  2816 Bytes with index= 2816 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1947 cycles, achieve throughput  6942 MB/s
transfer    4 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2065 cycles, achieve throughput  7140 MB/s
transfer    4 *  3328 Bytes with index= 3328 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2180 cycles, achieve throughput  7327 MB/s
transfer    4 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2290 cycles, achieve throughput  7512 MB/s
transfer    4 *  3840 Bytes with index= 3840 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2400 cycles, achieve throughput  7680 MB/s
transfer    4 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2509 cycles, achieve throughput  7836 MB/s
transfer    4 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2754 cycles, achieve throughput  8031 MB/s
transfer    4 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3065 cycles, achieve throughput  8018 MB/s
transfer    4 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3295 cycles, achieve throughput  8204 MB/s
transfer    4 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3514 cycles, achieve throughput  8392 MB/s
transfer    4 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   3758 cycles, achieve throughput  8501 MB/s
transfer    4 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4015 cycles, achieve throughput  8569 MB/s
transfer    4 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4288 cycles, achieve throughput  8597 MB/s
transfer    4 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4578 cycles, achieve throughput  8589 MB/s
transfer    4 *  9216 Bytes with index= 9216 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5035 cycles, achieve throughput  8785 MB/s
transfer    4 * 10240 Bytes with index=10240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   5474 cycles, achieve throughput  8979 MB/s
transfer    4 * 11264 Bytes with index=11264 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6059 cycles, achieve throughput  8923 MB/s
transfer    4 * 12288 Bytes with index=12288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6506 cycles, achieve throughput  9065 MB/s
transfer    4 * 13312 Bytes with index=13312 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   6998 cycles, achieve throughput  9130 MB/s
transfer    4 * 14336 Bytes with index=14336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8498 cycles, achieve throughput  8097 MB/s
transfer    4 * 15360 Bytes with index=15360 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   7905 cycles, achieve throughput  9326 MB/s
transfer    4 * 16384 Bytes with index=16384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8497 cycles, achieve throughput  9255 MB/s
transfer    4 * 17408 Bytes with index=17408 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8964 cycles, achieve throughput  9321 MB/s
transfer    4 * 18432 Bytes with index=18432 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   9485 cycles, achieve throughput  9327 MB/s
transfer    4 * 19456 Bytes with index=19456 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  10037 cycles, achieve throughput  9304 MB/s
transfer    4 * 20480 Bytes with index=20480 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  10510 cycles, achieve throughput  9353 MB/s
transfer    4 * 21504 Bytes with index=21504 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  10984 cycles, achieve throughput  9397 MB/s
transfer    4 * 22528 Bytes with index=22528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12462 cycles, achieve throughput  8677 MB/s
transfer    4 * 23552 Bytes with index=23552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  11990 cycles, achieve throughput  9428 MB/s
transfer    4 * 24576 Bytes with index=24576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12441 cycles, achieve throughput  9481 MB/s
EDMA Index test with EDMA0 TC0
transfer 1024 *     1 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33509 cycles, achieve throughput    36 MB/s
transfer 1024 *     2 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33313 cycles, achieve throughput    73 MB/s
transfer 1024 *     3 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31974 cycles, achieve throughput   115 MB/s
transfer 1024 *     4 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33195 cycles, achieve throughput   148 MB/s
transfer 1024 *     5 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33166 cycles, achieve throughput   185 MB/s
transfer 1024 *     6 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32057 cycles, achieve throughput   229 MB/s
transfer 1024 *     7 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33058 cycles, achieve throughput   260 MB/s
transfer 1024 *     8 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32052 cycles, achieve throughput   306 MB/s
transfer 1024 *     9 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33055 cycles, achieve throughput   334 MB/s
transfer 1024 *    10 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33057 cycles, achieve throughput   371 MB/s
transfer 1024 *    11 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32055 cycles, achieve throughput   421 MB/s
transfer 1024 *    12 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33094 cycles, achieve throughput   445 MB/s
transfer 1024 *    13 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32977 cycles, achieve throughput   484 MB/s
transfer 1024 *    14 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31975 cycles, achieve throughput   538 MB/s
transfer 1024 *    15 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33082 cycles, achieve throughput   557 MB/s
transfer 1024 *    16 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33975 cycles, achieve throughput   578 MB/s
transfer 1024 *    32 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31974 cycles, achieve throughput  1229 MB/s
transfer 1024 *    48 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33427 cycles, achieve throughput  1764 MB/s
transfer 1024 *    64 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34447 cycles, achieve throughput  2283 MB/s
transfer 1024 *    80 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34629 cycles, achieve throughput  2838 MB/s
transfer 1024 *    96 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33448 cycles, achieve throughput  3526 MB/s
transfer 1024 *   112 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34466 cycles, achieve throughput  3993 MB/s
transfer 1024 *   128 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33428 cycles, achieve throughput  4705 MB/s
transfer 1024 *   144 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34196 cycles, achieve throughput  5174 MB/s
transfer 1024 *   160 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34100 cycles, achieve throughput  5765 MB/s
transfer 1024 *   176 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35350 cycles, achieve throughput  6117 MB/s
transfer 1024 *   192 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35596 cycles, achieve throughput  6627 MB/s
transfer 1024 *   208 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35977 cycles, achieve throughput  7104 MB/s
transfer 1024 *   224 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  36197 cycles, achieve throughput  7604 MB/s
transfer 1024 *   240 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37502 cycles, achieve throughput  7863 MB/s
transfer 1024 *   256 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37884 cycles, achieve throughput  8303 MB/s
transfer 1024 *   320 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42104 cycles, achieve throughput  9339 MB/s
transfer 1024 *   384 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  49281 cycles, achieve throughput  9574 MB/s
transfer 1024 *   448 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59235 cycles, achieve throughput  9293 MB/s
transfer 1024 *   512 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  68939 cycles, achieve throughput  9126 MB/s
transfer 1024 *   768 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 101555 cycles, achieve throughput  9292 MB/s
transfer 1024 *  1024 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 136328 cycles, achieve throughput  9229 MB/s
transfer  682 *  1536 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 135439 cycles, achieve throughput  9281 MB/s
transfer  512 *  2048 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131287 cycles, achieve throughput  9584 MB/s
transfer  409 *  2560 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130607 cycles, achieve throughput  9620 MB/s
transfer  341 *  3072 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130474 cycles, achieve throughput  9634 MB/s
transfer  292 *  3584 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133006 cycles, achieve throughput  9441 MB/s
transfer  256 *  4096 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132837 cycles, achieve throughput  9472 MB/s
transfer  227 *  4608 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131127 cycles, achieve throughput  9572 MB/s
transfer  204 *  5120 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130654 cycles, achieve throughput  9593 MB/s
transfer  186 *  5632 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130910 cycles, achieve throughput  9602 MB/s
transfer  170 *  6144 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132422 cycles, achieve throughput  9465 MB/s
transfer  157 *  6656 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132317 cycles, achieve throughput  9477 MB/s
transfer  146 *  7168 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130818 cycles, achieve throughput  9599 MB/s
transfer  136 *  7680 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129996 cycles, achieve throughput  9641 MB/s
transfer  128 *  8192 Bytes with index=    0 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131090 cycles, achieve throughput  9598 MB/s
transfer 1024 *     1 Bytes with index=    1 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    811 cycles, achieve throughput  1515 MB/s
transfer 1024 *     2 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes    813 cycles, achieve throughput  3022 MB/s
transfer 1024 *     3 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33231 cycles, achieve throughput   110 MB/s
transfer 1024 *     4 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1054 cycles, achieve throughput  4663 MB/s
transfer 1024 *     5 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32331 cycles, achieve throughput   190 MB/s
transfer 1024 *     6 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31890 cycles, achieve throughput   231 MB/s
transfer 1024 *     7 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32672 cycles, achieve throughput   263 MB/s
transfer 1024 *     8 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   1507 cycles, achieve throughput  6523 MB/s
transfer 1024 *     9 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33984 cycles, achieve throughput   325 MB/s
transfer 1024 *    10 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32369 cycles, achieve throughput   379 MB/s
transfer 1024 *    11 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34104 cycles, achieve throughput   396 MB/s
transfer 1024 *    12 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31799 cycles, achieve throughput   463 MB/s
transfer 1024 *    13 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34438 cycles, achieve throughput   463 MB/s
transfer 1024 *    14 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35009 cycles, achieve throughput   491 MB/s
transfer 1024 *    15 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34778 cycles, achieve throughput   529 MB/s
transfer 1024 *    16 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   2568 cycles, achieve throughput  7656 MB/s
transfer 1024 *    32 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   4547 cycles, achieve throughput  8647 MB/s
transfer 1024 *    48 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33249 cycles, achieve throughput  1773 MB/s
transfer 1024 *    64 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes   8524 cycles, achieve throughput  9226 MB/s
transfer 1024 *    80 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  38462 cycles, achieve throughput  2555 MB/s
transfer 1024 *    96 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30196 cycles, achieve throughput  3906 MB/s
transfer 1024 *   112 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  43513 cycles, achieve throughput  3162 MB/s
transfer 1024 *   128 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  16281 cycles, achieve throughput  9660 MB/s
transfer 1024 *   144 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  47894 cycles, achieve throughput  3694 MB/s
transfer 1024 *   160 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  45350 cycles, achieve throughput  4335 MB/s
transfer 1024 *   176 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  52367 cycles, achieve throughput  4129 MB/s
transfer 1024 *   192 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28511 cycles, achieve throughput  8275 MB/s
transfer 1024 *   208 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  60175 cycles, achieve throughput  4247 MB/s
transfer 1024 *   224 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  52928 cycles, achieve throughput  5200 MB/s
transfer 1024 *   240 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  62915 cycles, achieve throughput  4687 MB/s
transfer 1024 *   256 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34785 cycles, achieve throughput  9043 MB/s
transfer 1024 *   320 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42879 cycles, achieve throughput  9170 MB/s
transfer 1024 *   384 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  49915 cycles, achieve throughput  9453 MB/s
transfer 1024 *   448 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59592 cycles, achieve throughput  9237 MB/s
transfer 1024 *   512 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  66998 cycles, achieve throughput  9390 MB/s
transfer 1024 *   768 Bytes with index=  768 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 100135 cycles, achieve throughput  9424 MB/s
transfer 1024 *  1024 Bytes with index= 1024 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 134588 cycles, achieve throughput  9349 MB/s
transfer  682 *  1536 Bytes with index= 1536 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133134 cycles, achieve throughput  9442 MB/s
transfer  512 *  2048 Bytes with index= 2048 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131126 cycles, achieve throughput  9596 MB/s
transfer  409 *  2560 Bytes with index= 2560 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133028 cycles, achieve throughput  9444 MB/s
transfer  341 *  3072 Bytes with index= 3072 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132454 cycles, achieve throughput  9490 MB/s
transfer  292 *  3584 Bytes with index= 3584 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131977 cycles, achieve throughput  9515 MB/s
transfer  256 *  4096 Bytes with index= 4096 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132956 cycles, achieve throughput  9463 MB/s
transfer  227 *  4608 Bytes with index= 4608 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130788 cycles, achieve throughput  9597 MB/s
transfer  204 *  5120 Bytes with index= 5120 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130336 cycles, achieve throughput  9616 MB/s
transfer  186 *  5632 Bytes with index= 5632 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132123 cycles, achieve throughput  9514 MB/s
transfer  170 *  6144 Bytes with index= 6144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130251 cycles, achieve throughput  9622 MB/s
transfer  157 *  6656 Bytes with index= 6656 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131532 cycles, achieve throughput  9533 MB/s
transfer  146 *  7168 Bytes with index= 7168 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133941 cycles, achieve throughput  9376 MB/s
transfer  136 *  7680 Bytes with index= 7680 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130474 cycles, achieve throughput  9606 MB/s
transfer  128 *  8192 Bytes with index= 8192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133429 cycles, achieve throughput  9430 MB/s
transfer 1024 *     1 Bytes with index=    2 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34117 cycles, achieve throughput    36 MB/s
transfer 1024 *     2 Bytes with index=    3 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31777 cycles, achieve throughput    77 MB/s
transfer 1024 *     3 Bytes with index=    4 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30555 cycles, achieve throughput   120 MB/s
transfer 1024 *     4 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32890 cycles, achieve throughput   149 MB/s
transfer 1024 *     5 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33003 cycles, achieve throughput   186 MB/s
transfer 1024 *     6 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32132 cycles, achieve throughput   229 MB/s
transfer 1024 *     7 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30096 cycles, achieve throughput   285 MB/s
transfer 1024 *     8 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32098 cycles, achieve throughput   306 MB/s
transfer 1024 *     9 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33476 cycles, achieve throughput   330 MB/s
transfer 1024 *    10 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32329 cycles, achieve throughput   380 MB/s
transfer 1024 *    11 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32896 cycles, achieve throughput   410 MB/s
transfer 1024 *    12 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32882 cycles, achieve throughput   448 MB/s
transfer 1024 *    13 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32882 cycles, achieve throughput   485 MB/s
transfer 1024 *    14 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34907 cycles, achieve throughput   492 MB/s
transfer 1024 *    15 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  25815 cycles, achieve throughput   714 MB/s
transfer 1024 *    16 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33255 cycles, achieve throughput   591 MB/s
transfer 1024 *    32 Bytes with index=   33 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35514 cycles, achieve throughput  1107 MB/s
transfer 1024 *    48 Bytes with index=   49 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41416 cycles, achieve throughput  1424 MB/s
transfer 1024 *    64 Bytes with index=   65 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  43810 cycles, achieve throughput  1795 MB/s
transfer 1024 *    80 Bytes with index=   81 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  45477 cycles, achieve throughput  2161 MB/s
transfer 1024 *    96 Bytes with index=   97 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  50711 cycles, achieve throughput  2326 MB/s
transfer 1024 *   112 Bytes with index=  113 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  50276 cycles, achieve throughput  2737 MB/s
transfer 1024 *   128 Bytes with index=  129 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  52696 cycles, achieve throughput  2984 MB/s
transfer 1024 *   144 Bytes with index=  145 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  53473 cycles, achieve throughput  3309 MB/s
transfer 1024 *   160 Bytes with index=  161 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  56564 cycles, achieve throughput  3475 MB/s
transfer 1024 *   176 Bytes with index=  177 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59272 cycles, achieve throughput  3648 MB/s
transfer 1024 *   192 Bytes with index=  193 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  61590 cycles, achieve throughput  3830 MB/s
transfer 1024 *   208 Bytes with index=  209 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  63103 cycles, achieve throughput  4050 MB/s
transfer 1024 *   224 Bytes with index=  225 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  68336 cycles, achieve throughput  4027 MB/s
transfer 1024 *   240 Bytes with index=  241 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  69698 cycles, achieve throughput  4231 MB/s
transfer 1024 *   256 Bytes with index=  257 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  77304 cycles, achieve throughput  4069 MB/s
transfer 1024 *   320 Bytes with index=  321 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  84626 cycles, achieve throughput  4646 MB/s
transfer 1024 *   384 Bytes with index=  385 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  90157 cycles, achieve throughput  5233 MB/s
transfer 1024 *   448 Bytes with index=  449 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 101725 cycles, achieve throughput  5411 MB/s
transfer 1024 *   512 Bytes with index=  513 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 107100 cycles, achieve throughput  5874 MB/s
transfer 1024 *   768 Bytes with index=  769 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 134770 cycles, achieve throughput  7002 MB/s
transfer 1023 *  1024 Bytes with index= 1025 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 170296 cycles, achieve throughput  7381 MB/s
transfer  682 *  1536 Bytes with index= 1537 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 165683 cycles, achieve throughput  7587 MB/s
transfer  511 *  2048 Bytes with index= 2049 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 161634 cycles, achieve throughput  7769 MB/s
transfer  409 *  2560 Bytes with index= 2561 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 160080 cycles, achieve throughput  7848 MB/s
transfer  341 *  3072 Bytes with index= 3073 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 161496 cycles, achieve throughput  7783 MB/s
transfer  292 *  3584 Bytes with index= 3585 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 157789 cycles, achieve throughput  7958 MB/s
transfer  255 *  4096 Bytes with index= 4097 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 160627 cycles, achieve throughput  7803 MB/s
transfer  227 *  4608 Bytes with index= 4609 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 159593 cycles, achieve throughput  7865 MB/s
transfer  204 *  5120 Bytes with index= 5121 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 158214 cycles, achieve throughput  7922 MB/s
transfer  186 *  5632 Bytes with index= 5633 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 158913 cycles, achieve throughput  7910 MB/s
transfer  170 *  6144 Bytes with index= 6145 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 160009 cycles, achieve throughput  7833 MB/s
transfer  157 *  6656 Bytes with index= 6657 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 162124 cycles, achieve throughput  7734 MB/s
transfer  146 *  7168 Bytes with index= 7169 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 159158 cycles, achieve throughput  7890 MB/s
transfer  136 *  7680 Bytes with index= 7681 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 159110 cycles, achieve throughput  7877 MB/s
transfer  127 *  8192 Bytes with index= 8193 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 160970 cycles, achieve throughput  7755 MB/s
transfer 1024 *     1 Bytes with index=    5 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31754 cycles, achieve throughput    38 MB/s
transfer 1024 *     2 Bytes with index=    6 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  29849 cycles, achieve throughput    82 MB/s
transfer 1024 *     3 Bytes with index=    7 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31665 cycles, achieve throughput   116 MB/s
transfer 1024 *     4 Bytes with index=    8 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30091 cycles, achieve throughput   163 MB/s
transfer 1024 *     5 Bytes with index=    9 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30669 cycles, achieve throughput   200 MB/s
transfer 1024 *     6 Bytes with index=   10 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31217 cycles, achieve throughput   236 MB/s
transfer 1024 *     7 Bytes with index=   11 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32230 cycles, achieve throughput   266 MB/s
transfer 1024 *     8 Bytes with index=   12 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30457 cycles, achieve throughput   322 MB/s
transfer 1024 *     9 Bytes with index=   13 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32353 cycles, achieve throughput   341 MB/s
transfer 1024 *    10 Bytes with index=   14 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31683 cycles, achieve throughput   387 MB/s
transfer 1024 *    11 Bytes with index=   15 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32228 cycles, achieve throughput   419 MB/s
transfer 1024 *    12 Bytes with index=   16 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26145 cycles, achieve throughput   563 MB/s
transfer 1024 *    13 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  31574 cycles, achieve throughput   505 MB/s
transfer 1024 *    14 Bytes with index=   18 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  32692 cycles, achieve throughput   526 MB/s
transfer 1024 *    15 Bytes with index=   19 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33387 cycles, achieve throughput   552 MB/s
transfer 1024 *    16 Bytes with index=   20 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30789 cycles, achieve throughput   638 MB/s
transfer 1024 *    32 Bytes with index=   36 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33848 cycles, achieve throughput  1161 MB/s
transfer 1024 *    48 Bytes with index=   52 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  38925 cycles, achieve throughput  1515 MB/s
transfer 1024 *    64 Bytes with index=   68 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41676 cycles, achieve throughput  1887 MB/s
transfer 1024 *    80 Bytes with index=   84 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  42646 cycles, achieve throughput  2305 MB/s
transfer 1024 *    96 Bytes with index=  100 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  44154 cycles, achieve throughput  2671 MB/s
transfer 1024 *   112 Bytes with index=  116 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  48272 cycles, achieve throughput  2851 MB/s
transfer 1024 *   128 Bytes with index=  132 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  49640 cycles, achieve throughput  3168 MB/s
transfer 1024 *   144 Bytes with index=  148 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  51868 cycles, achieve throughput  3411 MB/s
transfer 1024 *   160 Bytes with index=  164 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  54112 cycles, achieve throughput  3633 MB/s
transfer 1024 *   176 Bytes with index=  180 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59684 cycles, achieve throughput  3623 MB/s
transfer 1024 *   192 Bytes with index=  196 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59261 cycles, achieve throughput  3981 MB/s
transfer 1024 *   208 Bytes with index=  212 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  60315 cycles, achieve throughput  4237 MB/s
transfer 1024 *   224 Bytes with index=  228 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  64848 cycles, achieve throughput  4244 MB/s
transfer 1024 *   240 Bytes with index=  244 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  69201 cycles, achieve throughput  4261 MB/s
transfer 1024 *   256 Bytes with index=  260 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  73907 cycles, achieve throughput  4256 MB/s
transfer 1024 *   320 Bytes with index=  324 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  82414 cycles, achieve throughput  4771 MB/s
transfer 1024 *   384 Bytes with index=  388 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  88962 cycles, achieve throughput  5304 MB/s
transfer 1024 *   448 Bytes with index=  452 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  99319 cycles, achieve throughput  5542 MB/s
transfer 1024 *   512 Bytes with index=  516 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 105594 cycles, achieve throughput  5958 MB/s
transfer 1024 *   768 Bytes with index=  772 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130670 cycles, achieve throughput  7222 MB/s
transfer 1020 *  1024 Bytes with index= 1028 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 169181 cycles, achieve throughput  7408 MB/s
transfer  680 *  1536 Bytes with index= 1540 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 160145 cycles, achieve throughput  7826 MB/s
transfer  511 *  2048 Bytes with index= 2052 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 154740 cycles, achieve throughput  8115 MB/s
transfer  408 *  2560 Bytes with index= 2564 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 154070 cycles, achieve throughput  8135 MB/s
transfer  340 *  3072 Bytes with index= 3076 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155805 cycles, achieve throughput  8044 MB/s
transfer  292 *  3584 Bytes with index= 3588 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155380 cycles, achieve throughput  8082 MB/s
transfer  255 *  4096 Bytes with index= 4100 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155186 cycles, achieve throughput  8076 MB/s
transfer  227 *  4608 Bytes with index= 4612 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 154904 cycles, achieve throughput  8103 MB/s
transfer  204 *  5120 Bytes with index= 5124 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 156714 cycles, achieve throughput  7997 MB/s
transfer  186 *  5632 Bytes with index= 5636 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155856 cycles, achieve throughput  8065 MB/s
transfer  170 *  6144 Bytes with index= 6148 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155503 cycles, achieve throughput  8060 MB/s
transfer  157 *  6656 Bytes with index= 6660 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 157051 cycles, achieve throughput  7984 MB/s
transfer  146 *  7168 Bytes with index= 7172 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 155481 cycles, achieve throughput  8077 MB/s
transfer  136 *  7680 Bytes with index= 7684 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 157463 cycles, achieve throughput  7959 MB/s
transfer  127 *  8192 Bytes with index= 8196 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 159280 cycles, achieve throughput  7838 MB/s
transfer 1024 *     1 Bytes with index=   17 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26105 cycles, achieve throughput    47 MB/s
transfer 1024 *     2 Bytes with index=   18 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  25204 cycles, achieve throughput    97 MB/s
transfer 1024 *     3 Bytes with index=   19 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  25910 cycles, achieve throughput   142 MB/s
transfer 1024 *     4 Bytes with index=   20 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  25378 cycles, achieve throughput   193 MB/s
transfer 1024 *     5 Bytes with index=   21 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26004 cycles, achieve throughput   236 MB/s
transfer 1024 *     6 Bytes with index=   22 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  25589 cycles, achieve throughput   288 MB/s
transfer 1024 *     7 Bytes with index=   23 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26928 cycles, achieve throughput   319 MB/s
transfer 1024 *     8 Bytes with index=   24 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23103 cycles, achieve throughput   425 MB/s
transfer 1024 *     9 Bytes with index=   25 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26575 cycles, achieve throughput   416 MB/s
transfer 1024 *    10 Bytes with index=   26 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26572 cycles, achieve throughput   462 MB/s
transfer 1024 *    11 Bytes with index=   27 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  27344 cycles, achieve throughput   494 MB/s
transfer 1024 *    12 Bytes with index=   28 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  25805 cycles, achieve throughput   571 MB/s
transfer 1024 *    13 Bytes with index=   29 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28135 cycles, achieve throughput   567 MB/s
transfer 1024 *    14 Bytes with index=   30 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28934 cycles, achieve throughput   594 MB/s
transfer 1024 *    15 Bytes with index=   31 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  29703 cycles, achieve throughput   620 MB/s
transfer 1024 *    16 Bytes with index=   32 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22321 cycles, achieve throughput   880 MB/s
transfer 1024 *    32 Bytes with index=   48 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  24122 cycles, achieve throughput  1630 MB/s
transfer 1024 *    48 Bytes with index=   64 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  16889 cycles, achieve throughput  3492 MB/s
transfer 1024 *    64 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28503 cycles, achieve throughput  2759 MB/s
transfer 1024 *    80 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30660 cycles, achieve throughput  3206 MB/s
transfer 1024 *    96 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  36661 cycles, achieve throughput  3217 MB/s
transfer 1024 *   112 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22139 cycles, achieve throughput  6216 MB/s
transfer 1024 *   128 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  40249 cycles, achieve throughput  3907 MB/s
transfer 1024 *   144 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  43113 cycles, achieve throughput  4104 MB/s
transfer 1024 *   160 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  44478 cycles, achieve throughput  4420 MB/s
transfer 1024 *   176 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28548 cycles, achieve throughput  7575 MB/s
transfer 1024 *   192 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  52508 cycles, achieve throughput  4493 MB/s
transfer 1024 *   208 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  54014 cycles, achieve throughput  4731 MB/s
transfer 1024 *   224 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  51944 cycles, achieve throughput  5298 MB/s
transfer 1024 *   240 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35036 cycles, achieve throughput  8417 MB/s
transfer 1024 *   256 Bytes with index=  272 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  56144 cycles, achieve throughput  5602 MB/s
transfer 1024 *   320 Bytes with index=  336 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  62906 cycles, achieve throughput  6250 MB/s
transfer 1024 *   384 Bytes with index=  400 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  71566 cycles, achieve throughput  6593 MB/s
transfer 1024 *   448 Bytes with index=  464 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  80640 cycles, achieve throughput  6826 MB/s
transfer 1024 *   512 Bytes with index=  528 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  89480 cycles, achieve throughput  7031 MB/s
transfer 1024 *   768 Bytes with index=  784 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 122368 cycles, achieve throughput  7712 MB/s
transfer 1008 *  1024 Bytes with index= 1040 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 151816 cycles, achieve throughput  8158 MB/s
transfer  675 *  1536 Bytes with index= 1552 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 147554 cycles, achieve throughput  8431 MB/s
transfer  508 *  2048 Bytes with index= 2064 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145323 cycles, achieve throughput  8590 MB/s
transfer  407 *  2560 Bytes with index= 2576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145419 cycles, achieve throughput  8597 MB/s
transfer  339 *  3072 Bytes with index= 3088 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145795 cycles, achieve throughput  8571 MB/s
transfer  291 *  3584 Bytes with index= 3600 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144312 cycles, achieve throughput  8672 MB/s
transfer  255 *  4096 Bytes with index= 4112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 146245 cycles, achieve throughput  8570 MB/s
transfer  226 *  4608 Bytes with index= 4624 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 143299 cycles, achieve throughput  8720 MB/s
transfer  204 *  5120 Bytes with index= 5136 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 143268 cycles, achieve throughput  8748 MB/s
transfer  185 *  5632 Bytes with index= 5648 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145753 cycles, achieve throughput  8578 MB/s
transfer  170 *  6144 Bytes with index= 6160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144706 cycles, achieve throughput  8661 MB/s
transfer  157 *  6656 Bytes with index= 6672 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 143923 cycles, achieve throughput  8712 MB/s
transfer  145 *  7168 Bytes with index= 7184 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 146052 cycles, achieve throughput  8539 MB/s
transfer  136 *  7680 Bytes with index= 7696 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 145885 cycles, achieve throughput  8591 MB/s
transfer  127 *  8192 Bytes with index= 8208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 144055 cycles, achieve throughput  8666 MB/s
transfer 1024 *     1 Bytes with index=   65 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13023 cycles, achieve throughput    94 MB/s
transfer 1024 *     2 Bytes with index=   66 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12957 cycles, achieve throughput   189 MB/s
transfer 1024 *     3 Bytes with index=   67 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13062 cycles, achieve throughput   282 MB/s
transfer 1024 *     4 Bytes with index=   68 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12859 cycles, achieve throughput   382 MB/s
transfer 1024 *     5 Bytes with index=   69 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13272 cycles, achieve throughput   462 MB/s
transfer 1024 *     6 Bytes with index=   70 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13279 cycles, achieve throughput   555 MB/s
transfer 1024 *     7 Bytes with index=   71 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13431 cycles, achieve throughput   640 MB/s
transfer 1024 *     8 Bytes with index=   72 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13900 cycles, achieve throughput   707 MB/s
transfer 1024 *     9 Bytes with index=   73 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13696 cycles, achieve throughput   807 MB/s
transfer 1024 *    10 Bytes with index=   74 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13692 cycles, achieve throughput   897 MB/s
transfer 1024 *    11 Bytes with index=   75 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13877 cycles, achieve throughput   974 MB/s
transfer 1024 *    12 Bytes with index=   76 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  13654 cycles, achieve throughput  1079 MB/s
transfer 1024 *    13 Bytes with index=   77 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14086 cycles, achieve throughput  1134 MB/s
transfer 1024 *    14 Bytes with index=   78 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14063 cycles, achieve throughput  1223 MB/s
transfer 1024 *    15 Bytes with index=   79 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  14306 cycles, achieve throughput  1288 MB/s
transfer 1024 *    16 Bytes with index=   80 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12927 cycles, achieve throughput  1520 MB/s
transfer 1024 *    32 Bytes with index=   96 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  12913 cycles, achieve throughput  3045 MB/s
transfer 1024 *    48 Bytes with index=  112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  16011 cycles, achieve throughput  3683 MB/s
transfer 1024 *    64 Bytes with index=  128 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  16941 cycles, achieve throughput  4642 MB/s
transfer 1024 *    80 Bytes with index=  144 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19052 cycles, achieve throughput  5159 MB/s
transfer 1024 *    96 Bytes with index=  160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  19065 cycles, achieve throughput  6187 MB/s
transfer 1024 *   112 Bytes with index=  176 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  22397 cycles, achieve throughput  6144 MB/s
transfer 1024 *   128 Bytes with index=  192 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  23133 cycles, achieve throughput  6799 MB/s
transfer 1024 *   144 Bytes with index=  208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26839 cycles, achieve throughput  6592 MB/s
transfer 1024 *   160 Bytes with index=  224 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  26847 cycles, achieve throughput  7323 MB/s
transfer 1024 *   176 Bytes with index=  240 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  30998 cycles, achieve throughput  6976 MB/s
transfer 1024 *   192 Bytes with index=  256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  28456 cycles, achieve throughput  8291 MB/s
transfer 1024 *   208 Bytes with index=  272 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  33944 cycles, achieve throughput  7529 MB/s
transfer 1024 *   224 Bytes with index=  288 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  35081 cycles, achieve throughput  7846 MB/s
transfer 1024 *   240 Bytes with index=  304 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  37577 cycles, achieve throughput  7848 MB/s
transfer 1024 *   256 Bytes with index=  320 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  34930 cycles, achieve throughput  9005 MB/s
transfer 1024 *   320 Bytes with index=  384 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  41997 cycles, achieve throughput  9362 MB/s
transfer 1024 *   384 Bytes with index=  448 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  52332 cycles, achieve throughput  9016 MB/s
transfer 1024 *   448 Bytes with index=  512 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  59990 cycles, achieve throughput  9176 MB/s
transfer 1024 *   512 Bytes with index=  576 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  66997 cycles, achieve throughput  9390 MB/s
transfer 1024 *   768 Bytes with index=  832 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes  99836 cycles, achieve throughput  9452 MB/s
transfer  963 *  1024 Bytes with index= 1088 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 126311 cycles, achieve throughput  9368 MB/s
transfer  655 *  1536 Bytes with index= 1600 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129181 cycles, achieve throughput  9345 MB/s
transfer  496 *  2048 Bytes with index= 2112 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129767 cycles, achieve throughput  9393 MB/s
transfer  399 *  2560 Bytes with index= 2624 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129778 cycles, achieve throughput  9444 MB/s
transfer  334 *  3072 Bytes with index= 3136 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 130008 cycles, achieve throughput  9470 MB/s
transfer  287 *  3584 Bytes with index= 3648 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129370 cycles, achieve throughput  9541 MB/s
transfer  252 *  4096 Bytes with index= 4160 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129438 cycles, achieve throughput  9569 MB/s
transfer  224 *  4608 Bytes with index= 4672 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129676 cycles, achieve throughput  9551 MB/s
transfer  202 *  5120 Bytes with index= 5184 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132549 cycles, achieve throughput  9363 MB/s
transfer  184 *  5632 Bytes with index= 5696 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129557 cycles, achieve throughput  9598 MB/s
transfer  168 *  6144 Bytes with index= 6208 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 132351 cycles, achieve throughput  9358 MB/s
transfer  156 *  6656 Bytes with index= 6720 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 131612 cycles, achieve throughput  9467 MB/s
transfer  144 *  7168 Bytes with index= 7232 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129164 cycles, achieve throughput  9589 MB/s
transfer  135 *  7680 Bytes with index= 7744 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 129666 cycles, achieve throughput  9595 MB/s
transfer  127 *  8192 Bytes with index= 8256 from 0x c080000(MSMC RAM) to 0x80000000(DDR3A), consumes 133070 cycles, achieve throughput  9381 MB/s
EDMA test complete
Test complete
