JTAG ID= 0x0b9a602f. This is a K2E device, version variant = 0
DEVSTAT= 0x00000661. little endian, no boot or I2C slave boot, boot master is ARM core, PLL configuration implies the input clock for core is 100MHz
SmartReflex VID= 46, required core voltage= 0.995V.
Die ID= 0x0600c004, 0x0c00ea85, 0x00000000, 0x79900000
DSP speed grade = 800MHz, ARM speed grade= 800MHz
Enable IRQ and FIQ.
Enable Exception handling...
Initialize main core clock = 100.00MHz/1x12 = 1200MHz
DDR3A initialization
Initialize DDR data rate = 100.000/1*16/4*4= 1600.0 MTS, bus width = 64 bits.
DDR PHY status PGSR0=0xb0000fff.
Ethernet port 0 test setup: no connection  , forced 1000M fullduplex  , SerDes internal loopback
Ethernet port 1 test setup: no connection  , forced 1000M fullduplex  , SGMII loopback          
Ethernet port 2 test setup: no connection  , forced 1000M fullduplex  , SerDes internal loopback
Ethernet port 3 test setup: no connection  , forced 1000M fullduplex  , SGMII loopback          
Ethernet port 4 test setup: no connection  , forced 1000M fullduplex  , SerDes internal loopback
Ethernet port 5 test setup: no connection  , forced 1000M fullduplex  , SGMII loopback          
Ethernet port 6 test setup: no connection  , forced 1000M fullduplex  , SGMII loopback          
Ethernet port 7 test setup: no connection  , forced 1000M fullduplex  , MAC loopback            
Initialize PASS PLL clock = 100.00MHz/2x21 = 1050MHz
CPSW_port0.RxGoodFrames     =8
CPSW_port0.RxOctets         =1168
CPSW_port0.TxGoodFrames     =8
CPSW_port0.TxOctets         =1168
CPSW_port0.Frame128t255     =16
CPSW_port0.NetOctets        =2336
CPSW_port1.RxGoodFrames     =1
CPSW_port1.RxOctets         =146
CPSW_port1.TxGoodFrames     =1
CPSW_port1.TxOctets         =146
CPSW_port1.Frame128t255     =2
CPSW_port1.NetOctets        =292
CPSW_port2.RxGoodFrames     =1
CPSW_port2.RxOctets         =146
CPSW_port2.TxGoodFrames     =1
CPSW_port2.TxOctets         =146
CPSW_port2.Frame128t255     =2
CPSW_port2.NetOctets        =292
CPSW_port3.RxGoodFrames     =1
CPSW_port3.RxOctets         =146
CPSW_port3.TxGoodFrames     =1
CPSW_port3.TxOctets         =146
CPSW_port3.Frame128t255     =2
CPSW_port3.NetOctets        =292
CPSW_port4.RxGoodFrames     =1
CPSW_port4.RxOctets         =146
CPSW_port4.TxGoodFrames     =1
CPSW_port4.TxOctets         =146
CPSW_port4.Frame128t255     =2
CPSW_port4.NetOctets        =292
CPSW_port5.RxGoodFrames     =1
CPSW_port5.RxOctets         =146
CPSW_port5.TxGoodFrames     =1
CPSW_port5.TxOctets         =146
CPSW_port5.Frame128t255     =2
CPSW_port5.NetOctets        =292
CPSW_port6.RxGoodFrames     =1
CPSW_port6.RxOctets         =146
CPSW_port6.TxGoodFrames     =1
CPSW_port6.TxOctets         =146
CPSW_port6.Frame128t255     =2
CPSW_port6.NetOctets        =292
CPSW_port7.RxGoodFrames     =1
CPSW_port7.RxOctets         =146
CPSW_port7.TxGoodFrames     =1
CPSW_port7.TxOctets         =146
CPSW_port7.Frame128t255     =2
CPSW_port7.NetOctets        =292
CPSW_port8.RxGoodFrames     =1
CPSW_port8.RxOctets         =146
CPSW_port8.TxGoodFrames     =1
CPSW_port8.TxOctets         =146
CPSW_port8.Frame128t255     =2
CPSW_port8.NetOctets        =292
Ethernet port 0 TX  1 packets x  128 bytes, RX  1 packets,     4738 cycles,   259 Mbps
Ethernet port 1 TX  1 packets x  128 bytes, RX  1 packets,     4842 cycles,   253 Mbps
Ethernet port 2 TX  1 packets x  128 bytes, RX  1 packets,     5807 cycles,   211 Mbps
Ethernet port 3 TX  1 packets x  128 bytes, RX  1 packets,     4706 cycles,   261 Mbps
Ethernet port 4 TX  1 packets x  128 bytes, RX  1 packets,     4622 cycles,   265 Mbps
Ethernet port 5 TX  1 packets x  128 bytes, RX  1 packets,     5687 cycles,   216 Mbps
Ethernet port 6 TX  1 packets x  128 bytes, RX  1 packets,     5508 cycles,   223 Mbps
Ethernet port 7 TX  1 packets x  128 bytes, RX  1 packets,     5340 cycles,   230 Mbps

CPSW_port0.RxGoodFrames     =16
CPSW_port0.RxOctets         =9504
CPSW_port0.TxGoodFrames     =16
CPSW_port0.TxOctets         =9504
CPSW_port0.Frame1024tUp     =16
CPSW_port0.NetOctets        =19008
CPSW_port1.RxGoodFrames     =2
CPSW_port1.RxOctets         =1188
CPSW_port1.TxGoodFrames     =2
CPSW_port1.TxOctets         =1188
CPSW_port1.Frame1024tUp     =2
CPSW_port1.NetOctets        =2376
CPSW_port2.RxGoodFrames     =2
CPSW_port2.RxOctets         =1188
CPSW_port2.TxGoodFrames     =2
CPSW_port2.TxOctets         =1188
CPSW_port2.Frame1024tUp     =2
CPSW_port2.NetOctets        =2376
CPSW_port3.RxGoodFrames     =2
CPSW_port3.RxOctets         =1188
CPSW_port3.TxGoodFrames     =2
CPSW_port3.TxOctets         =1188
CPSW_port3.Frame1024tUp     =2
CPSW_port3.NetOctets        =2376
CPSW_port4.RxGoodFrames     =2
CPSW_port4.RxOctets         =1188
CPSW_port4.TxGoodFrames     =2
CPSW_port4.TxOctets         =1188
CPSW_port4.Frame1024tUp     =2
CPSW_port4.NetOctets        =2376
CPSW_port5.RxGoodFrames     =2
CPSW_port5.RxOctets         =1188
CPSW_port5.TxGoodFrames     =2
CPSW_port5.TxOctets         =1188
CPSW_port5.Frame1024tUp     =2
CPSW_port5.NetOctets        =2376
CPSW_port6.RxGoodFrames     =2
CPSW_port6.RxOctets         =1188
CPSW_port6.TxGoodFrames     =2
CPSW_port6.TxOctets         =1188
CPSW_port6.Frame1024tUp     =2
CPSW_port6.NetOctets        =2376
CPSW_port7.RxGoodFrames     =2
CPSW_port7.RxOctets         =1188
CPSW_port7.TxGoodFrames     =2
CPSW_port7.TxOctets         =1188
CPSW_port7.Frame1024tUp     =2
CPSW_port7.NetOctets        =2376
CPSW_port8.RxGoodFrames     =2
CPSW_port8.RxOctets         =1188
CPSW_port8.TxGoodFrames     =2
CPSW_port8.TxOctets         =1188
CPSW_port8.Frame1024tUp     =2
CPSW_port8.NetOctets        =2376
Ethernet port 0 TX  1 packets x 1024 bytes, RX  1 packets,    15409 cycles,   637 Mbps
Ethernet port 1 TX  1 packets x 1024 bytes, RX  1 packets,    14912 cycles,   659 Mbps
Ethernet port 2 TX  1 packets x 1024 bytes, RX  1 packets,    16601 cycles,   592 Mbps
Ethernet port 3 TX  1 packets x 1024 bytes, RX  1 packets,    16075 cycles,   611 Mbps
Ethernet port 4 TX  1 packets x 1024 bytes, RX  1 packets,    15596 cycles,   630 Mbps
Ethernet port 5 TX  1 packets x 1024 bytes, RX  1 packets,    15134 cycles,   649 Mbps
Ethernet port 6 TX  1 packets x 1024 bytes, RX  1 packets,    14672 cycles,   670 Mbps
Ethernet port 7 TX  1 packets x 1024 bytes, RX  1 packets,     8188 cycles,  1200 Mbps

CPSW_port0.RxGoodFrames     =24
CPSW_port0.RxOctets         =75184
CPSW_port0.TxGoodFrames     =24
CPSW_port0.TxOctets         =75184
CPSW_port0.Frame1024tUp     =32
CPSW_port0.NetOctets        =150368
CPSW_port1.RxGoodFrames     =3
CPSW_port1.RxOctets         =9398
CPSW_port1.TxGoodFrames     =3
CPSW_port1.TxOctets         =9398
CPSW_port1.Frame1024tUp     =4
CPSW_port1.NetOctets        =18796
CPSW_port2.RxGoodFrames     =3
CPSW_port2.RxOctets         =9398
CPSW_port2.TxGoodFrames     =3
CPSW_port2.TxOctets         =9398
CPSW_port2.Frame1024tUp     =4
CPSW_port2.NetOctets        =18796
CPSW_port3.RxGoodFrames     =3
CPSW_port3.RxOctets         =9398
CPSW_port3.TxGoodFrames     =3
CPSW_port3.TxOctets         =9398
CPSW_port3.Frame1024tUp     =4
CPSW_port3.NetOctets        =18796
CPSW_port4.RxGoodFrames     =3
CPSW_port4.RxOctets         =9398
CPSW_port4.TxGoodFrames     =3
CPSW_port4.TxOctets         =9398
CPSW_port4.Frame1024tUp     =4
CPSW_port4.NetOctets        =18796
CPSW_port5.RxGoodFrames     =3
CPSW_port5.RxOctets         =9398
CPSW_port5.TxGoodFrames     =3
CPSW_port5.TxOctets         =9398
CPSW_port5.Frame1024tUp     =4
CPSW_port5.NetOctets        =18796
CPSW_port6.RxGoodFrames     =3
CPSW_port6.RxOctets         =9398
CPSW_port6.TxGoodFrames     =3
CPSW_port6.TxOctets         =9398
CPSW_port6.Frame1024tUp     =4
CPSW_port6.NetOctets        =18796
CPSW_port7.RxGoodFrames     =3
CPSW_port7.RxOctets         =9398
CPSW_port7.TxGoodFrames     =3
CPSW_port7.TxOctets         =9398
CPSW_port7.Frame1024tUp     =4
CPSW_port7.NetOctets        =18796
CPSW_port8.RxGoodFrames     =3
CPSW_port8.RxOctets         =9398
CPSW_port8.TxGoodFrames     =3
CPSW_port8.TxOctets         =9398
CPSW_port8.Frame1024tUp     =4
CPSW_port8.NetOctets        =18796
Ethernet port 0 TX  1 packets x 8192 bytes, RX  1 packets,    96217 cycles,   817 Mbps
Ethernet port 1 TX  1 packets x 8192 bytes, RX  1 packets,   102200 cycles,   769 Mbps
Ethernet port 2 TX  1 packets x 8192 bytes, RX  1 packets,   108153 cycles,   727 Mbps
Ethernet port 3 TX  1 packets x 8192 bytes, RX  1 packets,   114160 cycles,   688 Mbps
Ethernet port 4 TX  1 packets x 8192 bytes, RX  1 packets,   120185 cycles,   654 Mbps
Ethernet port 5 TX  1 packets x 8192 bytes, RX  1 packets,   126204 cycles,   623 Mbps
Ethernet port 6 TX  1 packets x 8192 bytes, RX  1 packets,   132208 cycles,   594 Mbps
Ethernet port 7 TX  1 packets x 8192 bytes, RX  1 packets,    65155 cycles,  1207 Mbps

CPSW_port0.RxGoodFrames     =56
CPSW_port0.RxOctets         =79856
CPSW_port0.TxGoodFrames     =56
CPSW_port0.TxOctets         =79856
CPSW_port0.Frame128t255     =80
CPSW_port0.NetOctets        =159712
CPSW_port1.RxGoodFrames     =7
CPSW_port1.RxOctets         =9982
CPSW_port1.TxGoodFrames     =7
CPSW_port1.TxOctets         =9982
CPSW_port1.Frame128t255     =10
CPSW_port1.NetOctets        =19964
CPSW_port2.RxGoodFrames     =7
CPSW_port2.RxOctets         =9982
CPSW_port2.TxGoodFrames     =7
CPSW_port2.TxOctets         =9982
CPSW_port2.Frame128t255     =10
CPSW_port2.NetOctets        =19964
CPSW_port3.RxGoodFrames     =7
CPSW_port3.RxOctets         =9982
CPSW_port3.TxGoodFrames     =7
CPSW_port3.TxOctets         =9982
CPSW_port3.Frame128t255     =10
CPSW_port3.NetOctets        =19964
CPSW_port4.RxGoodFrames     =7
CPSW_port4.RxOctets         =9982
CPSW_port4.TxGoodFrames     =7
CPSW_port4.TxOctets         =9982
CPSW_port4.Frame128t255     =10
CPSW_port4.NetOctets        =19964
CPSW_port5.RxGoodFrames     =7
CPSW_port5.RxOctets         =9982
CPSW_port5.TxGoodFrames     =7
CPSW_port5.TxOctets         =9982
CPSW_port5.Frame128t255     =10
CPSW_port5.NetOctets        =19964
CPSW_port6.RxGoodFrames     =7
CPSW_port6.RxOctets         =9982
CPSW_port6.TxGoodFrames     =7
CPSW_port6.TxOctets         =9982
CPSW_port6.Frame128t255     =10
CPSW_port6.NetOctets        =19964
CPSW_port7.RxGoodFrames     =7
CPSW_port7.RxOctets         =9982
CPSW_port7.TxGoodFrames     =7
CPSW_port7.TxOctets         =9982
CPSW_port7.Frame128t255     =10
CPSW_port7.NetOctets        =19964
CPSW_port8.RxGoodFrames     =7
CPSW_port8.RxOctets         =9982
CPSW_port8.TxGoodFrames     =7
CPSW_port8.TxOctets         =9982
CPSW_port8.Frame128t255     =10
CPSW_port8.NetOctets        =19964
Ethernet port 0 TX  4 packets x  128 bytes, RX  4 packets,    74116 cycles,    66 Mbps
Ethernet port 1 TX  4 packets x  128 bytes, RX  4 packets,    78842 cycles,    62 Mbps
Ethernet port 2 TX  4 packets x  128 bytes, RX  4 packets,    80177 cycles,    61 Mbps
Ethernet port 3 TX  4 packets x  128 bytes, RX  4 packets,    73454 cycles,    66 Mbps
Ethernet port 4 TX  4 packets x  128 bytes, RX  4 packets,    79075 cycles,    62 Mbps
Ethernet port 5 TX  4 packets x  128 bytes, RX  4 packets,    78608 cycles,    62 Mbps
Ethernet port 6 TX  4 packets x  128 bytes, RX  4 packets,    74157 cycles,    66 Mbps
Ethernet port 7 TX  4 packets x  128 bytes, RX  4 packets,    73997 cycles,    66 Mbps

CPSW_port0.RxGoodFrames     =88
CPSW_port0.RxOctets         =113200
CPSW_port0.TxGoodFrames     =88
CPSW_port0.TxOctets         =113200
CPSW_port0.Frame1024tUp     =96
CPSW_port0.NetOctets        =226400
CPSW_port1.RxGoodFrames     =11
CPSW_port1.RxOctets         =14150
CPSW_port1.TxGoodFrames     =11
CPSW_port1.TxOctets         =14150
CPSW_port1.Frame1024tUp     =12
CPSW_port1.NetOctets        =28300
CPSW_port2.RxGoodFrames     =11
CPSW_port2.RxOctets         =14150
CPSW_port2.TxGoodFrames     =11
CPSW_port2.TxOctets         =14150
CPSW_port2.Frame1024tUp     =12
CPSW_port2.NetOctets        =28300
CPSW_port3.RxGoodFrames     =11
CPSW_port3.RxOctets         =14150
CPSW_port3.TxGoodFrames     =11
CPSW_port3.TxOctets         =14150
CPSW_port3.Frame1024tUp     =12
CPSW_port3.NetOctets        =28300
CPSW_port4.RxGoodFrames     =11
CPSW_port4.RxOctets         =14150
CPSW_port4.TxGoodFrames     =11
CPSW_port4.TxOctets         =14150
CPSW_port4.Frame1024tUp     =12
CPSW_port4.NetOctets        =28300
CPSW_port5.RxGoodFrames     =11
CPSW_port5.RxOctets         =14150
CPSW_port5.TxGoodFrames     =11
CPSW_port5.TxOctets         =14150
CPSW_port5.Frame1024tUp     =12
CPSW_port5.NetOctets        =28300
CPSW_port6.RxGoodFrames     =11
CPSW_port6.RxOctets         =14150
CPSW_port6.TxGoodFrames     =11
CPSW_port6.TxOctets         =14150
CPSW_port6.Frame1024tUp     =12
CPSW_port6.NetOctets        =28300
CPSW_port7.RxGoodFrames     =11
CPSW_port7.RxOctets         =14150
CPSW_port7.TxGoodFrames     =11
CPSW_port7.TxOctets         =14150
CPSW_port7.Frame1024tUp     =12
CPSW_port7.NetOctets        =28300
CPSW_port8.RxGoodFrames     =11
CPSW_port8.RxOctets         =14150
CPSW_port8.TxGoodFrames     =11
CPSW_port8.TxOctets         =14150
CPSW_port8.Frame1024tUp     =12
CPSW_port8.NetOctets        =28300
Ethernet port 0 TX  4 packets x 1024 bytes, RX  4 packets,    75294 cycles,   522 Mbps
Ethernet port 1 TX  4 packets x 1024 bytes, RX  4 packets,    74830 cycles,   525 Mbps
Ethernet port 2 TX  4 packets x 1024 bytes, RX  4 packets,    78328 cycles,   502 Mbps
Ethernet port 3 TX  4 packets x 1024 bytes, RX  4 packets,    85649 cycles,   459 Mbps
Ethernet port 4 TX  4 packets x 1024 bytes, RX  4 packets,    90313 cycles,   435 Mbps
Ethernet port 5 TX  4 packets x 1024 bytes, RX  4 packets,    89851 cycles,   437 Mbps
Ethernet port 6 TX  4 packets x 1024 bytes, RX  4 packets,    91255 cycles,   430 Mbps
Ethernet port 7 TX  4 packets x 1024 bytes, RX  4 packets,    84512 cycles,   465 Mbps

CPSW_port0.RxGoodFrames     =120
CPSW_port0.RxOctets         =375920
CPSW_port0.TxGoodFrames     =120
CPSW_port0.TxOctets         =375920
CPSW_port0.Frame1024tUp     =160
CPSW_port0.NetOctets        =751840
CPSW_port1.RxGoodFrames     =15
CPSW_port1.RxOctets         =46990
CPSW_port1.TxGoodFrames     =15
CPSW_port1.TxOctets         =46990
CPSW_port1.Frame1024tUp     =20
CPSW_port1.NetOctets        =93980
CPSW_port2.RxGoodFrames     =15
CPSW_port2.RxOctets         =46990
CPSW_port2.TxGoodFrames     =15
CPSW_port2.TxOctets         =46990
CPSW_port2.Frame1024tUp     =20
CPSW_port2.NetOctets        =93980
CPSW_port3.RxGoodFrames     =15
CPSW_port3.RxOctets         =46990
CPSW_port3.TxGoodFrames     =15
CPSW_port3.TxOctets         =46990
CPSW_port3.Frame1024tUp     =20
CPSW_port3.NetOctets        =93980
CPSW_port4.RxGoodFrames     =15
CPSW_port4.RxOctets         =46990
CPSW_port4.TxGoodFrames     =15
CPSW_port4.TxOctets         =46990
CPSW_port4.Frame1024tUp     =20
CPSW_port4.NetOctets        =93980
CPSW_port5.RxGoodFrames     =15
CPSW_port5.RxOctets         =46990
CPSW_port5.TxGoodFrames     =15
CPSW_port5.TxOctets         =46990
CPSW_port5.Frame1024tUp     =20
CPSW_port5.NetOctets        =93980
CPSW_port6.RxGoodFrames     =15
CPSW_port6.RxOctets         =46990
CPSW_port6.TxGoodFrames     =15
CPSW_port6.TxOctets         =46990
CPSW_port6.Frame1024tUp     =20
CPSW_port6.NetOctets        =93980
CPSW_port7.RxGoodFrames     =15
CPSW_port7.RxOctets         =46990
CPSW_port7.TxGoodFrames     =15
CPSW_port7.TxOctets         =46990
CPSW_port7.Frame1024tUp     =20
CPSW_port7.NetOctets        =93980
CPSW_port8.RxGoodFrames     =15
CPSW_port8.RxOctets         =46990
CPSW_port8.TxGoodFrames     =15
CPSW_port8.TxOctets         =46990
CPSW_port8.Frame1024tUp     =20
CPSW_port8.NetOctets        =93980
Ethernet port 0 TX  4 packets x 8192 bytes, RX  4 packets,   333277 cycles,   943 Mbps
Ethernet port 1 TX  4 packets x 8192 bytes, RX  4 packets,   339272 cycles,   927 Mbps
Ethernet port 2 TX  4 packets x 8192 bytes, RX  4 packets,   344817 cycles,   912 Mbps
Ethernet port 3 TX  4 packets x 8192 bytes, RX  4 packets,   350841 cycles,   896 Mbps
Ethernet port 4 TX  4 packets x 8192 bytes, RX  4 packets,   357275 cycles,   880 Mbps
Ethernet port 5 TX  4 packets x 8192 bytes, RX  4 packets,   363317 cycles,   865 Mbps
Ethernet port 6 TX  4 packets x 8192 bytes, RX  4 packets,   369333 cycles,   851 Mbps
Ethernet port 7 TX  4 packets x 8192 bytes, RX  4 packets,   173978 cycles,  1808 Mbps

CPSW_port0.RxGoodFrames     =248
CPSW_port0.RxOctets         =394608
CPSW_port0.TxGoodFrames     =248
CPSW_port0.TxOctets         =394608
CPSW_port0.Frame128t255     =336
CPSW_port0.NetOctets        =789216
CPSW_port1.RxGoodFrames     =31
CPSW_port1.RxOctets         =49326
CPSW_port1.TxGoodFrames     =31
CPSW_port1.TxOctets         =49326
CPSW_port1.Frame128t255     =42
CPSW_port1.NetOctets        =98652
CPSW_port2.RxGoodFrames     =31
CPSW_port2.RxOctets         =49326
CPSW_port2.TxGoodFrames     =31
CPSW_port2.TxOctets         =49326
CPSW_port2.Frame128t255     =42
CPSW_port2.NetOctets        =98652
CPSW_port3.RxGoodFrames     =31
CPSW_port3.RxOctets         =49326
CPSW_port3.TxGoodFrames     =31
CPSW_port3.TxOctets         =49326
CPSW_port3.Frame128t255     =42
CPSW_port3.NetOctets        =98652
CPSW_port4.RxGoodFrames     =31
CPSW_port4.RxOctets         =49326
CPSW_port4.TxGoodFrames     =31
CPSW_port4.TxOctets         =49326
CPSW_port4.Frame128t255     =42
CPSW_port4.NetOctets        =98652
CPSW_port5.RxGoodFrames     =31
CPSW_port5.RxOctets         =49326
CPSW_port5.TxGoodFrames     =31
CPSW_port5.TxOctets         =49326
CPSW_port5.Frame128t255     =42
CPSW_port5.NetOctets        =98652
CPSW_port6.RxGoodFrames     =31
CPSW_port6.RxOctets         =49326
CPSW_port6.TxGoodFrames     =31
CPSW_port6.TxOctets         =49326
CPSW_port6.Frame128t255     =42
CPSW_port6.NetOctets        =98652
CPSW_port7.RxGoodFrames     =31
CPSW_port7.RxOctets         =49326
CPSW_port7.TxGoodFrames     =31
CPSW_port7.TxOctets         =49326
CPSW_port7.Frame128t255     =42
CPSW_port7.NetOctets        =98652
CPSW_port8.RxGoodFrames     =31
CPSW_port8.RxOctets         =49326
CPSW_port8.TxGoodFrames     =31
CPSW_port8.TxOctets         =49326
CPSW_port8.Frame128t255     =42
CPSW_port8.NetOctets        =98652
Ethernet port 0 TX 16 packets x  128 bytes, RX 16 packets,   366628 cycles,    53 Mbps
Ethernet port 1 TX 16 packets x  128 bytes, RX 16 packets,   366169 cycles,    53 Mbps
Ethernet port 2 TX 16 packets x  128 bytes, RX 16 packets,   367088 cycles,    53 Mbps
Ethernet port 3 TX 16 packets x  128 bytes, RX 16 packets,   366008 cycles,    53 Mbps
Ethernet port 4 TX 16 packets x  128 bytes, RX 16 packets,   365935 cycles,    53 Mbps
Ethernet port 5 TX 16 packets x  128 bytes, RX 16 packets,   365460 cycles,    53 Mbps
Ethernet port 6 TX 16 packets x  128 bytes, RX 16 packets,   366396 cycles,    53 Mbps
Ethernet port 7 TX 16 packets x  128 bytes, RX 16 packets,   366239 cycles,    53 Mbps

CPSW_port0.RxGoodFrames     =376
CPSW_port0.RxOctets         =527984
CPSW_port0.TxGoodFrames     =376
CPSW_port0.TxOctets         =527984
CPSW_port0.Frame1024tUp     =416
CPSW_port0.NetOctets        =1055968
CPSW_port1.RxGoodFrames     =47
CPSW_port1.RxOctets         =65998
CPSW_port1.TxGoodFrames     =47
CPSW_port1.TxOctets         =65998
CPSW_port1.Frame1024tUp     =52
CPSW_port1.NetOctets        =131996
CPSW_port2.RxGoodFrames     =47
CPSW_port2.RxOctets         =65998
CPSW_port2.TxGoodFrames     =47
CPSW_port2.TxOctets         =65998
CPSW_port2.Frame1024tUp     =52
CPSW_port2.NetOctets        =131996
CPSW_port3.RxGoodFrames     =47
CPSW_port3.RxOctets         =65998
CPSW_port3.TxGoodFrames     =47
CPSW_port3.TxOctets         =65998
CPSW_port3.Frame1024tUp     =52
CPSW_port3.NetOctets        =131996
CPSW_port4.RxGoodFrames     =47
CPSW_port4.RxOctets         =65998
CPSW_port4.TxGoodFrames     =47
CPSW_port4.TxOctets         =65998
CPSW_port4.Frame1024tUp     =52
CPSW_port4.NetOctets        =131996
CPSW_port5.RxGoodFrames     =47
CPSW_port5.RxOctets         =65998
CPSW_port5.TxGoodFrames     =47
CPSW_port5.TxOctets         =65998
CPSW_port5.Frame1024tUp     =52
CPSW_port5.NetOctets        =131996
CPSW_port6.RxGoodFrames     =47
CPSW_port6.RxOctets         =65998
CPSW_port6.TxGoodFrames     =47
CPSW_port6.TxOctets         =65998
CPSW_port6.Frame1024tUp     =52
CPSW_port6.NetOctets        =131996
CPSW_port7.RxGoodFrames     =47
CPSW_port7.RxOctets         =65998
CPSW_port7.TxGoodFrames     =47
CPSW_port7.TxOctets         =65998
CPSW_port7.Frame1024tUp     =52
CPSW_port7.NetOctets        =131996
CPSW_port8.RxGoodFrames     =47
CPSW_port8.RxOctets         =65998
CPSW_port8.TxGoodFrames     =47
CPSW_port8.TxOctets         =65998
CPSW_port8.Frame1024tUp     =52
CPSW_port8.NetOctets        =131996
Ethernet port 0 TX 16 packets x 1024 bytes, RX 16 packets,   342109 cycles,   459 Mbps
Ethernet port 1 TX 16 packets x 1024 bytes, RX 16 packets,   343915 cycles,   457 Mbps
Ethernet port 2 TX 16 packets x 1024 bytes, RX 16 packets,   346451 cycles,   453 Mbps
Ethernet port 3 TX 16 packets x 1024 bytes, RX 16 packets,   348206 cycles,   451 Mbps
Ethernet port 4 TX 16 packets x 1024 bytes, RX 16 packets,   350138 cycles,   449 Mbps
Ethernet port 5 TX 16 packets x 1024 bytes, RX 16 packets,   349803 cycles,   449 Mbps
Ethernet port 6 TX 16 packets x 1024 bytes, RX 16 packets,   349475 cycles,   450 Mbps
Ethernet port 7 TX 16 packets x 1024 bytes, RX 16 packets,   344588 cycles,   456 Mbps

CPSW_port0.RxGoodFrames     =504
CPSW_port0.RxOctets         =1578864
CPSW_port0.TxGoodFrames     =504
CPSW_port0.TxOctets         =1578864
CPSW_port0.Frame1024tUp     =672
CPSW_port0.NetOctets        =3157728
CPSW_port1.RxGoodFrames     =63
CPSW_port1.RxOctets         =197358
CPSW_port1.TxGoodFrames     =63
CPSW_port1.TxOctets         =197358
CPSW_port1.Frame1024tUp     =84
CPSW_port1.NetOctets        =394716
CPSW_port2.RxGoodFrames     =63
CPSW_port2.RxOctets         =197358
CPSW_port2.TxGoodFrames     =63
CPSW_port2.TxOctets         =197358
CPSW_port2.Frame1024tUp     =84
CPSW_port2.NetOctets        =394716
CPSW_port3.RxGoodFrames     =63
CPSW_port3.RxOctets         =197358
CPSW_port3.TxGoodFrames     =63
CPSW_port3.TxOctets         =197358
CPSW_port3.Frame1024tUp     =84
CPSW_port3.NetOctets        =394716
CPSW_port4.RxGoodFrames     =63
CPSW_port4.RxOctets         =197358
CPSW_port4.TxGoodFrames     =63
CPSW_port4.TxOctets         =197358
CPSW_port4.Frame1024tUp     =84
CPSW_port4.NetOctets        =394716
CPSW_port5.RxGoodFrames     =63
CPSW_port5.RxOctets         =197358
CPSW_port5.TxGoodFrames     =63
CPSW_port5.TxOctets         =197358
CPSW_port5.Frame1024tUp     =84
CPSW_port5.NetOctets        =394716
CPSW_port6.RxGoodFrames     =63
CPSW_port6.RxOctets         =197358
CPSW_port6.TxGoodFrames     =63
CPSW_port6.TxOctets         =197358
CPSW_port6.Frame1024tUp     =84
CPSW_port6.NetOctets        =394716
CPSW_port7.RxGoodFrames     =63
CPSW_port7.RxOctets         =197358
CPSW_port7.TxGoodFrames     =63
CPSW_port7.TxOctets         =197358
CPSW_port7.Frame1024tUp     =84
CPSW_port7.NetOctets        =394716
CPSW_port8.RxGoodFrames     =63
CPSW_port8.RxOctets         =197358
CPSW_port8.TxGoodFrames     =63
CPSW_port8.TxOctets         =197358
CPSW_port8.Frame1024tUp     =84
CPSW_port8.NetOctets        =394716
Ethernet port 0 TX 16 packets x 8192 bytes, RX 16 packets,  1281494 cycles,   981 Mbps
Ethernet port 1 TX 16 packets x 8192 bytes, RX 16 packets,  1287594 cycles,   977 Mbps
Ethernet port 2 TX 16 packets x 8192 bytes, RX 16 packets,  1293738 cycles,   972 Mbps
Ethernet port 3 TX 16 packets x 8192 bytes, RX 16 packets,  1299906 cycles,   967 Mbps
Ethernet port 4 TX 16 packets x 8192 bytes, RX 16 packets,  1306072 cycles,   963 Mbps
Ethernet port 5 TX 16 packets x 8192 bytes, RX 16 packets,  1312252 cycles,   958 Mbps
Ethernet port 6 TX 16 packets x 8192 bytes, RX 16 packets,  1318482 cycles,   954 Mbps
Ethernet port 7 TX 16 packets x 8192 bytes, RX 16 packets,   621042 cycles,  2026 Mbps

GE test complete.

