Core Registers		Core Registers	
	PC	0x00000000808BA010	Program Counter [Core]	
	SP	0x0000000080477980	Stack Pointer [Core]	
	LR	0x00000000808BA010	Link Register [Core]	
	PC	0x00000000808BA010	Program Counter [Core]	
	SP	0x0000000080477980	Stack Pointer [Core]	
	DSPSR_EL0	0x200003C9	Saved PSTATE [Core]	
		N	0	Sign bit of result	
		Z	0	1 if result is zero, 0 otherwise	
		C	1	Carry/borrow bit of operation	
		V	0	Set to 1 if operation overflowed	
		Q	0	Cumulative saturation bit (AARCH32 only)	
		IT_10	00	Bits 1:0 of If-Then state (AARCH32 only)	
		J	0	Jazelle state - obsolete in ARMv8	
		RES0	00	Reserved 0	
		SS	0	Software step enabled	
		IL	0	Illegal execution state	
		GE	0000	Greater than or Equal flags for parallel add/sub (AARCH32 only)	
		IT_72	000000	Bits 7:2 of If-Then state (AARCH32 only)	
		E	1	Endian bit (0 little, 1 big) (AARCH32 only)	
		A	1	Asynchronous data abort mask bit	
		I	1	IRQ mask bit	
		F	1	FIQ mask bit	
		T	0	Thumb execution state bit	
		M4	0	Register width exception was taken from (1=AARCH32)	
		M30	1001	Mode exception was taken from	
	LR	0x00000000808BA010	General Purpose Register 30 [Core]	
	X0	0x0000000080903F80	64 Bit General Purpose Register 0 [Core]	
	X1	0x0000000080903F80	64 Bit General Purpose Register 1 [Core]	
	X2	0x00000000808F67AA	64 Bit General Purpose Register 2 [Core]	
	X3	0x0000000000000000	64 Bit General Purpose Register 3 [Core]	
	X4	0x00000000804774A0	64 Bit General Purpose Register 4 [Core]	
	X5	0x0000000000000077	64 Bit General Purpose Register 5 [Core]	
	X6	0x0000000000000000	64 Bit General Purpose Register 6 [Core]	
	X7	0x0000000080477990	64 Bit General Purpose Register 7 [Core]	
	X8	0x0000000000000001	64 Bit General Purpose Register 8 [Core]	
	X9	0x00000000FFFFFFD0	64 Bit General Purpose Register 9 [Core]	
	X10	0x000000000000000D	64 Bit General Purpose Register 10 [Core]	
	X11	0x0000000000000006	64 Bit General Purpose Register 11 [Core]	
	X12	0x0000000000000000	64 Bit General Purpose Register 12 [Core]	
	X13	0x0000000080948170	64 Bit General Purpose Register 13 [Core]	
	X14	0x0000000000000008	64 Bit General Purpose Register 14 [Core]	
	X15	0x0000000080477579	64 Bit General Purpose Register 15 [Core]	
	X16	0x0000000080870260	64 Bit General Purpose Register 16 [Core]	
	X17	0x0000000000000000	64 Bit General Purpose Register 17 [Core]	
	X18	0x0000000080477EA0	64 Bit General Purpose Register 18 [Core]	
	X19	0x0000000000000001	64 Bit General Purpose Register 19 [Core]	
	X20	0x0000000000000000	64 Bit General Purpose Register 20 [Core]	
	X21	0x0000000000000008	64 Bit General Purpose Register 21 [Core]	
	X22	0x00000000808F4F60	64 Bit General Purpose Register 22 [Core]	
	X23	0x0000000080948170	64 Bit General Purpose Register 23 [Core]	
	X24	0x0000000000000000	64 Bit General Purpose Register 24 [Core]	
	X25	0x0000000080950F14	64 Bit General Purpose Register 25 [Core]	
	X26	0x0000000000000005	64 Bit General Purpose Register 26 [Core]	
	X27	0x0000000000000000	64 Bit General Purpose Register 27 [Core]	
	X28	0x0000000000000A48	64 Bit General Purpose Register 28 [Core]	
	X29	0x0000000080477980	64 Bit General Purpose Register 29 [Core]	
	X30	0x00000000808BA010	64 Bit General Purpose Register 30 [Core]	
A64 Core Registers		AArch64 Core Registers	
	PC	0x00000000808BA010	Program Counter [Core]	
	SP	0x0000000080477980	Stack Pointer [Core]	
	DSPSR_EL0	0x200003C9	Saved PSTATE [Core]	
		N	0	Sign bit of result	
		Z	0	1 if result is zero, 0 otherwise	
		C	1	Carry/borrow bit of operation	
		V	0	Set to 1 if operation overflowed	
		Q	0	Cumulative saturation bit (AARCH32 only)	
		IT_10	00	Bits 1:0 of If-Then state (AARCH32 only)	
		J	0	Jazelle state - obsolete in ARMv8	
		RES0	00	Reserved 0	
		SS	0	Software step enabled	
		IL	0	Illegal execution state	
		GE	0000	Greater than or Equal flags for parallel add/sub (AARCH32 only)	
		IT_72	000000	Bits 7:2 of If-Then state (AARCH32 only)	
		E	1	Endian bit (0 little, 1 big) (AARCH32 only)	
		A	1	Asynchronous data abort mask bit	
		I	1	IRQ mask bit	
		F	1	FIQ mask bit	
		T	0	Thumb execution state bit	
		M4	0	Register width exception was taken from (1=AARCH32)	
		M30	1001	Mode exception was taken from	
	LR	0x00000000808BA010	General Purpose Register 30 [Core]	
	X0	0x0000000080903F80	64 Bit General Purpose Register 0 [Core]	
	X1	0x0000000080903F80	64 Bit General Purpose Register 1 [Core]	
	X2	0x00000000808F67AA	64 Bit General Purpose Register 2 [Core]	
	X3	0x0000000000000000	64 Bit General Purpose Register 3 [Core]	
	X4	0x00000000804774A0	64 Bit General Purpose Register 4 [Core]	
	X5	0x0000000000000077	64 Bit General Purpose Register 5 [Core]	
	X6	0x0000000000000000	64 Bit General Purpose Register 6 [Core]	
	X7	0x0000000080477990	64 Bit General Purpose Register 7 [Core]	
	X8	0x0000000000000001	64 Bit General Purpose Register 8 [Core]	
	X9	0x00000000FFFFFFD0	64 Bit General Purpose Register 9 [Core]	
	X10	0x000000000000000D	64 Bit General Purpose Register 10 [Core]	
	X11	0x0000000000000006	64 Bit General Purpose Register 11 [Core]	
	X12	0x0000000000000000	64 Bit General Purpose Register 12 [Core]	
	X13	0x0000000080948170	64 Bit General Purpose Register 13 [Core]	
	X14	0x0000000000000008	64 Bit General Purpose Register 14 [Core]	
	X15	0x0000000080477579	64 Bit General Purpose Register 15 [Core]	
	X16	0x0000000080870260	64 Bit General Purpose Register 16 [Core]	
	X17	0x0000000000000000	64 Bit General Purpose Register 17 [Core]	
	X18	0x0000000080477EA0	64 Bit General Purpose Register 18 [Core]	
	X19	0x0000000000000001	64 Bit General Purpose Register 19 [Core]	
	X20	0x0000000000000000	64 Bit General Purpose Register 20 [Core]	
	X21	0x0000000000000008	64 Bit General Purpose Register 21 [Core]	
	X22	0x00000000808F4F60	64 Bit General Purpose Register 22 [Core]	
	X23	0x0000000080948170	64 Bit General Purpose Register 23 [Core]	
	X24	0x0000000000000000	64 Bit General Purpose Register 24 [Core]	
	X25	0x0000000080950F14	64 Bit General Purpose Register 25 [Core]	
	X26	0x0000000000000005	64 Bit General Purpose Register 26 [Core]	
	X27	0x0000000000000000	64 Bit General Purpose Register 27 [Core]	
	X28	0x0000000000000A48	64 Bit General Purpose Register 28 [Core]	
	X29	0x0000000080477980	64 Bit General Purpose Register 29 [Core]	
	X30	0x00000000808BA010	64 Bit General Purpose Register 30 [Core]	
A32 Core Registers		AArch32 Core Registers	

Core Registers		Core Registers
	PC	0x00000000808BA010	Program Counter [Core]
	SP	0x0000000080477980	Stack Pointer [Core]
	LR	0x00000000808BA010	Link Register [Core]
	PC	0x00000000808BA010	Program Counter [Core]
	SP	0x0000000080477980	Stack Pointer [Core]
	DSPSR_EL0	0x200003C9	Saved PSTATE [Core]
		N	0	Sign bit of result
		Z	0	1 if result is zero, 0 otherwise
		C	1	Carry/borrow bit of operation
		V	0	Set to 1 if operation overflowed
		Q	0	Cumulative saturation bit (AARCH32 only)
		IT_10	00	Bits 1:0 of If-Then state (AARCH32 only)
		J	0	Jazelle state - obsolete in ARMv8
		RES0	00	Reserved 0
		SS	0	Software step enabled
		IL	0	Illegal execution state
		GE	0000	Greater than or Equal flags for parallel add/sub (AARCH32 only)
		IT_72	000000	Bits 7:2 of If-Then state (AARCH32 only)
		E	1	Endian bit (0 little, 1 big) (AARCH32 only)
		A	1	Asynchronous data abort mask bit
		I	1	IRQ mask bit
		F	1	FIQ mask bit
		T	0	Thumb execution state bit
		M4	0	Register width exception was taken from (1=AARCH32)
		M30	1001	Mode exception was taken from
	LR	0x00000000808BA010	General Purpose Register 30 [Core]
	X0	0x0000000080903F80	64 Bit General Purpose Register 0 [Core]
	X1	0x0000000080903F80	64 Bit General Purpose Register 1 [Core]
	X2	0x00000000808F67AA	64 Bit General Purpose Register 2 [Core]
	X3	0x0000000000000000	64 Bit General Purpose Register 3 [Core]
	X4	0x00000000804774A0	64 Bit General Purpose Register 4 [Core]
	X5	0x0000000000000077	64 Bit General Purpose Register 5 [Core]
	X6	0x0000000000000000	64 Bit General Purpose Register 6 [Core]
	X7	0x0000000080477990	64 Bit General Purpose Register 7 [Core]
	X8	0x0000000000000001	64 Bit General Purpose Register 8 [Core]
	X9	0x00000000FFFFFFD0	64 Bit General Purpose Register 9 [Core]
	X10	0x000000000000000D	64 Bit General Purpose Register 10 [Core]
	X11	0x0000000000000006	64 Bit General Purpose Register 11 [Core]
	X12	0x0000000000000000	64 Bit General Purpose Register 12 [Core]
	X13	0x0000000080948170	64 Bit General Purpose Register 13 [Core]
	X14	0x0000000000000008	64 Bit General Purpose Register 14 [Core]
	X15	0x0000000080477579	64 Bit General Purpose Register 15 [Core]
	X16	0x0000000080870260	64 Bit General Purpose Register 16 [Core]
	X17	0x0000000000000000	64 Bit General Purpose Register 17 [Core]
	X18	0x0000000080477EA0	64 Bit General Purpose Register 18 [Core]
	X19	0x0000000000000001	64 Bit General Purpose Register 19 [Core]
	X20	0x0000000000000000	64 Bit General Purpose Register 20 [Core]
	X21	0x0000000000000008	64 Bit General Purpose Register 21 [Core]
	X22	0x00000000808F4F60	64 Bit General Purpose Register 22 [Core]
	X23	0x0000000080948170	64 Bit General Purpose Register 23 [Core]
	X24	0x0000000000000000	64 Bit General Purpose Register 24 [Core]
	X25	0x0000000080950F14	64 Bit General Purpose Register 25 [Core]
	X26	0x0000000000000005	64 Bit General Purpose Register 26 [Core]
	X27	0x0000000000000000	64 Bit General Purpose Register 27 [Core]
	X28	0x0000000000000A48	64 Bit General Purpose Register 28 [Core]
	X29	0x0000000080477980	64 Bit General Purpose Register 29 [Core]
	X30	0x00000000808BA010	64 Bit General Purpose Register 30 [Core]
A64 Core Registers		AArch64 Core Registers
	PC	0x00000000808BA010	Program Counter [Core]
	SP	0x0000000080477980	Stack Pointer [Core]
	DSPSR_EL0	0x200003C9	Saved PSTATE [Core]
		N	0	Sign bit of result
		Z	0	1 if result is zero, 0 otherwise
		C	1	Carry/borrow bit of operation
		V	0	Set to 1 if operation overflowed
		Q	0	Cumulative saturation bit (AARCH32 only)
		IT_10	00	Bits 1:0 of If-Then state (AARCH32 only)
		J	0	Jazelle state - obsolete in ARMv8
		RES0	00	Reserved 0
		SS	0	Software step enabled
		IL	0	Illegal execution state
		GE	0000	Greater than or Equal flags for parallel add/sub (AARCH32 only)
		IT_72	000000	Bits 7:2 of If-Then state (AARCH32 only)
		E	1	Endian bit (0 little, 1 big) (AARCH32 only)
		A	1	Asynchronous data abort mask bit
		I	1	IRQ mask bit
		F	1	FIQ mask bit
		T	0	Thumb execution state bit
		M4	0	Register width exception was taken from (1=AARCH32)
		M30	1001	Mode exception was taken from
	LR	0x00000000808BA010	General Purpose Register 30 [Core]
	X0	0x0000000080903F80	64 Bit General Purpose Register 0 [Core]
	X1	0x0000000080903F80	64 Bit General Purpose Register 1 [Core]
	X2	0x00000000808F67AA	64 Bit General Purpose Register 2 [Core]
	X3	0x0000000000000000	64 Bit General Purpose Register 3 [Core]
	X4	0x00000000804774A0	64 Bit General Purpose Register 4 [Core]
	X5	0x0000000000000077	64 Bit General Purpose Register 5 [Core]
	X6	0x0000000000000000	64 Bit General Purpose Register 6 [Core]
	X7	0x0000000080477990	64 Bit General Purpose Register 7 [Core]
	X8	0x0000000000000001	64 Bit General Purpose Register 8 [Core]
	X9	0x00000000FFFFFFD0	64 Bit General Purpose Register 9 [Core]
	X10	0x000000000000000D	64 Bit General Purpose Register 10 [Core]
	X11	0x0000000000000006	64 Bit General Purpose Register 11 [Core]
	X12	0x0000000000000000	64 Bit General Purpose Register 12 [Core]
	X13	0x0000000080948170	64 Bit General Purpose Register 13 [Core]
	X14	0x0000000000000008	64 Bit General Purpose Register 14 [Core]
	X15	0x0000000080477579	64 Bit General Purpose Register 15 [Core]
	X16	0x0000000080870260	64 Bit General Purpose Register 16 [Core]
	X17	0x0000000000000000	64 Bit General Purpose Register 17 [Core]
	X18	0x0000000080477EA0	64 Bit General Purpose Register 18 [Core]
	X19	0x0000000000000001	64 Bit General Purpose Register 19 [Core]
	X20	0x0000000000000000	64 Bit General Purpose Register 20 [Core]
	X21	0x0000000000000008	64 Bit General Purpose Register 21 [Core]
	X22	0x00000000808F4F60	64 Bit General Purpose Register 22 [Core]
	X23	0x0000000080948170	64 Bit General Purpose Register 23 [Core]
	X24	0x0000000000000000	64 Bit General Purpose Register 24 [Core]
	X25	0x0000000080950F14	64 Bit General Purpose Register 25 [Core]
	X26	0x0000000000000005	64 Bit General Purpose Register 26 [Core]
	X27	0x0000000000000000	64 Bit General Purpose Register 27 [Core]
	X28	0x0000000000000A48	64 Bit General Purpose Register 28 [Core]
	X29	0x0000000080477980	64 Bit General Purpose Register 29 [Core]
	X30	0x00000000808BA010	64 Bit General Purpose Register 30 [Core]
A32 Core Registers		AArch32 Core Registers

AMAIR_EL1	0x0000000000000000	Auxiliary Memory Attribute Indirection Register (EL1) [Core]
AMAIR_EL2	0x0000000000000000	Auxiliary Memory Attribute Indirection Register (EL2) [Core]
AMAIR_EL3	0x0000000000000000	Auxiliary Memory Attribute Indirection Register (EL3) [Core]
CBAR_EL1	0x000000006F000000	Configuration Base Address Register [Core]
CCSIDR_EL1	0x201FE012	Current Cache Size ID Register [Core]
CLIDR_EL1	0x0A200023	Cache Level ID Register [Core]
CONTEXTIDR_EL1	0x00000000	Context ID Register [Core]
CPACR_EL1	0x00000000	Architectural Feature Access Control Register [Core]
CPTR_EL2	0x000033FF	Architectural Feature Trap Register (EL2) [Core]
CPTR_EL3	0x00000000	Architectural Feature Trap Register (EL3) [Core]
CPUACTLR_EL1	0x0000000000004010	CPU Auxiliary Control Register [Core]
CPUECTLR_EL1	0x0000001B00000040	CPU Extended Control Register [Core]
CPUMERRSR_EL1	0x0000000000000000	CPU Memory Error Syndrome Register [Core]
CSSELR_EL1	0x00000001	Cache Size Selection Register [Core]
CTR_EL0	0x8444C004	Cache Type Register [Core]
DACR32_EL2	0x00000000	Domain Access Control Register [Core]
DCZID_EL0	0x00000004	Data Cache Zero ID Register [Core]
ESR_EL1	0x00000000	Exception Syndrome Register (EL1) [Core]
ESR_EL2	0x02000000	Exception Syndrome Register (EL2) [Core]
ESR_EL3	0x5E000000	Exception Syndrome Register (EL3) [Core]
FAR_EL1	0x0000000000000000	Fault Address Register (EL1) [Core]
FAR_EL2	0x0000000000000000	Fault Address Register (EL2) [Core]
FAR_EL3	0x0000000000000000	Fault Address Register (EL3) [Core]
FPEXC32_EL2	0x00000700	Floating-point Exception Control Register [Core]
HACR_EL2	0x00000000	Hypervisor Auxiliary Control Register [Core]
HCR_EL2	0x0000000000000020	Hypervisor Configuration Register [Core]
HPFAR_EL2	0x0000000000000000	Hypervisor IPA Fault Address Register [Core]
HSTR_EL2	0x00000000	Hypervisor System Trap Register [Core]
ID_AA64AFR0_EL1	0x0000000000000000	AArch64 Auxiliary Feature Register 0 [Core]
ID_AA64AFR1_EL1	0x0000000000000000	AArch64 Auxiliary Feature Register 1 [Core]
ID_AA64DFR0_EL1	0x0000000010305106	AArch64 Debug Feature Register 0 [Core]
ID_AA64DFR1_EL1	0x0000000000000000	AArch64 Debug Feature Register 1 [Core]
ID_AA64ISAR0_EL1	0x0000000000011120	AArch64 Instruction Set Attribute Register 0 [Core]
ID_AA64ISAR1_EL1	0x0000000000000000	AArch64 Instruction Set Attribute Register 1 [Core]
ID_AA64MMFR0_EL1	0x0000000000001124	AArch64 Memory Model Feature Register 0 [Core]



System Registers		System Registers
	[0 ... 99]
		ACTLR_EL1	0x00000000	Auxiliary Control Register (EL1) [Core]
		ACTLR_EL2	0x00000000	Auxiliary Control Register (EL2) [Core]
		ACTLR_EL3	0x00000000	Auxiliary Control Register (EL3) [Core]
		AFSR0_EL1	0x00000000	Auxiliary Fault Status Register 0 (EL1) [Core]
		AFSR0_EL2	0x00000000	Auxiliary Fault Status Register 0 (EL2) [Core]
		AFSR0_EL3	0x00000000	Auxiliary Fault Status Register 0 (EL3) [Core]
		AFSR1_EL1	0x00000000	Auxiliary Fault Status Register 0 (EL1) [Core]
		AFSR1_EL2	0x00000000	Auxiliary Fault Status Register 0 (EL2) [Core]
		AFSR1_EL3	0x00000000	Auxiliary Fault Status Register 0 (EL3) [Core]
		AIDR_EL1	0x00000000	Auxiliary ID register [Core]
		AMAIR_EL1	0x0000000000000000	Auxiliary Memory Attribute Indirection Register (EL1) [Core]
		AMAIR_EL2	0x0000000000000000	Auxiliary Memory Attribute Indirection Register (EL2) [Core]
		AMAIR_EL3	0x0000000000000000	Auxiliary Memory Attribute Indirection Register (EL3) [Core]
		CBAR_EL1	0x000000006F000000	Configuration Base Address Register [Core]
		CCSIDR_EL1	0x201FE012	Current Cache Size ID Register [Core]
		CLIDR_EL1	0x0A200023	Cache Level ID Register [Core]
		CONTEXTIDR_EL1	0x00000000	Context ID Register [Core]
		CPACR_EL1	0x00000000	Architectural Feature Access Control Register [Core]
		CPTR_EL2	0x000033FF	Architectural Feature Trap Register (EL2) [Core]
		CPTR_EL3	0x00000000	Architectural Feature Trap Register (EL3) [Core]
		CPUACTLR_EL1	0x0000000000004010	CPU Auxiliary Control Register [Core]
		CPUECTLR_EL1	0x0000001B00000040	CPU Extended Control Register [Core]
		CPUMERRSR_EL1	0x0000000000000000	CPU Memory Error Syndrome Register [Core]
		CSSELR_EL1	0x00000001	Cache Size Selection Register [Core]
		CTR_EL0	0x8444C004	Cache Type Register [Core]
		DACR32_EL2	0x00000000	Domain Access Control Register [Core]
		DCZID_EL0	0x00000004	Data Cache Zero ID Register [Core]
		ESR_EL1	0x00000000	Exception Syndrome Register (EL1) [Core]
		ESR_EL2	0x02000000	Exception Syndrome Register (EL2) [Core]
		ESR_EL3	0x5E000000	Exception Syndrome Register (EL3) [Core]
		FAR_EL1	0x0000000000000000	Fault Address Register (EL1) [Core]
		FAR_EL2	0x0000000000000000	Fault Address Register (EL2) [Core]
		FAR_EL3	0x0000000000000000	Fault Address Register (EL3) [Core]
		FPEXC32_EL2	0x00000700	Floating-point Exception Control Register [Core]
		HACR_EL2	0x00000000	Hypervisor Auxiliary Control Register [Core]
		HCR_EL2	0x0000000000000020	Hypervisor Configuration Register [Core]
		HPFAR_EL2	0x0000000000000000	Hypervisor IPA Fault Address Register [Core]
		HSTR_EL2	0x00000000	Hypervisor System Trap Register [Core]
		ID_AA64AFR0_EL1	0x0000000000000000	AArch64 Auxiliary Feature Register 0 [Core]
		ID_AA64AFR1_EL1	0x0000000000000000	AArch64 Auxiliary Feature Register 1 [Core]
		ID_AA64DFR0_EL1	0x0000000010305106	AArch64 Debug Feature Register 0 [Core]
		ID_AA64DFR1_EL1	0x0000000000000000	AArch64 Debug Feature Register 1 [Core]
		ID_AA64ISAR0_EL1	0x0000000000011120	AArch64 Instruction Set Attribute Register 0 [Core]
		ID_AA64ISAR1_EL1	0x0000000000000000	AArch64 Instruction Set Attribute Register 1 [Core]
		ID_AA64MMFR0_EL1	0x0000000000001124	AArch64 Memory Model Feature Register 0 [Core]
		ID_AA64MMFR1_EL1	0x0000000000000000	AArch64 Memory Model Feature Register 1 [Core]
		ID_AA64PFR0_EL1	0x1100000001002222	AArch64 Processor Feature Register 0 [Core]
		ID_AA64PFR1_EL1	0x0000000000000000	AArch64 Processor Feature Register 1 [Core]
		ID_AFR0_EL1	0x00000000	AArch32 Auxiliary Feature Register 0 [Core]
		ID_DFR0_EL1	0x03010066	AArch32 Debug Feature Register 0 [Core]
		ID_ISAR0_EL1	0x02101110	AArch32 Instruction Set Attribute Register 0 [Core]
		ID_ISAR1_EL1	0x13112111	AArch32 Instruction Set Attribute Register 1 [Core]
		ID_ISAR2_EL1	0x21232042	AArch32 Instruction Set Attribute Register 2 [Core]
		ID_ISAR3_EL1	0x01112131	AArch32 Instruction Set Attribute Register 3 [Core]
		ID_ISAR4_EL1	0x00011142	AArch32 Instruction Set Attribute Register 4 [Core]
		ID_ISAR5_EL1	0x00011121	AArch32 Instruction Set Attribute Register 5 [Core]
		ID_MMFR0_EL1	0x10201105	AArch32 Memory Model Feature Register 0 [Core]
		ID_MMFR1_EL1	0x40000000	AArch32 Memory Model Feature Register 1 [Core]
		ID_MMFR2_EL1	0x01260000	AArch32 Memory Model Feature Register 2 [Core]
		ID_MMFR3_EL1	0x02102211	AArch32 Memory Model Feature Register 3 [Core]
		ID_PFR0_EL1	0x00010131	AArch32 Processor Feature Register 0 [Core]
		ID_PFR1_EL1	0x10011011	AArch32 Processor Feature Register 1 [Core]
		IFSR32_EL2	0x00000000	Instruction Fault Status Register (EL2) [Core]
		ISR_EL1	0x00000100	Interrupt Status Register [Core]
		L2CTLR_EL1	0x03F03403	L2 Control Register [Core]
		L2ACTLR_EL1	0x00004010	L2 Auxiliary Control Register [Core]
		L2ECTLR_EL1	0x00000000	L2 Extended Control Register [Core]
		L2MERRSR_EL1	0x0000000000000000	L2 Memory Error Syndrome Register [Core]
		MAIR_EL1	0x0000000000000000	Memory Attribute Indirection Register (EL1) [Core]
		MAIR_EL2	0x000000FF440C0400	Memory Attribute Indirection Register (EL2) [Core]
		MAIR_EL3	0x00000000004400FF	Memory Attribute Indirection Register (EL3) [Core]
		MIDR_EL1	0x411FD080	Main ID Register [Core]
		MPIDR_EL1	0x0000000080000000	Multiprocessor Affinity Register [Core]
		MVFR0_EL1	0x10110222	Media and VFP Feature Register 0 [Core]
		MVFR1_EL1	0x12111111	Media and VFP Feature Register 1 [Core]
		MVFR2_EL1	0x00000043	Media and VFP Feature Register 2 [Core]
		PAR_EL1	0x0000000000000000	Physical Address Register [Core]
		REVIDR_EL1	0x00000000	Revision ID Register [Core]
		RMR_EL3	0x00000001	Reset Management Register [Core]
		RVBAR_EL3	0x0000000070000000	Reset Vector Base Address Register [Core]
		SCR_EL3	0x00000735	Secure Configuration Register [Core]
		SCTLR_EL1	0x30D00800	System Control Register (EL1) [Core]
		SCTLR_EL2	0x30C51830	System Control Register (EL2) [Core]
		SCTLR_EL3	0x30CD183F	System Control Register (EL3) [Core]
		TCR_EL1	0x0000000000000000	Translation Control Register (EL1) [Core]
		TCR_EL2	0x8081351C	Translation Control Register (EL2) [Core]
		TCR_EL3	0x0000000080803520	Translation Control Register (EL3) [Core]
		TPIDR_EL0	0x0000000000000000	Thread Pointer/ID Register (EL0) [Core]
		TPIDR_EL1	0x0000000000000000	Thread Pointer/ID Register (EL1) [Core]
		TPIDR_EL2	0x0000000000000000	Thread Pointer/ID Register (EL2) [Core]
		TPIDR_EL3	0x0000000070010D40	Thread Pointer/ID Register (EL3) [Core]
		TPIDRR0_EL0	0x0000000000000000	Thread Pointer/ID Register Read-Only (EL0) [Core]
		TTBR0_EL1	0x0000000000000000	Translation Table Base Register 0 (EL1) [Core]
		TTBR0_EL2	0x00000000FFFF0000	Translation Table Base Register 0 (EL2) [Core]
		TTBR0_EL3	0x0000000070016900	Translation Table Base Register 0 (EL3) [Core]
		TTBR1_EL1	0x0000000000000000	Translation Table Base Register 1 (EL1) [Core]
		VBAR_EL1	0x0000000000000000	Vector Base Address Register (EL1) [Core]
		VBAR_EL2	0x0000000080802000	Vector Base Address Register (EL2) [Core]
		VBAR_EL3	0x0000000070009000	Vector Base Address Register (EL3) [Core]
		VMPIDR_EL2	0x0000000080000000	Virtualization Multiprocessor ID Register [Core]
	[100 ... 102]
		VPIDR_EL2	0x411FD080	Virtualization Processor ID Register [Core]
		VTCR_EL2	0x80000000	Virtualization Translation Control Register [Core]
		VTTBR_EL2	0x0000000000000000	Virtualization Translation Table Base Register [Core]

0x0000000002980000	68045100	00000000	00000000	00000000	00000000	00000000	00000000	00000000
0x0000000002980020	0FF18253	00000000	00000000	00000000	00000000	23456677	23456677	23456677
0x0000000002980040	00000000	00000000	00000000	00000000	00112345	00112345	00112345	00000020
0x0000000002980060	00000000	00000000	002000FF	004003FF	00000000	00000000	00000000	00000000
0x0000000002980080	00000000	00000000	00000000	00000000	00000000	00000000	00000000	00FFFFFF
0x00000000029800A0	00000000	00000000	00000000	00000000	00000000	00000000	00000000	00000000
0x00000000029800C0	00000000	00000000	00000000	00000000	00000000	00000000	00000000	00000000
0x00000000029800E0	00000000	00000000	00000000	00000000	00000000	00000000	00000000	00000000
0x0000000002980100	03020100	7260356E	493156FF	00000000	583746DE	00000000	00000000	00000000
0x0000000002980120	00000000	00000000	00000000	00000000	0007FFFF	00000000	0007FFFF	00000000
0x0000000002980140	0007FFFF	00000000	00000000	00000000	00000000	00000000	00000000	00000000
0x0000000002980160	00000000	00000000	00000000	00000000	00000000	00000000	00000000	00000000
0x0000000002980180	00000000	FFFFFFC0	00010000	02BF0000	00000000	00000000	00000000	00000000
0x00000000029801A0	FF003FFF	FFFFFFFF	0000000F	00000000	00000000	00000000	00000000	00000000
0x00000000029801C0	00000000	00000000	00000000	00000000	00000000	00000000	00000000	00000000
0x00000000029801E0	00000000	00000000	00000000	00000000	00000000	00000000	00000000	00000000
