- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_RtcAlarm Struct Reference
RTC Data Structures

RTC Alarm Time Structure. Contains the field of hour, minute, second and milli second for Alarm time. More...

`#include <csl_rtc.h>`

## Data Fields
Uint16 | year
Uint16 | month
Uint16 | day
Uint16 | hours
Uint16 | mins
Uint16 | secs
Uint16 | mSecs

## Detailed Description

RTC Alarm Time Structure. Contains the field of hour, minute, second and milli second for Alarm time.

## Field Documentation

Uint16 CSL_RtcAlarm::day

Day Alarm field value between 1 - 31

Uint16 CSL_RtcAlarm::hours

Hour Alarm field value between 0 - 23

Uint16 CSL_RtcAlarm::mins

Minute Alarm field value between 0 - 59

Uint16 CSL_RtcAlarm::month

Month Alarm field value between 1 - 12

Uint16 CSL_RtcAlarm::mSecs

MSecond Alarm field value between 0 - 1023

Uint16 CSL_RtcAlarm::secs

Second Alarm field value between 0 - 59

Uint16 CSL_RtcAlarm::year

Year Alarm field value between 0 - 99

The documentation for this struct was generated from the following file:

- csl_rtc.h