- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_UartIsrAddr Struct Reference
UART Data Structures

UART callback pointer structure. More...

`#include <csl_uart.h>`

## Data Fields
void(* | lsiAddr )(void)
void(* | rbiAddr )(void)
void(* | tbeiAddr )(void)
void(* | ctoi )(void)

## Detailed Description

UART callback pointer structure.

This structure contains pointers to UART interrupt callback functions

## Field Documentation

void(* CSL_UartIsrAddr::ctoi)(void)

Character timeout interrupt

Referenced by UART_setCallback().

void(* CSL_UartIsrAddr::lsiAddr)(void)

Receiver line status interrupt

Referenced by UART_setCallback().

void(* CSL_UartIsrAddr::rbiAddr)(void)

received data available and character timeout indication interrupt

Referenced by UART_setCallback().

void(* CSL_UartIsrAddr::tbeiAddr)(void)

transmiter holding register empty interrupt

Referenced by UART_setCallback().

The documentation for this struct was generated from the following file:

- csl_uart.h