- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_UsbSetupStruct Struct Reference
USB MUSB Data Structures

Data structure to hold USB setup packet. More...

`#include <csl_usb.h>`

## Data Fields
int | newPacket
| new = 1, structure holds new setup packet
Uint16 | bmRequestType
| Byte 0 of setup packet.
Uint16 | bRequest
| Byte 1 of setup packet.
Uint16 | wValue
| Byte 2 and 3 of setup packet.
Uint16 | wIndex
| Byte 4 and 5 setup packet.
Uint16 | wLength
| Byte 6 and 7 of setup packet.

## Detailed Description

Data structure to hold USB setup packet.

The documentation for this struct was generated from the following file:

- csl_usb.h