- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_NandAsyncCfg Struct Reference
NAND Data Structures

Nand Async config structure. More...

`#include <csl_nand.h>`

## Data Fields
Uint16 | selectStrobe
Uint16 | ewMode
Uint16 | w_setup
Uint16 | w_strobe
Uint16 | w_hold
Uint16 | r_setup
Uint16 | r_strobe
Uint16 | r_hold
Uint16 | turnAround
Uint16 | aSize

## Detailed Description

Nand Async config structure.

## Field Documentation

Uint16 CSL_NandAsyncCfg::aSize

Asynchronous memory size

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::ewMode

Enable extended wait mode

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::r_hold

Read strobe hold cycle

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::r_setup

Read strobe setup cycles

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::r_strobe

Read strobe duration cycles

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::selectStrobe

Strobe mode selection

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::turnAround

Turn around cycles

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::w_hold

Write strobe hold cycle

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::w_setup

Write strobe setup cycles

Referenced by NAND_getSetup(), and NAND_setup().

Uint16 CSL_NandAsyncCfg::w_strobe

Write strobe duration cycles

Referenced by NAND_getSetup(), and NAND_setup().

The documentation for this struct was generated from the following file:

- csl_nand.h