- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_AcLogicalUnit Struct Reference
USB AC Data Structures

Audio Class Logical unit structure. More...

`#include <csl_audioClass.h>`

## Data Fields
Uint16 | scsiInquiryData [CSL_AC_SCSI_INQUIRY_LEN]
| SCSI Inquiry Data.
Uint32 | mediaSize
| Number of logical blocks in the media During init this filed is set to value -1.
Uint32 | currLba
| the current LBA
Uint32 | lbaSize
| Logical Block Size.
Uint16 | removeable
| Removable or NonRemovable Media.
Uint16 | mediaState
| Media State.
Uint16 | readwrite
| Device is Readable and/or writeable.
Uint16 | lbaCnt
| Contains number of LB that has to be read/written.
Uint16 | verifyFlag
| Contains status of previous write in this variable.

## Detailed Description

Audio Class Logical unit structure.

Holds all the components for the logical unit This structure is filled with the data given by the application through CSL_AcLunAttribApp structure

The documentation for this struct was generated from the following file:

- csl_audioClass.h