- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_LcdcConfigDma Struct Reference
LCDC Data Structures

Configuration parameters for DMA engine. More...

`#include <csl_lcdc.h>`

## Data Fields
CSL_LcdcDmaBurst | burstSize
CSL_LcdcEofIntCtl | eofIntEn
CSL_LcdcEndianess | bigEndian
CSL_LcdcFrameMode | frameMode
Uint32 | fb0Base
Uint32 | fb0Ceil
Uint32 | fb1Base
Uint32 | fb1Ceil

## Detailed Description

Configuration parameters for DMA engine.

Used to configure DMA

## Field Documentation

CSL_LcdcEndianess CSL_LcdcConfigDma::bigEndian

Big Endian enable

Referenced by LCD_configDMA(), and LCD_getConfigDMA().

CSL_LcdcDmaBurst CSL_LcdcConfigDma::burstSize

Burst Size setting for DMA transfers

Referenced by LCD_configDMA(), and LCD_getConfigDMA().

CSL_LcdcEofIntCtl CSL_LcdcConfigDma::eofIntEn

End of Frame Interrupt Enable

Referenced by LCD_configDMA(), and LCD_getConfigDMA().

Uint32 CSL_LcdcConfigDma::fb0Base

The start address for frame buffer 0, specify most significant 30-bits

Referenced by LCD_configDMA(), and LCD_getConfigDMA().

Uint32 CSL_LcdcConfigDma::fb0Ceil

The end address for frame buffer 0, specify most significant 30-bits

Referenced by LCD_configDMA(), and LCD_getConfigDMA().

Uint32 CSL_LcdcConfigDma::fb1Base

The start address for frame buffer 1, specify most significant 30-bits

Referenced by LCD_configDMA(), and LCD_getConfigDMA().

Uint32 CSL_LcdcConfigDma::fb1Ceil

The end address for frame buffer 1, specify most significant 30-bits

Referenced by LCD_configDMA(), and LCD_getConfigDMA().

CSL_LcdcFrameMode CSL_LcdcConfigDma::frameMode

Frame Mode

Referenced by LCD_configDMA(), and LCD_getConfigDMA().

The documentation for this struct was generated from the following file:

- csl_lcdc.h