- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_MmcsdCmd Struct Reference
MMC/SD Data Structures

Command structure for the card. More...

`#include <csl_mmcsd.h>`

## Data Fields
Uint16 | idx
CSL_MmcsdRespType | respType
CSL_MmcsdRespBusy | busy
CSL_MmcsdCmdType | type
CSL_MmcsdDir | dir
CSL_MmcsdLineChr | lineChr

## Detailed Description

Command structure for the card.

This structure has parameters that is used to send a command to the MMC/SD device.

## Field Documentation

CSL_MmcsdRespBusy CSL_MmcsdCmd::busy

Response property with respect to busy signal

CSL_MmcsdDir CSL_MmcsdCmd::dir

Direction for the data incase of data transferred involved

Uint16 CSL_MmcsdCmd::idx

Index of the command

CSL_MmcsdLineChr CSL_MmcsdCmd::lineChr

Line characteristics of the command

CSL_MmcsdRespType CSL_MmcsdCmd::respType

Response expected for the command

CSL_MmcsdCmdType CSL_MmcsdCmd::type

Protocol type of the command

The documentation for this struct was generated from the following file:

- csl_mmcsd.h