- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_MMCConfig Struct Reference
MMC/SD Data Structures

MMC config structure for setting MMC/SD Control register. More...

`#include <csl_mmcsd.h>`

## Data Fields
Uint16 | mmcctl
Uint16 | mmcclk
Uint16 | mmcim
Uint16 | mmctor
Uint16 | mmctod
Uint16 | mmcblen
Uint16 | mmcnblk

## Detailed Description

MMC config structure for setting MMC/SD Control register.

## Field Documentation

Uint16 CSL_MMCConfig::mmcblen

no of bytes in a block of mmc or sd card

Referenced by MMC_config(), and MMC_getConfig().

Uint16 CSL_MMCConfig::mmcclk

MMCSD clock control register value

Referenced by MMC_config(), and MMC_getConfig().

Uint16 CSL_MMCConfig::mmcctl

MMCSD control register value

Referenced by MMC_config(), and MMC_getConfig().

Uint16 CSL_MMCConfig::mmcim

required interrupt field for MMCSD

Referenced by MMC_config(), and MMC_getConfig().

Uint16 CSL_MMCConfig::mmcnblk

total no of blocks for read or write

Referenced by MMC_config(), and MMC_getConfig().

Uint16 CSL_MMCConfig::mmctod

mmc data read time out register

Referenced by MMC_config(), and MMC_getConfig().

Uint16 CSL_MMCConfig::mmctor

mmc response time out register

Referenced by MMC_config(), and MMC_getConfig().

The documentation for this struct was generated from the following file:

- csl_mmcsd.h