- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_MMCSetupNative Struct Reference
MMC/SD Data Structures

Structure to store the some default configuration for MMCSD controller. More...

`#include <csl_mmcsd.h>`

## Data Fields
Uint16 | dmaEnable
Uint16 | dat3EdgeDetection
Uint16 | enableClkPin
Uint16 | cdiv
Uint16 | rspTimeout
Uint16 | dataTimeout
Uint16 | blockLen

## Detailed Description

Structure to store the some default configuration for MMCSD controller.

## Field Documentation

Uint16 CSL_MMCSetupNative::blockLen

Block Length - must be same as CSD

Referenced by MMC_setupNative().

Uint16 CSL_MMCSetupNative::cdiv

MMC function clk to memory clk divide down

Referenced by MMC_setupNative().

Uint16 CSL_MMCSetupNative::dat3EdgeDetection

Set level of edge detection for DAT3 pin

Referenced by MMC_setupNative().

Uint16 CSL_MMCSetupNative::dataTimeout

Number of memory clks to wait before data timeout

Referenced by MMC_setupNative().

Uint16 CSL_MMCSetupNative::dmaEnable

Enable/disable DMA for data read/write

Uint16 CSL_MMCSetupNative::enableClkPin

Memory clk reflected on CLK Pin

Uint16 CSL_MMCSetupNative::rspTimeout

Number of memory clks to wait before response timeout

Referenced by MMC_setupNative().

The documentation for this struct was generated from the following file:

- csl_mmcsd.h