- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_LcdcHwSetup Struct Reference
LCDC Data Structures

Input parameters for setting up LCD Controller Parameters used to put LCDC into useful state. More...

`#include <csl_lcdc.h>`

## Data Fields
void * | extendSetup
CSL_LcdcConfigLidd | config
CSL_LcdcLiddTiming | timingCs0
CSL_LcdcCs1Status | useCs1
CSL_LcdcLiddTiming | timingCs1

## Detailed Description

Input parameters for setting up LCD Controller Parameters used to put LCDC into useful state.

## Field Documentation

CSL_LcdcConfigLidd CSL_LcdcHwSetup::config

LCDC config sructure instance

Referenced by LCD_getSetup(), and LCD_setup().

void* CSL_LcdcHwSetup::extendSetup

place holder for future implementation

CSL_LcdcLiddTiming CSL_LcdcHwSetup::timingCs0

LCDC timing sructure instance for cs0

Referenced by LCD_getSetup(), and LCD_setup().

CSL_LcdcLiddTiming CSL_LcdcHwSetup::timingCs1

LCDC timing sructure instance for cs1

Referenced by LCD_getSetup(), and LCD_setup().

CSL_LcdcCs1Status CSL_LcdcHwSetup::useCs1

Enum for chosing the chip select

Referenced by LCD_getSetup(), and LCD_setup().

The documentation for this struct was generated from the following file:

- csl_lcdc.h