- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_UartSetup Struct Reference
UART Data Structures

UART Setup structure. More...

`#include <csl_uart.h>`

## Data Fields
Uint32 | clkInput
Uint32 | baud
Uint16 | wordLength
Uint16 | stopBits
Uint16 | parity
Uint16 | fifoControl
Uint16 | loopBackEnable
Uint16 | afeEnable
Uint16 | rtsEnable

## Detailed Description

UART Setup structure.

This structure contains the UART setup parameters. Using this structure individual parameters can be passed

## Field Documentation

Uint16 CSL_UartSetup::afeEnable

AFE enable/disable

Referenced by UART_setup().

Uint32 CSL_UartSetup::baud

Baud rate

Referenced by UART_setup().

Uint32 CSL_UartSetup::clkInput

Input clock in Hz

Referenced by UART_setup().

Uint16 CSL_UartSetup::fifoControl

Fifo control register

Referenced by UART_setup().

Uint16 CSL_UartSetup::loopBackEnable

Looppback mode enable/disable

Referenced by UART_setup().

Uint16 CSL_UartSetup::parity

Parity generation enable/disable

Referenced by UART_setup().

Uint16 CSL_UartSetup::rtsEnable

RTS enable/disable

Referenced by UART_setup().

Uint16 CSL_UartSetup::stopBits

Number of stop bits to be generated Valid values - 0 or 1

Referenced by UART_setup().

Uint16 CSL_UartSetup::wordLength

Word length selection Valid values - 5,6,7, or 8bits

Referenced by UART_setup().

The documentation for this struct was generated from the following file:

- csl_uart.h