- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_UsbEpStatus Struct Reference
USB MUSB Data Structures

USB end point status structure. More...

`#include <csl_usb.h>`

## Data Fields
DWORD | dwEndpoint
| Endpoint.
CSL_UsbXferType | xferType
| USB xfer type supported by the EP.
DWORD | dwPacketSizeAssigned
| Packet Size assigned.
Bool | fInitialized
| TRUE, if initialized.
DWORD * | pFifoAddr
| FIFO address of the EP.
CSL_UsbTransfer * | pTransfer
| Pointer to the Tx Buf.
WORD | wUSBEvents
| OR'ed combination of USB Events.
WORD | dataReadFromFifo
| Variable to store the most recent data size read from FIFO.
CSL_USB_EVENT_ISR | hEventHandler
| Call back for the associated event handler.
Bool | fStalled
| TRUE, if stalled.
Bool | fSelected
| TRUE, if selected.

## Detailed Description

USB end point status structure.

This structure is used to hold the status of an Endpoint

The documentation for this struct was generated from the following file:

- csl_usb.h