- Main Page
- Modules
- Data Structures
- Files

Enumerations
RTC Enumerated Data Types
RTC

## Enumerations
enum | CSL_RTCPeriodicInterruptType { CSL_RTC_DAY_PERIODIC_INTERRUPT, CSL_RTC_HR_PERIODIC_INTERRUPT, CSL_RTC_MINS_PERIODIC_INTERRUPT, CSL_RTC_SEC_PERIODIC_INTERRUPT, CSL_RTC_MS_PERIODIC_INTERRUPT }
| enum variable for the selection of rtc Periodic interrupt for Day , Hour , Minute , Second and MilliSecond Period.
enum | CSL_RTCEventType { CSL_RTC_MSEVENT_INTERRUPT, CSL_RTC_SECEVENT_INTERRUPT, CSL_RTC_MINSEVENT_INTERRUPT, CSL_RTC_HREVENT_INTERRUPT, CSL_RTC_DAYEVENT_INTERRUPT, CSL_RTC_EXTEVENT_INTERRUPT, CSL_RTC_ALARM_INTERRUPT, CSL_RTC_INTERRUPT_NONE }
| enum variable for the selection of rtc interrupt Alarm Int,External Event, Day Event, Hour Event, Minute Event, Second Event, MilliSecond Event.
enum | CSL_RTCCompType { CSL_RTC_COMPENSATION_NEGATIVE = 0, CSL_RTC_COMPENSATION_POSITIVE, CSL_RTC_COMPENSATION_INVALID }
| This enum holds type of the compensation required for the RTC.