- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_SdioControllerObj Struct Reference
SDIO Data Structures

structure for card specific information. More...

`#include <csl_sdio.h>`

## Data Fields
CSL_MmcsdRegsOvly | sdioRegs
CSL_SdioCardObj * | pSdioCardObj
CSL_SdioEndianMode | readEndianMode
CSL_SdioEndianMode | writeEndianMode
Bool | cmd8Resp

## Detailed Description

structure for card specific information.

## Field Documentation

Bool CSL_SdioControllerObj::cmd8Resp

Response status for CMD8

Referenced by SDIO_detectCard(), and SDIO_initCard().

CSL_SdioCardObj* CSL_SdioControllerObj::pSdioCardObj

Card Object structure pointer

Referenced by SDIO_deselectCard(), SDIO_detectCard(), SDIO_getRca(), SDIO_initCard(), and SDIO_selectCard().

CSL_SdioEndianMode CSL_SdioControllerObj::readEndianMode

Endian mode for read operation

Referenced by SDIO_open(), SDIO_readBlocks(), SDIO_readBytes(), SDIO_setEndianMode(), SDIO_writeBlocks(), and SDIO_writeBytes().

CSL_MmcsdRegsOvly CSL_SdioControllerObj::sdioRegs

Pointer to Hw regs structure

Referenced by SDIO_clearResponse(), SDIO_close(), SDIO_config(), SDIO_deselectCard(), SDIO_detectCard(), SDIO_eventDisable(), SDIO_eventEnable(), SDIO_getRca(), SDIO_getResponse(), SDIO_getSdioStatus(), SDIO_getStatus(), SDIO_initCard(), SDIO_open(), SDIO_readBlocks(), SDIO_readBytes(), SDIO_readSingleByte(), SDIO_readWaitDisable(), SDIO_readWaitEnable(), SDIO_resetCard(), SDIO_selectCard(), SDIO_sendCommand(), SDIO_setClock(), SDIO_setEndianMode(), SDIO_writeBlocks(), SDIO_writeBytes(), and SDIO_writeSingleByte().

CSL_SdioEndianMode CSL_SdioControllerObj::writeEndianMode

Endian mode for write operation

Referenced by SDIO_open(), SDIO_setEndianMode(), SDIO_writeBlocks(), and SDIO_writeBytes().

The documentation for this struct was generated from the following file:

- csl_sdio.h