- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_UartConfig Struct Reference
UART Data Structures

UART Config structure The members of this structure directly maps to a particular register of UART. More...

`#include <csl_uart.h>`

## Data Fields
Uint16 | DLL
Uint16 | DLH
Uint16 | LCR
Uint16 | FCR
Uint16 | MCR

## Detailed Description

UART Config structure The members of this structure directly maps to a particular register of UART.

## Field Documentation

Uint16 CSL_UartConfig::DLH

DLH holds most significant bits of the divisor

Referenced by UART_config(), and UART_getConfig().

Uint16 CSL_UartConfig::DLL

DLL holds least significant bits of the divisor

Referenced by UART_config(), and UART_getConfig().

Uint16 CSL_UartConfig::FCR

FCR controls fifo enable/disable,trigger level selection,dma selection

Referenced by UART_config(), and UART_getConfig().

Uint16 CSL_UartConfig::LCR

LCR controls word length,parity selection,stop bit generation

Referenced by UART_config(), and UART_getConfig().

Uint16 CSL_UartConfig::MCR

MCR controls autoflow selection,loopback feature,RTS selection

Referenced by UART_config(), and UART_getConfig().

The documentation for this struct was generated from the following file:

- csl_uart.h