**Power tree:**



**Detail:**

**Q1**: Confirm whether it has to be on all LDO of since we make 3 LDO in parallel if it can be only 1 per 3 LDO.( TPS7A96)

- I have read the TPS7A96’s datasheet. You can also see below, it is the place where we need to add the pi filter, and which type ferrite-bead they recommend. In my opinion, we should add pi filter in all of the TPS7A96. But we want to confirm whether it has to be on all LDO of since we make 3 LDO in parallel if it can be only 1 per 3 LDO.



