section {
 boot_mode = 50
 param_index = 0
 options = 1
 core_freq_mhz = 800
 exe_file = "simple.i2c.ccs"
 next_dev_addr_ext = 0x0
 sw_pll_prediv = 5
 sw_pll_mult = 32
 sw_pll_postdiv = 2
 sw_pll_flags = 1
 addr_width = 24
 n_pins = 4
 csel = 0
 mode = 0
 c2t_delay = 0
 bus_freq_mhz = 0
 bus_freq_khz = 500
}
