K2HK EVM # boot                                                                 
Creating 1 MTD partitions on "nand0":                                           
0x000000180000-0x000020000000 : "mtd=2"                                         
UBI: attaching mtd1 to ubi0                                                     
UBI: physical eraseblock size:   131072 bytes (128 KiB)                         
UBI: logical eraseblock size:    126976 bytes                                   
UBI: smallest flash I/O unit:    2048                                           
UBI: VID header offset:          2048 (aligned 2048)                            
UBI: data offset:                4096                                           
UBI: attached mtd1 to ubi0                                                      
UBI: MTD device name:            "mtd=2"                                        
UBI: MTD device size:            510 MiB                                        
UBI: number of good PEBs:        4080                                           
UBI: number of bad PEBs:         4                                              
UBI: max. allowed volumes:       128                                            
UBI: wear-leveling threshold:    4096                                           
UBI: number of internal volumes: 1                                              
UBI: number of user volumes:     5                                              
UBI: available PEBs:             0                                              
UBI: total number of reserved PEBs: 4080                                        
UBI: number of PEBs reserved for bad PEB handling: 40                           
UBI: max/mean erase counter: 2/0                                                
UBIFS: mounted UBI device 0, volume 0, name "boot"                              
UBIFS: mounted read-only                                                        
UBIFS: file system size:   9269248 bytes (9052 KiB, 8 MiB, 73 LEBs)             
UBIFS: journal size:       1650688 bytes (1612 KiB, 1 MiB, 13 LEBs)             
UBIFS: media format:       w4/r0 (latest is w4/r0)                              
UBIFS: default compressor: LZO                                                  
UBIFS: reserved for root:  0 bytes (0 KiB)                                      
Loading file 'securedb.key.bin' to addr 0x0c000000 with size 28 (0x0000001c)... 
Done                                                                            
Loading file 'uImage-k2hk-evm.dtb' to addr 0x87000000 with size 51080 (0x0000c7.
Done                                                                            
Loading file 'skern-k2hk-evm.bin' to addr 0x0c5f0000 with size 45056 (0x0000b00.
Done                                                                            
Loading file 'uImage-keystone-evm.bin' to addr 0x88000000 with size 3973208 (0x.
Done                                                                            
## installed monitor, freq [133120000], status 0                                
## Booting kernel from Legacy Image at 88000000 ...                             
   Image Name:   Linux-3.10.10                                                  
   Created:      2014-10-02   5:54:16 UTC                                       
   Image Type:   ARM Linux Kernel Image (uncompressed)                          
   Data Size:    3973144 Bytes = 3.8 MiB                                        
   Load Address: 80008000                                                       
   Entry Point:  80008000                                                       
   Verifying Checksum ... OK                                                    
## Flattened Device Tree blob at 87000000                                       
   Booting using the fdt blob at 0x87000000                                     
   Loading Kernel Image ... OK                                                  
OK                                                                              
   Using Device Tree in place at 87000000, end 8700f787                         
                                                                                
Starting kernel ...                                                             
                                                                                
[    0.000000] Booting Linux on physical CPU 0x0                                
[    0.000000] Linux version 3.10.10 (gtbldadm@ubuntu-12) (gcc version 4.7.3 204
[    0.000000] CPU: ARMv7 Processor [412fc0f4] revision 4 (ARMv7), cr=30c7387d  
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, PIPT instruction cache  
[    0.000000] Machine: KeyStone2, model: Texas Instruments Keystone 2 SoC      
[    0.000000] switching to high address space at 0x800000000                   
[    0.000000] cma: CMA: reserved 16 MiB at 1f000000                            
[    0.000000] Memory policy: ECC disabled, Data cache writealloc               
[    0.000000] PERCPU: Embedded 8 pages/cpu @c0bee000 s11840 r8192 d12736 u32768
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pa8
[    0.000000] Kernel command line: console=ttyS0,115200n8 rootwait=1 rootfstyp8
[    0.000000] PID hash table entries: 2048 (order: 1, 8192 bytes)              
[    0.000000] Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)  
[    0.000000] Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)   
[    0.000000] Memory: 512MB = 512MB total                                      
[    0.000000] Memory: 495056k/495056k available, 29232k reserved, 0K highmem   
[    0.000000] Virtual kernel memory layout:                                    
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)                
[    0.000000]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)                
[    0.000000]     vmalloc : 0xe0800000 - 0xff000000   ( 488 MB)                
[    0.000000]     lowmem  : 0xc0000000 - 0xe0000000   ( 512 MB)                
[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)                
[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)                
[    0.000000]       .text : 0xc0008000 - 0xc0708ad0   (7171 kB)                
[    0.000000]       .init : 0xc0709000 - 0xc075be40   ( 332 kB)                
[    0.000000]       .data : 0xc075c000 - 0xc07a2228   ( 281 kB)                
[    0.000000]        .bss : 0xc07a2228 - 0xc07d1d34   ( 191 kB)                
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1       
[    0.000000] Hierarchical RCU implementation.                                 
[    0.000000] NR_IRQS:16 nr_irqs:16 16                                         
[    0.000000] ipc irq: irqchip registered, range 512-539                       
[    0.000000] Main PLL clk (798720000 Hz), parent (122880000 Hz),postdiv = 2, 0
[    0.000000] Generic PLL clk (1200000000 Hz), parent (125000000 Hz),postdiv =4
[    0.000000] Generic PLL clk (983040000 Hz), parent (122880000 Hz),postdiv = 0
[    0.000000] Generic PLL clk (333333333 Hz), parent (100000000 Hz),postdiv = 0
[    0.000000] Generic PLL clk (333333333 Hz), parent (100000000 Hz),postdiv = 0
[    0.000000] Architected local timer running at 133.12MHz (phys).             
[    0.000000] Switching to timer-based delay loop                              
[    0.000000] sched_clock: ARM arch timer >56 bits at 133120kHz, resolution 96s
[    0.000000] keystone timer clock @133120000 MHz                              
[    0.000000] sched_clock: 32 bits at 100 Hz, resolution 10000000ns, wraps eves
[    0.000000] Console: colour dummy device 80x30                               
[  657.769808] Calibrating delay loop (skipped), value calculated using timer f)
[  657.769818] pid_max: default: 4096 minimum: 301                              
[  657.769937] Mount-cache hash table entries: 512                              
[  657.778747] CPU: Testing write buffer coherency: ok                          
[  657.778959] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000                 
[  657.778974] Setting up static identity map for 0xc04f8198 - 0xc04f81cc       
[  657.845306] CPU1: Booted secondary processor                                 
[  657.845335] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001                 
[  657.910724] CPU2: Booted secondary processor                                 
[  657.910752] CPU2: thread -1, cpu 2, socket 0, mpidr 80000002                 
[  657.976122] CPU3: Booted secondary processor                                 
[  657.976151] CPU3: thread -1, cpu 3, socket 0, mpidr 80000003                 
[  657.976271] Brought up 4 CPUs                                                
[  657.976291] SMP: Total of 4 processors activated (1064.96 BogoMIPS).         
[  657.976296] CPU: All CPU(s) started in SVC mode.                             
[  657.976753] devtmpfs: initialized                                            
[  657.989551] NET: Registered protocol family 16                               
[  657.990482] DMA: preallocated 256 KiB pool for atomic coherent allocations   
[  657.999752] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint.
[  657.999759] hw-breakpoint: maximum watchpoint size is 8 bytes.               
[  658.009608] bio: create slab <bio-0> at 0                                    
[  658.009965] keystone-pcie: keystone_pcie_rc_init - start                     
[  658.009987] keystone2_pcie_serdes_setup for domain 0                         
[  658.012091] keystone2_pcie_serdes_setup done domain 0, en_link_train = 1     
[  658.012122] keystone-pcie: MEM 0x0000000050000000..0x000000005fffffff -> 0x0 
[  658.012131] keystone-pcie: IO 0x0000000023250000..0x0000000023253fff -> 0x000
[  658.012163] keystone-pcie: pcie - number of legacy irqs = 4                  
[  658.012207] keystone-pcie: pcie - number of MSI host irqs = 8, msi_irqs = 32 
[  658.119697] keystone-pcie: Doing PCI Setup...Done                            
[  658.119703] keystone-pcie: Starting PCI scan, nr 0...                        
[  658.119820] PCI host bridge to bus 0000:00                                   
[  658.119832] pci_bus 0000:00: root bus resource [mem 0x50000000-0x5fffffff]   
[  658.119839] pci_bus 0000:00: root bus resource [io  0x0000-0x3fff]           
[  658.119846] pci_bus 0000:00: No busn resource found for root bus, will use []
[  658.119891] PCI: bus0: Fast back to back transfers enabled                   
[  658.119907] keystone-pcie: Ending PCI scan...                                
[  658.119915] keystone-pcie: keystone_pcie_rc_init - end                       
[  658.120166] vgaarb: loaded                                                   
[  658.120476] SCSI subsystem initialized                                       
[  658.121058] usbcore: registered new interface driver usbfs                   
[  658.121141] usbcore: registered new interface driver hub                     
[  658.121239] usbcore: registered new device driver usb                        
[  658.122301] pps_core: LinuxPPS API ver. 1 registered                         
[  658.122308] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giom>
[  658.122368] PTP clock support registered                                     
[  658.122479] keystone-hwqueue hwqueue.6: qmgr start queue 0, number of queues2
[  658.122562] keystone-hwqueue hwqueue.6: added qmgr start queue 0, num of que0
[  658.122571] keystone-hwqueue hwqueue.6: qmgr start queue 8192, number of que2
[  658.122645] keystone-hwqueue hwqueue.6: added qmgr start queue 8192, num of 0
[  658.123483] keystone-hwqueue hwqueue.6: qos: sched port @8096, drop sched @80
[  658.124483] keystone-hwqueue hwqueue.6: qos: sched port @6496, drop sched @60
[  658.125457] keystone-hwqueue hwqueue.6: added pool pool-rio: 128 descriptors6
[  658.125466] keystone-hwqueue hwqueue.6: added pool pool-xge: 1024 descriptor8
[  658.125475] keystone-hwqueue hwqueue.6: added pool pool-crypto: 1024 descrip8
[  658.125483] keystone-hwqueue hwqueue.6: added pool pool-net: 11264 descripto8
[  658.125491] keystone-hwqueue hwqueue.6: added pool pool-udma: 1920 descripto6
[  658.128330] keystone-hwqueue hwqueue.6: registered queues 0-16383            
[  658.128708] keystone-hwqueue hwqueue.6: qos version 0x2000108, magic valid   
[  658.129203] keystone-hwqueue hwqueue.6: qos version 0x2000108, magic valid   
[  658.136305] keystone-pktdma 2a08000.pktdma: registered 32 logical channels, k
[  658.139919] keystone-pktdma 2004000.pktdma: registered 33 logical channels, 4
[  658.140439] keystone-pktdma 2fa1000.pktdma: registered 4 logical channels, f6
[  658.140572] Switching to clocksource arch_sys_counter                        
[  658.158940] NET: Registered protocol family 2                                
[  658.159308] TCP established hash table entries: 4096 (order: 3, 32768 bytes) 
[  658.159368] TCP bind hash table entries: 4096 (order: 3, 32768 bytes)        
[  658.159425] TCP: Hash tables configured (established 4096 bind 4096)         
[  658.159471] TCP: reno registered                                             
[  658.159479] UDP hash table entries: 256 (order: 1, 8192 bytes)               
[  658.159494] UDP-Lite hash table entries: 256 (order: 1, 8192 bytes)          
[  658.159679] NET: Registered protocol family 1                                
[  658.159843] RPC: Registered named UNIX socket transport module.              
[  658.159849] RPC: Registered udp transport module.                            
[  658.159853] RPC: Registered tcp transport module.                            
[  658.159858] RPC: Registered tcp NFSv4.1 backchannel transport module.        
[  658.160210] hw perfevents: enabled with ARMv7 Cortex-A15 PMU driver, 7 counte
[  658.241401] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).         
[  658.241574] NTFS driver 2.1.30 [Flags: R/O].                                 
[  658.241810] jffs2: version 2.2. (NAND) © 2001-2006 Red Hat, Inc.             
[  658.242093] msgmni has been set to 998                                       
[  658.243013] NET: Registered protocol family 38                               
[  658.243201] Block layer SCSI generic (bsg) driver version 0.4 loaded (major )
[  658.243209] io scheduler noop registered                                     
[  658.243214] io scheduler deadline registered                                 
[  658.243326] io scheduler cfq registered (default)                            
[  658.244764] keystone-udma udma0.7: registered udma device udma0              
[  658.299906] Serial: 8250/16550 driver, 4 ports, IRQ sharing disabled         
[  658.302086] 2530c00.serial: ttyS0 at MMIO 0x2530c00 (irq = 309) is a 16550A  
[  659.127606] console [ttyS0] enabled                                          
[  659.131678] 2531000.serial: ttyS1 at MMIO 0x2531000 (irq = 312) is a 16550A  
[  659.141627] loop: module loaded                                              
[  659.144884] at24 0-0050: 131072 byte 24c1024 EEPROM, writable, 1 bytes/write 
[  659.153117] Generic platform RAM MTD, (c) 2004 Simtec Electronics            
[  659.160317] ONFI param page 0 valid                                          
[  659.163786] ONFI flash detected                                              
[  659.166912] NAND device: Manufacturer ID: 0x2c, Chip ID: 0xac (Micron MT29F44
[  659.178530] Bad block table found at page 262080, version 0x01               
[  659.184805] Bad block table found at page 262016, version 0x01               
[  659.190912] 3 ofpart partitions found on MTD device 30000000.nand            
[  659.196974] Creating 3 MTD partitions on "30000000.nand":                    
[  659.202355] 0x000000000000-0x000000100000 : "u-boot"                         
[  659.207944] 0x000000100000-0x000000180000 : "params"                         
[  659.213480] 0x000000180000-0x000020000000 : "ubifs"                          
[  659.219080] davinci_nand 30000000.nand: controller rev. 2.5                  
[  659.225228] spi_davinci 21000400.spi: master is unqueued, this is deprecated 
[  659.232527] m25p80 spi32766.0: found n25q128a11, expected n25q128            
[  659.238597] m25p80 spi32766.0: n25q128a11 (16384 Kbytes)                     
[  659.243900] 2 ofpart partitions found on MTD device spi32766.0               
[  659.249702] Creating 2 MTD partitions on "spi32766.0":                       
[  659.254821] 0x000000000000-0x000000080000 : "u-boot-spl"                     
[  659.260724] 0x000000080000-0x000001000000 : "test"                           
[  659.266403] spi_davinci 21000400.spi: Controller at 0xe087a400               
[  659.272524] spi_davinci 21000600.spi: master is unqueued, this is deprecated 
[  659.279541] spi_davinci 21000600.spi: Controller at 0xe087c600               
[  659.285646] spi_davinci 21000800.spi: master is unqueued, this is deprecated 
[  659.292675] spi_davinci 21000800.spi: Controller at 0xe087e800               
[  659.299497] tun: Universal TUN/TAP device driver, 1.6                        
[  659.304531] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>           
[  659.311097] keystone-netcp 2090000.netcp: missing num_serdes parameter       
[  659.317595] keystone-netcp 2090000.netcp: missing serdes_lanes parameter     
[  659.324276] keystone-netcp 2090000.netcp: missing serdes_ref_clk parameter   
[  659.331125] keystone-netcp 2090000.netcp: missing serdes_baud_rate parameter 
[  659.338141] keystone-netcp 2090000.netcp: missing serdes_rate_mode parameter 
[  659.345164] keystone-netcp 2090000.netcp: missing serdes_phy_intf parameter  
[  659.352099] keystone-netcp 2090000.netcp: missing serdes_loopback parameter  
[  659.359040] keystone-netcp 2090000.netcp: Missing cpts_clock_mult property i.
[  659.366840] keystone-netcp 2090000.netcp: Missing cpts_clock_shift property .
[  659.374727] keystone-netcp 2090000.netcp: Missing cpts_clock_div property in.
[  659.383279] keystone-netcp 2090000.netcp: Created interface "eth0"           
[  659.389434] keystone-netcp 2090000.netcp: dma_chan_name nettx0               
[  659.396020] keystone-netcp 2090000.netcp: Created interface "eth1"           
[  659.402187] keystone-netcp 2090000.netcp: dma_chan_name nettx1               
[  659.408783] keystone-netcp 2090000.netcp: Created interface "eth2"           
[  659.414949] keystone-netcp 2090000.netcp: dma_chan_name nettx2               
[  659.421539] keystone-netcp 2090000.netcp: Created interface "eth3"           
[  659.427695] keystone-netcp 2090000.netcp: dma_chan_name nettx3               
[  659.433648] keystone-netcp 2090000.netcp: pdsp 0 firmware: keystone/pa_pdsp0w
[  659.441798] keystone-netcp 2090000.netcp: pdsp 1 firmware: keystone/pa_pdsp1w
[  659.449947] keystone-netcp 2090000.netcp: pdsp 2 firmware: keystone/pa_pdsp2w
[  659.458087] keystone-netcp 2090000.netcp: pdsp 3 firmware: keystone/pa_pdsp3w
[  659.466234] keystone-netcp 2090000.netcp: pdsp 4 firmware: keystone/pa_pdsp4w
[  659.473948] keystone-netcp 2090000.netcp: pdsp 5 firmware: keystone/pa_pdsp4w
[  659.481738] keystone-netcp 2090000.netcp: could not find interface 2 node ine
[  659.489792] keystone-netcp 2090000.netcp: Attach of module keystone-qos decl9
[  659.497941] keystone-netcp 2090000.netcp: could not find interface 3 node ine
[  659.506002] keystone-netcp 2090000.netcp: Attach of module keystone-qos decl9
[  659.514161] keystone-netcp 2090000.netcp: Attach of module keystone-sa decli9
[  659.522222] keystone-netcp 2090000.netcp: Attach of module keystone-sa decli9
[  659.531165] keystone-dwc3 2690000.dwc: usbss revision 47914300               
[  659.536993] keystone-dwc3 2690000.dwc: mapped irq 425 to virq 608            
[  659.744604] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller                   
[  659.750089] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus n1
[  659.758295] xhci-hcd xhci-hcd.0.auto: irq 608, io mem 0x02690000             
[  659.764359] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002    
[  659.771123] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber1
[  659.778311] usb usb1: Product: xHCI Host Controller                          
[  659.783170] usb usb1: Manufacturer: Linux 3.10.10 xhci-hcd                   
[  659.788627] usb usb1: SerialNumber: xhci-hcd.0.auto                          
[  659.793893] hub 1-0:1.0: USB hub found                                       
[  659.797630] hub 1-0:1.0: 1 port detected                                     
[  659.801729] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller                   
[  659.807196] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus n2
[  659.814897] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003    
[  659.821661] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber1
[  659.828848] usb usb2: Product: xHCI Host Controller                          
[  659.833708] usb usb2: Manufacturer: Linux 3.10.10 xhci-hcd                   
[  659.839165] usb usb2: SerialNumber: xhci-hcd.0.auto                          
[  659.844406] hub 2-0:1.0: USB hub found                                       
[  659.848141] hub 2-0:1.0: 1 port detected                                     
[  659.852382] usbcore: registered new interface driver usb-storage             
[  659.858615] mousedev: PS/2 mouse device common for all mice                  
[  659.864370] i2c /dev entries driver                                          
[  659.868451] watchdog 22f0080.wdt: heartbeat 60 sec                           
[  659.875281] keystone-crypto 20c0000.crypto: crypto accelerator enabled       
[  659.882106] usbcore: registered new interface driver usbhid                  
[  659.887650] usbhid: USB HID core driver                                      
[  659.891780]  remoteproc0: 2620040.dsp0 is available                          
[  659.896633]  remoteproc0: Note: remoteproc is still under development and co.
[  659.905563]  remoteproc0: THE BINARY FORMAT IS NOT YET FINALIZED, and backwa.
[  659.915892]  remoteproc0: no firmware found                                  
[  659.920198] rproc-user 2620040.dsp0: registered misc device dsp0             
[  659.926398]  remoteproc1: 2620044.dsp1 is available                          
[  659.931262]  remoteproc1: Note: remoteproc is still under development and co.
[  659.940186]  remoteproc1: THE BINARY FORMAT IS NOT YET FINALIZED, and backwa.
[  659.950514]  remoteproc1: no firmware found                                  
[  659.954793] rproc-user 2620044.dsp1: registered misc device dsp1             
[  659.961000]  remoteproc2: 2620048.dsp2 is available                          
[  659.965852]  remoteproc2: Note: remoteproc is still under development and co.
[  659.974780]  remoteproc2: THE BINARY FORMAT IS NOT YET FINALIZED, and backwa.
[  659.985117]  remoteproc2: no firmware found                                  
[  659.989392] rproc-user 2620048.dsp2: registered misc device dsp2             
[  659.995592]  remoteproc3: 262004c.dsp3 is available                          
[  660.000454]  remoteproc3: Note: remoteproc is still under development and co.
[  660.009370]  remoteproc3: THE BINARY FORMAT IS NOT YET FINALIZED, and backwa.
[  660.019697]  remoteproc3: no firmware found                                  
[  660.023976] rproc-user 262004c.dsp3: registered misc device dsp3             
[  660.030181]  remoteproc4: 2620050.dsp4 is available                          
[  660.035032]  remoteproc4: Note: remoteproc is still under development and co.
[  660.043958]  remoteproc4: THE BINARY FORMAT IS NOT YET FINALIZED, and backwa.
[  660.054283]  remoteproc4: no firmware found                                  
[  660.058559] rproc-user 2620050.dsp4: registered misc device dsp4             
[  660.064765]  remoteproc5: 2620054.dsp5 is available                          
[  660.069627]  remoteproc5: Note: remoteproc is still under development and co.
[  660.078543]  remoteproc5: THE BINARY FORMAT IS NOT YET FINALIZED, and backwa.
[  660.088868]  remoteproc5: no firmware found                                  
[  660.093157] rproc-user 2620054.dsp5: registered misc device dsp5             
[  660.099348]  remoteproc6: 2620058.dsp6 is available                          
[  660.104211]  remoteproc6: Note: remoteproc is still under development and co.
[  660.113135]  remoteproc6: THE BINARY FORMAT IS NOT YET FINALIZED, and backwa.
[  660.123461]  remoteproc6: no firmware found                                  
[  660.127740] rproc-user 2620058.dsp6: registered misc device dsp6             
[  660.133944]  remoteproc7: 262005c.dsp7 is available                          
[  660.138797]  remoteproc7: Note: remoteproc is still under development and co.
[  660.147723]  remoteproc7: THE BINARY FORMAT IS NOT YET FINALIZED, and backwa.
[  660.158047]  remoteproc7: no firmware found                                  
[  660.162327] rproc-user 262005c.dsp7: registered misc device dsp7             
[  660.168323] rproc-user dspmem.9: kick gpio                                   
[  660.172531] rproc-user dspmem.9: registered misc device dspmem               
[  660.178627] oprofile: using arm/armv7-ca15                                   
[  660.182833] ipip: IPv4 over IPv4 tunneling driver                            
[  660.187898] gre: GRE over IPv4 demultiplexor driver                          
[  660.192761] ip_gre: GRE over IPv4 tunneling driver                           
[  660.198302] TCP: cubic registered                                            
[  660.201607] Initializing XFRM netlink socket                                 
[  660.206290] NET: Registered protocol family 10                               
[  660.211797] NET: Registered protocol family 17                               
[  660.216230] NET: Registered protocol family 15                               
[  660.220712] Bridge firewalling registered                                    
[  660.224704] 8021q: 802.1Q VLAN Support v1.8                                  
[  660.229321] sctp: Hash tables configured (established 16384 bind 16384)      
[  660.236037] NET: Registered protocol family 41                               
[  660.240600] VFP support v0.3: implementor 41 architecture 4 part 30 variant 0
[  660.248236] Registering SWP/SWPB emulation handler                           
[  660.253980] UBI: attaching mtd2 to ubi0                                      
[  662.143258] UBI: scanning is finished                                        
[  662.154562] UBI warning: print_rsvd_warning: cannot reserve enough PEBs for 6
[  662.167174] UBI: attached mtd2 (name "ubifs", size 510 MiB) to ubi0          
[  662.173423] UBI: PEB size: 131072 bytes (128 KiB), LEB size: 126976 bytes    
[  662.180187] UBI: min./max. I/O unit sizes: 2048/2048, sub-page size 2048     
[  662.186854] UBI: VID header offset: 2048 (aligned 2048), data offset: 4096   
[  662.193702] UBI: good PEBs: 4080, bad PEBs: 4, corrupted PEBs: 0             
[  662.199683] UBI: user volume: 5, internal volumes: 1, max. volumes count: 128
[  662.206783] UBI: max/mean erase counter: 2/0, WL threshold: 4096, image sequ9
[  662.215791] UBI: available PEBs: 0, total reserved PEBs: 4080, PEBs reserved0
[  662.224982] UBI: background thread "ubi_bgt0d" started, PID 1312             
[  662.231625] UBIFS: parse sync                                                
[  662.235138] UBIFS: background thread "ubifs_bgt0_2" started, PID 1315        
[  662.263744] UBIFS: recovery needed                                           
[  662.383524] UBIFS: recovery completed                                        
[  662.387231] UBIFS: mounted UBI device 0, volume 2, name "rootfs"             
[  662.393217] UBIFS: LEB size: 126976 bytes (124 KiB), min./max. I/O unit sizes
[  662.402315] UBIFS: FS size: 468795392 bytes (447 MiB, 3692 LEBs), journal si)
[  662.412189] UBIFS: reserved for root: 0 bytes (0 KiB)                        
[  662.417215] UBIFS: media format: w4/r0 (latest is w4/r0), UUID 20218911-28B8l
[  662.427975] VFS: Mounted root (ubifs filesystem) on device 0:12.             
[  662.435178] devtmpfs: mounted                                                
[  662.438304] Freeing unused kernel memory: 328K (c0709000 - c075b000)         
INIT: version 2.88 booting                                                      
Starting udev                                                                   
[  662.916836] udevd[1339]: starting version 182                                
[  663.214230] uio_module_drv mpax.3: registered misc device mpax               
[  663.221016] uio_module_drv edma3.4: registered misc device edma3             
[  663.229737] uio_module_drv secmgr.5: registered misc device secmgr           
[  663.258046] uio_module_drv hyperlink0.12: registered misc device hyperlink0  
[  663.291328] uio_module_drv hyperlink1.13: registered misc device hyperlink1  
Starting Bootlog daemon: bootlogd.                                              
Configuring network interfaces... [  664.134417] keystone-netcp 2090000.netcp: 1
[  664.144444] keystone-netcp 2090000.netcp: Created a cpsw ale engine          
[  664.247769] pps pps0: new PPS source ptp0                                    
[  664.251774] cpts rftclk rate(399360000 HZ),mult(2560),shift(10),div(1)       
[  664.307292] keystone-netcp 2090000.netcp: Using Packet Accelerator Firmware 0
[  664.315870] keystone-netcp 2090000.netcp: pa_clk_rate(163840000 HZ),mult(250)
[  664.597415] net eth0: netcp device eth0 opened                               
[  664.604680] 8021q: adding VLAN 0 to HW filter on device eth0                 
[  664.610328] net eth0: adding rx vlan id: 0                                   
udhcpc (v1.20.2) started                                                        
Sending discover...                                                             
Sending select for 157.87.43.158...                                             
Lease of 157.87.43.158 obtained, lease time 28800                               
/etc/udhcpc.d/50default: Adding DNS 192.0.2.2                                   
/etc/udhcpc.d/50default: Adding DNS 192.0.2.3                                   
done.                                                                           
net.ipv4.conf.default.rp_filter = 1                                             
net.ipv4.conf.all.rp_filter = 1                                                 
Thu Oct  2 04:52:00 UTC 2014                                                    
INIT: Entering runlevel: 5                                                      
Starting system message bus: dbus.                                              
Starting Dropbear SSH server: dropbear.                                         
Starting mpmsrv daemon.                                                         
Starting softhsm daemon[  666.355877]                                           
uio_read: Device read entered : dd901f88 : 2500100.                             
Starting telnet daemon.                                                         
#>>>>> LCD 12                                                                   
IP Address:                                                                     
157.87.43.158                                                                   
Starting tiipclad daemonstart-stop-daemon: can't execute 'Opened': No such filey
.                                                                               
Starting syslog-ng:.                                                            
Starting thttpd.                                                                
Starting Lighttpd Web Server: lighttpd.                                         
2014-10-02 04:52:01: (log.c.166) server started                                 
* starting FTP Server: vsftpd... done.                                          
***************************************************************                 
***************************************************************                 
NOTICE: This file system contains the followin GPLv3 packages:                  
        autoconf                                                                
        binutils-symlinks                                                       
        binutils                                                                
        coreutils                                                               
        cpp-symlinks                                                            
        cpp                                                                     
        g++-symlinks                                                            
        g++                                                                     
        gcc-symlinks                                                            
        gcc                                                                     
        gdb                                                                     
        gdbserver                                                               
        libgmp10                                                                
        libmpfr4                                                                
        m4                                                                      
        make                                                                    
                                                                                
If you do not wish to distribute GPLv3 components please remove                 
the above packages prior to distribution.  This can be done using               
the opkg remove command.  i.e.:                                                 
    opkg remove <package>                                                       
Where <package> is the name printed in the list above                           
                                                                                
NOTE: If the package is a dependency of another package you                     
      will be notified of the dependent packages.  You should                   
      use the --force-removal-of-dependent-packages option to                   
      also remove the dependent packages as well                                
***************************************************************                 
***************************************************************                 
Stopping Bootlog daemon: bootlogd.                                              
                                                                                
 _____                    _____           _         _                           
|  _  |___ ___ ___ ___   |  _  |___ ___  |_|___ ___| |_                         
|     |  _| .'| . | . |  |   __|  _| . | | | -_|  _|  _|                        
|__|__|_| |__,|_  |___|  |__|  |_| |___|_| |___|___|_|                          
              |___|                    |___|                                    
                                                                                
Arago Project http://arago-project.org k2hk-evm ttyS0                           
                                                                                
Arago 2013.12 k2hk-evm ttyS0                                                    
                                                                                
k2hk-evm login: 

