This example shows Ethernet data transfer between two DSP on TCI6482 EVM
Steps to run the test:
1, connect two DSP on the TCI6482 EVM with ethernet cable
2, load this project to both DSPs on TCI6482 EVM
3, run both DSP simultaneously through CCS parellel debug manager
4, check the stdout of both DSP for result
result on first DSP should look like:
-------------------------------------------------------
Calling EMAC_open()
Waiting for link...
Link Status  : 100Mb/s Full Duplex MII on PHY number 1
Packets Held : 32-RX  0-TX
Interrupt Pacing: 0 micro second
Starting packet transfer...
Sent 8192 packets (12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97538 kbps
Sent 8192 packets (10649600 Bytes), packet size is 1300 bytes, achieve bandwidth   87742 kbps
Sent 8192 packets ( 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth   96669 kbps
Sent 8192 packets ( 7372800 Bytes), packet size is  900 bytes, achieve bandwidth   95957 kbps
Sent 8192 packets ( 5734400 Bytes), packet size is  700 bytes, achieve bandwidth   79339 kbps
Sent 8192 packets ( 4096000 Bytes), packet size is  500 bytes, achieve bandwidth   92944 kbps
Sent 8192 packets ( 2457600 Bytes), packet size is  300 bytes, achieve bandwidth   88765 kbps
Sent 8192 packets (  819200 Bytes), packet size is  100 bytes, achieve bandwidth   72470 kbps
Calling EMAC_close()
-------------------------------------------------------
result on second DSP should look like:
-------------------------------------------------------
Calling EMAC_open()
Waiting for link...
Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
Packets Held : 32-RX  0-TX
Interrupt Pacing: 0 micro second
Starting packet receiving...
Received 16084 packets
Received 39779 packets
Received 65536 packets
