10:39:29 Calling EMAC_open()
10:39:29 Waiting for link...
10:39:32 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
10:39:32 Packets Held : 32-RX  0-TX
10:39:32 Interrupt Pacing: 0 micro second
10:39:32 
10:39:32 Starting packet transfer...
10:39:35 ERROR: 10:42:24 Calling EMAC_open()
10:42:24 Waiting for link...
10:42:26 Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
10:42:26 Packets Held : 32-RX  0-TX
10:42:26 Interrupt Pacing: 0 micro second
10:42:26 
10:42:26 Starting packet receiving and transfer...
10:51:22 Calling EMAC_open()
10:51:22 Waiting for link...
10:51:24 Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
10:51:24 Packets Held : 32-RX  0-TX
10:51:25 Interrupt Pacing: 0 micro second
10:51:25 
10:51:25 Starting packet receiving and transfer...
39:45 Sent/received 8192/   0 packets ( 7372800/       0 Bytes), packet size is  900 bytes, achieve bandwidth       0 kbps
10:39:48 ERROR: Timeout waiting for TX/RX
10:39:48 Sent/received 8192/   0 packets ( 5734400/       0 Bytes), packet size is  700 bytes, achieve bandwidth       0 kbps
10:39:53 ERROR: Timeout waiting for TX/RX
10:39:55 Sent/received 8192/   0 packets ( 4096000/       0 Bytes), packet size is  500 bytes, achieve bandwidth       0 kbps
10:39:59 ERROR: Timeout waiting for TX/RX
10:39:59 Sent/received 8192/   0 packets ( 2457600/       0 Bytes), packet size is  300 bytes, achieve bandwidth       0 kbps
10:40:02 ERROR: Timeout waiting for TX/RX
10:40:03 Sent/received 8192/   0 packets (  819200/       0 Bytes), packet size is  100 bytes, achieve bandwidth       0 kbps
10:40:03 Calling EMAC_close()
10:42:23 Calling EMAC_open()
10:42:23 Waiting for link...
10:42:26 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
10:42:26 Packets Held : 32-RX  0-TX
10:42:26 Interrupt Pacing: 0 micro second
10:42:26 
10:42:26 Starting packet transfer...
10:42:28 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97515 kbps
10:42:31 ERROR: Timeout waiting for TX/RX
10:42:31 Sent/received 8192/ 435 packets (10649600/  565500 Bytes), packet size is 1300 bytes, achieve bandwidth    1478 kbps
10:42:34 ERROR: Timeout waiting for TX/RX
10:42:34 Sent/received 8192/ 175 packets ( 9011200/  192500 Bytes), packet size is 1100 bytes, achieve bandwidth     509 kbps
10:42:37 ERROR: Timeout waiting for TX/RX
10:42:37 Sent/received 8192/ 174 packets ( 7372800/  156600 Bytes), packet size is  900 bytes, achieve bandwidth     405 kbps
10:42:40 ERROR: Timeout waiting for TX/RX
10:42:40 Sent/received 8192/ 174 packets ( 5734400/  121800 Bytes), packet size is  700 bytes, achieve bandwidth     319 kbps
10:42:43 ERROR: Timeout waiting for TX/RX
10:42:44 Sent/received 8192/ 175 packets ( 4096000/   87500 Bytes), packet size is  500 bytes, achieve bandwidth     227 kbps
10:42:47 ERROR: Timeout waiting for TX/RX
10:42:47 Sent/received 8192/ 174 packets ( 2457600/   52200 Bytes), packet size is  300 bytes, achieve bandwidth     138 kbps
10:42:50 ERROR: Timeout waiting for TX/RX
10:42:50 Sent/received 8192/  91 packets (  819200/    9100 Bytes), packet size is  100 bytes, achieve bandwidth      23 kbps
10:42:50 Calling EMAC_close()
10:51:22 Calling EMAC_open()
10:51:22 Waiting for link...
10:51:24 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
10:51:25 Packets Held : 32-RX  0-TX
10:51:25 Interrupt Pacing: 0 micro second
10:51:25 
10:51:25 Starting packet transfer...
10:51:26 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97515 kbps
10:51:29 ERROR: Timeout waiting for TX/RX
10:51:29 Sent/received 8192/ 419 packets (10649600/  544700 Bytes), packet size is 1300 bytes, achieve bandwidth    1407 kbps
10:51:32 ERROR: Timeout waiting for TX/RX
10:51:32 Sent/received 8192/  86 packets ( 9011200/   94600 Bytes), packet size is 1100 bytes, achieve bandwidth     252 kbps
10:51:35 ERROR: Timeout waiting for TX/RX
10:51:36 Sent/received 8192/  86 packets ( 7372800/   77400 Bytes), packet size is  900 bytes, achieve bandwidth     201 kbps
10:51:39 ERROR: Timeout waiting for TX/RX
10:51:39 Sent/received 8192/  86 packets ( 5734400/   60200 Bytes), packet size is  700 bytes, achieve bandwidth     157 kbps
10:51:42 ERROR: Timeout waiting for TX/RX
10:51:42 Sent/received 8192/  87 packets ( 4096000/   43500 Bytes), packet size is  500 bytes, achieve bandwidth     114 kbps
10:51:45 ERROR: Timeout waiting for TX/RX
10:51:45 Sent/received 8192/  86 packets ( 2457600/   25800 Bytes), packet size is  300 bytes, achieve bandwidth      67 kbps
10:51:48 ERROR: Timeout waiting for TX/RX
10:51:48 Sent/received 8192/  86 packets (  819200/    8600 Bytes), packet size is  100 bytes, achieve bandwidth      22 kbps
10:51:49 Calling EMAC_close()
11:26:58 Calling EMAC_open()
11:26:58 Waiting for link...
11:27:00 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
11:27:00 Packets Held : 32-RX  0-TX
11:27:00 Interrupt Pacing: 0 micro second
11:27:00 
11:27:00 Starting packet transfer...
11:27:04 ERROR: Timeout waiting for TX/RX
11:27:04 Sent/received 8192/   0 packets (12288000/       0 Bytes), packet size is 1500 bytes, achieve bandwidth       0 kbps
11:27:07 ERROR: Timeout waiting for TX/RX
11:27:07 Sent/received 8192/   0 packets (10649600/       0 Bytes), packet size is 1300 bytes, achieve bandwidth       0 kbps
11:27:10 ERROR: Timeout waiting for TX/RX
11:27:10 Sent/received 8192/   0 packets ( 9011200/       0 Bytes), packet size is 1100 bytes, achieve bandwidth       0 kbps
11:27:13 ERROR: Timeout waiting for TX/RX
11:27:13 Sent/received 8192/   0 packets ( 7372800/       0 Bytes), packet size is  900 bytes, achieve bandwidth       0 kbps
11:27:16 ERROR: Timeout waiting for TX/RX
11:27:16 Sent/received 8192/   0 packets ( 5734400/       0 Bytes), packet size is  700 bytes, achieve bandwidth       0 kbps
11:27:20 ERROR: Timeout waiting for TX/RX
11:27:20 Sent/received 8192/   0 packets ( 4096000/       0 Bytes), packet size is  500 bytes, achieve bandwidth       0 kbps
11:27:23 ERROR: Timeout waiting for TX/RX
11:27:23 Sent/received 8192/   0 packets ( 2457600/       0 Bytes), packet size is  300 bytes, achieve bandwidth       0 kbps
11:27:26 ERROR: Timeout waiting for TX/RX
11:27:26 Sent/received 8192/   0 packets (  819200/       0 Bytes), packet size is  100 bytes, achieve bandwidth       0 kbps
11:27:26 Calling EMAC_close()
11:29:44 Calling EMAC_open()
11:29:44 Waiting for link...
11:29:46 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
11:29:47 Packets Held : 32-RX  0-TX
11:29:47 Interrupt Pacing: 0 micro second
11:29:47 
11:29:47 Starting packet transfer...
11:29:50 ERROR: Timeout waiting for TX/RX
11:29:50 Sent/received 8192/   0 packets (12288000/       0 Bytes), packet size is 1500 bytes, achieve bandwidth       0 kbps
11:29:53 ERROR: Timeout waiting for TX/RX
11:29:53 Sent/received 8192/   0 packets (10649600/       0 Bytes), packet size is 1300 bytes, achieve bandwidth       0 kbps
11:29:56 ERROR: Timeout waiting for TX/RX
11:29:56 Sent/received 8192/   0 packets ( 9011200/       0 Bytes), packet size is 1100 bytes, achieve bandwidth       0 kbps
11:30:00 ERROR: Timeout waiting for TX/RX
11:30:00 Sent/received 8192/   0 packets ( 7372800/       0 Bytes), packet size is  900 bytes, achieve bandwidth       0 kbps
11:30:03 ERROR: Timeout waiting for TX/RX
11:30:03 Sent/received 8192/   0 packets ( 5734400/       0 Bytes), packet size is  700 bytes, achieve bandwidth       0 kbps
11:30:06 ERROR: Timeout waiting for TX/RX
11:30:06 Sent/received 8192/   0 packets ( 4096000/       0 Bytes), packet size is  500 bytes, achieve bandwidth       0 kbps
11:30:09 ERROR: Timeout waiting for TX/RX
11:30:09 Sent/received 8192/   0 packets ( 2457600/       0 Bytes), packet size is  300 bytes, achieve bandwidth       0 kbps
11:30:14 ERROR: Timeout waiting for TX/RX
11:30:16 Sent/received 8192/   0 packets (  819200/       0 Bytes), packet size is  100 bytes, achieve bandwidth       0 kbps
11:30:16 Calling EMAC_close()
11:38:23 Calling EMAC_open()
11:38:23 Waiting for link...
11:38:25 Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
11:38:25 Packets Held : 0-RX  0-TX
11:38:25 Interrupt Pacing: 0 micro second
11:38:25 
11:38:25 Starting packet receiving an11:38:28 ERROR:11:42:37 Calling EMAC_open()
11:42:37 Waiting for link...
11:42:43 Link Status  : No Link RGMII on PHY number 1
11:42:43 Packets Held : 32-RX  0-TX
11:42:43 
11:42:43 WARNING: No device LINK.
11:42:43 Interrupt Pacing: 0 micro second
11:42:43 
11:42:43 Starting packet receiving and transfer...
11:43:34 Calling EMAC_open()
11:43:34 Waiting for link...
11:43:40 Link Status  : No Link RGMII on PHY number 1
11:43:40 Packets Held : 32-RX  0-TX
11:43:40 
11:43:40 WARNING: No device LINK.
11:43:40 Interrupt Pacing: 0 micro second
11:43:40 
11:43:40 Starting packet receiving and transfer...
11:45:27 Calling EMAC_open()
11:45:27 Waiting for link...
11:45:29 Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
11:45:29 Packets Held : 0-RX  0-TX
11:45:29 Interrupt Pacing: 0 micro second
11:45:29 
11:45:29 Starting packet receiving and transfer...
11:52:55 Calling EMAC_open()
11:52:55 Waiting for link...
11:52:57 Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
11:52:57 Packets Held : 0-RX  0-TX
11:52:57 Interrupt Pacing: 0 micro second
11:52:57 
11:52:58 Starting packet receiving and transfer...
11:55:07 Calling EMAC_open()
11:55:07 Waiting for link...
11:55:09 Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
11:55:10 Packets Held : 32-RX  0-TX
11:55:10 Interrupt Pacing: 0 micro second
11:55:10 
11:55:10 Starting packet receiving and transfer...
aiting for link...
11:42:39 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
11:42:39 Packets Held : 32-RX  0-TX
11:42:39 Interrupt Pacing: 0 micro second
11:42:39 
11:42:39 Starting packet transfer...
11:42:43 ERROR: Timeout waiting for TX/RX
11:42:43 Sent/received 8192/   0 packets (12288000/       0 Bytes), packet size is 1500 bytes, achieve bandwidth       0 kbps
11:42:46 ERROR: Timeout waiting for TX/RX
11:42:46 Sent/received 8192/   0 packets (10649600/       0 Bytes), packet size is 1300 bytes, achieve bandwidth       0 kbps
11:42:49 ERROR: Timeout waiting for TX/RX
11:42:49 Sent/received 8192/   0 packets ( 9011200/       0 Bytes), packet size is 1100 bytes, achieve bandwidth       0 kbps
11:42:52 ERROR: Timeout waiting for TX/RX
11:42:52 Sent/received 8192/   0 packets ( 7372800/       0 Bytes), packet size is  900 bytes, achieve bandwidth       0 kbps
11:42:55 ERROR: Timeout waiting for TX/RX
11:42:55 Sent/received 8192/   0 packets ( 5734400/       0 Bytes), packet size is  700 bytes, achieve bandwidth       0 kbps
11:42:59 ERROR: Timeout waiting for TX/RX
11:42:59 Sent/received 8192/   0 packets ( 4096000/       0 Bytes), packet size is  500 bytes, achieve bandwidth       0 kbps
11:43:33 Calling EMAC_open()
11:43:33 Waiting for link...
11:43:35 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
11:43:35 Packets Held : 32-RX  0-TX
11:43:35 Interrupt Pacing: 0 micro second
11:43:35 
11:43:35 Starting packet transfer...
11:43:38 ERROR: Timeout waiting for TX/RX
11:43:38 Sent/received 8192/   0 packets (12288000/       0 Bytes), packet size is 1500 bytes, achieve bandwidth       0 kbps
11:43:42 ERROR: Timeout waiting for TX/RX
11:43:42 Sent/received 8192/   0 packets (10649600/       0 Bytes), packet size is 1300 bytes, achieve bandwidth       0 kbps
11:43:45 ERROR: Timeout waiting for TX/RX
11:43:45 Sent/received 8192/   0 packets ( 9011200/       0 Bytes), packet size is 1100 bytes, achieve bandwidth       0 kbps
11:43:48 ERROR: Timeout waiting for TX/RX
11:43:48 Sent/received 8192/   0 packets ( 7372800/       0 Bytes), packet size is  900 bytes, achieve bandwidth       0 kbps
11:43:51 ERROR: Timeout waiting for TX/RX
11:43:51 Sent/received 8192/   0 packets ( 5734400/       0 Bytes), packet size is  700 bytes, achieve bandwidth       0 kbps
11:43:55 ERROR: Timeout waiting for TX/RX
11:43:55 Sent/received 8192/   0 packets ( 4096000/       0 Bytes), packet size is  500 bytes, achieve bandwidth       0 kbps
11:43:58 ERROR: Timeout waiting for TX/RX
11:43:58 Sent/received 8192/   0 packets ( 2457600/       0 Bytes), packet size is  300 bytes, achieve bandwidth       0 kbps
11:44:01 ERROR: Timeout waiting for TX/RX
11:44:01 Sent/received 8192/   0 packets (  819200/       0 Bytes), packet size is  100 bytes, achieve bandwidth       0 kbps
11:44:01 Calling EMAC_close()
11:45:26 Calling EMAC_open()
11:45:26 Waiting for link...
11:45:28 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
11:45:28 Packets Held : 32-RX  0-TX
11:45:28 Interrupt Pacing: 0 micro second
11:45:28 
11:45:28 Starting packet transfer...
11:45:31 ERROR: Timeout waiting for TX/RX
11:45:31 Sent/received 8192/  32 packets (12288000/   48000 Bytes), packet size is 1500 bytes, achieve bandwidth     126 kbps
11:45:34 ERROR: Timeout waiting for TX/RX
11:45:34 Sent/received 8192/  64 packets (10649600/   83200 Bytes), packet size is 1300 bytes, achieve bandwidth     217 kbps
11:45:38 ERROR: Timeout waiting for TX/RX
11:45:38 Sent/received 8192/   0 packets ( 9011200/       0 Bytes), packet size is 1100 bytes, achieve bandwidth       0 kbps
11:45:41 ERROR: Timeout waiting for TX/RX
11:45:41 Sent/received 8192/   0 packets ( 7372800/       0 Bytes), packet size is  900 bytes, achieve bandwidth       0 kbps
11:45:44 ERROR: Timeout waiting for TX/RX
11:45:44 Sent/received 8192/   0 packets ( 5734400/       0 Bytes), packet size is  700 bytes, achieve bandwidth       0 kbps
11:45:47 ERROR: Timeout waiting for TX/RX
11:45:47 Sent/received 8192/   0 packets ( 4096000/       0 Bytes), packet size is  500 bytes, achieve bandwidth       0 kbps
11:45:50 ERROR: Timeout waiting for TX/RX
11:45:50 Sent/received 8192/   0 packets ( 2457600/       0 Bytes), packet size is  300 bytes, achieve bandwidth       0 kbps
11:45:54 ERROR: Timeout waiting for TX/RX
11:45:54 Sent/received 8192/   0 packets (  819200/       0 Bytes), packet size is  100 bytes, achieve bandwidth       0 kbps
11:45:54 Calling EMAC_close()
11:52:54 Calling EMAC_open()
11:52:54 Waiting for link...
11:52:56 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
11:52:56 Packets Held : 32-RX  0-TX
11:52:56 Interrupt Pacing: 0 micro second
11:52:56 
11:52:56 Starting packet transfer...
11:52:59 ERROR: Timeout waiting for TX/RX
11:52:59 Sent/received 8192/  32 packets (12288000/   48000 Bytes), packet size is 1500 bytes, achieve bandwidth     127 kbps
11:53:00 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth   97121 kbps
11:53:01 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth   96622 kbps
11:53:02 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth   95910 kbps
11:53:03 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth   94812 kbps
11:53:03 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth   92898 kbps
11:53:03 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth   88719 kbps
11:53:03 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth   72429 kbps
11:53:04 Calling EMAC_close()
11:55:07 Calling EMAC_open()
11:55:07 Waiting for link...
11:55:09 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
11:55:10 Packets Held : 32-RX  0-TX
11:55:10 Interrupt Pacing: 0 micro second
11:55:10 
11:55:10 Starting packet transfer...
11:55:11 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97491 kbps
11:55:12 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth   97121 kbps
11:55:13 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth   96622 kbps
11:55:14 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth   95910 kbps
11:55:14 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth   94812 kbps
11:55:15 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth   92898 kbps
11:55:15 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth   88720 kbps
11:55:15 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth   72429 kbps
11:55:15 Calling EMAC_close()
12:10:07 Calling EMAC_open()
12:10:07 Waiting for link...
12:10:09 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
12:10:09 Packets Held : 32-RX  0-TX
12:10:09 Interrupt Pacing: 0 micro second
12:10:09 
12:10:09 Starting packet transfer...
12:10:11 Sent/re12:10:12 Received and send back 16384 packets
12:10:14 Received and send back 40960 packets
12:10:16 Received and send back 65536 packets
12:13:40 Calling EMAC_open()
12:13:40 Waiting for link...
12:13:46 Link Status  : No Link RGMII on PHY number 1
12:13:46 Packets Held : 32-RX  0-TX
12:13:46 
12:13:46 WARNING: No device LINK.
12:13:46 Interrupt Pacing: 0 micro second
12:13:47 
12:13:47 Starting packet transfer...
12:13:47 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth  650173 kbps
12:13:47 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth  647708 kbps
12:13:47 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth  644377 kbps
12:13:47 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth  639625 kbps
12:13:47 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth  632297 kbps
12:13:48 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth  619524 kbps
12:13:48 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth  591647 kbps
12:13:48 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth  238589 kbps
12:13:48 Calling EMAC_close()
12:15:03 Calling EMAC_open()
12:15:03 Waiting for link...
12:15:09 Link Status  : No Link RGMII on PHY number 1
12:15:09 Packets Held : 32-RX  0-TX
12:15:09 
12:15:10 WARNING: No device LINK.
12:15:10 Interrupt Pacing: 5 micro second
12:15:10 
12:15:10 Starting packet transfer...
12:15:10 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth  650173 kbps
12:15:10 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth  647708 kbps
12:15:10 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth  644377 kbps
12:15:10 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth  639625 kbps
12:15:11 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth  632297 kbps
12:15:11 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth  619471 kbps
12:15:11 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth  591601 kbps
12:15:11 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth  390787 kbps
12:15:11 Calling EMAC_close()
12:16:06 Calling EMAC_open()
12:16:06 Waiting for link...
12:16:06 Link Status  : 1000Mb/s Full Duplex RGMII on PHY number 0
12:16:06 Packets Held : 32-RX  0-TX
12:16:07 Interrupt Pacing: 5 micro second
12:16:07 
12:16:07 Starting packet transfer...
12:16:07 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth  975229 kbps
12:16:08 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth  971529 kbps
12:16:08 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth  966529 kbps
12:16:08 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth  959338 kbps
12:16:08 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth  948391 kbps
12:16:08 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth  929121 kbps
12:16:08 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth  887265 kbps
12:16:08 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth  390796 kbps
12:16:08 Calling EMAC_close()
12:18:42 Calling EMAC_open()
12:18:42 Waiting for link...
12:18:43 Link Status  : 1000Mb/s Full Duplex RGMII on PHY number 0
12:18:43 Packets Held : 32-RX  0-TX
12:18:43 Interrupt Pacing: 5 micro second
12:18:43 
12:18:43 Starting packet transfer...
12:18:44 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth  189634 kbps
12:18:44 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth  186898 kbps
12:18:45 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth  184967 kbps
12:18:45 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth  183149 kbps
12:18:45 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth  179979 kbps
12:18:46 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth  175464 kbps
12:18:46 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth  165473 kbps
12:18:46 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth  124297 kbps
12:18:46 Calling EMAC_close()
12:19:05 Calling EMAC_open()
12:19:05 Waiting for link...
12:19:06 Link Status  : 1000Mb/s Full Duplex RGMII on PHY number 0
12:19:06 Packets Held : 32-RX  0-TX
12:19:06 Interrupt Pacing: 5 micro second
12:19:06 
12:19:06 Starting packet transfer...
12:19:06 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth  975229 kbps
12:19:06 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth  971520 kbps
12:19:07 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth  966528 kbps
12:19:07 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth  959333 kbps
12:19:07 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size i12:34:47 Calling EMAC_open()
12:34:47 Waiting for link...
12:34:48 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
12:34:48 Packets Held : 32-RX  0-TX
12:34:48 Interrupt Pacing: 5 micro second
12:34:48 
12:34:48 Starting packet transfer...
12:34:49 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97537 kbps
12:34:50 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth   97168 kbps
12:34:51 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth   96669 kbps
12:34:52 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth   95956 kbps
12:34:52 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth   94858 kbps
12:34:53 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth   92944 kbps
12:34:53 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth   88764 kbps
12:34:53 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth   72467 kbps
12:34:53 Calling EMAC_close()
12:35:24 Calling EMAC_open()
12:35:24 Waiting for link...
12:35:27 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
12:35:27 Packets Held : 32-RX  0-TX
12:35:27 Interrupt Pacing: 5 micro second
12:35:27 
12:35:27 Starting packet transfer...
12:35:29 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97515 kbps
12:35:30 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth   97145 kbps
12:35:30 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth   95128 kbps
12:35:31 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth   95934 kbps
12:35:32 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth   94836 kbps
12:35:32 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth   80196 kbps
12:35:33 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth   88742 kbps
12:35:33 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth   72444 kbps
12:35:33 Calling EMAC_close()
12:36:04 Calling EMAC_open()
12:36:05 Waiting for link...
12:36:05 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
12:36:05 Packets Held : 32-RX  0-TX
12:36:05 Interrupt Pacing: 5 micro second
12:36:05 
12:36:05 Starting packet transfer...
12:36:06 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97537 kbps
12:36:07 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth   97168 kbps
12:36:08 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth   96669 kbps
12:36:09 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth   95956 kbps
12:36:09 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth   94858 kbps
12:36:10 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth   92944 kbps
12:36:10 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth   88763 kbps
12:36:10 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth   72467 kbps
12:36:10 Calling EMAC_close()
s ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth  948306 kbps
12:34:52 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth  929186 kbps
12:34:52 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth  887073 kbps
12:34:52 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth  390546 kbps
12:34:52 Calling EMAC_close()
12:35:25 Calling EMAC_open()
12:35:25 Waiting for link...
12:35:27 Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
12:35:27 Packets Held : 32-RX  0-TX
12:35:27 Interrupt Pacing: 5 micro second
12:35:27 
12:35:27 Starting packet receiving and transfer...
12:35:30 Received and send back 16384 packets
12:35:32 Received and send back 40960 packets
12:35:34 Received and send back 65536 packets
12:36:05 Calling EMAC_open()
12:36:06 Waiting for link...
12:36:06 Link Status  : 1000Mb/s Full Duplex RGMII on PHY number 0
12:36:06 Packets Held : 32-RX  0-TX
12:36:06 Interrupt Pacing: 5 micro second
12:36:06 
12:36:06 Starting packet transfer...
12:36:07 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth  975229 kbps
12:36:07 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth  971520 kbps
12:36:07 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth  966529 kbps
12:36:07 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth  959341 kbps
12:36:07 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth  948308 kbps
12:36:08 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth  929144 kbps
12:36:08 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth  887101 kbps
12:36:08 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth  390546 kbps
12:36:08 Calling EMAC_close()
12:40:55 Calling EMAC_open()
12:40:56 Waiting for link...
12:40:56 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
12:40:56 Packets Held : 32-RX  0-TX
12:40:56 Interrupt Pacing: 5 micro second
12:40:56 
12:40:56 Starting packet transfer...
12:40:57 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97537 kbps
12:40:58 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth   97168 kbps
12:40:59 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth   96669 kbps
12:41:00 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth   95956 kbps
12:41:00 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth   94858 kbps
12:41:01 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth   92944 kbps
12:41:01 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth   88764 kbps
12:41:01 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth   72468 kbps
12:41:01 Calling EMAC_close()
12:44:16 Calling EMAC_open()
12:44:16 Waiting for link...
12:44:16 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
12:44:16 Packets Held : 32-RX  0-TX
12:44:16 Interrupt Pacing: 5 micro second
12:44:17 
12:44:17 Starting packet transfer...
12:44:18 Sent/received 8192/8192 packets (12288000/12288000 Bytes), packet size is 1500 bytes, achieve bandwidth   97537 kbps
12:44:19 Sent/received 8192/8192 packets (10649600/10649600 Bytes), packet size is 1300 bytes, achieve bandwidth   97168 kbps
12:44:20 Sent/received 8192/8192 packets ( 9011200/ 9011200 Bytes), packet size is 1100 bytes, achieve bandwidth   96669 kbps
12:44:20 Sent/received 8192/8192 packets ( 7372800/ 7372800 Bytes), packet size is  900 bytes, achieve bandwidth   95956 kbps
12:44:21 Sent/received 8192/8192 packets ( 5734400/ 5734400 Bytes), packet size is  700 bytes, achieve bandwidth   94858 kbps
12:44:21 Sent/received 8192/8192 packets ( 4096000/ 4096000 Bytes), packet size is  500 bytes, achieve bandwidth   92944 kbps
12:44:21 Sent/received 8192/8192 packets ( 2457600/ 2457600 Bytes), packet size is  300 bytes, achieve bandwidth   88764 kbps
12:44:22 Sent/received 8192/8192 packets (  819200/  819200 Bytes), packet size is  100 bytes, achieve bandwidth   72467 kbps
12:44:22 Calling EMAC_close()
)
13:19:25 Calling EMAC_open()
13:19:25 Waiting for link...
13:19:26 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
13:19:26 Packets Held : 32-RX  0-TX
13:19:26 
13:19:26 Starting packet transfer...
13:19:26 Interrupt Pacing: 0 micro second, init CPU load 100%
13:19:27 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with  26% CPU load
13:19:28 Sent/received 8192/8192 packets in  994 ms, packet size is 1480 bytes, achieve bandwidth   97505 kbps with   2% CPU load
13:19:29 Sent/received 8192/8192 packets in  981 ms, packet size is 1460 bytes, achieve bandwidth   97471 kbps with   2% CPU load
13:19:30 Sent/received 8192/8192 packets in  968 ms, packet size is 1440 bytes, achieve bandwidth   97437 kbps with   2% CPU load
13:19:31 Sent/received 8192/8192 packets in  955 ms, packet size is 1420 bytes, achieve bandwidth   97402 kbps with   2% CPU load
13:19:32 Sent/received 8192/8192 packets in  942 ms, packet size is 1400 bytes, achieve bandwidth   97365 kbps with   2% CPU load
13:19:33 Sent/received 8192/8192 packets in  929 ms, packet size is 1380 bytes, achieve bandwidth   97328 kbps with   2% CPU load
13:19:34 Sent/received 8192/8192 packets in  916 ms, packet size is 1360 bytes, achieve bandwidth   97290 kbps with   2% CPU load
13:19:35 Sent/received 8192/8192 packets in  903 ms, packet size is 1340 bytes, achieve bandwidth   97250 kbps with   2% CPU load
13:19:36 Sent/received 8192/8192 packets in  889 ms, packet size is 1320 bytes, achieve bandwidth   97210 kbps with   2% CPU load
13:19:37 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:19:38 Sent/received 8192/8192 packets in  863 ms, packet size is 1280 bytes, achieve bandwidth   97125 kbps with   2% CPU load
13:19:39 Sent/received 8192/8192 packets in  850 ms, packet size is 1260 bytes, achieve bandwidth   97080 kbps with   2% CPU load
13:19:40 Sent/received 8192/8192 packets in  837 ms, packet size is 1240 bytes, achieve bandwidth   97034 kbps with   2% CPU load
13:19:41 Sent/received 8192/8192 packets in  824 ms, packet size is 1220 bytes, achieve bandwidth   96987 kbps with   2% CPU load
13:19:42 Sent/received 8192/8192 packets in  811 ms, packet size is 1200 bytes, achieve bandwidth   96938 kbps with   2% CPU load
13:19:43 Sent/received 8192/8192 packets in  798 ms, packet size is 1180 bytes, achieve bandwidth   96888 kbps with   2% CPU load
13:19:44 Sent/received 8192/8192 packets in  785 ms, packet size is 1160 bytes, achieve bandwidth   96836 kbps with   2% CPU load
13:19:45 Sent/received 8192/8192 packets in  771 ms, packet size is 1140 bytes, achieve bandwidth   96782 kbps with   2% CPU load
13:19:45 Sent/received 8192/8192 packets in  758 ms, packet size is 1120 bytes, achieve bandwidth   96726 kbps with   2% CPU load
13:19:46 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:19:47 Sent/received 8192/8192 packets in  732 ms, packet size is 1080 bytes, achieve bandwidth   96609 kbps with   3% CPU load
13:19:48 Sent/received 8192/8192 packets in  719 ms, packet size is 1060 bytes, achieve bandwidth   96547 kbps with   3% CPU load
13:19:49 Sent/received 8192/8192 packets in  706 ms, packet size is 1040 bytes, achieve bandwidth   96483 kbps with   3% CPU load
13:19:49 Sent/received 8192/8192 packets in  693 ms, packet size is 1020 bytes, achieve bandwidth   96416 kbps with   3% CPU load
13:19:50 Sent/received 8192/8192 packets in  680 ms, packet size is 1000 bytes, achieve bandwidth   96347 kbps with   3% CPU load
13:19:51 Sent/received 8192/8192 packets in  667 ms, packet size is  980 bytes, achieve bandwidth   96275 kbps with   3% CPU load
13:19:51 Sent/received 8192/8192 packets in  653 ms, packet size is  960 bytes, achieve bandwidth   96200 kbps with   3% CPU load
13:19:52 Sent/received 8192/8192 packets in  640 ms, packet size is  940 bytes, achieve bandwidth   96122 kbps with   3% CPU load
13:19:53 Sent/received 8192/8192 packets in  627 ms, packet size is  920 bytes, achieve bandwidth   96041 kbps with   3% CPU load
13:19:54 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:19:54 Sent/received 8192/8192 packets in  601 ms, packet size is  880 bytes, achieve bandwidth   95868 kbps with   3% CPU load
13:19:55 Sent/received 8192/8192 packets in  588 ms, packet size is  860 bytes, achieve bandwidth   95776 kbps with   3% CPU load
13:19:55 Sent/received 8192/8192 packets in  575 ms, packet size is  840 bytes, achieve bandwidth   95680 kbps with   3% CPU load
13:19:56 Sent/received 8192/8192 packets in  562 ms, packet size is  820 bytes, achieve bandwidth   95579 kbps with   3% CPU load
13:19:57 Sent/received 8192/8192 packets in  549 ms, packet size is  800 bytes, achieve bandwidth   95473 kbps with   3% CPU load
13:19:57 Sent/received 8192/8192 packets in  536 ms, packet size is  780 bytes, achieve bandwidth   95362 kbps with   3% CPU load
13:19:58 Sent/received 8192/8192 packets in  522 ms, packet size is  760 bytes, achieve bandwidth   95246 kbps with   3% CPU load
13:19:58 Sent/received 8192/8192 packets in  509 ms, packet size is  740 bytes, achieve bandwidth   95123 kbps with   3% CPU load
13:19:59 Sent/received 8192/8192 packets in  496 ms, packet size is  720 bytes, achieve bandwidth   94994 kbps with   3% CPU load
13:20:00 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   4% CPU load
13:20:00 Sent/received 8192/8192 packets in  470 ms, packet size is  680 bytes, achieve bandwidth   94715 kbps with   4% CPU load
13:20:01 Sent/received 8192/8192 packets in  457 ms, packet size is  660 bytes, achieve bandwidth   94563 kbps with   4% CPU load
13:20:01 Sent/received 8192/8192 packets in  444 ms, packet size is  640 bytes, achieve bandwidth   94403 kbps with   4% CPU load
13:20:02 Sent/received 8192/8192 packets in  431 ms, packet size is  620 bytes, achieve bandwidth   94232 kbps with   4% CPU load
13:20:02 Sent/received 8192/8192 packets in  418 ms, packet size is  600 bytes, achieve bandwidth   94051 kbps with   4% CPU load
13:20:02 Sent/received 8192/8192 packets in  404 ms, packet size is  580 bytes, achieve bandwidth   93859 kbps with   4% CPU load
13:20:03 Sent/received 8192/8192 packets in  391 ms, packet size is  560 bytes, achieve bandwidth   93653 kbps with   4% CPU load
13:20:03 Sent/received 8192/8192 packets in  378 ms, packet size is  540 bytes, achieve bandwidth   93433 kbps with   4% CPU load
13:20:04 Sent/received 8192/8192 packets in  365 ms, packet size is  520 bytes, achieve bandwidth   93197 kbps with   5% CPU load
13:20:04 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:20:05 Sent/received 8192/8192 packets in  339 ms, packet size is  480 bytes, achieve bandwidth   92671 kbps with   5% CPU load
13:20:05 Sent/received 8192/8192 packets in  326 ms, packet size is  460 bytes, achieve bandwidth   92377 kbps with   5% CPU load
13:20:05 Sent/received 8192/8192 packets in  313 ms, packet size is  440 bytes, achieve bandwidth   92057 kbps with   5% CPU load
13:20:06 Sent/received 8192/8192 packets in  300 ms, packet size is  420 bytes, achieve bandwidth   91710 kbps with   5% CPU load
13:20:06 Sent/received 8192/8192 packets in  287 ms, packet size is  400 bytes, achieve bandwidth   91331 kbps with   6% CPU load
13:20:06 Sent/received 8192/8192 packets in  273 ms, packet size is  380 bytes, achieve bandwidth   90916 kbps with   6% CPU load
13:20:07 Sent/received 8192/8192 packets in  260 ms, packet size is  360 bytes, achieve bandwidth   90459 kbps with   6% CPU load
13:20:07 Sent/received 8192/8192 packets in  247 ms, packet size is  340 bytes, achieve bandwidth   89954 kbps with   6% CPU load
13:20:07 Sent/received 8192/8192 packets in  234 ms, packet size is  320 bytes, achieve bandwidth   89392 kbps with   7% CPU load
13:20:08 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:20:08 Sent/received 8192/8192 packets in  208 ms, packet size is  280 bytes, achieve bandwidth   88057 kbps with   8% CPU load
13:20:08 Sent/received 8192/8192 packets in  195 ms, packet size is  260 bytes, achieve bandwidth   87255 kbps with   8% CPU load
13:20:09 Sent/received 8192/8192 packets in  182 ms, packet size is  240 bytes, achieve bandwidth   86337 kbps with   9% CPU load
13:20:09 Sent/received 8192/8192 packets in  169 ms, packet size is  220 bytes, achieve bandwidth   85278 kbps with   9% CPU load
13:20:10 Sent/received 8192/8192 packets in  155 ms, packet size is  200 bytes, achieve bandwidth   84040 kbps with  10% CPU load
13:20:10 Sent/received 8192/8192 packets in  142 ms, packet size is  180 bytes, achieve bandwidth   82575 kbps with  11% CPU load
13:20:10 Sent/received 8192/8192 packets in  129 ms, packet size is  160 bytes, achieve bandwidth   80814 kbps with  12% CPU load
13:20:28 Calling EMAC_open()
13:20:28 Waiting for link...
13:20:29 Link Status  : 1000Mb/s Full Duplex RGMII on PHY number 0
13:20:29 Packets Held : 32-RX  0-TX
13:20:29 
13:20:29 Starting packet transfer...
13:20:29 Interrupt Pacing: 0 micro second, init CPU load 100%
13:20:29 Sent/received 8192/8192 packets in  103 ms, packet size is 1500 bytes, achieve bandwidth  951844 kbps with  85% CPU load
13:20:29 Sent/received 8192/8192 packets in   95 ms, packet size is 1400 bytes, achieve bandwidth  960195 kbps with  16% CPU load
13:20:30 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971519 kbps with  17% CPU load
13:20:30 Sent/received 8192/8192 packets in   81 ms, packet size is 1200 bytes, achieve bandwidth  969223 kbps with  19% CPU load
13:20:30 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966524 kbps with  20% CPU load
13:20:30 Sent/received 8192/8192 packets in   68 ms, packet size is 1000 bytes, achieve bandwidth  963304 kbps with  22% CPU load
13:20:30 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959400 kbps with  24% CPU load
13:20:30 Sent/received 8192/8192 packets in   54 ms, packet size is  800 bytes, achieve bandwidth  954561 kbps with  27% CPU load
13:20:31 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948413 kbps with  25% CPU load
13:20:31 Sent/received 8192/8192 packets in   41 ms, packet size is  600 bytes, achieve bandwidth  940339 kbps with  36% CPU load
13:20:31 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929260 kbps with  42% CPU load
13:20:31 Sent/received 8192/8192 packets in   28 ms, packet size is  400 bytes, achieve bandwidth  913126 kbps with  52% CPU load
13:20:31 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887447 kbps with  66% CPU load
13:20:31 Sent/received 8192/8192 packets in   15 ms, packet size is  200 bytes, achieve bandwidth  840182 kbps with  77% CPU load
13:20:31 Sent/received 8192/8192 packets in   12 ms, packet size is  100 bytes, achieve bandwidth  516906 kbps with 100% CPU load
13:20:31 Interrupt Pacing: 5 micro second, init CPU load 100%
13:20:32 Sent/received 8192/8192 packets in  103 ms, packet size is 1500 bytes, achieve bandwidth  951845 kbps with  22% CPU load
13:20:32 Sent/received 8192/8192 packets in   95 ms, packet size is 1400 bytes, achieve bandwidth  960195 kbps with  16% CPU load
13:20:32 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971518 kbps with  16% CPU load
13:20:32 Sent/received 8192/8192 packets in   81 ms, packet size is 1200 bytes, achieve bandwidth  969222 kbps with  17% CPU load
13:20:32 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966514 kbps with  19% CPU load
13:20:32 Sent/received 8192/8192 packets in   68 ms, packet size is 1000 bytes, achieve bandwidth  963300 kbps with 13:20:33 Sent/received 8192/8192 packets in  771 ms, packet size is 1140 bytes, achieve bandwidth   96782 kbps with   2% CPU load
13:20:34 Sent/received 8192/8192 packets in  758 ms, packet size is 1120 bytes, achieve bandwidth   96726 kbps with   2% CPU load
13:20:34 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:20:35 Sent/received 8192/8192 packets in  732 ms, packet size is 1080 bytes, achieve bandwidth   96609 kbps with   3% CPU load
13:20:36 Sent/received 8192/8192 packets in  719 ms, packet size is 1060 bytes, achieve bandwidth   96547 kbps with   3% CPU load
13:20:37 Sent/received 8192/8192 packets in  706 ms, packet size is 1040 bytes, achieve bandwidth   96483 kbps with   3% CPU load
13:20:38 Sent/received 8192/8192 packets in  693 ms, packet size is 1020 bytes, achieve bandwidth   96416 kbps with   3% CPU load
13:20:39 Sent/received 8192/8192 packets in  680 ms, packet size is 1000 bytes, achieve bandwidth   96347 kbps with   3% CPU load
13:20:39 Sent/received 8192/8192 packets in  667 ms, packet size is  980 bytes, achieve bandwidth   96275 kbps with   3% CPU load
13:20:40 Sent/received 8192/8192 packets in  653 ms, packet size is  960 bytes, achieve bandwidth   96200 kbps with   3% CPU load
13:20:41 Sent/received 8192/8192 packets in  640 ms, packet size is  940 bytes, achieve bandwidth   96122 kbps with   3% CPU load
13:20:42 Sent/received 8192/8192 packets in  627 ms, packet size is  920 bytes, achieve bandwidth   96041 kbps with   3% CPU load
13:20:42 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:20:43 Sent/received 8192/8192 packets in  601 ms, packet size is  880 bytes, achieve bandwidth   95868 kbps with   3% CPU load
13:20:44 Sent/received 8192/8192 packets in  588 ms, packet size is  860 bytes, achieve bandwidth   95776 kbps with   3% CPU load
13:20:44 Sent/received 8192/8192 packets in  575 ms, packet size is  840 bytes, achieve bandwidth   95680 kbps with   3% CPU load
13:20:45 Sent/received 8192/8192 packets in  562 ms, packet size is  820 bytes, achieve bandwidth   95579 kbps with   3% CPU load
13:20:46 Sent/received 8192/8192 packets in  549 ms, packet size is  800 bytes, achieve bandwidth   95473 kbps with   3% CPU load
13:20:46 Sent/received 8192/8192 packets in  536 ms, packet size is  780 bytes, achieve bandwidth   95362 kbps with   3% CPU load
13:20:47 Sent/received 8192/8192 packets in  522 ms, packet size is  760 bytes, achieve bandwidth   95246 kbps with   3% CPU load
13:20:48 Sent/received 8192/8192 packets in  509 ms, packet size is  740 bytes, achieve bandwidth   95123 kbps with   3% CPU load
13:20:48 Sent/received 8192/8192 packets in  496 ms, packet size is  720 bytes, achieve bandwidth   94994 kbps with   3% CPU load
13:20:49 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   4% CPU load
13:20:49 Sent/received 8192/8192 packets in  470 ms, packet size is  680 bytes, achieve bandwidth   94715 kbps with   4% CPU load
13:20:50 Sent/received 8192/8192 packets in  457 ms, packet size is  660 bytes, achieve bandwidth   94563 kbps with   4% CPU load
13:20:50 Sent/received 8192/8192 packets in  444 ms, packet size is  640 bytes, achieve bandwidth   94403 kbps with   4% CPU load
13:20:51 Sent/received 8192/8192 packets in  431 ms, packet size is  620 bytes, achieve bandwidth   94232 kbps with   4% CPU load
13:20:51 Sent/received 8192/8192 packets in  418 ms, packet size is  600 bytes, achieve bandwidth   94051 kbps with   4% CPU load
13:20:52 Sent/received 8192/8192 packets in  404 ms, packet size is  580 bytes, achieve bandwidth   93859 kbps with   4% CPU load
13:20:52 Sent/received 8192/8192 packets in  391 ms, packet size is  560 bytes, achieve bandwidth   93653 kbps with   4% CPU load
13:20:53 Sent/received 8192/8192 packets in  378 ms, packet size is  540 bytes, achieve bandwidth   93433 kbps with   4% CPU load
13:20:53 Sent/received 8192/8192 packets in  365 ms, packet size is  520 bytes, achieve bandwidth   93197 kbps with   5% CPU load
13:20:53 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:20:54 Sent/received 8192/8192 packets in  339 ms, packet size is  480 bytes, achieve bandwidth   92671 kbps with   5% CPU load
13:20:54 Sent/received 8192/8192 packets in  326 ms, packet size is  460 bytes, achieve bandwidth   92377 kbps with   5% CPU load
13:20:55 Sent/received 8192/8192 packets in  313 ms, packet size is  440 bytes, achieve bandwidth   92057 kbps with   5% CPU load
13:20:55 Sent/received 8192/8192 packets in  300 ms, packet size is  420 bytes, achieve bandwidth   91710 kbps with   5% CPU load
13:20:55 Sent/received 8192/8192 packets in  287 ms, packet size is  400 bytes, achieve bandwidth   91331 kbps with   6% CPU load
13:20:56 Sent/received 8192/8192 packets in  273 ms, packet size is  380 bytes, achieve bandwidth   90916 kbps with   6% CPU load
13:20:56 Sent/received 8192/8192 packets in  260 ms, packet size is  360 bytes, achieve bandwidth   90459 kbps with   6% CPU load
13:20:56 Sent/received 8192/8192 packets in  247 ms, packet size is  340 bytes, achieve bandwidth   89954 kbps with   6% CPU load
13:20:57 Sent/received 8192/8192 packets in  234 ms, packet size is  320 bytes, achieve bandwidth   89392 kbps with   7% CPU load
13:20:57 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:20:57 Sent/received 8192/8192 packets in  208 ms, packet size is  280 bytes, achieve bandwidth   88057 kbps with   8% CPU load
13:20:57 Sent/received 8192/8192 packets in  195 ms, packet size is  260 bytes, achieve bandwidth   87255 kbps with   8% CPU load
13:20:58 Sent/received 8192/8192 packets in  182 ms, packet size is  240 bytes, achieve bandwidth   86337 kbps with   9% CPU load
13:20:58 Sent/received 8192/8192 packets in  169 ms, packet size is  220 bytes, achieve bandwidth   85278 kbps with   9% CPU load
13:20:58 Sent/received 8192/8192 packets in  155 ms, packet size is  200 bytes, achieve bandwidth   84040 kbps with  10% CPU load
13:20:58 Sent/received 8192/8192 packets in  142 ms, packet size is  180 bytes, achieve bandwidth   82575 kbps with  11% CPU load
13:20:59 Sent/received 8192/8192 packets in  129 ms, packet size is  160 bytes, achieve bandwidth   80814 kbps with  12% CPU load
13:20:59 Sent/received 8192/8192 packets in  116 ms, packet size is  140 bytes, achieve bandwidth   78657 kbps with  13% CPU load
13:20:59 Sent/received 8192/8192 packets in  103 ms, packet size is  120 bytes, achieve bandwidth   75954 kbps with  15% CPU load
13:20:59 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  16% CPU load
13:20:59 Sent/received 8192/8192 packets in   77 ms, packet size is   80 bytes, achieve bandwidth   67801 kbps with  18% CPU load
13:20:59 Sent/received 8192/8192 packets in   64 ms, packet size is   60 bytes, achieve bandwidth   61228 kbps with  20% CPU load
13:20:59 Interrupt Pacing: 10 micro second, init CPU load 100%
13:21:01 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:21:02 Sent/received 8192/8192 packets in  994 ms, packet size is 1480 bytes, achieve bandwidth   97505 kbps with   2% CPU load
13:21:03 Sent/received 8192/8192 packets in  981 ms, packet size is 1460 bytes, achieve bandwidth   97471 kbps with   2% CPU load
13:21:04 Sent/received 8192/8192 packets in  968 ms, packet size is 1440 bytes, achieve bandwidth   97437 kbps with   2% CPU load
13:21:05 Sent/received 8192/8192 packets in  955 ms, packet size is 1420 bytes, achieve bandwidth   97402 kbps with   2% CPU load
13:21:06 Sent/received 8192/8192 packets in  942 ms, packet size is 1400 bytes, achieve bandwidth   97365 kbps with   2% CPU load
13:21:07 Sent/received 8192/8192 packets in  929 ms, packet size is 1380 bytes, achieve bandwidth   97328 kbps with   2% CPU load
13:21:08 Sent/received 8192/8192 packets in  916 ms, packet size is 1360 bytes, achieve bandwidth   97290 kbps with   2% CPU load
13:21:09 Sent/received 8192/8192 packets in  903 ms, packet size is 1340 bytes, achieve bandwidth   97250 kbps with   2% CPU load
13:21:10 Sent/received 8192/8192 packets in  889 ms, packet size is 1320 bytes, achieve bandwidth   97210 kbps with   2% CPU load
13:21:11 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:21:12 Sent/received 8192/8192 packets in  863 ms, packet size is 1280 bytes, achieve bandwidth   97125 kbps with   2% CPU load
13:21:13 Sent/received 8192/8192 packets in  850 ms, packet size is 1260 bytes, achieve bandwidth   97080 kbps with   2% CPU load
13:21:13 Sent/received 8192/8192 packets in  837 ms, packet size is 1240 bytes, achieve bandwidth   97034 kbps with   2% CPU load
13:21:15 Sent/received 8192/8192 packets in  824 ms, packet size is 1220 bytes, achieve bandwidth   96987 kbps with   2% CPU load
13:21:18 Sent/received 8192/8192 packets in  811 ms, packet size is 1200 bytes, achieve bandwidth   96938 kbps with   2% CPU load
13:21:21 Sent/received 8192/8192 packets in  798 ms, packet si13:23:06 Calling EMAC_open()
13:23:07 Waiting for link...
13:23:07 Link Status  : 1000Mb/s Full Duplex RGMII on PHY number 0
13:23:07 Packets Held : 32-RX  0-TX
13:23:07 
13:23:07 Starting packet transfer...
13:23:08 Interrupt Pacing: 0 micro second, init CPU load 100%
13:23:08 Sent/received 8192/8192 packets in  103 ms, p13:31:50 Calling EMAC_open()
13:31:50 Waiting for link...
13:31:50 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
13:31:50 Packets Held : 32-RX  0-TX
13:31:50 
13:31:50 Starting packet transfer...
13:31:50 Interrupt Pacing: 0 micro second, init CPU load 100%
13:31:52 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with  32% CPU load
13:31:52 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:31:53 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:31:54 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:31:55 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:31:55 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:31:55 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:31:55 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  16% CPU load
13:31:55 Interrupt Pacing: 5 micro second, init CPU load 100%
13:31:57 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:31:58 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:31:58 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:31:59 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:32:00 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:32:00 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:32:00 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:32:00 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  16% CPU load
13:32:01 Interrupt Pacing: 10 micro second, init CPU load 100%
13:32:02 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:32:03 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:32:03 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:32:04 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:32:05 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:32:05 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:32:05 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:32:05 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72466 kbps with  14% CPU load
13:32:06 Interrupt Pacing: 15 micro second, init CPU load 100%
13:32:07 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:32:08 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:32:08 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:32:09 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:32:10 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:32:10 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:32:10 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:32:11 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72465 kbps with  11% CPU load
13:32:11 Interrupt Pacing: 20 micro second, init CPU load 100%
13:32:12 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:32:13 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:32:14 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:32:14 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:32:15 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:32:15 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:32:16 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   6% CPU load
13:32:16 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72462 kbps with  10% CPU load
13:32:16 Interrupt Pacing: 25 micro second, init CPU load 100%
13:32:17 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:32:18 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:32:19 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:32:19 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:32:20 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:32:20 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   4% CPU load
13:32:21 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   6% CPU load
13:32:21 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72464 kbps with  10% CPU load
13:32:21 Calling EMAC_close()
13:38:33 Calling EMAC_open()
13:38:33 Waiting for link...
13:38:34 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
13:38:34 Packets Held : 32-RX  0-TX
13:38:34 
13:38:34 Starting packet transfer...
13:38:34 Interrupt Pacing: 0 micro second, init CPU load 100%
13:38:35 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with  31% CPU load
13:38:36 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:38:37 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:38:38 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:38:38 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   3% CPU load
13:38:39 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:38:39 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:38:39 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  16% CPU load
13:38:39 Interrupt Pacing: 5 micro second, init CPU load 100%
13:38:40 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:38:41 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:38:42 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:38:43 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:38:43 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   3% CPU load
13:38:44 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:38:44 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:38:44 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72469 kbps with  16% CPU load
13:38:45 Interrupt Pacing: 10 micro second, init CPU load 100%
13:38:46 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:38:47 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:38:48 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:38:48 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:38:49 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   3% CPU load
13:38:49 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:38:50 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:38:50 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72466 kbps with  14% CPU load
13:38:50 Interrupt Pacing: 15 micro second, init CPU load 100%
13:38:51 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:38:52 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:38:53 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:38:54 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:38:54 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   3% CPU load
13:38:55 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:38:55 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:38:55 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72465 kbps with  11% CPU load
13:38:56 Interrupt Pacing: 20 micro second, init CPU load 100%
13:38:57 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:38:58 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:38:59 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:38:59 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:39:00 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   3% CPU load
13:39:00 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:39:01 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   6% CPU load
13:39:01 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72462 kbps with  10% CPU load
13:39:01 Interrupt Pacing: 25 micro second, init CPU load 100%
13:39:02 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:39:03 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:39:04 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:39:05 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:39:05 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   3% CPU load
13:39:06 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   4% CPU load
13:39:06 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   6% CPU load
13:39:06 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72464 kbps with  10% CPU load
13:39:06 Calling EMAC_close()
13:45:07 Calling EMAC_open()
13:45:07 Waiting for link...
13:45:07 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
13:45:07 Packets Held : 32-RX  0-TX
13:45:07 
13:45:07 Starting packet transfer...
13:45:07 Interrupt Pacing: 0 micro second, init CPU load 100%
13:45:09 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with  32% CPU load
13:45:10 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:45:10 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:45:11 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:45:12 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:45:12 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:45:13 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:45:13 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  16% CPU load
13:45:13 Interrupt Pacing: 5 micro second, init CPU load 100%
13:45:14 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:45:15 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:45:16 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:45:17 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:45:17 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:45:18 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:45:18 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:45:18 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  16% CPU load
13:45:18 Interrupt Pacing: 10 micro second, init CPU load 100%
13:45:19 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:45:20 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:45:21 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:45:22 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:45:23 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:45:23 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:45:23 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:45:24 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72466 kbps with  14% CPU load
13:45:24 Interrupt Pacing: 15 micro second, init CPU load 100%
13:45:25 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:45:26 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:45:27 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:45:27 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:45:28 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:45:28 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:45:29 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
13:45:29 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72465 kbps with  11% CPU load
13:45:29 Interrupt Pacing: 20 micro second, init CPU load 100%
13:45:30 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:45:31 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:45:32 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:45:32 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:45:33 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:45:35 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
13:45:35 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   6% CPU load
13:45:35 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72462 kbps with  10% CPU load
13:45:35 Interrupt Pacing: 25 micro second, init CPU load 100%
13:45:36 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
13:45:37 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
13:45:38 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   2% CPU load
13:45:39 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
13:45:40 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   3% CPU load
13:45:40 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   4% CPU load
13:45:41 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   6% CPU load
13:45:41 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72464 kbps with  10% CPU load
13:45:41 Calling EMAC_close()
13:46:25 Calling EMAC_open()
13:46:26 Waiting for link...
13:46:28 Link Status  : No Link MII on PHY number 1
13:46:28 Packets Held : 32-RX  0-TX
13:46:28 
13:46:28 WARNING: No device LINK.
13:46:28 
13:46:28 Starting packet transfer...
13:46:28 Interrupt Pacing: 0 micro second, init CPU load 100%
13:46:29 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with  94% CPU load
13:46:32 ERROR: Timeout waiting for TX/RX
13:46:32 Sent/received 8192/8191 packets in 3048 ms, packet size is 1300 bytes, achieve bandwidth   27942 kbps with   1% CPU load
13:46:32 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644384 kbps with  13% CPU load
13:46:32 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639633 kbps with  16% CPU load
13:46:33 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632308 kbps with  17% CPU load
13:46:33 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619539 kbps with  28% CPU load
13:46:33 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591668 kbps with  44% CPU load
13:46:33 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  483020 kbps with 100% CPU load
13:46:33 Interrupt Pacing: 5 micro second, init CPU load 100%
13:46:33 EMAC_sendPacket() returned error 00000004
13:46:33 Sent/received   98/   1 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth  195147 kbps with 100% CPU load
13:46:34 EMAC_sendPacket() returned error 00000004
13:46:34 Sent/received   99/  35 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5702200 kbps with 100% CPU load
13:46:34 EMAC_sendPacket() returned error 00000004
13:46:34 Sent/received  100/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4570101 kbps with 100% CPU load
13:46:34 EMAC_sendPacket() returned error 00000004
13:46:34 Sent/received  100/  35 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3773584 kbps with 100% CPU load
13:46:34 EMAC_sendPacket() returned error 00000004
13:46:35 Sent/received  102/  37 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3060425 kbps with 100% CPU load
13:46:35 EMAC_sendPacket() returned error 00000004
13:46:35 Sent/received  105/  39 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2202301 kbps with 100% CPU load
13:46:35 EMAC_sendPacket() returned error 00000004
13:46:35 Sent/received  111/  43 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1356984 kbps with 100% CPU load
13:46:35 EMAC_sendPacket() returned error 00000004
13:46:35 Sent/received  148/  75 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  582365 kbps with 100% CPU load
13:46:35 Interrupt Pacing: 10 micro second, init CPU load 100%
13:46:36 EMAC_sendPacket() returned error 00000004
13:46:36 Sent/received   98/  41 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 7840762 kbps with 100% CPU load
13:46:36 EMAC_sendPacket() returned error 00000004
13:46:36 Sent/received   99/  35 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5744586 kbps with 100% CPU load
13:46:36 EMAC_sendPacket() returned error 00000004
13:46:36 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4652030 kbps with 100% CPU load
13:46:36 EMAC_sendPacket() returned error 00000004
13:46:36 Sent/received  100/  36 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3969189 kbps with 100% CPU load
13:46:37 EMAC_sendPacket() returned error 00000004
13:46:37 Sent/received  101/  36 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3058530 kbps with 100% CPU load
13:46:37 EMAC_sendPacket() returned error 00000004
13:46:37 Sent/received  103/  39 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2322119 kbps with 100% CPU load
13:46:37 EMAC_sendPacket() returned error 00000004
13:46:37 Sent/received  109/  41 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1386071 kbps with 100% CPU load
13:46:37 EMAC_sendPacket() returned error 00000004
13:46:38 Sent/received  132/  59 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  541912 kbps with 100% CPU load
13:46:38 Interrupt Pacing: 15 micro second, init CPU load 100%
13:46:38 EMAC_sendPacket() returned error 00000004
13:46:38 Sent/received   98/  41 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 7842012 kbps with 100% CPU load
13:46:38 EMAC_sendPacket() returned error 00000004
13:46:38 Sent/received   99/  35 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5771273 kbps with 100% CPU load
13:46:38 EMAC_sendPacket() returned error 00000004
13:46:38 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4745289 kbps with 100% CPU load
13:46:38 EMAC_sendPacket() returned error 00000004
13:46:38 Sent/received  100/  34 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3856636 kbps with 100% CPU load
13:46:39 EMAC_sendPacket() returned error 00000004
13:46:39 Sent/received  101/  35 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3054767 kbps with 100% CPU load
13:46:39 EMAC_sendPacket() returned error 00000004
13:46:39 Sent/received  103/  37 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2257956 kbps with 100% CPU load
13:46:39 EMAC_sendPacket() returned error 00000004
13:46:39 Sent/received  108/  40 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1369081 kbps with 100% CPU load
13:46:39 EMAC_sendPacket() returned error 00000004
13:46:40 Sent/received  119/  48 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  494450 kbps with 100% CPU load
13:46:40 Interrupt Pacing: 20 micro second, init CPU load 100%
13:46:40 EMAC_sendPacket() returned error 00000004
13:46:40 Sent/received   98/  44 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 8517640 kbps with 100% CPU load
13:46:40 EMAC_sendPacket() returned error 00000004
13:46:40 Sent/received   98/  33 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5573419 kbps with 100% CPU load
13:46:40 EMAC_sendPacket() returned error 00000004
13:46:40 Sent/received   98/  33 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4629806 kbps with 100% CPU load
13:46:40 EMAC_sendPacket() returned error 00000004
13:46:41 Sent/received   99/  35 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3985891 kbps with 100% CPU load
13:46:41 EMAC_sendPacket() returned error 00000004
13:46:41 Sent/received  100/  36 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3153498 kbps with 100% CPU load
13:46:41 EMAC_sendPacket() returned error 00000004
13:46:41 Sent/received  101/  37 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2282084 kbps with 100% CPU load
13:46:41 EMAC_sendPacket() returned error 00000004
13:46:41 Sent/received  105/  40 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1418879 kbps with 100% CPU load
13:46:41 EMAC_sendPacket() returned error 00000004
13:46:42 Sent/received   98/  39 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  473948 kbps with 100% CPU load
13:46:42 Interrupt Pacing: 25 micro second, init CPU load 100%
13:46:42 EMAC_sendPacket() returned error 00000004
13:46:42 Sent/received   98/  46 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 8899063 kbps with 100% CPU load
13:46:42 EMAC_sendPacket() returned error 00000004
13:46:42 Sent/received   98/  33 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5570795 kbps with 100% CPU load
13:46:42 EMAC_sendPacket() returned error 00000004
13:46:42 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4804341 kbps with 100% CPU load
13:46:42 EMAC_sendPacket() returned error 00000004
13:46:42 Sent/received   99/  34 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3926663 kbps with 100% CPU load
13:46:42 EMAC_sendPacket() returned error 00000004
13:46:42 Sent/received  100/  35 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3109235 kbps with 100% CPU load
13:46:42 EMAC_sendPacket() returned error 00000004
13:46:42 Sent/received  102/  36 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2243305 kbps with 100% CPU load
13:46:43 EMAC_sendPacket() returned error 00000004
13:46:43 Sent/received  107/  38 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1363983 kbps with 100% CPU load
13:46:43 EMAC_sendPacket() returned error 00000004
13:46:43 Sent/received   98/  34 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  439361 kbps with 100% CPU load
13:46:43 Calling EMAC_close()
13:48:57 Calling EMAC_open()
13:48:57 Waiting for link...
13:48:59 Link Status  : No Link MII on PHY number 1
13:48:59 Packets Held : 32-RX  0-TX
13:48:59 
13:48:59 WARNING: No device LINK.
13:48:59 
13:48:59 Starting packet transfer...
13:48:59 Interrupt Pacing: 0 micro second, init CPU load 100%
13:49:00 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with  94% CPU load
13:49:00 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  12% CPU load
13:49:00 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644384 kbps with  13% CPU load
13:49:00 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639633 kbps with  16% CPU load
13:49:00 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632307 kbps with  17% CPU load
13:49:00 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619538 kbps with  28% CPU load
13:49:01 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591666 kbps with  44% CPU load
13:49:01 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  483019 kbps with 100% CPU load
13:49:01 Interrupt Pacing: 5 micro second, init CPU load 100%
13:49:01 EMAC_sendPacket() returned error 00000004
13:49:01 Sent/received   98/   1 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth  194896 kbps with 100% CPU load
13:49:01 EMAC_sendPacket() returned error 00000004
13:49:01 Sent/received   99/  35 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5704792 kbps with 100% CPU load
13:49:01 EMAC_sendPacket() returned error 00000004
13:49:01 Sent/received  100/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4567869 kbps with 100% CPU load
13:49:01 EMAC_sendPacket() returned error 00000004
13:49:01 Sent/received  100/  35 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3773867 kbps with 100% CPU load
13:49:01 EMAC_sendPacket() returned error 00000004
13:49:01 Sent/received  102/  37 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3061284 kbps with 100% CPU load
13:49:01 EMAC_sendPacket() returned error 00000004
13:49:01 Sent/received  105/  39 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2203389 kbps with 100% CPU load
13:49:01 EMAC_sendPacket() returned error 00000004
13:49:02 Sent/received  111/  43 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1357448 kbps with 100% CPU load
13:49:02 EMAC_sendPacket() returned error 00000004
13:49:02 Sent/received  148/  75 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  582281 kbps with 100% CPU load
13:49:02 Interrupt Pacing: 10 micro second, init CPU load 100%
13:49:02 EMAC_sendPacket() returned error 00000004
13:49:02 Sent/received   98/  41 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 7837514 kbps with 100% CPU load
13:49:02 EMAC_sendPacket() returned error 00000004
13:49:02 Sent/received   99/  35 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5736619 kbps with 100% CPU load
13:49:02 EMAC_sendPacket() returned error 00000004
13:49:02 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4651885 kbps with 100% CPU load
13:49:02 EMAC_sendPacket() returned error 00000004
13:49:02 Sent/received  100/  36 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3968035 kbps with 100% CPU load
13:49:02 EMAC_sendPacket() returned error 00000004
13:49:02 Sent/received  101/  36 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3056027 kbps with 100% CPU load
13:49:02 EMAC_sendPacket() returned error 00000004
13:49:02 Sent/received  103/  39 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2320945 kbps with 100% CPU load
13:49:03 EMAC_sendPacket() returned error 00000004
13:49:03 Sent/received  109/  41 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1386384 kbps with 100% CPU load
13:49:03 EMAC_sendPacket() returned error 00000004
13:49:03 Sent/received  132/  59 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  542223 kbps with 100% CPU load
13:49:03 Interrupt Pacing: 15 micro second, init CPU load 100%
13:49:03 EMAC_sendPacket() returned error 00000004
13:49:03 Sent/received   98/  41 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 7838888 kbps with 100% CPU load
13:49:03 EMAC_sendPacket() returned error 00000004
13:49:03 Sent/received   99/  35 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5770175 kbps with 100% CPU load
13:49:03 EMAC_sendPacket() returned error 00000004
13:49:03 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4746644 kbps with 100% CPU load
13:49:03 EMAC_sendPacket() returned error 00000004
13:49:03 Sent/received  100/  34 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3857487 kbps with 100% CPU load
13:49:03 EMAC_sendPacket() returned error 00000004
13:49:03 Sent/received  101/  35 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3053768 kbps with 100% CPU load
13:49:04 EMAC_sendPacket() returned error 00000004
13:49:04 Sent/received  103/  37 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2257164 kbps with 100% CPU load
13:49:04 EMAC_sendPacket() returned error 00000004
13:49:04 Sent/received  108/  40 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1369823 kbps with 100% CPU load
13:49:04 EMAC_sendPacket() returned error 00000004
13:49:04 Sent/received  119/  48 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  494552 kbps with 100% CPU load
13:49:04 Interrupt Pacing: 20 micro second, init CPU load 100%
13:49:04 EMAC_sendPacket() returned error 00000004
13:49:04 Sent/received   98/  44 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 8518877 kbps with 100% CPU load
13:49:04 EMAC_sendPacket() returned error 00000004
13:51:08 Calling EMAC_open()
13:51:08 Waiting for link...
13:52:16 Calling EMAC_open()
13:52:16 Waiting for link...
13:52:18 Link Status  : No Link MII on PHY number 1
13:52:19 Packets Held : 32-RX  0-TX
13:52:19 
13:52:19 WARNING: No device LINK.
13:52:19 
13:52:19 Starting packet transfer...
13:52:19 Interrupt Pacing: 0 micro second, init CPU load 100%
13:52:19 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with  94% CPU load
13:52:20 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  12% CPU load
13:52:23 ERROR: Timeout waiting for TX/RX
13:52:23 Sent/received 8192/8187 packets in 3017 ms, packet size is 1100 bytes, achieve bandwidth   23879 kbps with   1% CPU load
13:52:23 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639633 kbps with  16% CPU load
13:52:23 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632308 kbps with  17% CPU load
13:52:24 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619538 kbps with  28% CPU load
13:52:24 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591667 kbps with  44% CPU load
13:52:24 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  478308 kbps with 100% CPU load
13:52:24 Interrupt Pacing: 5 micro second, init CPU load 100%
13:52:24 EMAC_sendPacket() returned error 00000004
13:52:24 Sent/received   98/   1 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth  194590 kbps with 100% CPU load
13:52:25 EMAC_sendPacket() returned error 00000004
13:52:25 Sent/received   99/  35 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5695687 kbps with 100% CPU load
13:52:25 EMAC_sendPacket() returned error 00000004
13:52:25 Sent/received  100/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4559168 kbps with 100% CPU load
13:52:25 EMAC_sendPacket() returned error 00000004
13:52:25 Sent/received  100/  35 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3769520 kbps with 100% CPU load
13:52:25 EMAC_sendPacket() returned error 00000004
13:52:26 Sent/received  102/  37 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3053705 kbps with 100% CPU load
13:52:26 EMAC_sendPacket() returned error 00000004
13:52:26 Sent/received  105/  39 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2195080 kbps with 100% CPU load
13:52:26 EMAC_sendPacket() returned error 00000004
13:52:26 Sent/received  113/  45 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1399326 kbps with 100% CPU load
13:52:26 EMAC_sendPacket() returned error 00000004
13:52:27 Sent/received  148/  73 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  566127 kbps with 100% CPU load
13:52:27 Interrupt Pacing: 10 micro second, init CPU load 100%
13:52:27 EMAC_sendPacket() returned error 00000004
13:52:27 Sent/received   99/  42 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 7948649 kbps with 100% CPU load
13:52:27 EMAC_sendPacket() returned error 00000004
13:52:27 Sent/received   99/  34 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5561934 kbps with 100% CPU load
13:52:28 EMAC_sendPacket() returned error 00000004
13:52:28 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4644448 kbps with 100% CPU load
13:52:28 EMAC_sendPacket() returned error 00000004
13:52:28 Sent/received  100/  36 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3961848 kbps with 100% CPU load
13:52:28 EMAC_sendPacket() returned error 00000004
13:52:28 Sent/received  101/  36 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3050524 kbps with 100% CPU load
13:52:28 EMAC_sendPacket() returned error 00000004
13:52:29 Sent/received  103/  39 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2319702 kbps with 100% CPU load
13:52:29 EMAC_sendPacket() returned error 00000004
13:52:29 Sent/received  109/  41 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1384180 kbps with 100% CPU load
13:52:29 EMAC_sendPacket() returned error 00000004
13:52:29 Sent/received  132/  60 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  550547 kbps with 100% CPU load
13:52:29 Interrupt Pacing: 15 micro second, init CPU load 100%
13:52:29 EMAC_sendPacket() returned error 00000004
13:52:30 Sent/received   99/  41 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 7762578 kbps with 100% CPU load
13:52:30 EMAC_sendPacket() returned error 00000004
13:52:30 Sent/received   99/  34 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5599721 kbps with 100% CPU load
13:52:30 EMAC_sendPacket() returned error 00000004
13:52:30 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4738450 kbps with 100% CPU load
13:52:30 EMAC_sendPacket() returned error 00000004
13:52:30 Sent/received  100/  34 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3851721 kbps with 100% CPU load
13:52:30 EMAC_sendPacket() returned error 00000004
13:52:31 Sent/received  101/  35 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3051676 kbps with 100% CPU load
13:52:31 EMAC_sendPacket() returned error 00000004
13:52:31 Sent/received  103/  37 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2253452 kbps with 100% CPU load
13:52:31 EMAC_sendPacket() returned error 00000004
13:52:31 Sent/received  108/  40 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1368574 kbps with 100% CPU load
13:52:31 EMAC_sendPacket() returned error 00000004
13:52:31 Sent/received  119/  48 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  493877 kbps with 100% CPU load
13:52:31 Interrupt Pacing: 20 micro second, init CPU load 100%
13:52:32 EMAC_sendPacket() returned error 00000004
13:52:32 Sent/received   98/  44 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 8500909 kbps with 100% CPU load
13:52:32 EMAC_sendPacket() returned error 00000004
13:52:32 Sent/received   98/  33 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5559605 kbps with 100% CPU load
13:52:32 EMAC_sendPacket() returned error 00000004
13:52:32 Sent/received   98/  33 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4618320 kbps with 100% CPU load
13:52:32 EMAC_sendPacket() returned error 00000004
13:52:33 Sent/received   99/  35 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3978151 kbps with 100% CPU load
13:52:33 EMAC_sendPacket() returned error 00000004
13:52:33 Sent/received  100/  36 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3146705 kbps with 100% CPU load
13:52:33 EMAC_sendPacket() returned error 00000004
13:52:33 Sent/received  101/  37 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2277203 kbps with 100% CPU load
13:52:33 EMAC_sendPacket() returned error 00000004
13:52:33 Sent/received  105/  40 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1417350 kbps with 100% CPU load
13:52:33 EMAC_sendPacket() returned error 00000004
13:52:33 Sent/received   98/  39 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  472798 kbps with 100% CPU load
13:52:34 Interrupt Pacing: 25 micro second, init CPU load 100%
13:52:34 EMAC_sendPacket() returned error 00000004
13:52:34 Sent/received   98/  46 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 8880451 kbps with 100% CPU load
13:52:34 EMAC_sendPacket() returned error 00000004
13:52:34 Sent/received   98/  33 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5559335 kbps with 100% CPU load
13:52:34 EMAC_sendPacket() returned error 00000004
13:52:34 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4789805 kbps with 100% CPU load
13:52:34 EMAC_sendPacket() returned error 00000004
13:52:34 Sent/received   99/  34 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3920249 kbps with 100% CPU load
13:52:34 EMAC_sendPacket() returned error 00000004
13:52:34 Sent/received  100/  35 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3102984 kbps with 100% CPU load
13:52:34 EMAC_sendPacket() returned error 00000004
13:52:34 Sent/received  102/  36 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2242746 kbps with 100% CPU load
13:52:35 EMAC_sendPacket() returned error 00000004
13:52:35 Sent/received  107/  38 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1362434 kbps with 100% CPU load
13:52:35 EMAC_sendPacket() returned error 00000004
13:52:35 Sent/received   98/  34 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  438419 kbps with 100% CPU load
13:52:35 Calling EMAC_close()
13:53:47 Calling EMAC_open()
13:53:47 Waiting for link...
13:53:49 Link Status  : No Link MII on PHY number 1
13:53:49 Packets Held : 32-RX  0-TX
13:53:49 
13:53:49 WARNING: No device LINK.
13:53:49 
13:53:49 Starting packet transfer...
13:53:49 Interrupt Pacing: 0 micro second, init CPU load 100%
13:53:49 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650174 kbps with  95% CPU load
13:53:50 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647710 kbps with  25% CPU load
13:53:50 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644379 kbps with  29% CPU load
13:53:50 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639625 kbps with  34% CPU load
13:53:50 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632298 kbps with  33% CPU load
13:53:50 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619527 kbps with  55% CPU load
13:53:50 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591648 kbps with  84% CPU load
13:53:50 Sent/received 8192/8192 packets in   23 ms, packet size is  100 bytes, achieve bandwidth  273158 kbps with 100% CPU load
13:53:50 Interrupt Pacing: 5 micro second, init CPU load 100%
13:53:51 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650174 kbps with  19% CPU load
13:53:51 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647710 kbps with  25% CPU load
13:53:51 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644379 kbps with  29% CPU load
13:53:51 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639626 kbps with  33% CPU load
13:53:51 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632300 kbps with  33% CPU load
13:53:51 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619472 kbps with  43% CPU load
13:53:55 ERROR: Timeout waiting for TX/RX
13:53:55 Sent/received 8192/8190 packets in 3017 ms, packet size is  300 bytes, achieve bandwidth    6513 kbps with   1% CPU load
13:53:55 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482685 kbps with  94% CPU load
13:53:55 Interrupt Pacing: 10 micro second, init CPU load 100%
13:53:55 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650175 kbps with  19% CPU load
13:53:55 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647710 kbps with  23% CPU load
13:53:55 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644378 kbps with  25% CPU load
13:53:56 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639608 kbps with  27% CPU load
13:53:56 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632247 kbps with  30% CPU load
13:53:56 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619441 kbps with  35% CPU load
13:53:56 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591472 kbps with  46% CPU load
13:53:56 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482404 kbps with  87% CPU load
13:53:56 Interrupt Pacing: 15 micro second, init CPU load 100%
13:53:56 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650175 kbps with  19% CPU load
13:53:57 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647692 kbps with  21% CPU load
13:53:57 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644351 kbps with  22% CPU load
13:53:57 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639531 kbps with  24% CPU load
13:53:57 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632192 kbps with  27% CPU load
13:53:57 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619504 kbps with  32% CPU load
13:53:58 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591530 kbps with  43% CPU load
13:53:58 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482029 kbps with  85% CPU load
13:53:58 Interrupt Pacing: 20 micro second, init CPU load 100%
13:53:58 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650089 kbps with  18% CPU load
13:53:58 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647707 kbps with  19% CPU load
13:53:59 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644292 kbps with  20% CPU load
13:53:59 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639516 kbps with  22% CPU load
13:53:59 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632256 kbps with  25% CPU load
13:53:59 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619459 kbps with  30% CPU load
13:53:59 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591418 kbps with  41% CPU load
13:53:59 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  481547 kbps with  84% CPU load
13:53:59 Interrupt Pacing: 25 micro second, init CPU load 100%
13:53:59 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650066 kbps with  17% CPU load
13:54:00 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647669 kbps with  18% CPU load
13:54:00 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644307 kbps with  19% CPU load
13:54:00 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639579 kbps with  21% CPU load
13:54:00 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632265 kbps with  24% CPU load
13:54:00 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619303 kbps with  29% CPU load
13:54:00 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591352 kbps with  40% CPU load
13:54:00 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  481534 kbps with  83% CPU load
13:54:00 Calling EMAC_close()
13:54:58 Calling EMAC_open()
13:54:59 Waiting for link...
13:55:01 Link Status  : No Link MII on PHY number 1
13:55:01 Packets Held : 32-RX  0-TX
13:55:01 
13:55:01 WARNING: No device LINK.
13:55:01 
13:55:02 Starting packet transfer...
13:55:02 Interrupt Pacing: 0 micro second, init CPU load 100%
13:55:18 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with  94% CPU load
13:55:19 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  12% CPU load
13:55:19 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644384 kbps with  13% CPU load
13:55:19 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639633 kbps with  16% CPU load
13:55:19 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632308 kbps with  17% CPU load
13:55:19 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619538 kbps with  28% CPU load
13:55:19 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591667 kbps with  44% CPU load
13:55:19 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  483017 kbps with 100% CPU load
13:55:19 Interrupt Pacing: 5 micro second, init CPU load 100%
13:55:20 EMAC_sendPacket() returned error 00000004
13:55:20 Sent/received   98/   1 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth  194388 kbps with 100% CPU load
13:55:20 EMAC_sendPacket() returned error 00000004
13:55:20 Sent/received   99/  35 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5638166 kbps with 100% CPU load
13:55:20 EMAC_sendPacket() returned error 00000004
13:55:20 Sent/received  100/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4556530 kbps with 100% CPU load
13:55:20 EMAC_sendPacket() returned error 00000004
13:55:20 Sent/received  100/  35 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3760464 kbps with 100% CPU load
13:55:20 EMAC_sendPacket() returned error 00000004
13:55:21 Sent/received  102/  37 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3050153 kbps with 100% CPU load
13:55:21 EMAC_sendPacket() returned error 00000004
13:55:21 Sent/received  105/  39 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2192458 kbps with 100% CPU load
13:55:21 EMAC_sendPacket() returned error 00000004
13:55:21 Sent/received  113/  45 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1398384 kbps with 100% CPU load
13:55:21 EMAC_sendPacket() returned error 00000004
13:55:21 Sent/received  148/  73 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  564169 kbps with 100% CPU load
13:55:21 Interrupt Pacing: 10 micro second, init CPU load 100%
13:55:21 EMAC_sendPacket() returned error 00000004
13:55:21 Sent/received   99/  42 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 7935508 kbps with 100% CPU load
13:55:22 EMAC_sendPacket() returned error 00000004
13:55:22 Sent/received   99/  34 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5554682 kbps with 100% CPU load
13:55:22 EMAC_sendPacket() returned error 00000004
13:55:22 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4636603 kbps with 100% CPU load
13:55:22 EMAC_sendPacket() returned error 00000004
13:55:22 Sent/received  100/  36 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3975155 kbps with 100% CPU load
13:55:22 EMAC_sendPacket() returned error 00000004
13:55:22 Sent/received  101/  35 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 2959562 kbps with 100% CPU load
13:55:22 EMAC_sendPacket() returned error 00000004
13:55:22 Sent/received  103/  39 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2316808 kbps with 100% CPU load
13:55:22 EMAC_sendPacket() returned error 00000004
13:55:23 Sent/received  112/  44 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1452804 kbps with 100% CPU load
13:55:23 EMAC_sendPacket() returned error 00000004
13:55:23 Sent/received  132/  57 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  522253 kbps with 100% CPU load
13:55:23 Interrupt Pacing: 15 micro second, init CPU load 100%
13:55:23 EMAC_sendPacket() returned error 00000004
13:55:23 Sent/received   99/  41 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 7753037 kbps with 100% CPU load
13:55:23 EMAC_sendPacket() returned error 00000004
13:55:23 Sent/received   99/  34 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5590779 kbps with 100% CPU load
13:55:23 EMAC_sendPacket() returned error 00000004
13:55:24 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4729387 kbps with 100% CPU load
13:55:24 EMAC_sendPacket() returned error 00000004
13:55:24 Sent/received  100/  34 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3845851 kbps with 100% CPU load
13:55:24 EMAC_sendPacket() returned error 00000004
13:55:24 Sent/received  101/  35 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3044707 kbps with 100% CPU load
13:55:24 EMAC_sendPacket() returned error 00000004
13:55:24 Sent/received  103/  37 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2250437 kbps with 100% CPU load
13:55:24 EMAC_sendPacket() returned error 00000004
13:55:24 Sent/received  108/  40 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1364877 kbps with 100% CPU load
13:55:25 EMAC_sendPacket() returned error 00000004
13:55:25 Sent/received  119/  48 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  492718 kbps with 100% CPU load
13:55:25 Interrupt Pacing: 20 micro second, init CPU load 100%
13:55:25 EMAC_sendPacket() returned error 00000004
13:55:25 Sent/received   98/  44 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 8485471 kbps with 100% CPU load
13:55:25 EMAC_sendPacket() returned error 00000004
13:55:25 Sent/received   98/  33 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5471502 kbps with 100% CPU load
13:55:25 EMAC_sendPacket() returned error 00000004
13:55:25 Sent/received   98/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4747473 kbps with 100% CPU load
13:55:25 EMAC_sendPacket() returned error 00000004
13:55:25 Sent/received   99/  35 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3967441 kbps with 100% CPU load
13:55:25 EMAC_sendPacket() returned error 00000004
13:55:26 Sent/received  100/  36 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3141459 kbps with 100% CPU load
13:55:26 EMAC_sendPacket() returned error 00000004
13:55:26 Sent/received  101/  37 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2274473 kbps with 100% CPU load
13:55:26 EMAC_sendPacket() returned error 00000004
13:55:26 Sent/received  105/  40 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1414739 kbps with 100% CPU load
13:55:26 EMAC_sendPacket() returned error 00000004
13:55:26 Sent/received   98/  39 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  472219 kbps with 100% CPU load
13:55:26 Interrupt Pacing: 25 micro second, init CPU load 100%
13:55:26 EMAC_sendPacket() returned error 00000004
13:55:26 Sent/received   98/  46 packets in    0 ms, packet size is 1500 bytes, achieve bandwidth 8866615 kbps with 100% CPU load
13:55:26 EMAC_sendPacket() returned error 00000004
13:55:26 Sent/received   98/  33 packets in    0 ms, packet size is 1300 bytes, achieve bandwidth 5548729 kbps with 100% CPU load
13:55:27 EMAC_sendPacket() returned error 00000004
13:55:27 Sent/received   99/  34 packets in    0 ms, packet size is 1100 bytes, achieve bandwidth 4778560 kbps with 100% CPU load
13:55:27 EMAC_sendPacket() returned error 00000004
13:55:27 Sent/received   99/  34 packets in    0 ms, packet size is  900 bytes, achieve bandwidth 3912543 kbps with 100% CPU load
13:55:27 EMAC_sendPacket() returned error 00000004
13:55:27 Sent/received  100/  35 packets in    0 ms, packet size is  700 bytes, achieve bandwidth 3099059 kbps with 100% CPU load
13:55:27 EMAC_sendPacket() returned error 00000004
13:55:27 Sent/received  102/  36 packets in    0 ms, packet size is  500 bytes, achieve bandwidth 2235747 kbps with 100% CPU load
13:55:27 EMAC_sendPacket() returned error 00000004
13:55:27 Sent/received  107/  38 packets in    0 ms, packet size is  300 bytes, achieve bandwidth 1359672 kbps with 100% CPU load
13:55:27 EMAC_sendPacket() returned error 00000004
13:55:27 Sent/received   98/  34 packets in    0 ms, packet size is  100 bytes, achieve bandwidth  437636 kbps with 100% CPU load
13:55:27 Calling EMAC_close()
13:58:20 Calling EMAC_open()
13:58:20 Waiting for link...
13:58:22 Link Status  : No Link MII on PHY number 1
13:58:22 Packets Held : 32-RX  0-TX
13:58:23 
13:58:23 WARNING: No device LINK.
13:58:23 
13:58:23 Starting packet transfer...
13:58:23 Interrupt Pacing: 0 micro second, init CPU load 100%
13:58:23 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with  94% CPU load
13:58:24 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  13% CPU load
13:58:24 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644384 kbps with  15% CPU load
13:58:24 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639632 kbps with  18% CPU load
13:58:24 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632307 kbps with  19% CPU load
13:58:24 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619537 kbps with  31% CPU load
13:58:25 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591667 kbps with  48% CPU load
13:58:25 Sent/received 8192/8192 packets in   14 ms, packet size is  100 bytes, achieve bandwidth  462764 kbps with 100% CPU load
13:58:25 Interrupt Pacing: 5 micro second, init CPU load 100%
13:58:25 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with   9% CPU load
13:58:25 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  13% CPU load
13:58:26 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644383 kbps with  15% CPU load
13:58:26 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639632 kbps with  18% CPU load
13:58:26 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632307 kbps with  19% CPU load
13:58:26 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619508 kbps with  26% CPU load
13:58:26 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591651 kbps with  34% CPU load
13:58:26 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482779 kbps with  61% CPU load
13:58:26 Interrupt Pacing: 10 micro second, init CPU load 100%
13:58:27 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with   9% CPU load
13:58:27 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  12% CPU load
13:58:27 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644364 kbps with  13% CPU load
13:58:27 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639611 kbps with  15% CPU load
13:58:27 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632301 kbps with  17% CPU load
13:58:27 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619509 kbps with  20% CPU load
13:58:28 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591487 kbps with  27% CPU load
13:58:28 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482551 kbps with  56% CPU load
13:58:28 Interrupt Pacing: 15 micro second, init CPU load 100%
13:58:28 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with   9% CPU load
13:58:28 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647657 kbps with  11% CPU load
13:58:28 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644318 kbps with  12% CPU load
13:58:28 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639547 kbps with  13% CPU load
13:58:29 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632254 kbps with  15% CPU load
13:58:29 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619519 kbps with  18% CPU load
13:58:29 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591518 kbps with  25% CPU load
13:58:29 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482271 kbps with  54% CPU load
13:58:29 Interrupt Pacing: 20 micro second, init CPU load 100%
13:58:32 ERROR: Timeout waiting for TX/RX
13:58:32 Sent/received 8192/8189 packets in 3062 ms, packet size is 1500 bytes, achieve bandwidth   32092 kbps with   1% CPU load
13:58:32 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647703 kbps with   9% CPU load
13:58:33 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644274 kbps with  10% CPU load
13:58:33 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639630 kbps with  12% CPU load
13:58:33 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632140 kbps with  14% CPU load
13:58:33 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619382 kbps with  17% CPU load
13:58:33 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591350 kbps with  24% CPU load
13:58:37 ERROR: Timeout waiting for TX/RX
13:58:37 Sent/received 8192/8158 packets in 3005 ms, packet size is  100 bytes, achieve bandwidth    2171 kbps with   1% CPU load
13:58:37 Interrupt Pacing: 25 micro second, init CPU load 100%
13:58:38 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650159 kbps with   8% CPU load
13:58:38 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647659 kbps with   9% CPU load
13:58:38 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644281 kbps with  10% CPU load
13:58:38 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639575 kbps with  11% CPU load
13:58:38 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632245 kbps with  13% CPU load
13:58:39 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619294 kbps with  16% CPU load
13:58:39 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591324 kbps with  24% CPU load
13:58:39 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  481210 kbps with  52% CPU load
13:58:39 Calling EMAC_close()
13:59:17 Calling EMAC_open()
13:59:17 Waiting for link...
13:59:19 Link Status  : No Link MII on PHY number 1
13:59:19 Packets Held : 32-RX  0-TX
13:59:19 
13:59:19 WARNING: No device LINK.
13:59:20 
13:59:20 Starting packet transfer...
13:59:20 Interrupt Pacing: 0 micro second, init CPU load 100%
13:59:20 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with  94% CPU load
13:59:20 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  13% CPU load
13:59:23 ERROR: Timeout waiting for TX/RX
13:59:23 Sent/received 8192/8187 packets in 3017 ms, packet size is 1100 bytes, achieve bandwidth   23879 kbps with   1% CPU load
13:59:24 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639632 kbps with  18% CPU load
13:59:24 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632306 kbps with  19% CPU load
13:59:24 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619537 kbps with  30% CPU load
13:59:24 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591667 kbps with  48% CPU load
13:59:24 Sent/received 8192/8192 packets in   14 ms, packet size is  100 bytes, achieve bandwidth  462797 kbps with 100% CPU load
13:59:24 Interrupt Pacing: 5 micro second, init CPU load 100%
13:59:25 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with   9% CPU load
13:59:25 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  13% CPU load
13:59:25 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644383 kbps with  15% CPU load
13:59:25 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639632 kbps with  18% CPU load
13:59:26 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632306 kbps with  19% CPU load
13:59:26 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619521 kbps with  26% CPU load
13:59:26 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591578 kbps with  33% CPU load
13:59:26 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482781 kbps with  61% CPU load
13:59:26 Interrupt Pacing: 10 micro second, init CPU load 100%
13:59:26 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with   9% CPU load
13:59:27 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647693 kbps with  11% CPU load
13:59:27 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644381 kbps with  13% CPU load
13:59:27 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639598 kbps with  15% CPU load
13:59:27 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632296 kbps with  17% CPU load
13:59:28 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619459 kbps with  20% CPU load
13:59:28 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591496 kbps with  27% CPU load
13:59:28 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482562 kbps with  56% CPU load
13:59:28 Interrupt Pacing: 15 micro second, init CPU load 100%
13:59:28 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with   9% CPU load
13:59:29 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647659 kbps with  11% CPU load
13:59:29 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644380 kbps with  11% CPU load
13:59:29 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639557 kbps with  13% CPU load
13:59:29 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632204 kbps with  15% CPU load
13:59:29 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619521 kbps with  18% CPU load
13:59:29 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591518 kbps with  25% CPU load
13:59:30 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482272 kbps with  54% CPU load
13:59:30 Interrupt Pacing: 20 micro second, init CPU load 100%
13:59:30 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650115 kbps with   9% CPU load
13:59:30 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647643 kbps with   9% CPU load
13:59:30 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644322 kbps with  10% CPU load
13:59:31 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639507 kbps with  11% CPU load
13:59:31 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632159 kbps with  13% CPU load
13:59:31 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619386 kbps with  17% CPU load
13:59:31 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591343 kbps with  24% CPU load
13:59:36 ERROR: Timeout waiting for TX/RX
13:59:37 Sent/received 8192/8165 packets in 3011 ms, packet size is  100 bytes, achieve bandwidth    2169 kbps with   1% CPU load
13:59:37 Interrupt Pacing: 25 micro second, init CPU load 100%
13:59:37 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650171 kbps with   8% CPU load
13:59:37 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647653 kbps with   9% CPU load
13:59:37 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644270 kbps with  10% CPU load
13:59:38 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639601 kbps with  11% CPU load
13:59:38 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632127 kbps with  13% CPU load
13:59:38 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619454 kbps with  16% CPU load
13:59:38 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591317 kbps with  24% CPU load
13:59:38 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  481190 kbps with  52% CPU load
13:59:38 Calling EMAC_close()
14:00:22 Calling EMAC_open()
14:00:22 Waiting for link...
14:00:23 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
14:00:23 Packets Held : 32-RX  0-TX
14:00:23 
14:00:23 Starting packet transfer...
14:00:23 Interrupt Pacing: 0 micro second, init CPU load 100%
14:00:24 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with  35% CPU load
14:00:25 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:00:26 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:00:27 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:00:27 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   4% CPU load
14:00:28 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:00:28 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   8% CPU load
14:00:28 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  18% CPU load
14:00:28 Interrupt Pacing: 5 micro second, init CPU load 100%
14:00:29 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:00:30 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:00:31 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:00:32 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:00:32 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   4% CPU load
14:00:33 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:00:33 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   8% CPU load
14:00:33 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  17% CPU load
14:00:33 Interrupt Pacing: 10 micro second, init CPU load 100%
14:00:34 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:00:35 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:00:36 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:00:37 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:00:37 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   4% CPU load
14:00:38 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:00:38 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   8% CPU load
14:00:38 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72466 kbps with  15% CPU load
14:00:38 Interrupt Pacing: 15 micro second, init CPU load 100%
14:00:40 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:00:40 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:00:41 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:00:42 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:00:42 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   4% CPU load
14:00:43 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:00:43 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
14:00:43 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72460 kbps with  13% CPU load
14:00:44 Interrupt Pacing: 20 micro second, init CPU load 100%
14:00:45 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:00:46 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:00:46 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:00:47 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:00:48 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   4% CPU load
14:00:48 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:00:48 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
14:00:48 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72457 kbps with  12% CPU load
14:00:48 Interrupt Pacing: 25 micro second, init CPU load 100%
14:00:50 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:00:51 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:00:51 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:00:52 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:00:53 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94858 kbps with   4% CPU load
14:00:53 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:00:53 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88757 kbps with   7% CPU load
14:00:53 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72454 kbps with  11% CPU load
14:00:53 Calling EMAC_close()
14:01:54 Calling EMAC_open()
14:01:55 Waiting for link...
14:01:55 Link Status  : 100Mb/s Full Duplex MII on PHY number 1
14:01:55 Packets Held : 32-RX  0-TX
14:01:55 
14:01:55 Starting packet transfer...
14:01:56 Interrupt Pacing: 0 micro second, init CPU load 100%
14:01:57 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with  35% CPU load
14:01:58 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:01:59 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:02:00 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:02:00 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   4% CPU load
14:02:01 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:02:01 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   8% CPU load
14:02:01 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  18% CPU load
14:02:02 Interrupt Pacing: 5 micro second, init CPU load 100%
14:02:03 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:02:04 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:02:05 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:02:05 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:02:06 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   4% CPU load
14:02:06 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:02:07 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   8% CPU load
14:02:07 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72468 kbps with  17% CPU load
14:02:07 Interrupt Pacing: 10 micro second, init CPU load 100%
14:02:08 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:02:09 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:02:10 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:02:11 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:02:11 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   4% CPU load
14:02:12 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:02:12 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   8% CPU load
14:02:12 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72466 kbps with  15% CPU load
14:02:12 Interrupt Pacing: 15 micro second, init CPU load 100%
14:02:14 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:02:14 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:02:15 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:02:16 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:02:17 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   4% CPU load
14:02:17 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:02:17 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
14:02:17 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72460 kbps with  13% CPU load
14:02:17 Interrupt Pacing: 20 micro second, init CPU load 100%
14:02:18 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:02:19 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:02:20 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:02:21 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:02:21 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   4% CPU load
14:02:22 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:02:22 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88764 kbps with   7% CPU load
14:02:22 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72457 kbps with  12% CPU load
14:02:22 Interrupt Pacing: 25 micro second, init CPU load 100%
14:02:23 Sent/received 8192/8192 packets in 1007 ms, packet size is 1500 bytes, achieve bandwidth   97537 kbps with   2% CPU load
14:02:24 Sent/received 8192/8192 packets in  876 ms, packet size is 1300 bytes, achieve bandwidth   97168 kbps with   2% CPU load
14:02:25 Sent/received 8192/8192 packets in  745 ms, packet size is 1100 bytes, achieve bandwidth   96669 kbps with   3% CPU load
14:02:26 Sent/received 8192/8192 packets in  614 ms, packet size is  900 bytes, achieve bandwidth   95957 kbps with   3% CPU load
14:02:26 Sent/received 8192/8192 packets in  483 ms, packet size is  700 bytes, achieve bandwidth   94859 kbps with   4% CPU load
14:02:27 Sent/received 8192/8192 packets in  352 ms, packet size is  500 bytes, achieve bandwidth   92944 kbps with   5% CPU load
14:02:27 Sent/received 8192/8192 packets in  221 ms, packet size is  300 bytes, achieve bandwidth   88757 kbps with   7% CPU load
14:02:27 Sent/received 8192/8192 packets in   90 ms, packet size is  100 bytes, achieve bandwidth   72454 kbps with  11% CPU load
14:02:27 Calling EMAC_close()
 device LINK.
13:58:09 
13:58:09 Starting packet transfer...
13:58:09 Interrupt Pacing: 0 micro second, init CPU load 100%
13:58:09 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with  94% CPU load
13:58:09 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  13% CPU load
13:58:09 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644383 kbps with  15% CPU load
13:58:10 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639633 kbps with  18% CPU load
13:58:10 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632307 kbps with  19% CPU load
13:58:10 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619537 kbps with  31% CPU load
13:58:10 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591666 kbps with  48% CPU load
13:58:10 Sent/received 8192/8192 packets in   14 ms, packet size is  100 bytes, achieve bandwidth  462780 kbps with 100% CPU load
13:58:10 Interrupt Pacing: 5 micro second, init CPU load 100%
13:58:10 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with   9% CPU load
13:58:11 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  13% CPU load
13:58:11 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644383 kbps with  15% CPU load
13:58:11 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639632 kbps with  18% CPU load
13:58:11 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632306 kbps with  19% CPU load
13:58:11 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619511 kbps with  26% CPU load
13:58:15 ERROR: Timeout waiting for TX/RX
13:58:15 Sent/received 8192/8189 packets in 3027 ms, packet size is  300 bytes, achieve bandwidth    6491 kbps with   1% CPU load
13:58:15 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482790 kbps with  61% CPU load
13:58:15 Interrupt Pacing: 10 micro second, init CPU load 100%
13:58:15 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with   9% CPU load
13:58:15 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  11% CPU load
13:58:15 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644368 kbps with  13% CPU load
13:58:15 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639571 kbps with  15% CPU load
13:58:16 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632302 kbps with  17% CPU load
13:58:16 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619443 kbps with  20% CPU load
13:58:16 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591494 kbps with  27% CPU load
13:58:16 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482572 kbps with  56% CPU load
13:58:16 Interrupt Pacing: 15 micro second, init CPU load 100%
13:58:16 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with   9% CPU load
13:58:16 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647658 kbps with  11% CPU load
13:58:17 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644361 kbps with  11% CPU load
13:58:18 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639598 kbps with  13% CPU load
13:58:18 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632214 kbps with  15% CPU load
13:58:18 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619525 kbps with  18% CPU load
13:58:18 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591445 kbps with  26% CPU load
13:58:18 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482265 kbps with  54% CPU load
13:58:18 Interrupt Pacing: 20 micro second, init CPU load 100%
13:58:19 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650094 kbps with   9% CPU load
13:58:19 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647634 kbps with   9% CPU load
13:58:20 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644382 kbps with  10% CPU load
13:58:20 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639562 kbps with  12% CPU load
13:58:20 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632160 kbps with  13% CPU load
13:58:20 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619328 kbps with  17% CPU load
13:58:20 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591342 kbps with  24% CPU load
13:58:20 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  481515 kbps with  53% CPU load
13:58:21 Interrupt Pacing: 25 micro second, init CPU load 100%
13:58:21 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650103 kbps with   8% CPU load
13:58:21 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647622 kbps with   9% CPU load
13:58:21 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644327 kbps with  10% CPU load
13:58:21 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639606 kbps with  11% CPU load
13:58:25 ERROR: Timeout waiting for TX/RX
13:58:25 Sent/received 8192/8158 packets in 3021 ms, packet size is  700 bytes, achieve bandwidth   15121 kbps with   1% CPU load
13:58:25 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619476 kbps with  16% CPU load
13:58:25 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591319 kbps with  24% CPU load
13:58:25 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  481206 kbps with  52% CPU load
13:58:25 Calling EMAC_close()
13:59:18 Calling EMAC_open()
13:59:18 Waiting for link...
13:59:20 Link Status  : 100Mb/s Full Duplex RGMII on PHY number 0
13:59:20 Packets Held : 32-RX  0-TX
13:59:20 
13:59:21 Starting packet transfer...
13:59:21 Interrupt Pacing: 0 micro second, init CPU load 100%
13:59:21 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with  94% CPU load
13:59:21 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  13% CPU load
13:59:21 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644384 kbps with  15% CPU load
13:59:22 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639632 kbps with  18% CPU load
13:59:22 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632306 kbps with  19% CPU load
13:59:22 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619537 kbps with  30% CPU load
13:59:22 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591665 kbps with  48% CPU load
13:59:22 Sent/received 8192/8192 packets in   14 ms, packet size is  100 bytes, achieve bandwidth  462754 kbps with 100% CPU load
13:59:22 Interrupt Pacing: 5 micro second, init CPU load 100%
13:59:23 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with   9% CPU load
13:59:23 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647714 kbps with  13% CPU load
13:59:23 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644383 kbps with  15% CPU load
13:59:23 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639633 kbps with  18% CPU load
13:59:23 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632306 kbps with  19% CPU load
13:59:24 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619518 kbps with  26% CPU load
13:59:24 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591654 kbps with  33% CPU load
13:59:24 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482784 kbps with  61% CPU load
13:59:24 Interrupt Pacing: 10 micro second, init CPU load 100%
13:59:24 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650179 kbps with   9% CPU load
13:59:25 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647691 kbps with  11% CPU load
13:59:25 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644384 kbps with  13% CPU load
13:59:25 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639596 kbps with  15% CPU load
13:59:25 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632296 kbps with  17% CPU load
13:59:25 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619471 kbps with  20% CPU load
13:59:25 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591484 kbps with  27% CPU load
13:59:26 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482560 kbps with  56% CPU load
13:59:26 Interrupt Pacing: 15 micro second, init CPU load 100%
13:59:26 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650178 kbps with   9% CPU load
13:59:26 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647659 kbps with  11% CPU load
13:59:26 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644378 kbps with  11% CPU load
13:59:27 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639558 kbps with  13% CPU load
13:59:27 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632201 kbps with  15% CPU load
13:59:27 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619525 kbps with  18% CPU load
13:59:27 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591517 kbps with  25% CPU load
13:59:27 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  482259 kbps with  54% CPU load
13:59:28 Interrupt Pacing: 20 micro second, init CPU load 100%
13:59:28 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650111 kbps with   9% CPU load
13:59:28 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647642 kbps with   9% CPU load
13:59:28 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644318 kbps with  10% CPU load
13:59:29 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639508 kbps with  11% CPU load
13:59:29 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632162 kbps with  13% CPU load
13:59:29 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619388 kbps with  17% CPU load
13:59:29 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591349 kbps with  24% CPU load
13:59:29 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  481515 kbps with  53% CPU load
13:59:29 Interrupt Pacing: 25 micro second, init CPU load 100%
13:59:30 Sent/received 8192/8192 packets in  151 ms, packet size is 1500 bytes, achieve bandwidth  650082 kbps with   8% CPU load
13:59:30 Sent/received 8192/8192 packets in  131 ms, packet size is 1300 bytes, achieve bandwidth  647619 kbps with   9% CPU load
13:59:30 Sent/received 8192/8192 packets in  111 ms, packet size is 1100 bytes, achieve bandwidth  644301 kbps with  10% CPU load
13:59:30 Sent/received 8192/8192 packets in   92 ms, packet size is  900 bytes, achieve bandwidth  639479 kbps with  11% CPU load
13:59:31 Sent/received 8192/8192 packets in   72 ms, packet size is  700 bytes, achieve bandwidth  632297 kbps with  13% CPU load
13:59:31 Sent/received 8192/8192 packets in   52 ms, packet size is  500 bytes, achieve bandwidth  619468 kbps with  16% CPU load
13:59:31 Sent/received 8192/8192 packets in   33 ms, packet size is  300 bytes, achieve bandwidth  591329 kbps with  24% CPU load
13:59:31 Sent/received 8192/8192 packets in   13 ms, packet size is  100 bytes, achieve bandwidth  481209 kbps with  52% CPU load
13:59:31 Calling EMAC_close()
14:01:02 Calling EMAC_open()
14:01:02 Waiting for link...
14:01:03 Link Status  : 1000Mb/s Full Duplex RGMII on PHY number 0
14:01:03 Packets Held : 32-RX  0-TX
14:01:03 
14:01:03 Starting packet transfer...
14:01:03 Interrupt Pacing: 0 micro second, init CPU load 100%
14:01:03 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975241 kbps with  86% CPU load
14:01:04 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971541 kbps with  19% CPU load
14:01:04 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966544 kbps with  22% CPU load
14:01:04 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959413 kbps with  26% CPU load
14:01:04 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948417 kbps with  28% CPU load
14:01:04 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929255 kbps with  45% CPU load
14:01:04 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887442 kbps with  72% CPU load
14:01:04 Sent/received 8192/8192 packets in   14 ms, packet size is  100 bytes, achieve bandwidth  462704 kbps with 100% CPU load
14:01:04 Interrupt Pacing: 5 micro second, init CPU load 100%
14:01:04 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975240 kbps with  14% CPU load
14:01:05 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971537 kbps with  17% CPU load
14:01:05 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966518 kbps with  20% CPU load
14:01:05 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959399 kbps with  23% CPU load
14:01:05 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948405 kbps with  27% CPU load
14:01:05 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929187 kbps with  32% CPU load
14:01:05 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887306 kbps with  43% CPU load
14:01:05 Sent/received 8192/8192 packets in    9 ms, packet size is  100 bytes, achieve bandwidth  723571 kbps with  84% CPU load
14:01:05 Interrupt Pacing: 10 micro second, init CPU load 100%
14:01:05 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975219 kbps with  14% CPU load
14:01:06 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971519 kbps with  15% CPU load
14:01:06 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966492 kbps with  17% CPU load
14:01:06 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959342 kbps with  18% CPU load
14:01:06 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948276 kbps with  21% CPU load
14:01:06 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929214 kbps with  26% CPU load
14:01:06 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887131 kbps with  37% CPU load
14:01:06 Sent/received 8192/8192 packets in    9 ms, packet size is  100 bytes, achieve bandwidth  723157 kbps with  80% CPU load
14:01:06 Interrupt Pacing: 15 micro second, init CPU load 100%
14:01:06 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975117 kbps with  12% CPU load
14:01:07 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971439 kbps with  13% CPU load
14:01:07 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966529 kbps with  14% CPU load
14:01:07 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959275 kbps with  16% CPU load
14:01:07 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948120 kbps with  19% CPU load
14:01:07 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929221 kbps with  24% CPU load
14:01:07 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887302 kbps with  35% CPU load
14:01:07 Sent/received 8192/8192 packets in    9 ms, packet size is  100 bytes, achieve bandwidth  722295 kbps with  78% CPU load
14:01:07 Interrupt Pacing: 20 micro second, init CPU load 100%
14:01:07 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975130 kbps with  11% CPU load
14:01:08 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971373 kbps with  12% CPU load
14:01:08 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966458 kbps with  13% CPU load
14:01:08 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959166 kbps with  15% CPU load
14:01:08 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948272 kbps with  18% CPU load
14:01:08 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929000 kbps with  23% CPU load
14:01:08 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  886583 kbps with  34% CPU load
14:01:11 ERROR: Timeout waiting for TX/RX
14:01:11 Sent/received 8192/5693 packets in 3005 ms, packet size is  100 bytes, achieve bandwidth    1515 kbps with   1% CPU load
14:01:11 Interrupt Pacing: 25 micro second, init CPU load 100%
14:01:11 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975109 kbps with  10% CPU load
14:01:12 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971299 kbps with  11% CPU load
14:01:12 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966250 kbps with  12% CPU load
14:01:12 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959031 kbps with  14% CPU load
14:01:12 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948001 kbps with  17% CPU load
14:01:12 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  928873 kbps with  22% CPU load
14:01:12 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  886410 kbps with  33% CPU load
14:01:15 ERROR: Timeout waiting for TX/RX
14:01:15 Sent/received 8192/4803 packets in 3069 ms, packet size is  100 bytes, achieve bandwidth    1251 kbps with   1% CPU load
14:01:15 Calling EMAC_close()
14:01:56 Calling EMAC_open()
14:01:56 Waiting for link...
14:01:56 Link Status  : 1000Mb/s Full Duplex RGMII on PHY number 0
14:01:56 Packets Held : 32-RX  0-TX
14:01:57 
14:01:57 Starting packet transfer...
14:01:57 Interrupt Pacing: 0 micro second, init CPU load 100%
14:01:57 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975240 kbps with  86% CPU load
14:01:57 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971541 kbps with  19% CPU load
14:01:57 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966544 kbps with  22% CPU load
14:01:58 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959412 kbps with  26% CPU load
14:01:58 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948418 kbps with  28% CPU load
14:01:58 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929256 kbps with  45% CPU load
14:01:58 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887442 kbps with  72% CPU load
14:01:58 Sent/received 8192/8192 packets in   14 ms, packet size is  100 bytes, achieve bandwidth  462699 kbps with 100% CPU load
14:01:58 Interrupt Pacing: 5 micro second, init CPU load 100%
14:01:58 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975239 kbps with  14% CPU load
14:01:59 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971542 kbps with  17% CPU load
14:01:59 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966520 kbps with  20% CPU load
14:01:59 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959388 kbps with  23% CPU load
14:01:59 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948318 kbps with  27% CPU load
14:01:59 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929187 kbps with  32% CPU load
14:01:59 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887283 kbps with  43% CPU load
14:02:00 Sent/received 8192/8192 packets in    9 ms, packet size is  100 bytes, achieve bandwidth  723888 kbps with  84% CPU load
14:02:00 Interrupt Pacing: 10 micro second, init CPU load 100%
14:02:00 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975231 kbps with  14% CPU load
14:02:00 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971516 kbps with  15% CPU load
14:02:00 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966495 kbps with  17% CPU load
14:02:00 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959343 kbps with  18% CPU load
14:02:01 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948281 kbps with  21% CPU load
14:02:01 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  929206 kbps with  26% CPU load
14:02:01 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887115 kbps with  37% CPU load
14:02:01 Sent/received 8192/8192 packets in    9 ms, packet size is  100 bytes, achieve bandwidth  723164 kbps with  80% CPU load
14:02:01 Interrupt Pacing: 15 micro second, init CPU load 100%
14:02:02 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975116 kbps with  12% CPU load
14:02:02 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971437 kbps with  13% CPU load
14:02:02 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966351 kbps with  14% CPU load
14:02:02 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959268 kbps with  16% CPU load
14:02:02 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948121 kbps with  19% CPU load
14:02:02 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  928849 kbps with  24% CPU load
14:02:03 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  887316 kbps with  35% CPU load
14:02:03 Sent/received 8192/8192 packets in    9 ms, packet size is  100 bytes, achieve bandwidth  722291 kbps with  78% CPU load
14:02:03 Interrupt Pacing: 20 micro second, init CPU load 100%
14:02:03 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975140 kbps with  11% CPU load
14:02:03 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971383 kbps with  12% CPU load
14:02:03 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966461 kbps with  13% CPU load
14:02:04 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959166 kbps with  15% CPU load
14:02:04 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  948271 kbps with  18% CPU load
14:02:04 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  928994 kbps with  23% CPU load
14:02:04 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  886588 kbps with  34% CPU load
14:02:07 ERROR: Timeout waiting for TX/RX
14:02:07 Sent/received 8192/5695 packets in 3005 ms, packet size is  100 bytes, achieve bandwidth    1515 kbps with   1% CPU load
14:02:07 Interrupt Pacing: 25 micro second, init CPU load 100%
14:02:07 Sent/received 8192/8192 packets in  100 ms, packet size is 1500 bytes, achieve bandwidth  975105 kbps with  10% CPU load
14:02:08 Sent/received 8192/8192 packets in   87 ms, packet size is 1300 bytes, achieve bandwidth  971294 kbps with  11% CPU load
14:02:08 Sent/received 8192/8192 packets in   74 ms, packet size is 1100 bytes, achieve bandwidth  966251 kbps with  12% CPU load
14:02:08 Sent/received 8192/8192 packets in   61 ms, packet size is  900 bytes, achieve bandwidth  959026 kbps with  14% CPU load
14:02:08 Sent/received 8192/8192 packets in   48 ms, packet size is  700 bytes, achieve bandwidth  947986 kbps with  17% CPU load
14:02:08 Sent/received 8192/8192 packets in   35 ms, packet size is  500 bytes, achieve bandwidth  928875 kbps with  22% CPU load
14:02:08 Sent/received 8192/8192 packets in   22 ms, packet size is  300 bytes, achieve bandwidth  886411 kbps with  33% CPU load
14:02:12 ERROR: Timeout waiting for TX/RX
14:02:12 Sent/received 8192/4735 packets in 3069 ms, packet size is  100 bytes, achieve bandwidth    1234 kbps with   1% CPU load
14:02:12 Calling EMAC_close()
14:17:28 PLLC configured: PLLM=20, PRE_DIV=1
14:17:28 Calling EMAC_open()
14:17:28 Calling EMAC_setReceiveFilter()
14:17:32 Waiting for EMAC link initialization...
14:17:32 
14:17:32 Starting packet transfer...
14:17:33 ERROR14:18:32 PLLC configured: PLLM=20, PRE_DIV=1
14:18:32 Calling EMAC_open()
14:18:32 Calling EMAC_setReceiveFilter()
14:18:32 Waiting for EMAC link initialization...
14:18:32 
14:18:32 Starting packet receiving and transfer...
14:19:28 PLLC configured: PLLM=20, PRE_DIV=1
14:19:28 Calling EMAC_open()
14:19:28 Calling EMAC_setReceiveFilter()
14:19:28 Waiting for EMAC link initialization...
14:19:28 
14:19:29 Starting packet receiving and transfer...
14:20:47 PLLC configured: PLLM=20, PRE_DIV=1
14:20:47 Calling EMAC_open()
14:20:47 Calling EMAC_setReceiveFilter()
14:20:48 Waiting for EMAC link initialization...
14:20:48 
14:20:48 Starting packet receiving and transfer...
14:25:44 PLLC configured: PLLM=20, PRE_DIV=1
14:25:44 Calling EMAC_open()
14:25:44 Calling EMAC_setReceiveFilter()
14:25:44 Waiting for EMAC link initialization...
14:25:44 
14:25:44 Starting packet receiving and transfer...
14:26:13 PLLC configured: PLLM=20, PRE_DIV=1
14:26:13 Calling EMAC_open()
14:26:13 Calling EMAC_setReceiveFilter()
14:26:14 Waiting for EMAC link initialization...
14:26:14 
14:26:14 Starting packet receiving and transfer...
14:48:22 PLLC configured: PLLM=20, PRE_DIV=1
14:48:22 Calling EMAC_open()
14:48:22 Calling EMAC_setReceiveFilter()
14:48:22 Waiting for EMAC link initialization...
14:48:22 
14:48:22 Starting packet receiving and transfer...
14:52:40 PLLC configured: PLLM=20, PRE_DIV=1
14:52:40 Calling EMAC_open()
14:52:40 Calling EMAC_setReceiveFilter()
14:52:40 Waiting for EMAC link initialization...
14:52:43 
14:52:43 Starting packet receiving and transfer...
15:46:19 PLLC configured: PLLM=20, PRE_DIV=1
15:46:19 Calling EMAC_open()
15:46:19 Calling EMAC_setReceiveFilter()
15:47:49 PLLC configured: PLLM=20, PRE_DIV=1
15:47:50 Calling EMAC_open()
15:47:50 Calling EMAC_setReceiveFilter()
15:48:38 PLLC configured: PLLM=20, PRE_DIV=1
15:48:38 Calling EMAC_open()
15:48:38 Calling EMAC_setReceiveFilter()
15:48:38 Waiting for EMAC link initialization...
15:48:41 
15:48:41 Starting packet receiving and transfer...
15:49:20 PLLC configured: PLLM=20, PRE_DIV=1
15:49:20 Calling EMAC_open()
15:49:20 Calling EMAC_setReceiveFilter()
15:49:20 Waiting for EMAC link initialization...
15:49:23 
15:49:23 Starting packet receiving and transfer...
15:56:55 PLLC configured: PLLM=20, PRE_DIV=1
15:56:56 Calling EMAC_open()
15:56:56 Calling EMAC_setReceiveFilter()
15:56:56 Waiting for EMAC link initialization...
15:56:58 
15:56:59 Starting packet receiving and transfer...
16:01:48 PLLC configured: PLLM=20, PRE_DIV=1
16:01:48 Calling EMAC_open()
16:01:48 Calling EMAC_setReceiveFilter()
16:01:49 Waiting for EMAC link initialization...
16:01:51 
16:01:51 Starting packet receiving and transfer...
16:01:57 Received and send back 1 packets
16:02:00 Received and send back 33 packets
16:02:02 Received and send back 57377 packets
16:02:40 PLLC configured: PLLM=20, PRE_DIV=1
16:02:40 Calling EMAC_open()
16:02:40 Calling EMAC_setReceiveFilter()
16:02:41 Waiting for EMAC link initialization...
16:02:43 
16:02:43 Starting packet receiving and transfer...
16:02:49 Received and send back 1 packets
16:02:51 Received and send back 33 packets
16:02:54 Received and send back 57377 packets
16:07:38 PLLC configured: PLLM=20, PRE_DIV=1
16:07:38 Calling EMAC_open()
16:07:38 Calling EMAC_setReceiveFilter()
16:07:38 
16:07:38 Starting packet receiving and transfer...
16:07:46 Received and send back 1 packets
16:07:49 Received and send back 33 packets
16:07:51 Received and send back 57377 packets
16:08:16 PLLC configured: PLLM=20, PRE_DIV=1
16:08:16 Calling EMAC_open()
16:08:16 Calling EMAC_setReceiveFilter()
16:08:16 
16:08:17 Starting packet receiving and transfer...
16:08:24 Received and send back 1 packets
16:08:26 Received and send back 33 packets
16:08:28 Received and send back 57377 packets
16:09:24 PLLC configured: PLLM=20, PRE_DIV=1
16:09:24 Calling EMAC_open()
16:09:24 Calling EMAC_setReceiveFilter()
16:09:24 
16:09:24 Starting packet receiving and transfer...
16:09:32 Received and send back 1 packets
16:09:35 Received and send back 342 packets
16:09:37 Received and send back 57686 packets
16:11:26 PLLC configured: PLLM=20, PRE_DIV=1
16:11:26 Calling EMAC_open()
16:11:26 Calling EMAC_setReceiveFilter()
16:11:26 
16:11:26 Starting packet receiving and transfer...
16:11:28 Received and send back 14364 packets
16:11:31 Received and send back 14397 packets
16:11:33 Received and send back 63549 packets
16:12:07 PLLC configured: PLLM=20, PRE_DIV=1
16:12:07 Calling EMAC_open()
16:12:07 Calling EMAC_setReceiveFilter()
16:12:07 
16:12:07 Starting packet receiving and transfer...
16:12:11 Received and send back 1 packets
16:12:13 Received and send back 1724 packets
16:12:15 Received and send back 57681 packets
16:12:18 Received and send back 57717 packets
16:12:56 PLLC configured: PLLM=20, PRE_DIV=1
16:12:56 Calling EMAC_open()
16:12:56 Calling EMAC_setReceiveFilter()
16:12:56 
16:12:56 Starting packet receiving and transfer...
16:13:01 Received and send back 1 packets
16:13:03 Received and send back 343 packets
16:13:05 Received and send back 50663 packets
16:13:07 Received and send back 50699 packets
16:20:17 PLLC configured: PLLM=20, PRE_DIV=1
16:20:17 Calling EMAC_open()
16:20:17 Calling EMAC_setReceiveFilter()
16:20:17 
16:20:17 Starting packet transfer...
16:20:17 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656240 kbps
16:20:17 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654681 kbps
16:20:17 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652576 kbps
16:20:18 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649571 kbps
16:20:18 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644939 kbps
16:20:18 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636867 kbps
16:20:18 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619251 kbps
16:20:18 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  241199 kbps
16:20:18 Calling EMAC_close()
16:22:11 PLLC configured: PLLM=20, PRE_DIV=1
16:22:11 Calling EMAC_open()
16:22:11 Calling EMAC_setReceiveFilter()
16:24:34 PLLC configured: PLLM=20, PRE_DIV=1
16:24:34 Calling EMAC_open()
16:24:35 Calling EMAC_setReceiveFilter()
16:24:35 
16:24:35 Starting packet receiving and transfer...
16:24:39 Received and send back 1 packets
16:24:41 Received and send back 33 packets
16:24:43 Received and send back 57377 packets
16:33:44 PLLC configured: PLLM=20, PRE_DIV=1
16:33:44 Calling EMAC_open()
16:33:44 Calling EMAC_setReceiveFilter()
16:33:44 
16:33:44 Starting packet receiving and transfer...
16:33:54 Received and send back 1 packets
16:33:56 Received and send back 33 packets
16:33:58 Received and send back 57377 packets
16:34:50 PLLC configured: PLLM=20, PRE_DIV=1
16:34:50 Calling EMAC_open()
16:34:50 Calling EMAC_setReceiveFilter()
16:34:51 
16:34:51 Starting packet receiving and transfer...
16:35:01 Received and send back 1 packets
16:35:03 Received and send back 33 packets
16:35:05 Received and send back 57377 packets
16:38:34 Received and send back 57378 packets
16:38:36 Received and send back 57410 packets
16:38:38 Received and send back 114754 packets
16:44:59 PLLC configured: PLLM=20, PRE_DIV=1
16:44:59 Calling EMAC_open()
16:44:59 Calling EMAC_setReceiveFilter()
16:44:59 
16:44:59 Starting packet receiving and transfer...
16:45:12 Received and send back 1 packets
16:45:14 Received and send back 33 packets
16:45:17 Received and send back 57377 packets
16:47:06 PLLC configured: PLLM=20, PRE_DIV=1
16:47:06 Calling EMAC_open()
16:47:06 Calling EMAC_setReceiveFilter()
16:47:06 
16:47:06 Starting packet receiving and transfer...
16:47:10 Received and send back 1 packets
16:47:12 Received and send back 1886 packets
16:47:14 Received and send back 59230 packets
16:48:13 PLLC configured: PLLM=20, PRE_DIV=1
16:48:13 Calling EMAC_open()
16:48:13 Calling EMAC_setReceiveFilter()
16:48:14 
16:48:14 Starting packet receiving and transfer...
16:48:17 Received and send back 1 packets
16:48:20 Received and send back 830 packets
16:48:22 Received and send back 58174 packets
16:49:31 PLLC configured: PLLM=20, PRE_DIV=1
16:49:31 Calling EMAC_open()
16:49:31 Calling EMAC_setReceiveFilter()
16:49:32 
16:49:32 Starting packet receiving and transfer...
16:49:36 Received and send back 1 packets
16:49:38 Received and send back 33 packets
16:49:40 Received and send back 57377 packets
16:55:01 PLLC configured: PLLM=20, PRE_DIV=1
16:55:01 Calling EMAC_open()
16:55:01 Calling EMAC_setReceiveFilter()
16:55:02 
16:55:02 Starting packet receiving and transfer...
16:55:06 Received and send back 1 packets
16:55:09 Received and send back 1886 packets
16:55:11 Received and send back 59230 packets
17:01:34 PLLC configured: PLLM=20, PRE_DIV=1
17:01:34 Calling EMAC_open()
17:01:34 Calling EMAC_setReceiveFilter()
17:01:34 
17:01:34 Starting packet transfer...
17:01:35 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656245 kbps
17:01:35 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654687 kbps
17:01:35 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652582 kbps
17:01:35 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649580 kbps
17:01:35 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644949 kbps
17:01:35 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636880 kbps
17:01:35 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619273 kbps
17:01:35 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  433027 kbps
17:01:35 Calling EMAC_close()
17:20:19 PLLC configured: PLLM=20, PRE_DIV=1
17:20:19 Calling EMAC_open()
17:20:20 Calling EMAC_setReceiveFilter()
17:20:20 
17:20:20 Starting packet transfer...
17:20:20 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656245 kbps
17:20:20 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654687 kbps
17:20:21 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652582 kbps
17:20:21 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649580 kbps
17:20:21 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644949 kbps
17:20:21 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636880 kbps
17:20:21 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619273 kbps
17:20:21 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  433027 kbps
17:20:21 Calling EMAC_close()
17:20:57 PLLC configured: PLLM=20, PRE_DIV=1
17:20:57 Calling EMAC_open()
17:20:57 Calling EMAC_setReceiveFilter()
17:20:57 
17:20:57 Starting packet receiving and transfer...
17:21:01 Received and send back 1 packets
17:21:03 Received and send back 1073 packets
17:21:05 Received and send back 58417 packets
17:28:59 PLLC configured: PLLM=20, PRE_DIV=1
17:28:59 Calling EMAC_open()
17:28:59 Calling EMAC_setReceiveFilter()
17:28:59 
17:29:00 Starting packet receiving and transfer...
17:29:03 Received and send back 1 packets
17:29:05 Received and send back 669 packets
17:29:08 Received and send back 58013 packets
17:30:59 PLLC configured: PLLM=20, PRE_DIV=1
17:30:59 Calling EMAC_open()
17:30:59 Calling EMAC_setReceiveFilter()
17:30:59 
17:30:59 Starting packet transfer...
17:31:00 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656245 kbps
17:31:00 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654687 kbps
17:31:00 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652582 kbps
17:31:00 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649579 kbps
17:31:01 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644950 kbps
17:31:01 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636880 kbps
17:31:01 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619273 kbps
17:31:01 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  433029 kbps
17:31:01 Calling EMAC_close()
17:31:55 PLLC configured: PLLM=20, PRE_DIV=1
17:31:55 Calling EMAC_open()
17:31:55 Calling EMAC_setReceiveFilter()
17:31:55 
17:31:55 Starting packet receiving and transfer...
17:31:59 Received and send back 1 packets
17:32:01 Received and send back 1478 packets
17:32:03 Received and send back 58822 packets
17:35:24 PLLC configured: PLLM=20, PRE_DIV=1
17:35:24 Calling EMAC_open()
17:35:24 Calling EMAC_setReceiveFilter()
17:35:25 
17:35:25 Starting packet receiving and transfer...
17:35:28 Received and send back 1 packets
17:35:31 Received and send back 991 packets
17:35:33 Received and send back 58335 packets
17:50:31 PLLC configured: PLLM=20, PRE_DIV=1
17:50:31 Calling EMAC_open()
17:50:31 Calling EMAC_setReceiveFilter()
17:50:31 
17:50:31 Starting packet receiving and transfer...
17:50:35 Received and send back 1 packets
17:50:37 Received and send back 65536 packets
17:51:44 PLLC configured: PLLM=20, PRE_DIV=1
17:51:44 Calling EMAC_open()
17:51:44 Calling EMAC_setReceiveFilter()
17:51:44 
17:51:44 Starting packet receiving and transfer...
17:51:49 Received and send back 1 packets
17:51:51 Received and send back 65536 packets
18:00:14 PLLC configured: PLLM=20, PRE_DIV=1
18:00:14 Calling EMAC_open()
18:00:14 Calling EMAC_setReceiveFilter()
18:00:14 
18:00:14 Starting packet transfer...
18:00:14 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984335 kbps
18:00:14 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981995 kbps
18:00:14 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978833 kbps
18:00:15 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974321 kbps
18:00:15 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967365 kbps
18:00:15 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955244 kbps
18:00:15 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  660955 kbps
18:00:15 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240120 kbps
18:00:15 Calling EMAC_close()
18:00:48 PLLC configured: PLLM=20, PRE_DIV=1
18:00:48 Calling EMAC_open()
18:00:48 Calling EMAC_setReceiveFilter()
18:00:48 
18:00:48 Starting packet receiving and transfer...
18:00:50 Received and send back 16384 packets
18:00:52 Received and send back 65536 packets
18:01:52 PLLC configured: PLLM=20, PRE_DIV=1
18:01:52 Calling EMAC_open()
18:01:52 Calling EMAC_setReceiveFilter()
18:01:52 
18:01:52 Starting packet receiving and transfer...
18:01:54 Received and send back 8192 packets
18:01:56 Received and send back 65536 packets
18:02:44 PLLC configured: PLLM=20, PRE_DIV=1
18:02:45 Calling EMAC_open()
18:02:45 Calling EMAC_setReceiveFilter()
18:02:45 
18:02:45 Starting packet transfer...
18:02:45 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656239 kbps
18:02:45 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654682 kbps
18:02:46 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652576 kbps
18:02:46 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649571 kbps
18:02:46 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644939 kbps
18:02:46 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636866 kbps
18:02:46 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619251 kbps
18:02:46 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240120 kbps
18:02:47 Calling EMAC_close()
18:03:24 PLLC configured: PLLM=20, PRE_DIV=1
18:03:24 Calling EMAC_open()
18:03:24 Calling EMAC_setReceiveFilter()
18:03:24 
18:03:24 Starting packet transfer...
18:03:24 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984335 kbps
18:03:25 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981995 kbps
18:03:25 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978833 kbps
18:03:25 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974322 kbps
18:03:25 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967365 kbps
18:03:25 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955245 kbps
18:03:25 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  660928 kbps
18:03:25 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240121 kbps
18:03:26 Calling EMAC_close()
18:06:20 PLLC configured: PLLM=20, PRE_DIV=1
18:06:20 Calling EMAC_open()
18:06:20 Calling EMAC_setReceiveFilter()
18:06:20 
18:06:20 Starting packet receiving and transfer...
18:06:22 Received and send back 9309 packets
18:06:24 Received and send back 65536 packets
18:39:40 PLLC configured: PLLM=20, PRE_DIV=1
18:39:40 Calling EMAC_open()
18:39:40 Calling EMAC_setReceiveFilter()
18:39:40 
18:39:40 Starting packet transfer...
18:39:41 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984335 kbps
18:39:41 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981995 kbps
18:39:41 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978833 kbps
18:39:41 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974322 kbps
18:39:41 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967366 kbps
18:39:41 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955245 kbps
18:39:41 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  660910 kbps
18:39:41 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240114 kbps
18:39:42 Calling EMAC_close()
18:39:56 PLLC configured: PLLM=20, PRE_DIV=1
18:39:56 Calling EMAC_open()
18:39:56 Calling EMAC_setReceiveFilter()
18:39:56 
18:39:57 Starting packet transfer...
18:39:57 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984335 kbps
18:40:00 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  984775 kbps
18:40:00 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978833 kbps
18:40:00 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974321 kbps
18:40:00 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967366 kbps
18:40:00 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955244 kbps
18:40:00 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  660926 kbps
18:40:00 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240109 kbps
18:40:01 Calling EMAC_close()
18:40:08 PLLC configured: PLLM=20, PRE_DIV=1
18:40:08 Calling EMAC_open()
18:40:08 Calling EMAC_setReceiveFilter()
18:40:08 
18:40:08 Starting packet transfer...
18:40:08 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984335 kbps
18:40:08 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981996 kbps
18:40:08 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978833 kbps
18:40:08 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974322 kbps
18:40:08 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967366 kbps
18:40:08 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955246 kbps
18:40:09 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  660897 kbps
18:40:12 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240110 kbps
18:40:12 Calling EMAC_close()
18:40:21 PLLC configured: PLLM=20, PRE_DIV=1
18:40:21 Calling EMAC_open()
18:40:21 Calling EMAC_setReceiveFilter()
18:40:21 
18:40:21 Starting packet transfer...
18:40:22 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984336 kbps
18:40:22 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981995 kbps
18:40:22 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978833 kbps
18:40:22 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974322 kbps
18:40:22 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967365 kbps
18:40:22 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955245 kbps
18:40:22 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  660923 kbps
18:40:22 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240121 kbps
18:40:22 Calling EMAC_close()
18:41:04 PLLC configured: PLLM=20, PRE_DIV=1
18:41:04 Calling EMAC_open()
18:41:04 Calling EMAC_setReceiveFilter()
18:41:04 
18:41:04 Starting packet receiving and transfer...
18:41:06 Received and send back 17287 packets
18:41:09 Received and send back 65536 packets
18:43:34 PLLC configured: PLLM=20, PRE_DIV=1
18:43:34 Calling EMAC_open()
18:43:34 Calling EMAC_setReceiveFilter()
18:43:34 
18:43:34 Starting packet receiving and transfer...
18:43:36 Received and send back 11922 packets
18:43:38 Received and send back 65536 packets
width  981547 kbps
16:33:57 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978363 kbps
16:33:57 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973805 kbps
16:33:57 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966820 kbps
16:33:57 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954649 kbps
16:33:57 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  648261 kbps
16:33:58 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  235893 kbps
16:33:58 Calling EMAC_close()
16:34:49 PLLC configured: PLLM=20, PRE_DIV=1
16:34:49 Calling EMAC_open()
16:34:49 Calling EMAC_setReceiveFilter()
16:34:49 Waiting for PHY link initialization...
16:35:00 
16:35:01 Starting packet transfer...
16:35:04 ERROR: Timeout waiting for TX/RX
16:35:04 Sent 8192 packets, received 33 packets, packet size is 1514 bytes, achieve bandwidth    132 kbps
16:35:04 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981547 kbps
16:35:04 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978372 kbps
16:35:04 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973815 kbps
16:35:04 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966820 kbps
16:35:05 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954647 kbps
16:35:05 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  648282 kbps
16:35:05 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  235897 kbps
16:35:05 Calling EMAC_close()
16:38:19 PLLC configured: PLLM=20, PRE_DIV=1
16:38:19 Calling EMAC_open()
16:38:19 Calling EMAC_setReceiveFilter()
16:38:19 Waiting for PHY link initialization...
16:38:33 
16:38:33 Starting packet transfer...
16:38:36 ERROR: Timeout waiting for TX/RX
16:38:36 Sent 8192 packets, received 33 packets, packet size is 1514 bytes, achieve bandwidth    129 kbps
16:38:36 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981547 kbps
16:38:37 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978371 kbps
16:38:37 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973816 kbps
16:38:37 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966819 kbps
16:38:37 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954648 kbps
16:38:37 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  648253 kbps
16:38:37 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  235882 kbps
16:38:37 Calling EMAC_close()
16:44:58 PLLC configured: PLLM=20, PRE_DIV=1
16:44:58 Calling EMAC_open()
16:44:58 Calling EMAC_setReceiveFilter()
16:44:58 Waiting for PHY link initialization...
16:45:12 
16:45:12 Starting packet transfer...
16:45:15 ERROR: Timeout waiting for TX/RX
16:45:15 Sent 8192 packets, received 33 packets, packet size is 1514 bytes, achieve bandwidth    133 kbps
16:45:15 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981547 kbps
16:45:16 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978371 kbps
16:45:16 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973816 kbps
16:45:16 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966819 kbps
16:45:16 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954648 kbps
16:45:16 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  648286 kbps
16:45:16 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  235880 kbps
16:45:16 Calling EMAC_close()
16:47:05 PLLC configured: PLLM=20, PRE_DIV=1
16:47:05 Calling EMAC_open()
16:47:05 Calling EMAC_setReceiveFilter()
16:47:05 Waiting for PHY link initialization...
16:47:10 
16:47:10 Starting packet transfer...
16:47:13 ERROR: Timeout waiting for TX/RX
16:47:13 Sent 8192 packets, received 1886 packets, packet size is 1514 bytes, achieve bandwidth   7553 kbps
16:47:13 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981544 kbps
16:47:13 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978370 kbps
16:47:14 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973806 kbps
16:47:14 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966809 kbps
16:47:14 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954647 kbps
16:47:14 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  648271 kbps
16:47:14 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  235901 kbps
16:47:14 Calling EMAC_close()
16:48:12 PLLC configured: PLLM=20, PRE_DIV=1
16:48:12 Calling EMAC_open()
16:48:12 Calling EMAC_setReceiveFilter()
16:48:12 Waiting for PHY link initialization...
16:48:17 
16:48:17 Starting packet transfer...
16:48:20 ERROR: Timeout waiting for TX/RX
16:48:20 Sent 8192 packets, received 830 packets, packet size is 1514 bytes, achieve bandwidth   3333 kbps
16:48:21 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981542 kbps
16:48:21 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978372 kbps
16:48:21 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973817 kbps
16:48:21 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966811 kbps
16:48:21 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954650 kbps
16:48:21 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  650413 kbps
16:48:22 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  236820 kbps
16:48:22 Calling EMAC_close()
16:49:30 PLLC configured: PLLM=20, PRE_DIV=1
16:49:30 Calling EMAC_open()
16:49:31 Calling EMAC_setReceiveFilter()
16:49:31 Waiting for PHY link initialization...
16:49:35 
16:49:35 Starting packet transfer...
16:49:39 ERROR: Timeout waiting for TX/RX
16:49:39 Sent 8192 packets, received 33 packets, packet size is 1514 bytes, achieve bandwidth    132 kbps
16:49:39 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981575 kbps
16:49:39 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978402 kbps
16:49:39 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973877 kbps
16:49:39 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966900 kbps
16:49:39 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954722 kbps
16:49:40 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  928253 kbps
16:49:40 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  449839 kbps
16:49:40 Calling EMAC_close()
16:55:01 PLLC configured: PLLM=20, PRE_DIV=1
16:55:01 Calling EMAC_open()
16:55:01 Calling EMAC_setReceiveFilter()
16:55:02 Waiting for PHY link initialization...
16:55:06 
16:55:06 Starting packet transfer...
16:55:09 ERROR: Timeout waiting for TX/RX
16:55:10 Sent 8192 packets, received 1886 packets, packet size is 1514 bytes, achieve bandwidth   7386 kbps
16:55:10 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981573 kbps
16:55:10 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978402 kbps
16:55:10 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973877 kbps
16:55:10 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966899 kbps
16:55:10 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954720 kbps
16:55:10 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  928252 kbps
16:55:11 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  437006 kbps
16:55:11 Calling EMAC_close()
17:01:01 PLLC configured: PLLM=20, PRE_DIV=1
17:01:01 Calling EMAC_open()
17:01:01 Calling EMAC_setReceiveFilter()
17:01:01 
17:01:02 Starting packet transfer...
17:01:02 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656245 kbps
17:01:02 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654687 kbps
17:01:02 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652582 kbps
17:01:02 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649579 kbps
17:01:02 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644950 kbps
17:01:02 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636880 kbps
17:01:03 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619273 kbps
17:01:03 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  434272 kbps
17:01:03 Calling EMAC_close()
17:20:18 PLLC configured: PLLM=20, PRE_DIV=1
17:20:18 Calling EMAC_open()
17:20:19 Calling EMAC_setReceiveFilter()
17:20:19 
17:20:19 Starting packet transfer...
17:20:19 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656245 kbps
17:20:19 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654687 kbps
17:20:19 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652582 kbps
17:20:19 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649579 kbps
17:20:20 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644950 kbps
17:20:20 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636880 kbps
17:20:20 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619273 kbps
17:20:20 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  434272 kbps
17:20:20 Calling EMAC_close()
17:20:56 PLLC configured: PLLM=20, PRE_DIV=1
17:20:56 Calling EMAC_open()
17:20:56 Calling EMAC_setReceiveFilter()
17:20:56 Waiting for PHY link initialization...
17:21:01 
17:21:01 Starting packet transfer...
17:21:04 ERROR: Timeout waiting for TX/RX
17:21:04 Sent 8192 packets, received 1073 packets, packet size is 1514 bytes, achieve bandwidth   4290 kbps
17:21:05 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981574 kbps
17:21:05 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978402 kbps
17:21:05 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973877 kbps
17:21:05 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966900 kbps
17:21:05 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954727 kbps
17:21:05 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  928251 kbps
17:21:05 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  435585 kbps
17:21:05 Calling EMAC_close()
17:28:58 PLLC configured: PLLM=20, PRE_DIV=1
17:28:58 Calling EMAC_open()
17:28:58 Calling EMAC_setReceiveFilter()
17:28:58 Waiting for PHY link initialization...
17:29:03 
17:29:03 Starting packet transfer...
17:29:06 ERROR: Timeout waiting for TX/RX
17:29:06 Sent 8192 packets, received 669 packets, packet size is 1514 bytes, achieve bandwidth   2694 kbps
17:29:07 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981574 kbps
17:29:07 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978402 kbps
17:29:07 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973877 kbps
17:29:07 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966900 kbps
17:29:07 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954727 kbps
17:29:07 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  928252 kbps
17:29:07 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  436315 kbps
17:29:08 Calling EMAC_close()
17:30:59 PLLC configured: PLLM=20, PRE_DIV=1
17:30:59 Calling EMAC_open()
17:30:59 Calling EMAC_setReceiveFilter()
17:30:59 
17:30:59 Starting packet transfer...
17:31:00 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656245 kbps
17:31:00 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654687 kbps
17:31:00 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652582 kbps
17:31:00 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649579 kbps
17:31:00 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644950 kbps
17:31:01 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636880 kbps
17:31:01 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619273 kbps
17:31:01 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  434264 kbps
17:31:01 Calling EMAC_close()
17:31:54 PLLC configured: PLLM=20, PRE_DIV=1
17:31:54 Calling EMAC_open()
17:31:54 Calling EMAC_setReceiveFilter()
17:31:54 Waiting for PHY link initialization...
17:31:59 
17:31:59 Starting packet transfer...
17:32:02 ERROR: Timeout waiting for TX/RX
17:32:02 Sent 8192 packets, received 1478 packets, packet size is 1514 bytes, achieve bandwidth   5892 kbps
17:32:02 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981573 kbps
17:32:03 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978402 kbps
17:32:03 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973877 kbps
17:32:03 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966900 kbps
17:32:03 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954727 kbps
17:32:03 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  928252 kbps
17:32:03 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  435453 kbps
17:32:03 Calling EMAC_close()
17:35:23 PLLC configured: PLLM=20, PRE_DIV=1
17:35:23 Calling EMAC_open()
17:35:24 Calling EMAC_setReceiveFilter()
17:35:24 Waiting for PHY link initialization...
17:35:28 
17:35:28 Starting packet transfer...
17:35:32 ERROR: Timeout waiting for TX/RX
17:35:32 Sent 8192 packets, received 991 packets, packet size is 1514 bytes, achieve bandwidth   3942 kbps
17:35:32 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981574 kbps
17:35:32 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978402 kbps
17:35:32 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973877 kbps
17:35:32 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966899 kbps
17:35:32 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954727 kbps
17:35:33 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  928251 kbps
17:35:33 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  435998 kbps
17:35:33 Calling EMAC_close()
17:50:30 PLLC configured: PLLM=20, PRE_DIV=1
17:50:30 Calling EMAC_open()
17:50:30 Calling EMAC_setReceiveFilter()
17:50:30 Waiting for PHY link initialization...
17:50:35 
17:50:35 Starting packet transfer...
17:50:35 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  520092 kbps
17:50:35 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981571 kbps
17:50:36 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978402 kbps
17:50:36 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973877 kbps
17:50:36 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966900 kbps
17:50:36 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954727 kbps
17:50:36 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  928248 kbps
17:50:36 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  434863 kbps
17:50:36 Calling EMAC_close()
17:51:44 PLLC configured: PLLM=20, PRE_DIV=1
17:51:44 Calling EMAC_open()
17:51:44 Calling EMAC_setReceiveFilter()
17:51:44 Waiting for PHY link initialization...
17:51:49 
17:51:49 Starting packet transfer...
17:51:49 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  534053 kbps
17:51:49 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981574 kbps
17:51:50 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978402 kbps
17:51:50 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973877 kbps
17:51:50 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966900 kbps
17:51:50 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954721 kbps
17:51:50 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  928252 kbps
17:51:50 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  435165 kbps
17:51:50 Calling EMAC_close()
17:52:40 PLLC configured: PLLM=20, PRE_DIV=1
17:52:40 Calling EMAC_open()
17:52:40 Calling EMAC_setReceiveFilter()
17:52:41 
17:52:41 Starting packet transfer...
17:52:41 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656245 kbps
17:52:41 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654688 kbps
17:52:41 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652582 kbps
17:52:41 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649580 kbps
17:52:41 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644950 kbps
17:52:42 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636880 kbps
17:52:42 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619273 kbps
17:52:42 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  434108 kbps
17:52:42 Calling EMAC_close()
17:54:52 PLLC configured: PLLM=20, PRE_DIV=1
17:54:52 Calling EMAC_open()
17:54:53 Calling EMAC_setReceiveFilter()
17:54:53 Waiting for PHY link initialization...
17:56:25 PLLC configured: PLLM=20, PRE_DIV=1
17:56:25 Calling EMAC_open()
17:56:25 Calling EMAC_setReceiveFilter()
17:56:25 Waiting for PHY link initialization...
17:59:24 PLLC configured: PLLM=20, PRE_DIV=1
17:59:25 Calling EMAC_open()
17:59:25 Calling EMAC_setReceiveFilter()
17:59:25 Waiting for PHY link initialization...
17:59:29 
17:59:29 Starting packet transfer...
17:59:30 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984335 kbps
17:59:30 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981995 kbps
17:59:30 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978832 kbps
17:59:30 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974321 kbps
17:59:30 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967363 kbps
17:59:30 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955243 kbps
17:59:30 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  651402 kbps
17:59:30 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  236495 kbps
17:59:30 Calling EMAC_close()
18:00:06 PLLC configured: PLLM=20, PRE_DIV=1
18:00:06 Calling EMAC_open()
18:00:06 Calling EMAC_setReceiveFilter()
18:00:06 
18:00:06 Starting packet transfer...
18:00:07 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984335 kbps
18:00:07 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981996 kbps
18:00:07 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978833 kbps
18:00:07 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974321 kbps
18:00:07 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967364 kbps
18:00:07 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955245 kbps
18:00:07 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  660709 kbps
18:00:07 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240114 kbps
18:00:07 Calling EMAC_close()
18:00:47 PLLC configured: PLLM=20, PRE_DIV=1
18:00:47 Calling EMAC_open()
18:00:47 Calling EMAC_setReceiveFilter()
18:00:47 Waiting for PHY link initialization...
18:00:50 
18:00:50 Starting packet transfer...
18:00:50 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  983900 kbps
18:00:50 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981543 kbps
18:00:50 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  494629 kbps
18:00:51 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973833 kbps
18:00:51 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966829 kbps
18:00:51 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954639 kbps
18:00:51 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  646188 kbps
18:00:51 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  234719 kbps
18:00:51 Calling EMAC_close()
18:01:51 PLLC configured: PLLM=20, PRE_DIV=1
18:01:51 Calling EMAC_open()
18:01:51 Calling EMAC_setReceiveFilter()
18:01:51 Waiting for PHY link initialization...
18:01:54 
18:01:54 Starting packet transfer...
18:01:54 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  983899 kbps
18:01:54 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  499268 kbps
18:01:54 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978376 kbps
18:01:55 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973846 kbps
18:01:55 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966830 kbps
18:01:55 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954660 kbps
18:01:55 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  646522 kbps
18:01:55 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  234712 kbps
18:01:55 Calling EMAC_close()
18:02:43 PLLC configured: PLLM=20, PRE_DIV=1
18:02:44 Calling EMAC_open()
18:02:44 Calling EMAC_setReceiveFilter()
18:02:44 
18:02:44 Starting packet transfer...
18:02:44 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  656240 kbps
18:02:44 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  654681 kbps
18:02:44 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  652575 kbps
18:02:45 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  649571 kbps
18:02:45 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  644939 kbps
18:02:45 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  636866 kbps
18:02:45 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  619251 kbps
18:02:45 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240124 kbps
18:02:45 Calling EMAC_close()
18:03:23 PLLC configured: PLLM=20, PRE_DIV=1
18:03:23 Calling EMAC_open()
18:03:23 Calling EMAC_setReceiveFilter()
18:03:23 
18:03:23 Starting packet transfer...
18:03:23 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  984335 kbps
18:03:23 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  981996 kbps
18:03:24 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978833 kbps
18:03:24 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  974321 kbps
18:03:24 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  967365 kbps
18:03:24 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  955245 kbps
18:03:24 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  660719 kbps
18:03:24 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  240125 kbps
18:03:24 Calling EMAC_close()
18:06:19 PLLC configured: PLLM=20, PRE_DIV=1
18:06:19 Calling EMAC_open()
18:06:19 Calling EMAC_setReceiveFilter()
18:06:19 Waiting for PHY link initialization...
18:06:22 
18:06:22 Starting packet transfer...
18:06:22 Sent 8192 packets, received 8192 packets, packet size is 1514 bytes, achieve bandwidth  983899 kbps
18:06:22 Sent 8192 packets, received 8192 packets, packet size is 1314 bytes, achieve bandwidth  512739 kbps
18:06:22 Sent 8192 packets, received 8192 packets, packet size is 1114 bytes, achieve bandwidth  978366 kbps
18:06:23 Sent 8192 packets, received 8192 packets, packet size is  914 bytes, achieve bandwidth  973846 kbps
18:06:23 Sent 8192 packets, received 8192 packets, packet size is  714 bytes, achieve bandwidth  966829 kbps
18:06:23 Sent 8192 packets, received 8192 packets, packet size is  514 bytes, achieve bandwidth  954649 kbps
18:06:23 Sent 8192 packets, received 8192 packets, packet size is  314 bytes, achieve bandwidth  646255 kbps
18:06:23 Sent 8192 packets, received 8192 packets, packet size is  114 bytes, achieve bandwidth  234801 kbps
18:06:23 Calling EMAC_close()
