<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<configurations XML_version="1.2" id="configurations_0">
<configuration XML_version="1.2" id="SEED XDS560V2 USB Emulator_0">
        <instance XML_version="1.2" desc="SEED XDS560V2 USB Emulator_0" href="connections/SEEDXDS560V2USB_Connection.xml" id="SEED XDS560V2 USB Emulator_0" xml="SEEDXDS560V2USB_Connection.xml" xmlpath="connections"/>
        <connection XML_version="1.2" id="SEED XDS560V2 USB Emulator_0">
            <instance XML_version="1.2" href="drivers/tixds560icepick_d.xml" id="drivers" xml="tixds560icepick_d.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560c66xx.xml" id="drivers" xml="tixds560c66xx.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560cs_dap.xml" id="drivers" xml="tixds560cs_dap.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560csstm.xml" id="drivers" xml="tixds560csstm.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560etbcs.xml" id="drivers" xml="tixds560etbcs.xml" xmlpath="drivers"/>
            <platform XML_version="1.2" id="platform_0">
                <instance XML_version="1.2" desc="TMS320C6657_0" href="devices/C6657.xml" id="TMS320C6657_0" xml="C6657.xml" xmlpath="devices"/>
            <device HW_revision="1" XML_version="1.2" description="C66x core" id="TMS320C6657_0" partnum="TMS320C6657">
                    <router HW_revision="1.0" XML_version="1.2" description="ICEPick_D Router" id="IcePick_D_0" isa="ICEPICK_D">
                        <subpath id="DAP">
                            <router HW_revision="1.0" XML_version="1.2" description="CS DAP Router" id="CS_DAP_DebugSS" isa="CS_DAP">
                                <subpath id="STM">
                                    <cpu HW_revision="1.0" XML_version="1.2" description="CS System Trace" id="CSSTM_0" isa="TMS470R26X">
                                        <property Type="choicelist" Value="1" id="bypass"/>
                                    </cpu>
                                    <cpu HW_revision="1.0" XML_version="1.2" description="CS Embedded Trace Buffer" id="TETB_STM" isa="CS_ETB">
                                        <property Type="choicelist" Value="1" id="bypass"/>
                                    </cpu>
                                </subpath>
                            </router>
                        </subpath>
                        <subpath id="subpath_1">
                            <cpu HW_revision="1.0" XML_version="1.2" description="C66xx CPU" id="C66xx_1" isa="TMS320c66xx">
                                <property Type="choicelist" Value="1" id="bypass"/>
                            </cpu>
                        </subpath>
                    </router>
                </device>
            </platform>
        </connection>
    </configuration>
</configurations>
