!_TAG_FILE_FORMAT	2	/extended format; --format=1 will not append ;" to lines/
!_TAG_FILE_SORTED	1	/0=unsorted, 1=sorted, 2=foldcase/
!_TAG_PROGRAM_AUTHOR	Darren Hiebert	/dhiebert@users.sourceforge.net/
!_TAG_PROGRAM_NAME	Exuberant Ctags	//
!_TAG_PROGRAM_URL	http://ctags.sourceforge.net	/official site/
!_TAG_PROGRAM_VERSION	5.8	//
ADC1	stm8s_stdperiph_driver\inc\stm8s.h	2492;"	macro
ADC1_ALIGN_LEFT	stm8s_stdperiph_driver\inc\stm8s_adc1.h	64;"	enumerator	enum:__anon45
ADC1_ALIGN_RIGHT	stm8s_stdperiph_driver\inc\stm8s_adc1.h	65;"	enumerator	enum:__anon45
ADC1_AWCRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	337;"	macro
ADC1_AWCRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	338;"	macro
ADC1_AWDChannelConfig	stm8s_stdperiph_driver\inc\stm8s_adc1.h	314;"	prototype	signature:(ADC1_Channel_TypeDef Channel, FunctionalState NewState)
ADC1_Align_TypeDef	stm8s_stdperiph_driver\inc\stm8s_adc1.h	66;"	typedef	typeref:enum:__anon45
ADC1_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2475;"	macro
ADC1_CHANNEL_0	stm8s_stdperiph_driver\inc\stm8s_adc1.h	151;"	enumerator	enum:__anon50
ADC1_CHANNEL_1	stm8s_stdperiph_driver\inc\stm8s_adc1.h	152;"	enumerator	enum:__anon50
ADC1_CHANNEL_12	stm8s_stdperiph_driver\inc\stm8s_adc1.h	161;"	enumerator	enum:__anon50
ADC1_CHANNEL_2	stm8s_stdperiph_driver\inc\stm8s_adc1.h	153;"	enumerator	enum:__anon50
ADC1_CHANNEL_3	stm8s_stdperiph_driver\inc\stm8s_adc1.h	154;"	enumerator	enum:__anon50
ADC1_CHANNEL_4	stm8s_stdperiph_driver\inc\stm8s_adc1.h	155;"	enumerator	enum:__anon50
ADC1_CHANNEL_5	stm8s_stdperiph_driver\inc\stm8s_adc1.h	156;"	enumerator	enum:__anon50
ADC1_CHANNEL_6	stm8s_stdperiph_driver\inc\stm8s_adc1.h	157;"	enumerator	enum:__anon50
ADC1_CHANNEL_7	stm8s_stdperiph_driver\inc\stm8s_adc1.h	158;"	enumerator	enum:__anon50
ADC1_CHANNEL_8	stm8s_stdperiph_driver\inc\stm8s_adc1.h	159;"	enumerator	enum:__anon50
ADC1_CHANNEL_9	stm8s_stdperiph_driver\inc\stm8s_adc1.h	160;"	enumerator	enum:__anon50
ADC1_CONVERSIONMODE_CONTINUOUS	stm8s_stdperiph_driver\inc\stm8s_adc1.h	142;"	enumerator	enum:__anon49
ADC1_CONVERSIONMODE_SINGLE	stm8s_stdperiph_driver\inc\stm8s_adc1.h	141;"	enumerator	enum:__anon49
ADC1_CR1_ADON	stm8s_stdperiph_driver\inc\stm8s.h	354;"	macro
ADC1_CR1_CONT	stm8s_stdperiph_driver\inc\stm8s.h	353;"	macro
ADC1_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	328;"	macro
ADC1_CR1_SPSEL	stm8s_stdperiph_driver\inc\stm8s.h	352;"	macro
ADC1_CR2_ALIGN	stm8s_stdperiph_driver\inc\stm8s.h	358;"	macro
ADC1_CR2_EXTSEL	stm8s_stdperiph_driver\inc\stm8s.h	357;"	macro
ADC1_CR2_EXTTRIG	stm8s_stdperiph_driver\inc\stm8s.h	356;"	macro
ADC1_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	329;"	macro
ADC1_CR2_SCAN	stm8s_stdperiph_driver\inc\stm8s.h	359;"	macro
ADC1_CR3_DBUF	stm8s_stdperiph_driver\inc\stm8s.h	361;"	macro
ADC1_CR3_OVR	stm8s_stdperiph_driver\inc\stm8s.h	362;"	macro
ADC1_CR3_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	330;"	macro
ADC1_CSR_AWD	stm8s_stdperiph_driver\inc\stm8s.h	347;"	macro
ADC1_CSR_AWDIE	stm8s_stdperiph_driver\inc\stm8s.h	349;"	macro
ADC1_CSR_CH	stm8s_stdperiph_driver\inc\stm8s.h	350;"	macro
ADC1_CSR_EOC	stm8s_stdperiph_driver\inc\stm8s.h	346;"	macro
ADC1_CSR_EOCIE	stm8s_stdperiph_driver\inc\stm8s.h	348;"	macro
ADC1_CSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	327;"	macro
ADC1_Channel_TypeDef	stm8s_stdperiph_driver\inc\stm8s_adc1.h	163;"	typedef	typeref:enum:__anon50
ADC1_ClearFlag	stm8s_stdperiph_driver\inc\stm8s_adc1.h	322;"	prototype	signature:(ADC1_Flag_TypeDef Flag)
ADC1_ClearITPendingBit	stm8s_stdperiph_driver\inc\stm8s_adc1.h	324;"	prototype	signature:(ADC1_IT_TypeDef ITPendingBit)
ADC1_Cmd	stm8s_stdperiph_driver\inc\stm8s_adc1.h	303;"	prototype	signature:(FunctionalState NewState)
ADC1_ConvMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_adc1.h	143;"	typedef	typeref:enum:__anon49
ADC1_ConversionConfig	stm8s_stdperiph_driver\inc\stm8s_adc1.h	310;"	prototype	signature:(ADC1_ConvMode_TypeDef ADC1_ConversionMode, ADC1_Channel_TypeDef ADC1_Channel, ADC1_Align_TypeDef ADC1_Align)
ADC1_DataBufferCmd	stm8s_stdperiph_driver\inc\stm8s_adc1.h	305;"	prototype	signature:(FunctionalState NewState)
ADC1_DeInit	stm8s_stdperiph_driver\inc\stm8s_adc1.h	295;"	prototype	signature:(void)
ADC1_EXTTRIG_GPIO	stm8s_stdperiph_driver\inc\stm8s_adc1.h	56;"	enumerator	enum:__anon44
ADC1_EXTTRIG_TIM	stm8s_stdperiph_driver\inc\stm8s_adc1.h	55;"	enumerator	enum:__anon44
ADC1_ExtTrig_TypeDef	stm8s_stdperiph_driver\inc\stm8s_adc1.h	57;"	typedef	typeref:enum:__anon44
ADC1_ExternalTriggerConfig	stm8s_stdperiph_driver\inc\stm8s_adc1.h	313;"	prototype	signature:(ADC1_ExtTrig_TypeDef ADC1_ExtTrigger, FunctionalState NewState)
ADC1_FLAG_AWD	stm8s_stdperiph_driver\inc\stm8s_adc1.h	98;"	enumerator	enum:__anon47
ADC1_FLAG_AWS0	stm8s_stdperiph_driver\inc\stm8s_adc1.h	99;"	enumerator	enum:__anon47
ADC1_FLAG_AWS1	stm8s_stdperiph_driver\inc\stm8s_adc1.h	100;"	enumerator	enum:__anon47
ADC1_FLAG_AWS12	stm8s_stdperiph_driver\inc\stm8s_adc1.h	109;"	enumerator	enum:__anon47
ADC1_FLAG_AWS2	stm8s_stdperiph_driver\inc\stm8s_adc1.h	101;"	enumerator	enum:__anon47
ADC1_FLAG_AWS3	stm8s_stdperiph_driver\inc\stm8s_adc1.h	102;"	enumerator	enum:__anon47
ADC1_FLAG_AWS4	stm8s_stdperiph_driver\inc\stm8s_adc1.h	103;"	enumerator	enum:__anon47
ADC1_FLAG_AWS5	stm8s_stdperiph_driver\inc\stm8s_adc1.h	104;"	enumerator	enum:__anon47
ADC1_FLAG_AWS6	stm8s_stdperiph_driver\inc\stm8s_adc1.h	105;"	enumerator	enum:__anon47
ADC1_FLAG_AWS7	stm8s_stdperiph_driver\inc\stm8s_adc1.h	106;"	enumerator	enum:__anon47
ADC1_FLAG_AWS8	stm8s_stdperiph_driver\inc\stm8s_adc1.h	107;"	enumerator	enum:__anon47
ADC1_FLAG_AWS9	stm8s_stdperiph_driver\inc\stm8s_adc1.h	108;"	enumerator	enum:__anon47
ADC1_FLAG_EOC	stm8s_stdperiph_driver\inc\stm8s_adc1.h	111;"	enumerator	enum:__anon47
ADC1_FLAG_OVR	stm8s_stdperiph_driver\inc\stm8s_adc1.h	97;"	enumerator	enum:__anon47
ADC1_Flag_TypeDef	stm8s_stdperiph_driver\inc\stm8s_adc1.h	112;"	typedef	typeref:enum:__anon47
ADC1_GetAWDChannelStatus	stm8s_stdperiph_driver\inc\stm8s_adc1.h	320;"	prototype	signature:(ADC1_Channel_TypeDef Channel)
ADC1_GetBufferValue	stm8s_stdperiph_driver\inc\stm8s_adc1.h	319;"	prototype	signature:(uint8_t Buffer)
ADC1_GetConversionValue	stm8s_stdperiph_driver\inc\stm8s_adc1.h	316;"	prototype	signature:(void)
ADC1_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_adc1.h	321;"	prototype	signature:(ADC1_Flag_TypeDef Flag)
ADC1_GetITStatus	stm8s_stdperiph_driver\inc\stm8s_adc1.h	323;"	prototype	signature:(ADC1_IT_TypeDef ITPendingBit)
ADC1_HTRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	334;"	macro
ADC1_HTRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	333;"	macro
ADC1_ITConfig	stm8s_stdperiph_driver\inc\stm8s_adc1.h	306;"	prototype	signature:(ADC1_IT_TypeDef ADC1_IT, FunctionalState NewState)
ADC1_IT_AWD	stm8s_stdperiph_driver\inc\stm8s_adc1.h	75;"	enumerator	enum:__anon46
ADC1_IT_AWDIE	stm8s_stdperiph_driver\inc\stm8s_adc1.h	73;"	enumerator	enum:__anon46
ADC1_IT_AWS0	stm8s_stdperiph_driver\inc\stm8s_adc1.h	76;"	enumerator	enum:__anon46
ADC1_IT_AWS1	stm8s_stdperiph_driver\inc\stm8s_adc1.h	77;"	enumerator	enum:__anon46
ADC1_IT_AWS12	stm8s_stdperiph_driver\inc\stm8s_adc1.h	86;"	enumerator	enum:__anon46
ADC1_IT_AWS2	stm8s_stdperiph_driver\inc\stm8s_adc1.h	78;"	enumerator	enum:__anon46
ADC1_IT_AWS3	stm8s_stdperiph_driver\inc\stm8s_adc1.h	79;"	enumerator	enum:__anon46
ADC1_IT_AWS4	stm8s_stdperiph_driver\inc\stm8s_adc1.h	80;"	enumerator	enum:__anon46
ADC1_IT_AWS5	stm8s_stdperiph_driver\inc\stm8s_adc1.h	81;"	enumerator	enum:__anon46
ADC1_IT_AWS6	stm8s_stdperiph_driver\inc\stm8s_adc1.h	82;"	enumerator	enum:__anon46
ADC1_IT_AWS7	stm8s_stdperiph_driver\inc\stm8s_adc1.h	83;"	enumerator	enum:__anon46
ADC1_IT_AWS8	stm8s_stdperiph_driver\inc\stm8s_adc1.h	84;"	enumerator	enum:__anon46
ADC1_IT_AWS9	stm8s_stdperiph_driver\inc\stm8s_adc1.h	85;"	enumerator	enum:__anon46
ADC1_IT_EOC	stm8s_stdperiph_driver\inc\stm8s_adc1.h	88;"	enumerator	enum:__anon46
ADC1_IT_EOCIE	stm8s_stdperiph_driver\inc\stm8s_adc1.h	74;"	enumerator	enum:__anon46
ADC1_IT_TypeDef	stm8s_stdperiph_driver\inc\stm8s_adc1.h	90;"	typedef	typeref:enum:__anon46
ADC1_Init	stm8s_stdperiph_driver\inc\stm8s_adc1.h	296;"	prototype	signature:(ADC1_ConvMode_TypeDef ADC1_ConversionMode, ADC1_Channel_TypeDef ADC1_Channel, ADC1_PresSel_TypeDef ADC1_PrescalerSelection, ADC1_ExtTrig_TypeDef ADC1_ExtTrigger, FunctionalState ADC1_ExtTriggerState, ADC1_Align_TypeDef ADC1_Align, ADC1_SchmittTrigg_TypeDef ADC1_SchmittTriggerChannel, FunctionalState ADC1_SchmittTriggerState)
ADC1_LTRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	335;"	macro
ADC1_LTRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	336;"	macro
ADC1_PRESSEL_FCPU_D10	stm8s_stdperiph_driver\inc\stm8s_adc1.h	45;"	enumerator	enum:__anon43
ADC1_PRESSEL_FCPU_D12	stm8s_stdperiph_driver\inc\stm8s_adc1.h	46;"	enumerator	enum:__anon43
ADC1_PRESSEL_FCPU_D18	stm8s_stdperiph_driver\inc\stm8s_adc1.h	47;"	enumerator	enum:__anon43
ADC1_PRESSEL_FCPU_D2	stm8s_stdperiph_driver\inc\stm8s_adc1.h	40;"	enumerator	enum:__anon43
ADC1_PRESSEL_FCPU_D3	stm8s_stdperiph_driver\inc\stm8s_adc1.h	41;"	enumerator	enum:__anon43
ADC1_PRESSEL_FCPU_D4	stm8s_stdperiph_driver\inc\stm8s_adc1.h	42;"	enumerator	enum:__anon43
ADC1_PRESSEL_FCPU_D6	stm8s_stdperiph_driver\inc\stm8s_adc1.h	43;"	enumerator	enum:__anon43
ADC1_PRESSEL_FCPU_D8	stm8s_stdperiph_driver\inc\stm8s_adc1.h	44;"	enumerator	enum:__anon43
ADC1_PresSel_TypeDef	stm8s_stdperiph_driver\inc\stm8s_adc1.h	48;"	typedef	typeref:enum:__anon43
ADC1_PrescalerConfig	stm8s_stdperiph_driver\inc\stm8s_adc1.h	307;"	prototype	signature:(ADC1_PresSel_TypeDef ADC1_Prescaler)
ADC1_SCHMITTTRIG_ALL	stm8s_stdperiph_driver\inc\stm8s_adc1.h	132;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL0	stm8s_stdperiph_driver\inc\stm8s_adc1.h	120;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL1	stm8s_stdperiph_driver\inc\stm8s_adc1.h	121;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL12	stm8s_stdperiph_driver\inc\stm8s_adc1.h	130;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL2	stm8s_stdperiph_driver\inc\stm8s_adc1.h	122;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL3	stm8s_stdperiph_driver\inc\stm8s_adc1.h	123;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL4	stm8s_stdperiph_driver\inc\stm8s_adc1.h	124;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL5	stm8s_stdperiph_driver\inc\stm8s_adc1.h	125;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL6	stm8s_stdperiph_driver\inc\stm8s_adc1.h	126;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL7	stm8s_stdperiph_driver\inc\stm8s_adc1.h	127;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL8	stm8s_stdperiph_driver\inc\stm8s_adc1.h	128;"	enumerator	enum:__anon48
ADC1_SCHMITTTRIG_CHANNEL9	stm8s_stdperiph_driver\inc\stm8s_adc1.h	129;"	enumerator	enum:__anon48
ADC1_ScanModeCmd	stm8s_stdperiph_driver\inc\stm8s_adc1.h	304;"	prototype	signature:(FunctionalState NewState)
ADC1_SchmittTrigg_TypeDef	stm8s_stdperiph_driver\inc\stm8s_adc1.h	133;"	typedef	typeref:enum:__anon48
ADC1_SchmittTriggerConfig	stm8s_stdperiph_driver\inc\stm8s_adc1.h	308;"	prototype	signature:(ADC1_SchmittTrigg_TypeDef ADC1_SchmittTriggerChannel, FunctionalState NewState)
ADC1_SetHighThreshold	stm8s_stdperiph_driver\inc\stm8s_adc1.h	317;"	prototype	signature:(uint16_t Threshold)
ADC1_SetLowThreshold	stm8s_stdperiph_driver\inc\stm8s_adc1.h	318;"	prototype	signature:(uint16_t Threshold)
ADC1_StartConversion	stm8s_stdperiph_driver\inc\stm8s_adc1.h	315;"	prototype	signature:(void)
ADC1_TDRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	332;"	macro
ADC1_TDRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	331;"	macro
ADC1_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	322;"	typedef	typeref:struct:ADC1_struct
ADC1_struct	stm8s_stdperiph_driver\inc\stm8s.h	282;"	struct
ADC2	stm8s_stdperiph_driver\inc\stm8s.h	2497;"	macro
ADC2_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2476;"	macro
ADC2_CR1_ADON	stm8s_stdperiph_driver\inc\stm8s.h	408;"	macro
ADC2_CR1_CONT	stm8s_stdperiph_driver\inc\stm8s.h	407;"	macro
ADC2_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	391;"	macro
ADC2_CR1_SPSEL	stm8s_stdperiph_driver\inc\stm8s.h	406;"	macro
ADC2_CR2_ALIGN	stm8s_stdperiph_driver\inc\stm8s.h	412;"	macro
ADC2_CR2_EXTSEL	stm8s_stdperiph_driver\inc\stm8s.h	411;"	macro
ADC2_CR2_EXTTRIG	stm8s_stdperiph_driver\inc\stm8s.h	410;"	macro
ADC2_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	392;"	macro
ADC2_CSR_CH	stm8s_stdperiph_driver\inc\stm8s.h	404;"	macro
ADC2_CSR_EOC	stm8s_stdperiph_driver\inc\stm8s.h	402;"	macro
ADC2_CSR_EOCIE	stm8s_stdperiph_driver\inc\stm8s.h	403;"	macro
ADC2_CSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	390;"	macro
ADC2_TDRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	394;"	macro
ADC2_TDRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	393;"	macro
ADC2_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	385;"	typedef	typeref:struct:ADC2_struct
ADC2_struct	stm8s_stdperiph_driver\inc\stm8s.h	374;"	struct
ADC_CH_LUSB_CUR	user\main.h	69;"	macro
ADC_CH_LUSB_VOL	user\main.h	68;"	macro
ADC_Configuration	user\config.c	95;"	function	signature:(void)
ADC_Configuration	user\main.h	144;"	prototype	signature:(void)
ADC_Convert	user\adc.c	3;"	function	signature:(uint8_t ch, uint8_t times)
ADC_Convert	user\main.h	130;"	prototype	signature:(uint8_t ch, uint8_t times)
APR	stm8s_stdperiph_driver\inc\stm8s.h	427;"	member	struct:AWU_struct
APR_Array	stm8s_stdperiph_driver\src\stm8s_awu.c	43;"	variable
AREA	stm8s_stdperiph_driver\inc\stm8s.h	2704;"	macro
ARR	stm8s_stdperiph_driver\inc\stm8s.h	1054;"	member	struct:TIM4_struct
ARR	stm8s_stdperiph_driver\inc\stm8s.h	1254;"	member	struct:TIM6_struct
ARRH	stm8s_stdperiph_driver\inc\stm8s.h	1122;"	member	struct:TIM5_struct
ARRH	stm8s_stdperiph_driver\inc\stm8s.h	616;"	member	struct:TIM1_struct
ARRH	stm8s_stdperiph_driver\inc\stm8s.h	827;"	member	struct:TIM2_struct
ARRH	stm8s_stdperiph_driver\inc\stm8s.h	949;"	member	struct:TIM3_struct
ARRL	stm8s_stdperiph_driver\inc\stm8s.h	1123;"	member	struct:TIM5_struct
ARRL	stm8s_stdperiph_driver\inc\stm8s.h	617;"	member	struct:TIM1_struct
ARRL	stm8s_stdperiph_driver\inc\stm8s.h	828;"	member	struct:TIM2_struct
ARRL	stm8s_stdperiph_driver\inc\stm8s.h	950;"	member	struct:TIM3_struct
AWCRH	stm8s_stdperiph_driver\inc\stm8s.h	319;"	member	struct:ADC1_struct
AWCRL	stm8s_stdperiph_driver\inc\stm8s.h	320;"	member	struct:ADC1_struct
AWSRH	stm8s_stdperiph_driver\inc\stm8s.h	317;"	member	struct:ADC1_struct
AWSRL	stm8s_stdperiph_driver\inc\stm8s.h	318;"	member	struct:ADC1_struct
AWU	stm8s_stdperiph_driver\inc\stm8s.h	2500;"	macro
AWU_APR_APR	stm8s_stdperiph_driver\inc\stm8s.h	451;"	macro
AWU_APR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	436;"	macro
AWU_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2462;"	macro
AWU_CSR_AWUEN	stm8s_stdperiph_driver\inc\stm8s.h	448;"	macro
AWU_CSR_AWUF	stm8s_stdperiph_driver\inc\stm8s.h	447;"	macro
AWU_CSR_MSR	stm8s_stdperiph_driver\inc\stm8s.h	449;"	macro
AWU_CSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	435;"	macro
AWU_Cmd	stm8s_stdperiph_driver\inc\stm8s_awu.h	129;"	prototype	signature:(FunctionalState NewState)
AWU_Cmd	stm8s_stdperiph_driver\src\stm8s_awu.c	108;"	function	signature:(FunctionalState NewState)
AWU_Configuration	user\config.c	142;"	function	signature:(void)
AWU_Configuration	user\main.h	146;"	prototype	signature:(void)
AWU_DeInit	stm8s_stdperiph_driver\inc\stm8s_awu.h	127;"	prototype	signature:(void)
AWU_DeInit	stm8s_stdperiph_driver\src\stm8s_awu.c	67;"	function	signature:(void)
AWU_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_awu.h	132;"	prototype	signature:(void)
AWU_GetFlagStatus	stm8s_stdperiph_driver\src\stm8s_awu.c	180;"	function	signature:(void)
AWU_IRQHandler	stm8_interrupt_vector.c	23;"	function	signature:(void)
AWU_IdleModeEnable	stm8s_stdperiph_driver\inc\stm8s_awu.h	131;"	prototype	signature:(void)
AWU_IdleModeEnable	stm8s_stdperiph_driver\src\stm8s_awu.c	165;"	function	signature:(void)
AWU_Init	stm8s_stdperiph_driver\inc\stm8s_awu.h	128;"	prototype	signature:(AWU_Timebase_TypeDef AWU_TimeBase)
AWU_Init	stm8s_stdperiph_driver\src\stm8s_awu.c	82;"	function	signature:(AWU_Timebase_TypeDef AWU_TimeBase)
AWU_LSICalibrationConfig	stm8s_stdperiph_driver\inc\stm8s_awu.h	130;"	prototype	signature:(uint32_t LSIFreqHz)
AWU_LSICalibrationConfig	stm8s_stdperiph_driver\src\stm8s_awu.c	135;"	function	signature:(uint32_t LSIFreqHz)
AWU_Start	user\main.h	65;"	macro
AWU_Stop	user\main.h	66;"	macro
AWU_TBR_AWUTB	stm8s_stdperiph_driver\inc\stm8s.h	453;"	macro
AWU_TBR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	437;"	macro
AWU_TIMEBASE_128MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	51;"	enumerator	enum:__anon14
AWU_TIMEBASE_12S	stm8s_stdperiph_driver\inc\stm8s_awu.h	56;"	enumerator	enum:__anon14
AWU_TIMEBASE_16MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	48;"	enumerator	enum:__anon14
AWU_TIMEBASE_1MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	44;"	enumerator	enum:__anon14
AWU_TIMEBASE_1S	stm8s_stdperiph_driver\inc\stm8s_awu.h	54;"	enumerator	enum:__anon14
AWU_TIMEBASE_250US	stm8s_stdperiph_driver\inc\stm8s_awu.h	42;"	enumerator	enum:__anon14
AWU_TIMEBASE_256MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	52;"	enumerator	enum:__anon14
AWU_TIMEBASE_2MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	45;"	enumerator	enum:__anon14
AWU_TIMEBASE_2S	stm8s_stdperiph_driver\inc\stm8s_awu.h	55;"	enumerator	enum:__anon14
AWU_TIMEBASE_30S	stm8s_stdperiph_driver\inc\stm8s_awu.h	57;"	enumerator	enum:__anon14
AWU_TIMEBASE_32MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	49;"	enumerator	enum:__anon14
AWU_TIMEBASE_4MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	46;"	enumerator	enum:__anon14
AWU_TIMEBASE_500US	stm8s_stdperiph_driver\inc\stm8s_awu.h	43;"	enumerator	enum:__anon14
AWU_TIMEBASE_512MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	53;"	enumerator	enum:__anon14
AWU_TIMEBASE_64MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	50;"	enumerator	enum:__anon14
AWU_TIMEBASE_8MS	stm8s_stdperiph_driver\inc\stm8s_awu.h	47;"	enumerator	enum:__anon14
AWU_TIMEBASE_NO_IT	stm8s_stdperiph_driver\inc\stm8s_awu.h	41;"	enumerator	enum:__anon14
AWU_Timebase_TypeDef	stm8s_stdperiph_driver\inc\stm8s_awu.h	58;"	typedef	typeref:enum:__anon14
AWU_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	430;"	typedef	typeref:struct:AWU_struct
AWU_struct	stm8s_stdperiph_driver\inc\stm8s.h	424;"	struct
AffBit	stm8s_stdperiph_driver\inc\stm8s.h	2678;"	macro
BAT_Charge	user\battery.c	40;"	function	signature:(void)
BAT_Charge	user\main.h	137;"	prototype	signature:(void)
BAT_Discharge	user\battery.c	3;"	function	signature:(void)
BAT_Discharge	user\main.h	136;"	prototype	signature:(void)
BAT_VOL_HIGH	user\main.h	101;"	macro
BAT_VOL_HIGHEST	user\main.h	102;"	macro
BAT_VOL_LEVEL_1	user\main.h	104;"	macro
BAT_VOL_LEVEL_2	user\main.h	105;"	macro
BAT_VOL_LEVEL_3	user\main.h	106;"	macro
BAT_VOL_LEVEL_4	user\main.h	107;"	macro
BAT_VOL_LEVEL_5	user\main.h	108;"	macro
BAT_VOL_LOW	user\main.h	99;"	macro
BAT_VOL_LOWEST	user\main.h	98;"	macro
BAT_VOL_MIDDLE	user\main.h	100;"	macro
BAT_VolLevel	user\main.c	5;"	variable
BEEP	stm8s_stdperiph_driver\inc\stm8s.h	2502;"	macro
BEEP_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2463;"	macro
BEEP_CALIBRATION_DEFAULT	stm8s_stdperiph_driver\inc\stm8s_beep.h	55;"	macro
BEEP_CSR_BEEPDIV	stm8s_stdperiph_driver\inc\stm8s.h	483;"	macro
BEEP_CSR_BEEPEN	stm8s_stdperiph_driver\inc\stm8s.h	482;"	macro
BEEP_CSR_BEEPSEL	stm8s_stdperiph_driver\inc\stm8s.h	481;"	macro
BEEP_CSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	473;"	macro
BEEP_Cmd	stm8s_stdperiph_driver\inc\stm8s_beep.h	102;"	prototype	signature:(FunctionalState NewState)
BEEP_DeInit	stm8s_stdperiph_driver\inc\stm8s_beep.h	100;"	prototype	signature:(void)
BEEP_FREQUENCY_1KHZ	stm8s_stdperiph_driver\inc\stm8s_beep.h	40;"	enumerator	enum:__anon51
BEEP_FREQUENCY_2KHZ	stm8s_stdperiph_driver\inc\stm8s_beep.h	41;"	enumerator	enum:__anon51
BEEP_FREQUENCY_4KHZ	stm8s_stdperiph_driver\inc\stm8s_beep.h	42;"	enumerator	enum:__anon51
BEEP_Frequency_TypeDef	stm8s_stdperiph_driver\inc\stm8s_beep.h	43;"	typedef	typeref:enum:__anon51
BEEP_Init	stm8s_stdperiph_driver\inc\stm8s_beep.h	101;"	prototype	signature:(BEEP_Frequency_TypeDef BEEP_Frequency)
BEEP_LSICalibrationConfig	stm8s_stdperiph_driver\inc\stm8s_beep.h	103;"	prototype	signature:(uint32_t LSIFreqHz)
BEEP_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	468;"	typedef	typeref:struct:BEEP_struct
BEEP_struct	stm8s_stdperiph_driver\inc\stm8s.h	464;"	struct
BKR	stm8s_stdperiph_driver\inc\stm8s.h	627;"	member	struct:TIM1_struct
BQ24195_Init	user\i2c_bq24195.c	67;"	function	signature:(void)
BQ24195_Init	user\main.h	127;"	prototype	signature:(void)
BRR1	stm8s_stdperiph_driver\inc\stm8s.h	1755;"	member	struct:UART1_struct
BRR1	stm8s_stdperiph_driver\inc\stm8s.h	1853;"	member	struct:UART2_struct
BRR1	stm8s_stdperiph_driver\inc\stm8s.h	1961;"	member	struct:UART3_struct
BRR2	stm8s_stdperiph_driver\inc\stm8s.h	1756;"	member	struct:UART1_struct
BRR2	stm8s_stdperiph_driver\inc\stm8s.h	1854;"	member	struct:UART2_struct
BRR2	stm8s_stdperiph_driver\inc\stm8s.h	1962;"	member	struct:UART3_struct
BTR1	stm8s_stdperiph_driver\inc\stm8s.h	2179;"	member	struct:__anon5::__anon6::__anon12
BTR2	stm8s_stdperiph_driver\inc\stm8s.h	2180;"	member	struct:__anon5::__anon6::__anon12
BYTE_0	stm8s_stdperiph_driver\inc\stm8s.h	2685;"	macro
BYTE_1	stm8s_stdperiph_driver\inc\stm8s.h	2686;"	macro
BYTE_2	stm8s_stdperiph_driver\inc\stm8s.h	2687;"	macro
BYTE_3	stm8s_stdperiph_driver\inc\stm8s.h	2688;"	macro
BitAction	stm8s_stdperiph_driver\inc\stm8s.h	221;"	typedef	typeref:enum:__anon2
BitClr	stm8s_stdperiph_driver\inc\stm8s.h	2706;"	macro
BitSet	stm8s_stdperiph_driver\inc\stm8s.h	2707;"	macro
BitStatus	stm8s_stdperiph_driver\inc\stm8s.h	221;"	typedef	typeref:enum:__anon2
BitVal	stm8s_stdperiph_driver\inc\stm8s.h	2708;"	macro
CAN	stm8s_stdperiph_driver\inc\stm8s.h	2505;"	macro
CAN_BTR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2390;"	macro
CAN_BTR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2391;"	macro
CAN_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2477;"	macro
CAN_DGR_LBKM	stm8s_stdperiph_driver\inc\stm8s.h	2266;"	macro
CAN_DGR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2383;"	macro
CAN_DGR_RX	stm8s_stdperiph_driver\inc\stm8s.h	2269;"	macro
CAN_DGR_SAMP	stm8s_stdperiph_driver\inc\stm8s.h	2268;"	macro
CAN_DGR_SLIM	stm8s_stdperiph_driver\inc\stm8s.h	2267;"	macro
CAN_DGR_TXM2E	stm8s_stdperiph_driver\inc\stm8s.h	2270;"	macro
CAN_EIER_BOFIE	stm8s_stdperiph_driver\inc\stm8s.h	2307;"	macro
CAN_EIER_EPVIE	stm8s_stdperiph_driver\inc\stm8s.h	2306;"	macro
CAN_EIER_ERRIE	stm8s_stdperiph_driver\inc\stm8s.h	2309;"	macro
CAN_EIER_EWGIE	stm8s_stdperiph_driver\inc\stm8s.h	2305;"	macro
CAN_EIER_LECIE	stm8s_stdperiph_driver\inc\stm8s.h	2308;"	macro
CAN_EIER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2387;"	macro
CAN_ESR_BOFF	stm8s_stdperiph_driver\inc\stm8s.h	2298;"	macro
CAN_ESR_EPVF	stm8s_stdperiph_driver\inc\stm8s.h	2297;"	macro
CAN_ESR_EWGF	stm8s_stdperiph_driver\inc\stm8s.h	2296;"	macro
CAN_ESR_LEC	stm8s_stdperiph_driver\inc\stm8s.h	2302;"	macro
CAN_ESR_LEC0	stm8s_stdperiph_driver\inc\stm8s.h	2299;"	macro
CAN_ESR_LEC1	stm8s_stdperiph_driver\inc\stm8s.h	2300;"	macro
CAN_ESR_LEC2	stm8s_stdperiph_driver\inc\stm8s.h	2301;"	macro
CAN_ESR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2386;"	macro
CAN_FCR1_FACT0	stm8s_stdperiph_driver\inc\stm8s.h	2347;"	macro
CAN_FCR1_FACT1	stm8s_stdperiph_driver\inc\stm8s.h	2348;"	macro
CAN_FCR1_FSC00	stm8s_stdperiph_driver\inc\stm8s.h	2354;"	macro
CAN_FCR1_FSC01	stm8s_stdperiph_driver\inc\stm8s.h	2355;"	macro
CAN_FCR1_FSC10	stm8s_stdperiph_driver\inc\stm8s.h	2356;"	macro
CAN_FCR1_FSC11	stm8s_stdperiph_driver\inc\stm8s.h	2357;"	macro
CAN_FCR2_FACT2	stm8s_stdperiph_driver\inc\stm8s.h	2349;"	macro
CAN_FCR2_FACT3	stm8s_stdperiph_driver\inc\stm8s.h	2350;"	macro
CAN_FCR2_FSC20	stm8s_stdperiph_driver\inc\stm8s.h	2358;"	macro
CAN_FCR2_FSC21	stm8s_stdperiph_driver\inc\stm8s.h	2359;"	macro
CAN_FCR2_FSC30	stm8s_stdperiph_driver\inc\stm8s.h	2360;"	macro
CAN_FCR2_FSC31	stm8s_stdperiph_driver\inc\stm8s.h	2361;"	macro
CAN_FCR3_FACT4	stm8s_stdperiph_driver\inc\stm8s.h	2351;"	macro
CAN_FCR3_FACT5	stm8s_stdperiph_driver\inc\stm8s.h	2352;"	macro
CAN_FCR3_FSC40	stm8s_stdperiph_driver\inc\stm8s.h	2362;"	macro
CAN_FCR3_FSC41	stm8s_stdperiph_driver\inc\stm8s.h	2363;"	macro
CAN_FCR3_FSC50	stm8s_stdperiph_driver\inc\stm8s.h	2364;"	macro
CAN_FCR3_FSC51	stm8s_stdperiph_driver\inc\stm8s.h	2365;"	macro
CAN_FCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2394;"	macro
CAN_FMR1_FMH0	stm8s_stdperiph_driver\inc\stm8s.h	2333;"	macro
CAN_FMR1_FMH1	stm8s_stdperiph_driver\inc\stm8s.h	2335;"	macro
CAN_FMR1_FMH2	stm8s_stdperiph_driver\inc\stm8s.h	2337;"	macro
CAN_FMR1_FMH3	stm8s_stdperiph_driver\inc\stm8s.h	2339;"	macro
CAN_FMR1_FML0	stm8s_stdperiph_driver\inc\stm8s.h	2332;"	macro
CAN_FMR1_FML1	stm8s_stdperiph_driver\inc\stm8s.h	2334;"	macro
CAN_FMR1_FML2	stm8s_stdperiph_driver\inc\stm8s.h	2336;"	macro
CAN_FMR1_FML3	stm8s_stdperiph_driver\inc\stm8s.h	2338;"	macro
CAN_FMR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2392;"	macro
CAN_FMR2_FMH4	stm8s_stdperiph_driver\inc\stm8s.h	2342;"	macro
CAN_FMR2_FMH5	stm8s_stdperiph_driver\inc\stm8s.h	2344;"	macro
CAN_FMR2_FML4	stm8s_stdperiph_driver\inc\stm8s.h	2341;"	macro
CAN_FMR2_FML5	stm8s_stdperiph_driver\inc\stm8s.h	2343;"	macro
CAN_FMR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2393;"	macro
CAN_IER_FFIE	stm8s_stdperiph_driver\inc\stm8s.h	2260;"	macro
CAN_IER_FMPIE	stm8s_stdperiph_driver\inc\stm8s.h	2259;"	macro
CAN_IER_FOVIE	stm8s_stdperiph_driver\inc\stm8s.h	2261;"	macro
CAN_IER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2382;"	macro
CAN_IER_TMEIE	stm8s_stdperiph_driver\inc\stm8s.h	2258;"	macro
CAN_IER_WKUIE	stm8s_stdperiph_driver\inc\stm8s.h	2262;"	macro
CAN_MCR_ABOM	stm8s_stdperiph_driver\inc\stm8s.h	2224;"	macro
CAN_MCR_AWUM	stm8s_stdperiph_driver\inc\stm8s.h	2223;"	macro
CAN_MCR_INRQ	stm8s_stdperiph_driver\inc\stm8s.h	2218;"	macro
CAN_MCR_NART	stm8s_stdperiph_driver\inc\stm8s.h	2222;"	macro
CAN_MCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2377;"	macro
CAN_MCR_RFLM	stm8s_stdperiph_driver\inc\stm8s.h	2221;"	macro
CAN_MCR_SLEEP	stm8s_stdperiph_driver\inc\stm8s.h	2219;"	macro
CAN_MCR_TTCM	stm8s_stdperiph_driver\inc\stm8s.h	2225;"	macro
CAN_MCR_TXFP	stm8s_stdperiph_driver\inc\stm8s.h	2220;"	macro
CAN_MCSR_ABRQ	stm8s_stdperiph_driver\inc\stm8s.h	2280;"	macro
CAN_MCSR_ALST	stm8s_stdperiph_driver\inc\stm8s.h	2283;"	macro
CAN_MCSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2398;"	macro
CAN_MCSR_RQCP	stm8s_stdperiph_driver\inc\stm8s.h	2281;"	macro
CAN_MCSR_TERR	stm8s_stdperiph_driver\inc\stm8s.h	2284;"	macro
CAN_MCSR_TXOK	stm8s_stdperiph_driver\inc\stm8s.h	2282;"	macro
CAN_MCSR_TXRQ	stm8s_stdperiph_driver\inc\stm8s.h	2279;"	macro
CAN_MDLCR_DLC	stm8s_stdperiph_driver\inc\stm8s.h	2286;"	macro
CAN_MDLCR_TGT	stm8s_stdperiph_driver\inc\stm8s.h	2287;"	macro
CAN_MDLC_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2397;"	macro
CAN_MFMI_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2396;"	macro
CAN_MIDR1_IDE	stm8s_stdperiph_driver\inc\stm8s.h	2290;"	macro
CAN_MIDR1_RTR	stm8s_stdperiph_driver\inc\stm8s.h	2289;"	macro
CAN_MSR_ERRI	stm8s_stdperiph_driver\inc\stm8s.h	2230;"	macro
CAN_MSR_INAK	stm8s_stdperiph_driver\inc\stm8s.h	2228;"	macro
CAN_MSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2378;"	macro
CAN_MSR_RX	stm8s_stdperiph_driver\inc\stm8s.h	2233;"	macro
CAN_MSR_SLAK	stm8s_stdperiph_driver\inc\stm8s.h	2229;"	macro
CAN_MSR_TX	stm8s_stdperiph_driver\inc\stm8s.h	2232;"	macro
CAN_MSR_WKUI	stm8s_stdperiph_driver\inc\stm8s.h	2231;"	macro
CAN_PSR_PS0	stm8s_stdperiph_driver\inc\stm8s.h	2274;"	macro
CAN_PSR_PS1	stm8s_stdperiph_driver\inc\stm8s.h	2275;"	macro
CAN_PSR_PS2	stm8s_stdperiph_driver\inc\stm8s.h	2276;"	macro
CAN_PSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2384;"	macro
CAN_RECR_REC0	stm8s_stdperiph_driver\inc\stm8s.h	2322;"	macro
CAN_RECR_REC1	stm8s_stdperiph_driver\inc\stm8s.h	2323;"	macro
CAN_RECR_REC2	stm8s_stdperiph_driver\inc\stm8s.h	2324;"	macro
CAN_RECR_REC3	stm8s_stdperiph_driver\inc\stm8s.h	2325;"	macro
CAN_RECR_REC4	stm8s_stdperiph_driver\inc\stm8s.h	2326;"	macro
CAN_RECR_REC5	stm8s_stdperiph_driver\inc\stm8s.h	2327;"	macro
CAN_RECR_REC6	stm8s_stdperiph_driver\inc\stm8s.h	2328;"	macro
CAN_RECR_REC7	stm8s_stdperiph_driver\inc\stm8s.h	2329;"	macro
CAN_RECR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2389;"	macro
CAN_RFR_FMP01	stm8s_stdperiph_driver\inc\stm8s.h	2252;"	macro
CAN_RFR_FOVR	stm8s_stdperiph_driver\inc\stm8s.h	2254;"	macro
CAN_RFR_FULL	stm8s_stdperiph_driver\inc\stm8s.h	2253;"	macro
CAN_RFR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2381;"	macro
CAN_RFR_RFOM	stm8s_stdperiph_driver\inc\stm8s.h	2255;"	macro
CAN_TECR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2388;"	macro
CAN_TECR_TEC0	stm8s_stdperiph_driver\inc\stm8s.h	2312;"	macro
CAN_TECR_TEC1	stm8s_stdperiph_driver\inc\stm8s.h	2313;"	macro
CAN_TECR_TEC2	stm8s_stdperiph_driver\inc\stm8s.h	2314;"	macro
CAN_TECR_TEC3	stm8s_stdperiph_driver\inc\stm8s.h	2315;"	macro
CAN_TECR_TEC4	stm8s_stdperiph_driver\inc\stm8s.h	2316;"	macro
CAN_TECR_TEC5	stm8s_stdperiph_driver\inc\stm8s.h	2317;"	macro
CAN_TECR_TEC6	stm8s_stdperiph_driver\inc\stm8s.h	2318;"	macro
CAN_TECR_TEC7	stm8s_stdperiph_driver\inc\stm8s.h	2319;"	macro
CAN_TPR_CODE0	stm8s_stdperiph_driver\inc\stm8s.h	2244;"	macro
CAN_TPR_LOW0	stm8s_stdperiph_driver\inc\stm8s.h	2248;"	macro
CAN_TPR_LOW1	stm8s_stdperiph_driver\inc\stm8s.h	2249;"	macro
CAN_TPR_LOW2	stm8s_stdperiph_driver\inc\stm8s.h	2250;"	macro
CAN_TPR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2380;"	macro
CAN_TPR_TME0	stm8s_stdperiph_driver\inc\stm8s.h	2245;"	macro
CAN_TPR_TME1	stm8s_stdperiph_driver\inc\stm8s.h	2246;"	macro
CAN_TPR_TME2	stm8s_stdperiph_driver\inc\stm8s.h	2247;"	macro
CAN_TSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2379;"	macro
CAN_TSR_RQCP0	stm8s_stdperiph_driver\inc\stm8s.h	2236;"	macro
CAN_TSR_RQCP012	stm8s_stdperiph_driver\inc\stm8s.h	2239;"	macro
CAN_TSR_RQCP1	stm8s_stdperiph_driver\inc\stm8s.h	2237;"	macro
CAN_TSR_RQCP2	stm8s_stdperiph_driver\inc\stm8s.h	2238;"	macro
CAN_TSR_TXOK0	stm8s_stdperiph_driver\inc\stm8s.h	2240;"	macro
CAN_TSR_TXOK1	stm8s_stdperiph_driver\inc\stm8s.h	2241;"	macro
CAN_TSR_TXOK2	stm8s_stdperiph_driver\inc\stm8s.h	2242;"	macro
CAN_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	2212;"	typedef	typeref:struct:__anon5
CCER1	stm8s_stdperiph_driver\inc\stm8s.h	1117;"	member	struct:TIM5_struct
CCER1	stm8s_stdperiph_driver\inc\stm8s.h	610;"	member	struct:TIM1_struct
CCER1	stm8s_stdperiph_driver\inc\stm8s.h	822;"	member	struct:TIM2_struct
CCER1	stm8s_stdperiph_driver\inc\stm8s.h	945;"	member	struct:TIM3_struct
CCER2	stm8s_stdperiph_driver\inc\stm8s.h	1118;"	member	struct:TIM5_struct
CCER2	stm8s_stdperiph_driver\inc\stm8s.h	611;"	member	struct:TIM1_struct
CCER2	stm8s_stdperiph_driver\inc\stm8s.h	823;"	member	struct:TIM2_struct
CCMR1	stm8s_stdperiph_driver\inc\stm8s.h	1114;"	member	struct:TIM5_struct
CCMR1	stm8s_stdperiph_driver\inc\stm8s.h	606;"	member	struct:TIM1_struct
CCMR1	stm8s_stdperiph_driver\inc\stm8s.h	819;"	member	struct:TIM2_struct
CCMR1	stm8s_stdperiph_driver\inc\stm8s.h	943;"	member	struct:TIM3_struct
CCMR2	stm8s_stdperiph_driver\inc\stm8s.h	1115;"	member	struct:TIM5_struct
CCMR2	stm8s_stdperiph_driver\inc\stm8s.h	607;"	member	struct:TIM1_struct
CCMR2	stm8s_stdperiph_driver\inc\stm8s.h	820;"	member	struct:TIM2_struct
CCMR2	stm8s_stdperiph_driver\inc\stm8s.h	944;"	member	struct:TIM3_struct
CCMR3	stm8s_stdperiph_driver\inc\stm8s.h	1116;"	member	struct:TIM5_struct
CCMR3	stm8s_stdperiph_driver\inc\stm8s.h	608;"	member	struct:TIM1_struct
CCMR3	stm8s_stdperiph_driver\inc\stm8s.h	821;"	member	struct:TIM2_struct
CCMR4	stm8s_stdperiph_driver\inc\stm8s.h	609;"	member	struct:TIM1_struct
CCMR_TIxDirect_Set	stm8s_stdperiph_driver\inc\stm8s.h	739;"	macro
CCOR	stm8s_stdperiph_driver\inc\stm8s.h	503;"	member	struct:CLK_struct
CCR1H	stm8s_stdperiph_driver\inc\stm8s.h	1124;"	member	struct:TIM5_struct
CCR1H	stm8s_stdperiph_driver\inc\stm8s.h	619;"	member	struct:TIM1_struct
CCR1H	stm8s_stdperiph_driver\inc\stm8s.h	829;"	member	struct:TIM2_struct
CCR1H	stm8s_stdperiph_driver\inc\stm8s.h	951;"	member	struct:TIM3_struct
CCR1L	stm8s_stdperiph_driver\inc\stm8s.h	1125;"	member	struct:TIM5_struct
CCR1L	stm8s_stdperiph_driver\inc\stm8s.h	620;"	member	struct:TIM1_struct
CCR1L	stm8s_stdperiph_driver\inc\stm8s.h	830;"	member	struct:TIM2_struct
CCR1L	stm8s_stdperiph_driver\inc\stm8s.h	952;"	member	struct:TIM3_struct
CCR2H	stm8s_stdperiph_driver\inc\stm8s.h	1126;"	member	struct:TIM5_struct
CCR2H	stm8s_stdperiph_driver\inc\stm8s.h	621;"	member	struct:TIM1_struct
CCR2H	stm8s_stdperiph_driver\inc\stm8s.h	831;"	member	struct:TIM2_struct
CCR2H	stm8s_stdperiph_driver\inc\stm8s.h	953;"	member	struct:TIM3_struct
CCR2L	stm8s_stdperiph_driver\inc\stm8s.h	1127;"	member	struct:TIM5_struct
CCR2L	stm8s_stdperiph_driver\inc\stm8s.h	622;"	member	struct:TIM1_struct
CCR2L	stm8s_stdperiph_driver\inc\stm8s.h	832;"	member	struct:TIM2_struct
CCR2L	stm8s_stdperiph_driver\inc\stm8s.h	954;"	member	struct:TIM3_struct
CCR3H	stm8s_stdperiph_driver\inc\stm8s.h	1128;"	member	struct:TIM5_struct
CCR3H	stm8s_stdperiph_driver\inc\stm8s.h	623;"	member	struct:TIM1_struct
CCR3H	stm8s_stdperiph_driver\inc\stm8s.h	833;"	member	struct:TIM2_struct
CCR3L	stm8s_stdperiph_driver\inc\stm8s.h	1129;"	member	struct:TIM5_struct
CCR3L	stm8s_stdperiph_driver\inc\stm8s.h	624;"	member	struct:TIM1_struct
CCR3L	stm8s_stdperiph_driver\inc\stm8s.h	834;"	member	struct:TIM2_struct
CCR4H	stm8s_stdperiph_driver\inc\stm8s.h	625;"	member	struct:TIM1_struct
CCR4L	stm8s_stdperiph_driver\inc\stm8s.h	626;"	member	struct:TIM1_struct
CCRH	stm8s_stdperiph_driver\inc\stm8s.h	1326;"	member	struct:I2C_struct
CCRL	stm8s_stdperiph_driver\inc\stm8s.h	1325;"	member	struct:I2C_struct
CFG	stm8s_stdperiph_driver\inc\stm8s.h	2587;"	macro
CFG_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2478;"	macro
CFG_GCR_AL	stm8s_stdperiph_driver\inc\stm8s.h	2429;"	macro
CFG_GCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	2418;"	macro
CFG_GCR_SWD	stm8s_stdperiph_driver\inc\stm8s.h	2428;"	macro
CFG_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	2412;"	typedef	typeref:struct:CFG_struct
CFG_struct	stm8s_stdperiph_driver\inc\stm8s.h	2408;"	struct
CKDIVR	stm8s_stdperiph_driver\inc\stm8s.h	500;"	member	struct:CLK_struct
CLK	stm8s_stdperiph_driver\inc\stm8s.h	2508;"	macro
CLKPrescTable	stm8s_stdperiph_driver\src\stm8s_clk.c	43;"	variable
CLK_AdjustHSICalibrationValue	stm8s_stdperiph_driver\inc\stm8s_clk.h	363;"	prototype	signature:(CLK_HSITrimValue_TypeDef CLK_HSICalibrationValue)
CLK_AdjustHSICalibrationValue	stm8s_stdperiph_driver\src\stm8s_clk.c	616;"	function	signature:(CLK_HSITrimValue_TypeDef CLK_HSICalibrationValue)
CLK_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2459;"	macro
CLK_CCOCmd	stm8s_stdperiph_driver\inc\stm8s_clk.h	350;"	prototype	signature:(FunctionalState NewState)
CLK_CCOCmd	stm8s_stdperiph_driver\src\stm8s_clk.c	192;"	function	signature:(FunctionalState NewState)
CLK_CCOConfig	stm8s_stdperiph_driver\inc\stm8s_clk.h	357;"	prototype	signature:(CLK_Output_TypeDef CLK_CCO)
CLK_CCOConfig	stm8s_stdperiph_driver\src\stm8s_clk.c	439;"	function	signature:(CLK_Output_TypeDef CLK_CCO)
CLK_CCOR_CCOBSY	stm8s_stdperiph_driver\inc\stm8s.h	578;"	macro
CLK_CCOR_CCOEN	stm8s_stdperiph_driver\inc\stm8s.h	581;"	macro
CLK_CCOR_CCORDY	stm8s_stdperiph_driver\inc\stm8s.h	579;"	macro
CLK_CCOR_CCOSEL	stm8s_stdperiph_driver\inc\stm8s.h	580;"	macro
CLK_CCOR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	524;"	macro
CLK_CKDIVR_CPUDIV	stm8s_stdperiph_driver\inc\stm8s.h	555;"	macro
CLK_CKDIVR_HSIDIV	stm8s_stdperiph_driver\inc\stm8s.h	554;"	macro
CLK_CKDIVR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	520;"	macro
CLK_CMSR_CKM	stm8s_stdperiph_driver\inc\stm8s.h	545;"	macro
CLK_CMSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	517;"	macro
CLK_CSSCONFIG_DISABLE	stm8s_stdperiph_driver\inc\stm8s_clk.h	58;"	enumerator	enum:__anon17
CLK_CSSCONFIG_ENABLE	stm8s_stdperiph_driver\inc\stm8s_clk.h	57;"	enumerator	enum:__anon17
CLK_CSSCONFIG_ENABLEWITHIT	stm8s_stdperiph_driver\inc\stm8s_clk.h	56;"	enumerator	enum:__anon17
CLK_CSSConfig_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	59;"	typedef	typeref:enum:__anon17
CLK_CSSR_AUX	stm8s_stdperiph_driver\inc\stm8s.h	575;"	macro
CLK_CSSR_CSSD	stm8s_stdperiph_driver\inc\stm8s.h	573;"	macro
CLK_CSSR_CSSDIE	stm8s_stdperiph_driver\inc\stm8s.h	574;"	macro
CLK_CSSR_CSSEN	stm8s_stdperiph_driver\inc\stm8s.h	576;"	macro
CLK_CSSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	523;"	macro
CLK_CURRENTCLOCKSTATE_DISABLE	stm8s_stdperiph_driver\inc\stm8s_clk.h	48;"	enumerator	enum:__anon16
CLK_CURRENTCLOCKSTATE_ENABLE	stm8s_stdperiph_driver\inc\stm8s_clk.h	49;"	enumerator	enum:__anon16
CLK_ClearITPendingBit	stm8s_stdperiph_driver\inc\stm8s_clk.h	368;"	prototype	signature:(CLK_IT_TypeDef CLK_IT)
CLK_ClearITPendingBit	stm8s_stdperiph_driver\src\stm8s_clk.c	747;"	function	signature:(CLK_IT_TypeDef CLK_IT)
CLK_ClockSecuritySystemEnable	stm8s_stdperiph_driver\inc\stm8s_clk.h	361;"	prototype	signature:(void)
CLK_ClockSecuritySystemEnable	stm8s_stdperiph_driver\src\stm8s_clk.c	557;"	function	signature:(void)
CLK_ClockSwitchCmd	stm8s_stdperiph_driver\inc\stm8s_clk.h	351;"	prototype	signature:(FunctionalState NewState)
CLK_ClockSwitchCmd	stm8s_stdperiph_driver\src\stm8s_clk.c	218;"	function	signature:(FunctionalState NewState)
CLK_ClockSwitchConfig	stm8s_stdperiph_driver\inc\stm8s_clk.h	355;"	prototype	signature:(CLK_SwitchMode_TypeDef CLK_SwitchMode, CLK_Source_TypeDef CLK_NewClock, FunctionalState ITState, CLK_CurrentClockState_TypeDef CLK_CurrentClockState)
CLK_ClockSwitchConfig	stm8s_stdperiph_driver\src\stm8s_clk.c	319;"	function	signature:(CLK_SwitchMode_TypeDef CLK_SwitchMode, CLK_Source_TypeDef CLK_NewClock, FunctionalState ITState, CLK_CurrentClockState_TypeDef CLK_CurrentClockState)
CLK_Configuration	user\config.c	3;"	function	signature:(void)
CLK_Configuration	user\main.h	140;"	prototype	signature:(void)
CLK_CurrentClockState_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	50;"	typedef	typeref:enum:__anon16
CLK_DeInit	stm8s_stdperiph_driver\inc\stm8s_clk.h	346;"	prototype	signature:(void)
CLK_DeInit	stm8s_stdperiph_driver\src\stm8s_clk.c	66;"	function	signature:(void)
CLK_ECKR_HSEEN	stm8s_stdperiph_driver\inc\stm8s.h	543;"	macro
CLK_ECKR_HSERDY	stm8s_stdperiph_driver\inc\stm8s.h	542;"	macro
CLK_ECKR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	516;"	macro
CLK_FLAG_AUX	stm8s_stdperiph_driver\inc\stm8s_clk.h	152;"	enumerator	enum:__anon22
CLK_FLAG_CCOBSY	stm8s_stdperiph_driver\inc\stm8s_clk.h	153;"	enumerator	enum:__anon22
CLK_FLAG_CCORDY	stm8s_stdperiph_driver\inc\stm8s_clk.h	154;"	enumerator	enum:__anon22
CLK_FLAG_CSSD	stm8s_stdperiph_driver\inc\stm8s_clk.h	151;"	enumerator	enum:__anon22
CLK_FLAG_HSERDY	stm8s_stdperiph_driver\inc\stm8s_clk.h	148;"	enumerator	enum:__anon22
CLK_FLAG_HSIRDY	stm8s_stdperiph_driver\inc\stm8s_clk.h	147;"	enumerator	enum:__anon22
CLK_FLAG_LSIRDY	stm8s_stdperiph_driver\inc\stm8s_clk.h	146;"	enumerator	enum:__anon22
CLK_FLAG_SWBSY	stm8s_stdperiph_driver\inc\stm8s_clk.h	150;"	enumerator	enum:__anon22
CLK_FLAG_SWIF	stm8s_stdperiph_driver\inc\stm8s_clk.h	149;"	enumerator	enum:__anon22
CLK_FastHaltWakeUpCmd	stm8s_stdperiph_driver\inc\stm8s_clk.h	352;"	prototype	signature:(FunctionalState NewState)
CLK_FastHaltWakeUpCmd	stm8s_stdperiph_driver\src\stm8s_clk.c	95;"	function	signature:(FunctionalState NewState)
CLK_Flag_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	156;"	typedef	typeref:enum:__anon22
CLK_GetClockFreq	stm8s_stdperiph_driver\inc\stm8s_clk.h	364;"	prototype	signature:(void)
CLK_GetClockFreq	stm8s_stdperiph_driver\src\stm8s_clk.c	579;"	function	signature:(void)
CLK_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_clk.h	366;"	prototype	signature:(CLK_Flag_TypeDef CLK_FLAG)
CLK_GetFlagStatus	stm8s_stdperiph_driver\src\stm8s_clk.c	648;"	function	signature:(CLK_Flag_TypeDef CLK_FLAG)
CLK_GetITStatus	stm8s_stdperiph_driver\inc\stm8s_clk.h	367;"	prototype	signature:(CLK_IT_TypeDef CLK_IT)
CLK_GetITStatus	stm8s_stdperiph_driver\src\stm8s_clk.c	703;"	function	signature:(CLK_IT_TypeDef CLK_IT)
CLK_GetSYSCLKSource	stm8s_stdperiph_driver\inc\stm8s_clk.h	365;"	prototype	signature:(void)
CLK_GetSYSCLKSource	stm8s_stdperiph_driver\src\stm8s_clk.c	569;"	function	signature:(void)
CLK_HSECmd	stm8s_stdperiph_driver\inc\stm8s_clk.h	347;"	prototype	signature:(FunctionalState NewState)
CLK_HSECmd	stm8s_stdperiph_driver\src\stm8s_clk.c	119;"	function	signature:(FunctionalState NewState)
CLK_HSICmd	stm8s_stdperiph_driver\inc\stm8s_clk.h	348;"	prototype	signature:(FunctionalState NewState)
CLK_HSICmd	stm8s_stdperiph_driver\src\stm8s_clk.c	143;"	function	signature:(FunctionalState NewState)
CLK_HSIPrescalerConfig	stm8s_stdperiph_driver\inc\stm8s_clk.h	356;"	prototype	signature:(CLK_Prescaler_TypeDef HSIPrescaler)
CLK_HSIPrescalerConfig	stm8s_stdperiph_driver\src\stm8s_clk.c	416;"	function	signature:(CLK_Prescaler_TypeDef HSIPrescaler)
CLK_HSITRIMR_HSITRIM	stm8s_stdperiph_driver\inc\stm8s.h	583;"	macro
CLK_HSITRIMR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	525;"	macro
CLK_HSITRIMVALUE_0	stm8s_stdperiph_driver\inc\stm8s_clk.h	74;"	enumerator	enum:__anon19
CLK_HSITRIMVALUE_1	stm8s_stdperiph_driver\inc\stm8s_clk.h	75;"	enumerator	enum:__anon19
CLK_HSITRIMVALUE_2	stm8s_stdperiph_driver\inc\stm8s_clk.h	76;"	enumerator	enum:__anon19
CLK_HSITRIMVALUE_3	stm8s_stdperiph_driver\inc\stm8s_clk.h	77;"	enumerator	enum:__anon19
CLK_HSITRIMVALUE_4	stm8s_stdperiph_driver\inc\stm8s_clk.h	78;"	enumerator	enum:__anon19
CLK_HSITRIMVALUE_5	stm8s_stdperiph_driver\inc\stm8s_clk.h	79;"	enumerator	enum:__anon19
CLK_HSITRIMVALUE_6	stm8s_stdperiph_driver\inc\stm8s_clk.h	80;"	enumerator	enum:__anon19
CLK_HSITRIMVALUE_7	stm8s_stdperiph_driver\inc\stm8s_clk.h	81;"	enumerator	enum:__anon19
CLK_HSITrimValue_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	82;"	typedef	typeref:enum:__anon19
CLK_ICKR_FHWU	stm8s_stdperiph_driver\inc\stm8s.h	538;"	macro
CLK_ICKR_HSIEN	stm8s_stdperiph_driver\inc\stm8s.h	540;"	macro
CLK_ICKR_HSIRDY	stm8s_stdperiph_driver\inc\stm8s.h	539;"	macro
CLK_ICKR_LSIEN	stm8s_stdperiph_driver\inc\stm8s.h	537;"	macro
CLK_ICKR_LSIRDY	stm8s_stdperiph_driver\inc\stm8s.h	536;"	macro
CLK_ICKR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	515;"	macro
CLK_ICKR_SWUAH	stm8s_stdperiph_driver\inc\stm8s.h	535;"	macro
CLK_ITConfig	stm8s_stdperiph_driver\inc\stm8s_clk.h	358;"	prototype	signature:(CLK_IT_TypeDef CLK_IT, FunctionalState NewState)
CLK_ITConfig	stm8s_stdperiph_driver\src\stm8s_clk.c	464;"	function	signature:(CLK_IT_TypeDef CLK_IT, FunctionalState NewState)
CLK_IT_CSSD	stm8s_stdperiph_driver\inc\stm8s_clk.h	162;"	enumerator	enum:__anon23
CLK_IT_SWIF	stm8s_stdperiph_driver\inc\stm8s_clk.h	163;"	enumerator	enum:__anon23
CLK_IT_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	164;"	typedef	typeref:enum:__anon23
CLK_LSICmd	stm8s_stdperiph_driver\inc\stm8s_clk.h	349;"	prototype	signature:(FunctionalState NewState)
CLK_LSICmd	stm8s_stdperiph_driver\src\stm8s_clk.c	167;"	function	signature:(FunctionalState NewState)
CLK_OUTPUT_CPU	stm8s_stdperiph_driver\inc\stm8s_clk.h	91;"	enumerator	enum:__anon20
CLK_OUTPUT_CPUDIV16	stm8s_stdperiph_driver\inc\stm8s_clk.h	95;"	enumerator	enum:__anon20
CLK_OUTPUT_CPUDIV2	stm8s_stdperiph_driver\inc\stm8s_clk.h	92;"	enumerator	enum:__anon20
CLK_OUTPUT_CPUDIV32	stm8s_stdperiph_driver\inc\stm8s_clk.h	96;"	enumerator	enum:__anon20
CLK_OUTPUT_CPUDIV4	stm8s_stdperiph_driver\inc\stm8s_clk.h	93;"	enumerator	enum:__anon20
CLK_OUTPUT_CPUDIV64	stm8s_stdperiph_driver\inc\stm8s_clk.h	97;"	enumerator	enum:__anon20
CLK_OUTPUT_CPUDIV8	stm8s_stdperiph_driver\inc\stm8s_clk.h	94;"	enumerator	enum:__anon20
CLK_OUTPUT_HSE	stm8s_stdperiph_driver\inc\stm8s_clk.h	90;"	enumerator	enum:__anon20
CLK_OUTPUT_HSI	stm8s_stdperiph_driver\inc\stm8s_clk.h	88;"	enumerator	enum:__anon20
CLK_OUTPUT_HSIRC	stm8s_stdperiph_driver\inc\stm8s_clk.h	98;"	enumerator	enum:__anon20
CLK_OUTPUT_LSI	stm8s_stdperiph_driver\inc\stm8s_clk.h	89;"	enumerator	enum:__anon20
CLK_OUTPUT_MASTER	stm8s_stdperiph_driver\inc\stm8s_clk.h	99;"	enumerator	enum:__anon20
CLK_OUTPUT_OTHERS	stm8s_stdperiph_driver\inc\stm8s_clk.h	100;"	enumerator	enum:__anon20
CLK_Output_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	101;"	typedef	typeref:enum:__anon20
CLK_PCKENR1_I2C	stm8s_stdperiph_driver\inc\stm8s.h	567;"	macro
CLK_PCKENR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	521;"	macro
CLK_PCKENR1_SPI	stm8s_stdperiph_driver\inc\stm8s.h	566;"	macro
CLK_PCKENR1_TIM1	stm8s_stdperiph_driver\inc\stm8s.h	557;"	macro
CLK_PCKENR1_TIM2	stm8s_stdperiph_driver\inc\stm8s.h	559;"	macro
CLK_PCKENR1_TIM3	stm8s_stdperiph_driver\inc\stm8s.h	558;"	macro
CLK_PCKENR1_TIM4	stm8s_stdperiph_driver\inc\stm8s.h	561;"	macro
CLK_PCKENR1_TIM5	stm8s_stdperiph_driver\inc\stm8s.h	560;"	macro
CLK_PCKENR1_TIM6	stm8s_stdperiph_driver\inc\stm8s.h	562;"	macro
CLK_PCKENR1_UART1	stm8s_stdperiph_driver\inc\stm8s.h	565;"	macro
CLK_PCKENR1_UART2	stm8s_stdperiph_driver\inc\stm8s.h	564;"	macro
CLK_PCKENR1_UART3	stm8s_stdperiph_driver\inc\stm8s.h	563;"	macro
CLK_PCKENR2_ADC	stm8s_stdperiph_driver\inc\stm8s.h	570;"	macro
CLK_PCKENR2_AWU	stm8s_stdperiph_driver\inc\stm8s.h	571;"	macro
CLK_PCKENR2_CAN	stm8s_stdperiph_driver\inc\stm8s.h	569;"	macro
CLK_PCKENR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	522;"	macro
CLK_PERIPHERAL_ADC	stm8s_stdperiph_driver\inc\stm8s_clk.h	129;"	enumerator	enum:__anon21
CLK_PERIPHERAL_AWU	stm8s_stdperiph_driver\inc\stm8s_clk.h	128;"	enumerator	enum:__anon21
CLK_PERIPHERAL_CAN	stm8s_stdperiph_driver\inc\stm8s_clk.h	130;"	enumerator	enum:__anon21
CLK_PERIPHERAL_I2C	stm8s_stdperiph_driver\inc\stm8s_clk.h	113;"	enumerator	enum:__anon21
CLK_PERIPHERAL_SPI	stm8s_stdperiph_driver\inc\stm8s_clk.h	114;"	enumerator	enum:__anon21
CLK_PERIPHERAL_TIMER1	stm8s_stdperiph_driver\inc\stm8s_clk.h	127;"	enumerator	enum:__anon21
CLK_PERIPHERAL_TIMER2	stm8s_stdperiph_driver\inc\stm8s_clk.h	125;"	enumerator	enum:__anon21
CLK_PERIPHERAL_TIMER3	stm8s_stdperiph_driver\inc\stm8s_clk.h	126;"	enumerator	enum:__anon21
CLK_PERIPHERAL_TIMER4	stm8s_stdperiph_driver\inc\stm8s_clk.h	123;"	enumerator	enum:__anon21
CLK_PERIPHERAL_TIMER5	stm8s_stdperiph_driver\inc\stm8s_clk.h	124;"	enumerator	enum:__anon21
CLK_PERIPHERAL_TIMER6	stm8s_stdperiph_driver\inc\stm8s_clk.h	122;"	enumerator	enum:__anon21
CLK_PERIPHERAL_UART1	stm8s_stdperiph_driver\inc\stm8s_clk.h	116;"	enumerator	enum:__anon21
CLK_PERIPHERAL_UART2	stm8s_stdperiph_driver\inc\stm8s_clk.h	120;"	enumerator	enum:__anon21
CLK_PERIPHERAL_UART3	stm8s_stdperiph_driver\inc\stm8s_clk.h	121;"	enumerator	enum:__anon21
CLK_PRESCALER_CPUDIV1	stm8s_stdperiph_driver\inc\stm8s_clk.h	179;"	enumerator	enum:__anon24
CLK_PRESCALER_CPUDIV128	stm8s_stdperiph_driver\inc\stm8s_clk.h	186;"	enumerator	enum:__anon24
CLK_PRESCALER_CPUDIV16	stm8s_stdperiph_driver\inc\stm8s_clk.h	183;"	enumerator	enum:__anon24
CLK_PRESCALER_CPUDIV2	stm8s_stdperiph_driver\inc\stm8s_clk.h	180;"	enumerator	enum:__anon24
CLK_PRESCALER_CPUDIV32	stm8s_stdperiph_driver\inc\stm8s_clk.h	184;"	enumerator	enum:__anon24
CLK_PRESCALER_CPUDIV4	stm8s_stdperiph_driver\inc\stm8s_clk.h	181;"	enumerator	enum:__anon24
CLK_PRESCALER_CPUDIV64	stm8s_stdperiph_driver\inc\stm8s_clk.h	185;"	enumerator	enum:__anon24
CLK_PRESCALER_CPUDIV8	stm8s_stdperiph_driver\inc\stm8s_clk.h	182;"	enumerator	enum:__anon24
CLK_PRESCALER_HSIDIV1	stm8s_stdperiph_driver\inc\stm8s_clk.h	175;"	enumerator	enum:__anon24
CLK_PRESCALER_HSIDIV2	stm8s_stdperiph_driver\inc\stm8s_clk.h	176;"	enumerator	enum:__anon24
CLK_PRESCALER_HSIDIV4	stm8s_stdperiph_driver\inc\stm8s_clk.h	177;"	enumerator	enum:__anon24
CLK_PRESCALER_HSIDIV8	stm8s_stdperiph_driver\inc\stm8s_clk.h	178;"	enumerator	enum:__anon24
CLK_PeripheralClockConfig	stm8s_stdperiph_driver\inc\stm8s_clk.h	354;"	prototype	signature:(CLK_Peripheral_TypeDef CLK_Peripheral, FunctionalState NewState)
CLK_PeripheralClockConfig	stm8s_stdperiph_driver\src\stm8s_clk.c	272;"	function	signature:(CLK_Peripheral_TypeDef CLK_Peripheral, FunctionalState NewState)
CLK_Peripheral_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	131;"	typedef	typeref:enum:__anon21
CLK_Prescaler_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	187;"	typedef	typeref:enum:__anon24
CLK_SOURCE_HSE	stm8s_stdperiph_driver\inc\stm8s_clk.h	67;"	enumerator	enum:__anon18
CLK_SOURCE_HSI	stm8s_stdperiph_driver\inc\stm8s_clk.h	65;"	enumerator	enum:__anon18
CLK_SOURCE_LSI	stm8s_stdperiph_driver\inc\stm8s_clk.h	66;"	enumerator	enum:__anon18
CLK_SWCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	519;"	macro
CLK_SWCR_SWBSY	stm8s_stdperiph_driver\inc\stm8s.h	552;"	macro
CLK_SWCR_SWEN	stm8s_stdperiph_driver\inc\stm8s.h	551;"	macro
CLK_SWCR_SWIEN	stm8s_stdperiph_driver\inc\stm8s.h	550;"	macro
CLK_SWCR_SWIF	stm8s_stdperiph_driver\inc\stm8s.h	549;"	macro
CLK_SWIMCCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	526;"	macro
CLK_SWIMCCR_SWIMDIV	stm8s_stdperiph_driver\inc\stm8s.h	585;"	macro
CLK_SWIMConfig	stm8s_stdperiph_driver\inc\stm8s_clk.h	360;"	prototype	signature:(CLK_SWIMDivider_TypeDef CLK_SWIMDivider)
CLK_SWIMConfig	stm8s_stdperiph_driver\src\stm8s_clk.c	531;"	function	signature:(CLK_SWIMDivider_TypeDef CLK_SWIMDivider)
CLK_SWIMDIVIDER_2	stm8s_stdperiph_driver\inc\stm8s_clk.h	193;"	enumerator	enum:__anon25
CLK_SWIMDIVIDER_OTHER	stm8s_stdperiph_driver\inc\stm8s_clk.h	194;"	enumerator	enum:__anon25
CLK_SWIMDivider_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	195;"	typedef	typeref:enum:__anon25
CLK_SWITCHMODE_AUTO	stm8s_stdperiph_driver\inc\stm8s_clk.h	41;"	enumerator	enum:__anon15
CLK_SWITCHMODE_MANUAL	stm8s_stdperiph_driver\inc\stm8s_clk.h	40;"	enumerator	enum:__anon15
CLK_SWR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	518;"	macro
CLK_SWR_SWI	stm8s_stdperiph_driver\inc\stm8s.h	547;"	macro
CLK_SYSCLKConfig	stm8s_stdperiph_driver\inc\stm8s_clk.h	359;"	prototype	signature:(CLK_Prescaler_TypeDef CLK_Prescaler)
CLK_SYSCLKConfig	stm8s_stdperiph_driver\src\stm8s_clk.c	507;"	function	signature:(CLK_Prescaler_TypeDef CLK_Prescaler)
CLK_SYSCLKEmergencyClear	stm8s_stdperiph_driver\inc\stm8s_clk.h	362;"	prototype	signature:(void)
CLK_SYSCLKEmergencyClear	stm8s_stdperiph_driver\src\stm8s_clk.c	636;"	function	signature:(void)
CLK_SlowActiveHaltWakeUpCmd	stm8s_stdperiph_driver\inc\stm8s_clk.h	353;"	prototype	signature:(FunctionalState NewState)
CLK_SlowActiveHaltWakeUpCmd	stm8s_stdperiph_driver\src\stm8s_clk.c	245;"	function	signature:(FunctionalState NewState)
CLK_Source_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	68;"	typedef	typeref:enum:__anon18
CLK_SwitchMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_clk.h	42;"	typedef	typeref:enum:__anon15
CLK_TIMEOUT	stm8s_stdperiph_driver\inc\stm8s_clk.h	206;"	macro
CLK_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	509;"	typedef	typeref:struct:CLK_struct
CLK_struct	stm8s_stdperiph_driver\inc\stm8s.h	492;"	struct
CMSR	stm8s_stdperiph_driver\inc\stm8s.h	497;"	member	struct:CLK_struct
CNTR	stm8s_stdperiph_driver\inc\stm8s.h	1052;"	member	struct:TIM4_struct
CNTR	stm8s_stdperiph_driver\inc\stm8s.h	1252;"	member	struct:TIM6_struct
CNTRH	stm8s_stdperiph_driver\inc\stm8s.h	1119;"	member	struct:TIM5_struct
CNTRH	stm8s_stdperiph_driver\inc\stm8s.h	612;"	member	struct:TIM1_struct
CNTRH	stm8s_stdperiph_driver\inc\stm8s.h	824;"	member	struct:TIM2_struct
CNTRH	stm8s_stdperiph_driver\inc\stm8s.h	946;"	member	struct:TIM3_struct
CNTRL	stm8s_stdperiph_driver\inc\stm8s.h	1120;"	member	struct:TIM5_struct
CNTRL	stm8s_stdperiph_driver\inc\stm8s.h	613;"	member	struct:TIM1_struct
CNTRL	stm8s_stdperiph_driver\inc\stm8s.h	825;"	member	struct:TIM2_struct
CNTRL	stm8s_stdperiph_driver\inc\stm8s.h	947;"	member	struct:TIM3_struct
CONST	stm8s_stdperiph_driver\inc\stm8s.h	116;"	macro
CONST	stm8s_stdperiph_driver\inc\stm8s.h	122;"	macro
CONST	stm8s_stdperiph_driver\inc\stm8s.h	136;"	macro
CPU_CC_I1I0	stm8s_stdperiph_driver\inc\stm8s.h	1446;"	macro
CPU_SOFT_INT_DISABLED	stm8s_stdperiph_driver\inc\stm8s_itc.h	122;"	macro
CR	stm8s_stdperiph_driver\inc\stm8s.h	1619;"	member	struct:WWDG_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1044;"	member	struct:TIM4_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1107;"	member	struct:TIM5_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1246;"	member	struct:TIM6_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1314;"	member	struct:I2C_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1459;"	member	struct:EXTI_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1500;"	member	struct:FLASH_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1682;"	member	struct:SPI_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1757;"	member	struct:UART1_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1855;"	member	struct:UART2_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	1963;"	member	struct:UART3_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	258;"	member	struct:GPIO_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	306;"	member	struct:ADC1_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	377;"	member	struct:ADC2_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	598;"	member	struct:TIM1_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	810;"	member	struct:TIM2_struct
CR1	stm8s_stdperiph_driver\inc\stm8s.h	938;"	member	struct:TIM3_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1108;"	member	struct:TIM5_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1247;"	member	struct:TIM6_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1315;"	member	struct:I2C_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1460;"	member	struct:EXTI_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1501;"	member	struct:FLASH_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1683;"	member	struct:SPI_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1758;"	member	struct:UART1_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1856;"	member	struct:UART2_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	1964;"	member	struct:UART3_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	259;"	member	struct:GPIO_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	307;"	member	struct:ADC1_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	378;"	member	struct:ADC2_struct
CR2	stm8s_stdperiph_driver\inc\stm8s.h	599;"	member	struct:TIM1_struct
CR3	stm8s_stdperiph_driver\inc\stm8s.h	1759;"	member	struct:UART1_struct
CR3	stm8s_stdperiph_driver\inc\stm8s.h	1857;"	member	struct:UART2_struct
CR3	stm8s_stdperiph_driver\inc\stm8s.h	1965;"	member	struct:UART3_struct
CR3	stm8s_stdperiph_driver\inc\stm8s.h	308;"	member	struct:ADC1_struct
CR4	stm8s_stdperiph_driver\inc\stm8s.h	1760;"	member	struct:UART1_struct
CR4	stm8s_stdperiph_driver\inc\stm8s.h	1858;"	member	struct:UART2_struct
CR4	stm8s_stdperiph_driver\inc\stm8s.h	1966;"	member	struct:UART3_struct
CR5	stm8s_stdperiph_driver\inc\stm8s.h	1761;"	member	struct:UART1_struct
CR5	stm8s_stdperiph_driver\inc\stm8s.h	1859;"	member	struct:UART2_struct
CR6	stm8s_stdperiph_driver\inc\stm8s.h	1860;"	member	struct:UART2_struct
CR6	stm8s_stdperiph_driver\inc\stm8s.h	1968;"	member	struct:UART3_struct
CRCPR	stm8s_stdperiph_driver\inc\stm8s.h	1687;"	member	struct:SPI_struct
CSR	stm8s_stdperiph_driver\inc\stm8s.h	305;"	member	struct:ADC1_struct
CSR	stm8s_stdperiph_driver\inc\stm8s.h	376;"	member	struct:ADC2_struct
CSR	stm8s_stdperiph_driver\inc\stm8s.h	426;"	member	struct:AWU_struct
CSR	stm8s_stdperiph_driver\inc\stm8s.h	466;"	member	struct:BEEP_struct
CSSR	stm8s_stdperiph_driver\inc\stm8s.h	502;"	member	struct:CLK_struct
CUSB_CHGING	user\main.h	94;"	macro
CUSB_EXTRACT	user\main.h	95;"	macro
CUSB_INSERT	user\main.h	93;"	macro
CUSB_Status	user\main.c	4;"	variable
CUSB_TERMINA	user\main.h	96;"	macro
ChgBit	stm8s_stdperiph_driver\inc\stm8s.h	2677;"	macro
ClrBit	stm8s_stdperiph_driver\inc\stm8s.h	2675;"	macro
Config	stm8s_stdperiph_driver\inc\stm8s.h	2189;"	member	union:__anon5::__anon6	typeref:struct:__anon5::__anon6::__anon12
DB0RH	stm8s_stdperiph_driver\inc\stm8s.h	284;"	member	struct:ADC1_struct
DB0RL	stm8s_stdperiph_driver\inc\stm8s.h	285;"	member	struct:ADC1_struct
DB1RH	stm8s_stdperiph_driver\inc\stm8s.h	286;"	member	struct:ADC1_struct
DB1RL	stm8s_stdperiph_driver\inc\stm8s.h	287;"	member	struct:ADC1_struct
DB2RH	stm8s_stdperiph_driver\inc\stm8s.h	288;"	member	struct:ADC1_struct
DB2RL	stm8s_stdperiph_driver\inc\stm8s.h	289;"	member	struct:ADC1_struct
DB3RH	stm8s_stdperiph_driver\inc\stm8s.h	290;"	member	struct:ADC1_struct
DB3RL	stm8s_stdperiph_driver\inc\stm8s.h	291;"	member	struct:ADC1_struct
DB4RH	stm8s_stdperiph_driver\inc\stm8s.h	292;"	member	struct:ADC1_struct
DB4RL	stm8s_stdperiph_driver\inc\stm8s.h	293;"	member	struct:ADC1_struct
DB5RH	stm8s_stdperiph_driver\inc\stm8s.h	294;"	member	struct:ADC1_struct
DB5RL	stm8s_stdperiph_driver\inc\stm8s.h	295;"	member	struct:ADC1_struct
DB6RH	stm8s_stdperiph_driver\inc\stm8s.h	296;"	member	struct:ADC1_struct
DB6RL	stm8s_stdperiph_driver\inc\stm8s.h	297;"	member	struct:ADC1_struct
DB7RH	stm8s_stdperiph_driver\inc\stm8s.h	298;"	member	struct:ADC1_struct
DB7RL	stm8s_stdperiph_driver\inc\stm8s.h	299;"	member	struct:ADC1_struct
DB8RH	stm8s_stdperiph_driver\inc\stm8s.h	300;"	member	struct:ADC1_struct
DB8RL	stm8s_stdperiph_driver\inc\stm8s.h	301;"	member	struct:ADC1_struct
DB9RH	stm8s_stdperiph_driver\inc\stm8s.h	302;"	member	struct:ADC1_struct
DB9RL	stm8s_stdperiph_driver\inc\stm8s.h	303;"	member	struct:ADC1_struct
DDR	stm8s_stdperiph_driver\inc\stm8s.h	257;"	member	struct:GPIO_struct
DGR	stm8s_stdperiph_driver\inc\stm8s.h	2058;"	member	struct:__anon5
DISABLE	stm8s_stdperiph_driver\inc\stm8s.h	223;"	enumerator	enum:__anon3
DM	stm8s_stdperiph_driver\inc\stm8s.h	2589;"	macro
DM_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2480;"	macro
DR	stm8s_stdperiph_driver\inc\stm8s.h	1320;"	member	struct:I2C_struct
DR	stm8s_stdperiph_driver\inc\stm8s.h	1686;"	member	struct:SPI_struct
DR	stm8s_stdperiph_driver\inc\stm8s.h	1754;"	member	struct:UART1_struct
DR	stm8s_stdperiph_driver\inc\stm8s.h	1852;"	member	struct:UART2_struct
DR	stm8s_stdperiph_driver\inc\stm8s.h	1960;"	member	struct:UART3_struct
DRH	stm8s_stdperiph_driver\inc\stm8s.h	309;"	member	struct:ADC1_struct
DRH	stm8s_stdperiph_driver\inc\stm8s.h	380;"	member	struct:ADC2_struct
DRL	stm8s_stdperiph_driver\inc\stm8s.h	310;"	member	struct:ADC1_struct
DRL	stm8s_stdperiph_driver\inc\stm8s.h	381;"	member	struct:ADC2_struct
DTR	stm8s_stdperiph_driver\inc\stm8s.h	628;"	member	struct:TIM1_struct
DUKR	stm8s_stdperiph_driver\inc\stm8s.h	1510;"	member	struct:FLASH_struct
DelayMs	user\main.c	42;"	function	signature:(uint16_t t)
DelayMs	user\main.h	150;"	prototype	signature:(uint16_t t)
DelaySoft	user\main.c	52;"	function	signature:(uint16_t t)
DelaySoft	user\main.h	151;"	prototype	signature:(uint16_t t)
DelayVal	user\main.c	6;"	variable
ECKR	stm8s_stdperiph_driver\inc\stm8s.h	495;"	member	struct:CLK_struct
EEPROM	stm8s_stdperiph_driver\inc\stm8s.h	115;"	macro
EEPROM	stm8s_stdperiph_driver\inc\stm8s.h	121;"	macro
EEPROM	stm8s_stdperiph_driver\inc\stm8s.h	135;"	macro
EGR	stm8s_stdperiph_driver\inc\stm8s.h	1051;"	member	struct:TIM4_struct
EGR	stm8s_stdperiph_driver\inc\stm8s.h	1113;"	member	struct:TIM5_struct
EGR	stm8s_stdperiph_driver\inc\stm8s.h	1251;"	member	struct:TIM6_struct
EGR	stm8s_stdperiph_driver\inc\stm8s.h	605;"	member	struct:TIM1_struct
EGR	stm8s_stdperiph_driver\inc\stm8s.h	818;"	member	struct:TIM2_struct
EGR	stm8s_stdperiph_driver\inc\stm8s.h	942;"	member	struct:TIM3_struct
EIER	stm8s_stdperiph_driver\inc\stm8s.h	2176;"	member	struct:__anon5::__anon6::__anon12
ENABLE	stm8s_stdperiph_driver\inc\stm8s.h	223;"	enumerator	enum:__anon3
ERROR	stm8s_stdperiph_driver\inc\stm8s.h	226;"	enumerator	enum:__anon4
ESR	stm8s_stdperiph_driver\inc\stm8s.h	2175;"	member	struct:__anon5::__anon6::__anon12
ETR	stm8s_stdperiph_driver\inc\stm8s.h	601;"	member	struct:TIM1_struct
EXTI	stm8s_stdperiph_driver\inc\stm8s.h	2510;"	macro
EXTI_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2457;"	macro
EXTI_CR1_PAIS	stm8s_stdperiph_driver\inc\stm8s.h	1482;"	macro
EXTI_CR1_PBIS	stm8s_stdperiph_driver\inc\stm8s.h	1481;"	macro
EXTI_CR1_PCIS	stm8s_stdperiph_driver\inc\stm8s.h	1480;"	macro
EXTI_CR1_PDIS	stm8s_stdperiph_driver\inc\stm8s.h	1479;"	macro
EXTI_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1468;"	macro
EXTI_CR2_PEIS	stm8s_stdperiph_driver\inc\stm8s.h	1485;"	macro
EXTI_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1469;"	macro
EXTI_CR2_TLIS	stm8s_stdperiph_driver\inc\stm8s.h	1484;"	macro
EXTI_Configuration	user\config.c	129;"	function	signature:(void)
EXTI_Configuration	user\main.h	147;"	prototype	signature:(void)
EXTI_DeInit	stm8s_stdperiph_driver\inc\stm8s_exti.h	115;"	prototype	signature:(void)
EXTI_GetExtIntSensitivity	stm8s_stdperiph_driver\inc\stm8s_exti.h	118;"	prototype	signature:(EXTI_Port_TypeDef Port)
EXTI_GetTLISensitivity	stm8s_stdperiph_driver\inc\stm8s_exti.h	119;"	prototype	signature:(void)
EXTI_PORT_GPIOA	stm8s_stdperiph_driver\inc\stm8s_exti.h	57;"	enumerator	enum:__anon54
EXTI_PORT_GPIOB	stm8s_stdperiph_driver\inc\stm8s_exti.h	58;"	enumerator	enum:__anon54
EXTI_PORT_GPIOC	stm8s_stdperiph_driver\inc\stm8s_exti.h	59;"	enumerator	enum:__anon54
EXTI_PORT_GPIOD	stm8s_stdperiph_driver\inc\stm8s_exti.h	60;"	enumerator	enum:__anon54
EXTI_PORT_GPIOE	stm8s_stdperiph_driver\inc\stm8s_exti.h	61;"	enumerator	enum:__anon54
EXTI_PortD_IRQHandler	stm8_interrupt_vector.c	39;"	function	signature:(void)
EXTI_Port_TypeDef	stm8s_stdperiph_driver\inc\stm8s_exti.h	62;"	typedef	typeref:enum:__anon54
EXTI_SENSITIVITY_FALL_LOW	stm8s_stdperiph_driver\inc\stm8s_exti.h	39;"	enumerator	enum:__anon52
EXTI_SENSITIVITY_FALL_ONLY	stm8s_stdperiph_driver\inc\stm8s_exti.h	41;"	enumerator	enum:__anon52
EXTI_SENSITIVITY_RISE_FALL	stm8s_stdperiph_driver\inc\stm8s_exti.h	42;"	enumerator	enum:__anon52
EXTI_SENSITIVITY_RISE_ONLY	stm8s_stdperiph_driver\inc\stm8s_exti.h	40;"	enumerator	enum:__anon52
EXTI_Sensitivity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_exti.h	43;"	typedef	typeref:enum:__anon52
EXTI_SetExtIntSensitivity	stm8s_stdperiph_driver\inc\stm8s_exti.h	116;"	prototype	signature:(EXTI_Port_TypeDef Port, EXTI_Sensitivity_TypeDef SensitivityValue)
EXTI_SetTLISensitivity	stm8s_stdperiph_driver\inc\stm8s_exti.h	117;"	prototype	signature:(EXTI_TLISensitivity_TypeDef SensitivityValue)
EXTI_TLISENSITIVITY_FALL_ONLY	stm8s_stdperiph_driver\inc\stm8s_exti.h	49;"	enumerator	enum:__anon53
EXTI_TLISENSITIVITY_RISE_ONLY	stm8s_stdperiph_driver\inc\stm8s_exti.h	50;"	enumerator	enum:__anon53
EXTI_TLISensitivity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_exti.h	51;"	typedef	typeref:enum:__anon53
EXTI_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1462;"	typedef	typeref:struct:EXTI_struct
EXTI_struct	stm8s_stdperiph_driver\inc\stm8s.h	1457;"	struct
ErrorStatus	stm8s_stdperiph_driver\inc\stm8s.h	226;"	typedef	typeref:enum:__anon4
F0R1	stm8s_stdperiph_driver\inc\stm8s.h	2109;"	member	struct:__anon5::__anon6::__anon9
F0R2	stm8s_stdperiph_driver\inc\stm8s.h	2110;"	member	struct:__anon5::__anon6::__anon9
F0R3	stm8s_stdperiph_driver\inc\stm8s.h	2111;"	member	struct:__anon5::__anon6::__anon9
F0R4	stm8s_stdperiph_driver\inc\stm8s.h	2112;"	member	struct:__anon5::__anon6::__anon9
F0R5	stm8s_stdperiph_driver\inc\stm8s.h	2113;"	member	struct:__anon5::__anon6::__anon9
F0R6	stm8s_stdperiph_driver\inc\stm8s.h	2114;"	member	struct:__anon5::__anon6::__anon9
F0R7	stm8s_stdperiph_driver\inc\stm8s.h	2115;"	member	struct:__anon5::__anon6::__anon9
F0R8	stm8s_stdperiph_driver\inc\stm8s.h	2116;"	member	struct:__anon5::__anon6::__anon9
F1R1	stm8s_stdperiph_driver\inc\stm8s.h	2118;"	member	struct:__anon5::__anon6::__anon9
F1R2	stm8s_stdperiph_driver\inc\stm8s.h	2119;"	member	struct:__anon5::__anon6::__anon9
F1R3	stm8s_stdperiph_driver\inc\stm8s.h	2120;"	member	struct:__anon5::__anon6::__anon9
F1R4	stm8s_stdperiph_driver\inc\stm8s.h	2121;"	member	struct:__anon5::__anon6::__anon9
F1R5	stm8s_stdperiph_driver\inc\stm8s.h	2122;"	member	struct:__anon5::__anon6::__anon9
F1R6	stm8s_stdperiph_driver\inc\stm8s.h	2123;"	member	struct:__anon5::__anon6::__anon9
F1R7	stm8s_stdperiph_driver\inc\stm8s.h	2124;"	member	struct:__anon5::__anon6::__anon9
F1R8	stm8s_stdperiph_driver\inc\stm8s.h	2125;"	member	struct:__anon5::__anon6::__anon9
F2R1	stm8s_stdperiph_driver\inc\stm8s.h	2131;"	member	struct:__anon5::__anon6::__anon10
F2R2	stm8s_stdperiph_driver\inc\stm8s.h	2132;"	member	struct:__anon5::__anon6::__anon10
F2R3	stm8s_stdperiph_driver\inc\stm8s.h	2133;"	member	struct:__anon5::__anon6::__anon10
F2R4	stm8s_stdperiph_driver\inc\stm8s.h	2134;"	member	struct:__anon5::__anon6::__anon10
F2R5	stm8s_stdperiph_driver\inc\stm8s.h	2135;"	member	struct:__anon5::__anon6::__anon10
F2R6	stm8s_stdperiph_driver\inc\stm8s.h	2136;"	member	struct:__anon5::__anon6::__anon10
F2R7	stm8s_stdperiph_driver\inc\stm8s.h	2137;"	member	struct:__anon5::__anon6::__anon10
F2R8	stm8s_stdperiph_driver\inc\stm8s.h	2138;"	member	struct:__anon5::__anon6::__anon10
F3R1	stm8s_stdperiph_driver\inc\stm8s.h	2140;"	member	struct:__anon5::__anon6::__anon10
F3R2	stm8s_stdperiph_driver\inc\stm8s.h	2141;"	member	struct:__anon5::__anon6::__anon10
F3R3	stm8s_stdperiph_driver\inc\stm8s.h	2142;"	member	struct:__anon5::__anon6::__anon10
F3R4	stm8s_stdperiph_driver\inc\stm8s.h	2143;"	member	struct:__anon5::__anon6::__anon10
F3R5	stm8s_stdperiph_driver\inc\stm8s.h	2144;"	member	struct:__anon5::__anon6::__anon10
F3R6	stm8s_stdperiph_driver\inc\stm8s.h	2145;"	member	struct:__anon5::__anon6::__anon10
F3R7	stm8s_stdperiph_driver\inc\stm8s.h	2146;"	member	struct:__anon5::__anon6::__anon10
F3R8	stm8s_stdperiph_driver\inc\stm8s.h	2147;"	member	struct:__anon5::__anon6::__anon10
F4R1	stm8s_stdperiph_driver\inc\stm8s.h	2153;"	member	struct:__anon5::__anon6::__anon11
F4R2	stm8s_stdperiph_driver\inc\stm8s.h	2154;"	member	struct:__anon5::__anon6::__anon11
F4R3	stm8s_stdperiph_driver\inc\stm8s.h	2155;"	member	struct:__anon5::__anon6::__anon11
F4R4	stm8s_stdperiph_driver\inc\stm8s.h	2156;"	member	struct:__anon5::__anon6::__anon11
F4R5	stm8s_stdperiph_driver\inc\stm8s.h	2157;"	member	struct:__anon5::__anon6::__anon11
F4R6	stm8s_stdperiph_driver\inc\stm8s.h	2158;"	member	struct:__anon5::__anon6::__anon11
F4R7	stm8s_stdperiph_driver\inc\stm8s.h	2159;"	member	struct:__anon5::__anon6::__anon11
F4R8	stm8s_stdperiph_driver\inc\stm8s.h	2160;"	member	struct:__anon5::__anon6::__anon11
F5R1	stm8s_stdperiph_driver\inc\stm8s.h	2162;"	member	struct:__anon5::__anon6::__anon11
F5R2	stm8s_stdperiph_driver\inc\stm8s.h	2163;"	member	struct:__anon5::__anon6::__anon11
F5R3	stm8s_stdperiph_driver\inc\stm8s.h	2164;"	member	struct:__anon5::__anon6::__anon11
F5R4	stm8s_stdperiph_driver\inc\stm8s.h	2165;"	member	struct:__anon5::__anon6::__anon11
F5R5	stm8s_stdperiph_driver\inc\stm8s.h	2166;"	member	struct:__anon5::__anon6::__anon11
F5R6	stm8s_stdperiph_driver\inc\stm8s.h	2167;"	member	struct:__anon5::__anon6::__anon11
F5R7	stm8s_stdperiph_driver\inc\stm8s.h	2168;"	member	struct:__anon5::__anon6::__anon11
F5R8	stm8s_stdperiph_driver\inc\stm8s.h	2169;"	member	struct:__anon5::__anon6::__anon11
FALSE	stm8s_stdperiph_driver\inc\stm8s.h	219;"	enumerator	enum:__anon1
FAR	stm8s_stdperiph_driver\inc\stm8s.h	112;"	macro
FAR	stm8s_stdperiph_driver\inc\stm8s.h	118;"	macro
FAR	stm8s_stdperiph_driver\inc\stm8s.h	132;"	macro
FCR1	stm8s_stdperiph_driver\inc\stm8s.h	2184;"	member	struct:__anon5::__anon6::__anon12
FCR2	stm8s_stdperiph_driver\inc\stm8s.h	2185;"	member	struct:__anon5::__anon6::__anon12
FCR3	stm8s_stdperiph_driver\inc\stm8s.h	2186;"	member	struct:__anon5::__anon6::__anon12
FLASH	stm8s_stdperiph_driver\inc\stm8s.h	2512;"	macro
FLASH_BLOCK_SIZE	stm8s_stdperiph_driver\inc\stm8s_flash.h	43;"	macro
FLASH_BLOCK_SIZE	stm8s_stdperiph_driver\inc\stm8s_flash.h	52;"	macro
FLASH_BLOCK_SIZE	stm8s_stdperiph_driver\inc\stm8s_flash.h	61;"	macro
FLASH_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2456;"	macro
FLASH_CR1_AHALT	stm8s_stdperiph_driver\inc\stm8s.h	1534;"	macro
FLASH_CR1_FIX	stm8s_stdperiph_driver\inc\stm8s.h	1536;"	macro
FLASH_CR1_HALT	stm8s_stdperiph_driver\inc\stm8s.h	1533;"	macro
FLASH_CR1_IE	stm8s_stdperiph_driver\inc\stm8s.h	1535;"	macro
FLASH_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1518;"	macro
FLASH_CR2_ERASE	stm8s_stdperiph_driver\inc\stm8s.h	1540;"	macro
FLASH_CR2_FPRG	stm8s_stdperiph_driver\inc\stm8s.h	1541;"	macro
FLASH_CR2_OPT	stm8s_stdperiph_driver\inc\stm8s.h	1538;"	macro
FLASH_CR2_PRG	stm8s_stdperiph_driver\inc\stm8s.h	1542;"	macro
FLASH_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1519;"	macro
FLASH_CR2_WPRG	stm8s_stdperiph_driver\inc\stm8s.h	1539;"	macro
FLASH_DATA_BLOCKS_NUMBER	stm8s_stdperiph_driver\inc\stm8s_flash.h	42;"	macro
FLASH_DATA_BLOCKS_NUMBER	stm8s_stdperiph_driver\inc\stm8s_flash.h	51;"	macro
FLASH_DATA_BLOCKS_NUMBER	stm8s_stdperiph_driver\inc\stm8s_flash.h	60;"	macro
FLASH_DATA_END_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	41;"	macro
FLASH_DATA_END_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	50;"	macro
FLASH_DATA_END_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	59;"	macro
FLASH_DATA_START_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	40;"	macro
FLASH_DATA_START_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	49;"	macro
FLASH_DATA_START_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	58;"	macro
FLASH_DUKR_DUK	stm8s_stdperiph_driver\inc\stm8s.h	1558;"	macro
FLASH_DUKR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1523;"	macro
FLASH_DeInit	stm8s_stdperiph_driver\inc\stm8s_flash.h	252;"	prototype	signature:(void)
FLASH_EraseByte	stm8s_stdperiph_driver\inc\stm8s_flash.h	254;"	prototype	signature:(uint32_t Address)
FLASH_EraseOptionByte	stm8s_stdperiph_driver\inc\stm8s_flash.h	260;"	prototype	signature:(uint16_t Address)
FLASH_FLAG_DUL	stm8s_stdperiph_driver\inc\stm8s_flash.h	138;"	enumerator	enum:__anon60
FLASH_FLAG_EOP	stm8s_stdperiph_driver\inc\stm8s_flash.h	139;"	enumerator	enum:__anon60
FLASH_FLAG_HVOFF	stm8s_stdperiph_driver\inc\stm8s_flash.h	136;"	enumerator	enum:__anon60
FLASH_FLAG_PUL	stm8s_stdperiph_driver\inc\stm8s_flash.h	140;"	enumerator	enum:__anon60
FLASH_FLAG_WR_PG_DIS	stm8s_stdperiph_driver\inc\stm8s_flash.h	141;"	enumerator	enum:__anon60
FLASH_Flag_TypeDef	stm8s_stdperiph_driver\inc\stm8s_flash.h	142;"	typedef	typeref:enum:__anon60
FLASH_GetBootSize	stm8s_stdperiph_driver\inc\stm8s_flash.h	265;"	prototype	signature:(void)
FLASH_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_flash.h	266;"	prototype	signature:(FLASH_Flag_TypeDef FLASH_FLAG)
FLASH_GetLowPowerMode	stm8s_stdperiph_driver\inc\stm8s_flash.h	263;"	prototype	signature:(void)
FLASH_GetProgrammingTime	stm8s_stdperiph_driver\inc\stm8s_flash.h	264;"	prototype	signature:(void)
FLASH_IAPSR_DUL	stm8s_stdperiph_driver\inc\stm8s.h	1551;"	macro
FLASH_IAPSR_EOP	stm8s_stdperiph_driver\inc\stm8s.h	1552;"	macro
FLASH_IAPSR_HVOFF	stm8s_stdperiph_driver\inc\stm8s.h	1550;"	macro
FLASH_IAPSR_PUL	stm8s_stdperiph_driver\inc\stm8s.h	1553;"	macro
FLASH_IAPSR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1521;"	macro
FLASH_IAPSR_WR_PG_DIS	stm8s_stdperiph_driver\inc\stm8s.h	1554;"	macro
FLASH_ITConfig	stm8s_stdperiph_driver\inc\stm8s_flash.h	253;"	prototype	signature:(FunctionalState NewState)
FLASH_LPMODE_POWERDOWN	stm8s_stdperiph_driver\inc\stm8s_flash.h	109;"	enumerator	enum:__anon58
FLASH_LPMODE_POWERDOWN_STANDBY	stm8s_stdperiph_driver\inc\stm8s_flash.h	111;"	enumerator	enum:__anon58
FLASH_LPMODE_STANDBY	stm8s_stdperiph_driver\inc\stm8s_flash.h	110;"	enumerator	enum:__anon58
FLASH_LPMODE_STANDBY_POWERDOWN	stm8s_stdperiph_driver\inc\stm8s_flash.h	112;"	enumerator	enum:__anon58
FLASH_LPMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_flash.h	114;"	typedef	typeref:enum:__anon58
FLASH_Lock	stm8s_stdperiph_driver\inc\stm8s_flash.h	251;"	prototype	signature:(FLASH_MemType_TypeDef FLASH_MemType)
FLASH_MEMTYPE_DATA	stm8s_stdperiph_driver\inc\stm8s_flash.h	86;"	enumerator	enum:__anon55
FLASH_MEMTYPE_PROG	stm8s_stdperiph_driver\inc\stm8s_flash.h	85;"	enumerator	enum:__anon55
FLASH_MemType_TypeDef	stm8s_stdperiph_driver\inc\stm8s_flash.h	87;"	typedef	typeref:enum:__anon55
FLASH_NCR2_NERASE	stm8s_stdperiph_driver\inc\stm8s.h	1546;"	macro
FLASH_NCR2_NFPRG	stm8s_stdperiph_driver\inc\stm8s.h	1547;"	macro
FLASH_NCR2_NOPT	stm8s_stdperiph_driver\inc\stm8s.h	1544;"	macro
FLASH_NCR2_NPRG	stm8s_stdperiph_driver\inc\stm8s.h	1548;"	macro
FLASH_NCR2_NWPRG	stm8s_stdperiph_driver\inc\stm8s.h	1545;"	macro
FLASH_NCR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1520;"	macro
FLASH_OPTIONBYTE_ERROR	stm8s_stdperiph_driver\inc\stm8s_flash.h	69;"	macro
FLASH_PROGRAMMODE_FAST	stm8s_stdperiph_driver\inc\stm8s_flash.h	94;"	enumerator	enum:__anon56
FLASH_PROGRAMMODE_STANDARD	stm8s_stdperiph_driver\inc\stm8s_flash.h	93;"	enumerator	enum:__anon56
FLASH_PROGRAMTIME_STANDARD	stm8s_stdperiph_driver\inc\stm8s_flash.h	101;"	enumerator	enum:__anon57
FLASH_PROGRAMTIME_TPROG	stm8s_stdperiph_driver\inc\stm8s_flash.h	102;"	enumerator	enum:__anon57
FLASH_PROG_BLOCKS_NUMBER	stm8s_stdperiph_driver\inc\stm8s_flash.h	39;"	macro
FLASH_PROG_BLOCKS_NUMBER	stm8s_stdperiph_driver\inc\stm8s_flash.h	48;"	macro
FLASH_PROG_BLOCKS_NUMBER	stm8s_stdperiph_driver\inc\stm8s_flash.h	57;"	macro
FLASH_PROG_END_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	38;"	macro
FLASH_PROG_END_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	47;"	macro
FLASH_PROG_END_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	56;"	macro
FLASH_PROG_START_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	35;"	macro
FLASH_PUKR_PUK	stm8s_stdperiph_driver\inc\stm8s.h	1556;"	macro
FLASH_PUKR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1522;"	macro
FLASH_ProgramByte	stm8s_stdperiph_driver\inc\stm8s_flash.h	255;"	prototype	signature:(uint32_t Address, uint8_t Data)
FLASH_ProgramMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_flash.h	95;"	typedef	typeref:enum:__anon56
FLASH_ProgramOptionByte	stm8s_stdperiph_driver\inc\stm8s_flash.h	259;"	prototype	signature:(uint16_t Address, uint8_t Data)
FLASH_ProgramTime_TypeDef	stm8s_stdperiph_driver\inc\stm8s_flash.h	103;"	typedef	typeref:enum:__anon57
FLASH_ProgramWord	stm8s_stdperiph_driver\inc\stm8s_flash.h	257;"	prototype	signature:(uint32_t Address, uint32_t Data)
FLASH_RASS_KEY1	stm8s_stdperiph_driver\inc\stm8s_flash.h	64;"	macro
FLASH_RASS_KEY2	stm8s_stdperiph_driver\inc\stm8s_flash.h	65;"	macro
FLASH_ReadByte	stm8s_stdperiph_driver\inc\stm8s_flash.h	256;"	prototype	signature:(uint32_t Address)
FLASH_ReadOptionByte	stm8s_stdperiph_driver\inc\stm8s_flash.h	258;"	prototype	signature:(uint16_t Address)
FLASH_STATUS_END_HIGH_VOLTAGE	stm8s_stdperiph_driver\inc\stm8s_flash.h	122;"	enumerator	enum:__anon59
FLASH_STATUS_SUCCESSFUL_OPERATION	stm8s_stdperiph_driver\inc\stm8s_flash.h	124;"	enumerator	enum:__anon59
FLASH_STATUS_TIMEOUT	stm8s_stdperiph_driver\inc\stm8s_flash.h	125;"	enumerator	enum:__anon59
FLASH_STATUS_WRITE_PROTECTION_ERROR	stm8s_stdperiph_driver\inc\stm8s_flash.h	126;"	enumerator	enum:__anon59
FLASH_SetLowPowerMode	stm8s_stdperiph_driver\inc\stm8s_flash.h	261;"	prototype	signature:(FLASH_LPMode_TypeDef FLASH_LPMode)
FLASH_SetProgrammingTime	stm8s_stdperiph_driver\inc\stm8s_flash.h	262;"	prototype	signature:(FLASH_ProgramTime_TypeDef FLASH_ProgTime)
FLASH_Status_TypeDef	stm8s_stdperiph_driver\inc\stm8s_flash.h	127;"	typedef	typeref:enum:__anon59
FLASH_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1512;"	typedef	typeref:struct:FLASH_struct
FLASH_Unlock	stm8s_stdperiph_driver\inc\stm8s_flash.h	250;"	prototype	signature:(FLASH_MemType_TypeDef FLASH_MemType)
FLASH_WaitForLastOperation	stm8s_stdperiph_driver\inc\stm8s_flash.h	285;"	prototype	signature:(FLASH_MemType_TypeDef FLASH_MemType)
FLASH_struct	stm8s_stdperiph_driver\inc\stm8s.h	1498;"	struct
FMR1	stm8s_stdperiph_driver\inc\stm8s.h	2182;"	member	struct:__anon5::__anon6::__anon12
FMR2	stm8s_stdperiph_driver\inc\stm8s.h	2183;"	member	struct:__anon5::__anon6::__anon12
FPR	stm8s_stdperiph_driver\inc\stm8s.h	1503;"	member	struct:FLASH_struct
FR01	stm8s_stdperiph_driver\inc\stm8s.h	2086;"	member	struct:__anon5::__anon6::__anon8
FR02	stm8s_stdperiph_driver\inc\stm8s.h	2087;"	member	struct:__anon5::__anon6::__anon8
FR03	stm8s_stdperiph_driver\inc\stm8s.h	2088;"	member	struct:__anon5::__anon6::__anon8
FR04	stm8s_stdperiph_driver\inc\stm8s.h	2089;"	member	struct:__anon5::__anon6::__anon8
FR05	stm8s_stdperiph_driver\inc\stm8s.h	2090;"	member	struct:__anon5::__anon6::__anon8
FR06	stm8s_stdperiph_driver\inc\stm8s.h	2091;"	member	struct:__anon5::__anon6::__anon8
FR07	stm8s_stdperiph_driver\inc\stm8s.h	2092;"	member	struct:__anon5::__anon6::__anon8
FR08	stm8s_stdperiph_driver\inc\stm8s.h	2093;"	member	struct:__anon5::__anon6::__anon8
FR09	stm8s_stdperiph_driver\inc\stm8s.h	2095;"	member	struct:__anon5::__anon6::__anon8
FR10	stm8s_stdperiph_driver\inc\stm8s.h	2096;"	member	struct:__anon5::__anon6::__anon8
FR11	stm8s_stdperiph_driver\inc\stm8s.h	2097;"	member	struct:__anon5::__anon6::__anon8
FR12	stm8s_stdperiph_driver\inc\stm8s.h	2098;"	member	struct:__anon5::__anon6::__anon8
FR13	stm8s_stdperiph_driver\inc\stm8s.h	2099;"	member	struct:__anon5::__anon6::__anon8
FR14	stm8s_stdperiph_driver\inc\stm8s.h	2100;"	member	struct:__anon5::__anon6::__anon8
FR15	stm8s_stdperiph_driver\inc\stm8s.h	2101;"	member	struct:__anon5::__anon6::__anon8
FR16	stm8s_stdperiph_driver\inc\stm8s.h	2102;"	member	struct:__anon5::__anon6::__anon8
FREQR	stm8s_stdperiph_driver\inc\stm8s.h	1316;"	member	struct:I2C_struct
Filter	stm8s_stdperiph_driver\inc\stm8s.h	2104;"	member	union:__anon5::__anon6	typeref:struct:__anon5::__anon6::__anon8
Filter01	stm8s_stdperiph_driver\inc\stm8s.h	2127;"	member	union:__anon5::__anon6	typeref:struct:__anon5::__anon6::__anon9
Filter23	stm8s_stdperiph_driver\inc\stm8s.h	2149;"	member	union:__anon5::__anon6	typeref:struct:__anon5::__anon6::__anon10
Filter45	stm8s_stdperiph_driver\inc\stm8s.h	2171;"	member	union:__anon5::__anon6	typeref:struct:__anon5::__anon6::__anon11
FlagStatus	stm8s_stdperiph_driver\inc\stm8s.h	221;"	typedef	typeref:enum:__anon2
FunctionalState	stm8s_stdperiph_driver\inc\stm8s.h	223;"	typedef	typeref:enum:__anon3
GCR	stm8s_stdperiph_driver\inc\stm8s.h	2410;"	member	struct:CFG_struct
GPIOA	stm8s_stdperiph_driver\inc\stm8s.h	2516;"	macro
GPIOA_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2447;"	macro
GPIOB	stm8s_stdperiph_driver\inc\stm8s.h	2518;"	macro
GPIOB_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2448;"	macro
GPIOC	stm8s_stdperiph_driver\inc\stm8s.h	2520;"	macro
GPIOC_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2449;"	macro
GPIOD	stm8s_stdperiph_driver\inc\stm8s.h	2522;"	macro
GPIOD_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2450;"	macro
GPIOE	stm8s_stdperiph_driver\inc\stm8s.h	2524;"	macro
GPIOE_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2451;"	macro
GPIOF	stm8s_stdperiph_driver\inc\stm8s.h	2526;"	macro
GPIOF_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2452;"	macro
GPIOG	stm8s_stdperiph_driver\inc\stm8s.h	2530;"	macro
GPIOG_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2453;"	macro
GPIOH	stm8s_stdperiph_driver\inc\stm8s.h	2535;"	macro
GPIOH_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2454;"	macro
GPIOI	stm8s_stdperiph_driver\inc\stm8s.h	2536;"	macro
GPIOI_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2455;"	macro
GPIO_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	269;"	macro
GPIO_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	270;"	macro
GPIO_Configuration	user\config.c	26;"	function	signature:(void)
GPIO_Configuration	user\main.h	141;"	prototype	signature:(void)
GPIO_DDR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	268;"	macro
GPIO_DeInit	stm8s_stdperiph_driver\inc\stm8s_gpio.h	133;"	prototype	signature:(GPIO_TypeDef* GPIOx)
GPIO_DeInit	stm8s_stdperiph_driver\src\stm8s_gpio.c	47;"	function	signature:(GPIO_TypeDef* GPIOx)
GPIO_ExternalPullUpConfig	stm8s_stdperiph_driver\inc\stm8s_gpio.h	142;"	prototype	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef GPIO_Pin, FunctionalState NewState)
GPIO_ExternalPullUpConfig	stm8s_stdperiph_driver\src\stm8s_gpio.c	219;"	function	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef GPIO_Pin, FunctionalState NewState)
GPIO_Init	stm8s_stdperiph_driver\inc\stm8s_gpio.h	134;"	prototype	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef GPIO_Pin, GPIO_Mode_TypeDef GPIO_Mode)
GPIO_Init	stm8s_stdperiph_driver\src\stm8s_gpio.c	65;"	function	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef GPIO_Pin, GPIO_Mode_TypeDef GPIO_Mode)
GPIO_Input	user\main.h	39;"	macro
GPIO_MODE_IN_FL_IT	stm8s_stdperiph_driver\inc\stm8s_gpio.h	52;"	enumerator	enum:__anon26
GPIO_MODE_IN_FL_NO_IT	stm8s_stdperiph_driver\inc\stm8s_gpio.h	50;"	enumerator	enum:__anon26
GPIO_MODE_IN_PU_IT	stm8s_stdperiph_driver\inc\stm8s_gpio.h	53;"	enumerator	enum:__anon26
GPIO_MODE_IN_PU_NO_IT	stm8s_stdperiph_driver\inc\stm8s_gpio.h	51;"	enumerator	enum:__anon26
GPIO_MODE_OUT_OD_HIZ_FAST	stm8s_stdperiph_driver\inc\stm8s_gpio.h	58;"	enumerator	enum:__anon26
GPIO_MODE_OUT_OD_HIZ_SLOW	stm8s_stdperiph_driver\inc\stm8s_gpio.h	60;"	enumerator	enum:__anon26
GPIO_MODE_OUT_OD_LOW_FAST	stm8s_stdperiph_driver\inc\stm8s_gpio.h	54;"	enumerator	enum:__anon26
GPIO_MODE_OUT_OD_LOW_SLOW	stm8s_stdperiph_driver\inc\stm8s_gpio.h	56;"	enumerator	enum:__anon26
GPIO_MODE_OUT_PP_HIGH_FAST	stm8s_stdperiph_driver\inc\stm8s_gpio.h	59;"	enumerator	enum:__anon26
GPIO_MODE_OUT_PP_HIGH_SLOW	stm8s_stdperiph_driver\inc\stm8s_gpio.h	61;"	enumerator	enum:__anon26
GPIO_MODE_OUT_PP_LOW_FAST	stm8s_stdperiph_driver\inc\stm8s_gpio.h	55;"	enumerator	enum:__anon26
GPIO_MODE_OUT_PP_LOW_SLOW	stm8s_stdperiph_driver\inc\stm8s_gpio.h	57;"	enumerator	enum:__anon26
GPIO_Mode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_gpio.h	62;"	typedef	typeref:enum:__anon26
GPIO_ODR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	267;"	macro
GPIO_Out	user\main.h	36;"	macro
GPIO_OutHigh	user\main.h	37;"	macro
GPIO_OutLow	user\main.h	38;"	macro
GPIO_PIN_0	stm8s_stdperiph_driver\inc\stm8s_gpio.h	71;"	enumerator	enum:__anon27
GPIO_PIN_1	stm8s_stdperiph_driver\inc\stm8s_gpio.h	72;"	enumerator	enum:__anon27
GPIO_PIN_2	stm8s_stdperiph_driver\inc\stm8s_gpio.h	73;"	enumerator	enum:__anon27
GPIO_PIN_3	stm8s_stdperiph_driver\inc\stm8s_gpio.h	74;"	enumerator	enum:__anon27
GPIO_PIN_4	stm8s_stdperiph_driver\inc\stm8s_gpio.h	75;"	enumerator	enum:__anon27
GPIO_PIN_5	stm8s_stdperiph_driver\inc\stm8s_gpio.h	76;"	enumerator	enum:__anon27
GPIO_PIN_6	stm8s_stdperiph_driver\inc\stm8s_gpio.h	77;"	enumerator	enum:__anon27
GPIO_PIN_7	stm8s_stdperiph_driver\inc\stm8s_gpio.h	78;"	enumerator	enum:__anon27
GPIO_PIN_ALL	stm8s_stdperiph_driver\inc\stm8s_gpio.h	81;"	enumerator	enum:__anon27
GPIO_PIN_HNIB	stm8s_stdperiph_driver\inc\stm8s_gpio.h	80;"	enumerator	enum:__anon27
GPIO_PIN_LNIB	stm8s_stdperiph_driver\inc\stm8s_gpio.h	79;"	enumerator	enum:__anon27
GPIO_Pin_TypeDef	stm8s_stdperiph_driver\inc\stm8s_gpio.h	82;"	typedef	typeref:enum:__anon27
GPIO_ReadInputData	stm8s_stdperiph_driver\inc\stm8s_gpio.h	139;"	prototype	signature:(GPIO_TypeDef* GPIOx)
GPIO_ReadInputData	stm8s_stdperiph_driver\src\stm8s_gpio.c	196;"	function	signature:(GPIO_TypeDef* GPIOx)
GPIO_ReadInputPin	stm8s_stdperiph_driver\inc\stm8s_gpio.h	141;"	prototype	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef GPIO_Pin)
GPIO_ReadInputPin	stm8s_stdperiph_driver\src\stm8s_gpio.c	207;"	function	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef GPIO_Pin)
GPIO_ReadOutputData	stm8s_stdperiph_driver\inc\stm8s_gpio.h	140;"	prototype	signature:(GPIO_TypeDef* GPIOx)
GPIO_ReadOutputData	stm8s_stdperiph_driver\src\stm8s_gpio.c	185;"	function	signature:(GPIO_TypeDef* GPIOx)
GPIO_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	261;"	typedef	typeref:struct:GPIO_struct
GPIO_Write	stm8s_stdperiph_driver\inc\stm8s_gpio.h	135;"	prototype	signature:(GPIO_TypeDef* GPIOx, uint8_t PortVal)
GPIO_Write	stm8s_stdperiph_driver\src\stm8s_gpio.c	135;"	function	signature:(GPIO_TypeDef* GPIOx, uint8_t PortVal)
GPIO_WriteHigh	stm8s_stdperiph_driver\inc\stm8s_gpio.h	136;"	prototype	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef PortPins)
GPIO_WriteHigh	stm8s_stdperiph_driver\src\stm8s_gpio.c	148;"	function	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef PortPins)
GPIO_WriteLow	stm8s_stdperiph_driver\inc\stm8s_gpio.h	137;"	prototype	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef PortPins)
GPIO_WriteLow	stm8s_stdperiph_driver\src\stm8s_gpio.c	161;"	function	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef PortPins)
GPIO_WriteReverse	stm8s_stdperiph_driver\inc\stm8s_gpio.h	138;"	prototype	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef PortPins)
GPIO_WriteReverse	stm8s_stdperiph_driver\src\stm8s_gpio.c	174;"	function	signature:(GPIO_TypeDef* GPIOx, GPIO_Pin_TypeDef PortPins)
GPIO_struct	stm8s_stdperiph_driver\inc\stm8s.h	253;"	struct
GTR	stm8s_stdperiph_driver\inc\stm8s.h	1762;"	member	struct:UART1_struct
GTR	stm8s_stdperiph_driver\inc\stm8s.h	1861;"	member	struct:UART2_struct
HSE_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	101;"	macro
HSE_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	99;"	macro
HSIDivFactor	stm8s_stdperiph_driver\src\stm8s_clk.c	42;"	variable
HSITRIMR	stm8s_stdperiph_driver\inc\stm8s.h	506;"	member	struct:CLK_struct
HSI_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	108;"	macro
HTRH	stm8s_stdperiph_driver\inc\stm8s.h	313;"	member	struct:ADC1_struct
HTRL	stm8s_stdperiph_driver\inc\stm8s.h	314;"	member	struct:ADC1_struct
I2C	stm8s_stdperiph_driver\inc\stm8s.h	2545;"	macro
I2C_7BIT_ADDR	user\main.h	45;"	macro
I2C_ACK_CURR	stm8s_stdperiph_driver\inc\stm8s_i2c.h	50;"	enumerator	enum:__anon62
I2C_ACK_NEXT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	51;"	enumerator	enum:__anon62
I2C_ACK_NONE	stm8s_stdperiph_driver\inc\stm8s_i2c.h	49;"	enumerator	enum:__anon62
I2C_ADDMODE_10BIT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	60;"	enumerator	enum:__anon63
I2C_ADDMODE_7BIT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	59;"	enumerator	enum:__anon63
I2C_Ack_TypeDef	stm8s_stdperiph_driver\inc\stm8s_i2c.h	52;"	typedef	typeref:enum:__anon62
I2C_AcknowledgeConfig	stm8s_stdperiph_driver\inc\stm8s_i2c.h	509;"	prototype	signature:(I2C_Ack_TypeDef Ack)
I2C_AddMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_i2c.h	61;"	typedef	typeref:enum:__anon63
I2C_BQ24195_ADDR	user\main.h	44;"	macro
I2C_BQ24195_ByteRead	user\i2c_bq24195.c	31;"	function	signature:(uint8_t addr)
I2C_BQ24195_ByteRead	user\main.h	126;"	prototype	signature:(uint8_t addr)
I2C_BQ24195_ByteWrite	user\i2c_bq24195.c	3;"	function	signature:(uint8_t addr, uint8_t data)
I2C_BQ24195_ByteWrite	user\main.h	125;"	prototype	signature:(uint8_t addr, uint8_t data)
I2C_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2465;"	macro
I2C_CCRH_CCR	stm8s_stdperiph_driver\inc\stm8s.h	1406;"	macro
I2C_CCRH_DUTY	stm8s_stdperiph_driver\inc\stm8s.h	1405;"	macro
I2C_CCRH_FS	stm8s_stdperiph_driver\inc\stm8s.h	1404;"	macro
I2C_CCRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1347;"	macro
I2C_CCRL_CCR	stm8s_stdperiph_driver\inc\stm8s.h	1402;"	macro
I2C_CCRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1346;"	macro
I2C_CR1_ENGC	stm8s_stdperiph_driver\inc\stm8s.h	1359;"	macro
I2C_CR1_NOSTRETCH	stm8s_stdperiph_driver\inc\stm8s.h	1358;"	macro
I2C_CR1_PE	stm8s_stdperiph_driver\inc\stm8s.h	1360;"	macro
I2C_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1336;"	macro
I2C_CR2_ACK	stm8s_stdperiph_driver\inc\stm8s.h	1364;"	macro
I2C_CR2_POS	stm8s_stdperiph_driver\inc\stm8s.h	1363;"	macro
I2C_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1337;"	macro
I2C_CR2_START	stm8s_stdperiph_driver\inc\stm8s.h	1366;"	macro
I2C_CR2_STOP	stm8s_stdperiph_driver\inc\stm8s.h	1365;"	macro
I2C_CR2_SWRST	stm8s_stdperiph_driver\inc\stm8s.h	1362;"	macro
I2C_CheckEvent	stm8s_stdperiph_driver\inc\stm8s_i2c.h	597;"	prototype	signature:(I2C_Event_TypeDef I2C_Event)
I2C_ClearAddrFlag	user\main.h	60;"	macro
I2C_ClearBTFFlag	user\main.h	61;"	macro
I2C_ClearFlag	stm8s_stdperiph_driver\inc\stm8s_i2c.h	614;"	prototype	signature:(I2C_Flag_TypeDef I2C_FLAG)
I2C_ClearITPendingBit	stm8s_stdperiph_driver\inc\stm8s_i2c.h	616;"	prototype	signature:(I2C_ITPendingBit_TypeDef I2C_ITPendingBit)
I2C_Close	user\main.h	47;"	macro
I2C_Cmd	stm8s_stdperiph_driver\inc\stm8s_i2c.h	503;"	prototype	signature:(FunctionalState NewState)
I2C_Configuration	user\config.c	69;"	function	signature:(void)
I2C_Configuration	user\main.h	143;"	prototype	signature:(void)
I2C_DIRECTION_RX	stm8s_stdperiph_driver\inc\stm8s_i2c.h	81;"	enumerator	enum:__anon65
I2C_DIRECTION_TX	stm8s_stdperiph_driver\inc\stm8s_i2c.h	80;"	enumerator	enum:__anon65
I2C_DR_DR	stm8s_stdperiph_driver\inc\stm8s.h	1377;"	macro
I2C_DR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1341;"	macro
I2C_DUTYCYCLE_16_9	stm8s_stdperiph_driver\inc\stm8s_i2c.h	41;"	enumerator	enum:__anon61
I2C_DUTYCYCLE_2	stm8s_stdperiph_driver\inc\stm8s_i2c.h	40;"	enumerator	enum:__anon61
I2C_DeInit	stm8s_stdperiph_driver\inc\stm8s_i2c.h	499;"	prototype	signature:(void)
I2C_Direction_TypeDef	stm8s_stdperiph_driver\inc\stm8s_i2c.h	82;"	typedef	typeref:enum:__anon65
I2C_DisableAck	user\main.h	51;"	macro
I2C_DutyCycle_TypeDef	stm8s_stdperiph_driver\inc\stm8s_i2c.h	42;"	typedef	typeref:enum:__anon61
I2C_EVENT_MASTER_BYTE_RECEIVED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	236;"	enumerator	enum:__anon68
I2C_EVENT_MASTER_BYTE_TRANSMITTED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	243;"	enumerator	enum:__anon68
I2C_EVENT_MASTER_BYTE_TRANSMITTING	stm8s_stdperiph_driver\inc\stm8s_i2c.h	240;"	enumerator	enum:__anon68
I2C_EVENT_MASTER_MODE_ADDRESS10	stm8s_stdperiph_driver\inc\stm8s_i2c.h	204;"	enumerator	enum:__anon68
I2C_EVENT_MASTER_MODE_SELECT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	172;"	enumerator	enum:__anon68
I2C_EVENT_MASTER_RECEIVER_MODE_SELECTED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	202;"	enumerator	enum:__anon68
I2C_EVENT_MASTER_TRANSMITTER_MODE_SELECTED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	201;"	enumerator	enum:__anon68
I2C_EVENT_SLAVE_ACK_FAILURE	stm8s_stdperiph_driver\inc\stm8s_i2c.h	318;"	enumerator	enum:__anon68
I2C_EVENT_SLAVE_BYTE_RECEIVED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	309;"	enumerator	enum:__anon68
I2C_EVENT_SLAVE_BYTE_TRANSMITTED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	315;"	enumerator	enum:__anon68
I2C_EVENT_SLAVE_BYTE_TRANSMITTING	stm8s_stdperiph_driver\inc\stm8s_i2c.h	316;"	enumerator	enum:__anon68
I2C_EVENT_SLAVE_GENERALCALLADDRESS_MATCHED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	278;"	enumerator	enum:__anon68
I2C_EVENT_SLAVE_RECEIVER_ADDRESS_MATCHED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	274;"	enumerator	enum:__anon68
I2C_EVENT_SLAVE_STOP_DETECTED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	311;"	enumerator	enum:__anon68
I2C_EVENT_SLAVE_TRANSMITTER_ADDRESS_MATCHED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	275;"	enumerator	enum:__anon68
I2C_EnableAck	user\main.h	50;"	macro
I2C_Event_TypeDef	stm8s_stdperiph_driver\inc\stm8s_i2c.h	319;"	typedef	typeref:enum:__anon68
I2C_FLAG_ACKNOWLEDGEFAILURE	stm8s_stdperiph_driver\inc\stm8s_i2c.h	108;"	enumerator	enum:__anon66
I2C_FLAG_ADDRESSSENTMATCHED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	102;"	enumerator	enum:__anon66
I2C_FLAG_ARBITRATIONLOSS	stm8s_stdperiph_driver\inc\stm8s_i2c.h	109;"	enumerator	enum:__anon66
I2C_FLAG_BUSBUSY	stm8s_stdperiph_driver\inc\stm8s_i2c.h	115;"	enumerator	enum:__anon66
I2C_FLAG_BUSERROR	stm8s_stdperiph_driver\inc\stm8s_i2c.h	110;"	enumerator	enum:__anon66
I2C_FLAG_GENERALCALL	stm8s_stdperiph_driver\inc\stm8s_i2c.h	113;"	enumerator	enum:__anon66
I2C_FLAG_HEADERSENT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	100;"	enumerator	enum:__anon66
I2C_FLAG_MASTERSLAVE	stm8s_stdperiph_driver\inc\stm8s_i2c.h	116;"	enumerator	enum:__anon66
I2C_FLAG_OVERRUNUNDERRUN	stm8s_stdperiph_driver\inc\stm8s_i2c.h	107;"	enumerator	enum:__anon66
I2C_FLAG_RXNOTEMPTY	stm8s_stdperiph_driver\inc\stm8s_i2c.h	98;"	enumerator	enum:__anon66
I2C_FLAG_STARTDETECTION	stm8s_stdperiph_driver\inc\stm8s_i2c.h	103;"	enumerator	enum:__anon66
I2C_FLAG_STOPDETECTION	stm8s_stdperiph_driver\inc\stm8s_i2c.h	99;"	enumerator	enum:__anon66
I2C_FLAG_TRANSFERFINISHED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	101;"	enumerator	enum:__anon66
I2C_FLAG_TRANSMITTERRECEIVER	stm8s_stdperiph_driver\inc\stm8s_i2c.h	114;"	enumerator	enum:__anon66
I2C_FLAG_TXEMPTY	stm8s_stdperiph_driver\inc\stm8s_i2c.h	97;"	enumerator	enum:__anon66
I2C_FLAG_WAKEUPFROMHALT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	106;"	enumerator	enum:__anon66
I2C_FREQR_FREQ	stm8s_stdperiph_driver\inc\stm8s.h	1368;"	macro
I2C_FREQR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1338;"	macro
I2C_FastModeDutyCycleConfig	stm8s_stdperiph_driver\inc\stm8s_i2c.h	510;"	prototype	signature:(I2C_DutyCycle_TypeDef I2C_DutyCycle)
I2C_Flag_TypeDef	stm8s_stdperiph_driver\inc\stm8s_i2c.h	117;"	typedef	typeref:enum:__anon66
I2C_GeneralCallCmd	stm8s_stdperiph_driver\inc\stm8s_i2c.h	504;"	prototype	signature:(FunctionalState NewState)
I2C_GenerateSTART	stm8s_stdperiph_driver\inc\stm8s_i2c.h	505;"	prototype	signature:(FunctionalState NewState)
I2C_GenerateSTOP	stm8s_stdperiph_driver\inc\stm8s_i2c.h	506;"	prototype	signature:(FunctionalState NewState)
I2C_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_i2c.h	609;"	prototype	signature:(I2C_Flag_TypeDef I2C_Flag)
I2C_GetITStatus	stm8s_stdperiph_driver\inc\stm8s_i2c.h	615;"	prototype	signature:(I2C_ITPendingBit_TypeDef I2C_ITPendingBit)
I2C_GetLastEvent	stm8s_stdperiph_driver\inc\stm8s_i2c.h	603;"	prototype	signature:(void)
I2C_INPUT_FRE	user\main.h	42;"	macro
I2C_INTER_ADDR	user\main.h	43;"	macro
I2C_ITConfig	stm8s_stdperiph_driver\inc\stm8s_i2c.h	511;"	prototype	signature:(I2C_IT_TypeDef I2C_IT, FunctionalState NewState)
I2C_ITPENDINGBIT_ACKNOWLEDGEFAILURE	stm8s_stdperiph_driver\inc\stm8s_i2c.h	143;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_ADDRESSSENTMATCHED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	137;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_ARBITRATIONLOSS	stm8s_stdperiph_driver\inc\stm8s_i2c.h	144;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_BUSERROR	stm8s_stdperiph_driver\inc\stm8s_i2c.h	145;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_HEADERSENT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	135;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_OVERRUNUNDERRUN	stm8s_stdperiph_driver\inc\stm8s_i2c.h	142;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_RXNOTEMPTY	stm8s_stdperiph_driver\inc\stm8s_i2c.h	133;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_STARTDETECTION	stm8s_stdperiph_driver\inc\stm8s_i2c.h	138;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_STOPDETECTION	stm8s_stdperiph_driver\inc\stm8s_i2c.h	134;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_TRANSFERFINISHED	stm8s_stdperiph_driver\inc\stm8s_i2c.h	136;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_TXEMPTY	stm8s_stdperiph_driver\inc\stm8s_i2c.h	132;"	enumerator	enum:__anon67
I2C_ITPENDINGBIT_WAKEUPFROMHALT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	141;"	enumerator	enum:__anon67
I2C_ITPendingBit_TypeDef	stm8s_stdperiph_driver\inc\stm8s_i2c.h	146;"	typedef	typeref:enum:__anon67
I2C_ITR_ITBUFEN	stm8s_stdperiph_driver\inc\stm8s.h	1398;"	macro
I2C_ITR_ITERREN	stm8s_stdperiph_driver\inc\stm8s.h	1400;"	macro
I2C_ITR_ITEVTEN	stm8s_stdperiph_driver\inc\stm8s.h	1399;"	macro
I2C_ITR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1345;"	macro
I2C_IT_BUF	stm8s_stdperiph_driver\inc\stm8s_i2c.h	71;"	enumerator	enum:__anon64
I2C_IT_ERR	stm8s_stdperiph_driver\inc\stm8s_i2c.h	69;"	enumerator	enum:__anon64
I2C_IT_EVT	stm8s_stdperiph_driver\inc\stm8s_i2c.h	70;"	enumerator	enum:__anon64
I2C_IT_TypeDef	stm8s_stdperiph_driver\inc\stm8s_i2c.h	72;"	typedef	typeref:enum:__anon64
I2C_Init	stm8s_stdperiph_driver\inc\stm8s_i2c.h	500;"	prototype	signature:(uint32_t OutputClockFrequencyHz, uint16_t OwnAddress, I2C_DutyCycle_TypeDef I2C_DutyCycle, I2C_Ack_TypeDef Ack, I2C_AddMode_TypeDef AddMode, uint8_t InputClockFrequencyMHz )
I2C_IsAddrFinished	user\main.h	56;"	macro
I2C_IsBusy	user\main.h	54;"	macro
I2C_IsRecvNotEmpty	user\main.h	59;"	macro
I2C_IsSendEmpty	user\main.h	58;"	macro
I2C_IsSendFinished	user\main.h	57;"	macro
I2C_IsStartFinished	user\main.h	55;"	macro
I2C_MAX_FAST_FREQ	stm8s_stdperiph_driver\inc\stm8s_i2c.h	330;"	macro
I2C_MAX_INPUT_FREQ	stm8s_stdperiph_driver\inc\stm8s_i2c.h	332;"	macro
I2C_MAX_INPUT_FREQ	stm8s_stdperiph_driver\inc\stm8s_i2c.h	334;"	macro
I2C_MAX_STANDARD_FREQ	stm8s_stdperiph_driver\inc\stm8s_i2c.h	329;"	macro
I2C_OARH_ADD	stm8s_stdperiph_driver\inc\stm8s.h	1375;"	macro
I2C_OARH_ADDCONF	stm8s_stdperiph_driver\inc\stm8s.h	1374;"	macro
I2C_OARH_ADDMODE	stm8s_stdperiph_driver\inc\stm8s.h	1373;"	macro
I2C_OARH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1340;"	macro
I2C_OARL_ADD	stm8s_stdperiph_driver\inc\stm8s.h	1370;"	macro
I2C_OARL_ADD0	stm8s_stdperiph_driver\inc\stm8s.h	1371;"	macro
I2C_OARL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1339;"	macro
I2C_OUTPUT_FRE	user\main.h	41;"	macro
I2C_Open	user\main.h	46;"	macro
I2C_ReceiveData	stm8s_stdperiph_driver\inc\stm8s_i2c.h	512;"	prototype	signature:(void)
I2C_RecvByte	user\main.h	52;"	macro
I2C_SR1_ADD10	stm8s_stdperiph_driver\inc\stm8s.h	1382;"	macro
I2C_SR1_ADDR	stm8s_stdperiph_driver\inc\stm8s.h	1384;"	macro
I2C_SR1_BTF	stm8s_stdperiph_driver\inc\stm8s.h	1383;"	macro
I2C_SR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1342;"	macro
I2C_SR1_RXNE	stm8s_stdperiph_driver\inc\stm8s.h	1380;"	macro
I2C_SR1_SB	stm8s_stdperiph_driver\inc\stm8s.h	1385;"	macro
I2C_SR1_STOPF	stm8s_stdperiph_driver\inc\stm8s.h	1381;"	macro
I2C_SR1_TXE	stm8s_stdperiph_driver\inc\stm8s.h	1379;"	macro
I2C_SR2_AF	stm8s_stdperiph_driver\inc\stm8s.h	1389;"	macro
I2C_SR2_ARLO	stm8s_stdperiph_driver\inc\stm8s.h	1390;"	macro
I2C_SR2_BERR	stm8s_stdperiph_driver\inc\stm8s.h	1391;"	macro
I2C_SR2_OVR	stm8s_stdperiph_driver\inc\stm8s.h	1388;"	macro
I2C_SR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1343;"	macro
I2C_SR2_WUFH	stm8s_stdperiph_driver\inc\stm8s.h	1387;"	macro
I2C_SR3_BUSY	stm8s_stdperiph_driver\inc\stm8s.h	1395;"	macro
I2C_SR3_GENCALL	stm8s_stdperiph_driver\inc\stm8s.h	1393;"	macro
I2C_SR3_MSL	stm8s_stdperiph_driver\inc\stm8s.h	1396;"	macro
I2C_SR3_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1344;"	macro
I2C_SR3_TRA	stm8s_stdperiph_driver\inc\stm8s.h	1394;"	macro
I2C_Send7bitAddress	stm8s_stdperiph_driver\inc\stm8s_i2c.h	513;"	prototype	signature:(uint8_t Address, I2C_Direction_TypeDef Direction)
I2C_SendByte	user\main.h	53;"	macro
I2C_SendData	stm8s_stdperiph_driver\inc\stm8s_i2c.h	514;"	prototype	signature:(uint8_t Data)
I2C_SoftwareResetCmd	stm8s_stdperiph_driver\inc\stm8s_i2c.h	507;"	prototype	signature:(FunctionalState NewState)
I2C_Start	user\main.h	48;"	macro
I2C_Stop	user\main.h	49;"	macro
I2C_StretchClockCmd	stm8s_stdperiph_driver\inc\stm8s_i2c.h	508;"	prototype	signature:(FunctionalState NewState)
I2C_TRISER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1348;"	macro
I2C_TRISER_TRISE	stm8s_stdperiph_driver\inc\stm8s.h	1408;"	macro
I2C_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1330;"	typedef	typeref:struct:I2C_struct
I2C_struct	stm8s_stdperiph_driver\inc\stm8s.h	1312;"	struct
IAPSR	stm8s_stdperiph_driver\inc\stm8s.h	1505;"	member	struct:FLASH_struct
ICKR	stm8s_stdperiph_driver\inc\stm8s.h	494;"	member	struct:CLK_struct
ICR	stm8s_stdperiph_driver\inc\stm8s.h	1684;"	member	struct:SPI_struct
IDI_BAT_CHGING	user\main.h	88;"	macro
IDI_LUSB_OVERTOP_C	user\main.h	84;"	macro
IDI_LUSB_OVERTOP_V	user\main.h	86;"	macro
IDI_LUSB_TOOLOW_C	user\main.h	85;"	macro
IDI_LUSB_TOOLOW_V	user\main.h	87;"	macro
IDR	stm8s_stdperiph_driver\inc\stm8s.h	256;"	member	struct:GPIO_struct
IER	stm8s_stdperiph_driver\inc\stm8s.h	1049;"	member	struct:TIM4_struct
IER	stm8s_stdperiph_driver\inc\stm8s.h	1110;"	member	struct:TIM5_struct
IER	stm8s_stdperiph_driver\inc\stm8s.h	1249;"	member	struct:TIM6_struct
IER	stm8s_stdperiph_driver\inc\stm8s.h	2057;"	member	struct:__anon5
IER	stm8s_stdperiph_driver\inc\stm8s.h	602;"	member	struct:TIM1_struct
IER	stm8s_stdperiph_driver\inc\stm8s.h	815;"	member	struct:TIM2_struct
IER	stm8s_stdperiph_driver\inc\stm8s.h	939;"	member	struct:TIM3_struct
INTERRUPT	stm8s_stdperiph_driver\inc\stm8s.h	2655;"	macro
INTERRUPT	stm8s_stdperiph_driver\inc\stm8s.h	2657;"	macro
INTERRUPT_HANDLER	stm8s_stdperiph_driver\inc\stm8s.h	2633;"	macro
INTERRUPT_HANDLER	stm8s_stdperiph_driver\inc\stm8s.h	2638;"	macro
INTERRUPT_HANDLER	stm8s_stdperiph_driver\inc\stm8s.h	2645;"	macro
INTERRUPT_HANDLER_TRAP	stm8s_stdperiph_driver\inc\stm8s.h	2634;"	macro
INTERRUPT_HANDLER_TRAP	stm8s_stdperiph_driver\inc\stm8s.h	2639;"	macro
INTERRUPT_HANDLER_TRAP	stm8s_stdperiph_driver\inc\stm8s.h	2648;"	macro
IN_RAM	stm8s_stdperiph_driver\inc\stm8s.h	159;"	macro
IN_RAM	stm8s_stdperiph_driver\inc\stm8s.h	161;"	macro
IN_RAM	stm8s_stdperiph_driver\inc\stm8s.h	163;"	macro
IN_RAM	stm8s_stdperiph_driver\inc\stm8s.h	166;"	macro
ISPR1	stm8s_stdperiph_driver\inc\stm8s.h	1421;"	member	struct:ITC_struct
ISPR2	stm8s_stdperiph_driver\inc\stm8s.h	1422;"	member	struct:ITC_struct
ISPR3	stm8s_stdperiph_driver\inc\stm8s.h	1423;"	member	struct:ITC_struct
ISPR4	stm8s_stdperiph_driver\inc\stm8s.h	1424;"	member	struct:ITC_struct
ISPR5	stm8s_stdperiph_driver\inc\stm8s.h	1425;"	member	struct:ITC_struct
ISPR6	stm8s_stdperiph_driver\inc\stm8s.h	1426;"	member	struct:ITC_struct
ISPR7	stm8s_stdperiph_driver\inc\stm8s.h	1427;"	member	struct:ITC_struct
ISPR8	stm8s_stdperiph_driver\inc\stm8s.h	1428;"	member	struct:ITC_struct
IS_ADC1_ALIGN_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	201;"	macro
IS_ADC1_BUFFER_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	284;"	macro
IS_ADC1_CHANNEL_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	269;"	macro
IS_ADC1_CONVERSIONMODE_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	263;"	macro
IS_ADC1_EXTTRIG_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	195;"	macro
IS_ADC1_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	213;"	macro
IS_ADC1_ITPENDINGBIT_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	230;"	macro
IS_ADC1_IT_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	207;"	macro
IS_ADC1_PRESSEL_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	183;"	macro
IS_ADC1_SCHMITTTRIG_OK	stm8s_stdperiph_driver\inc\stm8s_adc1.h	247;"	macro
IS_AWU_TIMEBASE_OK	stm8s_stdperiph_driver\inc\stm8s_awu.h	92;"	macro
IS_BEEP_FREQUENCY_OK	stm8s_stdperiph_driver\inc\stm8s_beep.h	78;"	macro
IS_CLK_CSSCONFIG_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	234;"	macro
IS_CLK_CURRENTCLOCKSTATE_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	228;"	macro
IS_CLK_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	295;"	macro
IS_CLK_HSIPRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	313;"	macro
IS_CLK_HSITRIMVALUE_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	248;"	macro
IS_CLK_IT_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	308;"	macro
IS_CLK_OUTPUT_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	260;"	macro
IS_CLK_PERIPHERAL_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	277;"	macro
IS_CLK_PRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	321;"	macro
IS_CLK_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	241;"	macro
IS_CLK_SWIMDIVIDER_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	337;"	macro
IS_CLK_SWITCHMODE_OK	stm8s_stdperiph_driver\inc\stm8s_clk.h	223;"	macro
IS_EXTI_PINMASK_OK	stm8s_stdperiph_driver\inc\stm8s_exti.h	103;"	macro
IS_EXTI_PORT_OK	stm8s_stdperiph_driver\inc\stm8s_exti.h	93;"	macro
IS_EXTI_SENSITIVITY_OK	stm8s_stdperiph_driver\inc\stm8s_exti.h	77;"	macro
IS_EXTI_TLISENSITIVITY_OK	stm8s_stdperiph_driver\inc\stm8s_exti.h	86;"	macro
IS_FLASH_ADDRESS_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	173;"	macro
IS_FLASH_DATA_ADDRESS_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	167;"	macro
IS_FLASH_DATA_BLOCK_NUMBER_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	184;"	macro
IS_FLASH_FLAGS_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	230;"	macro
IS_FLASH_FLAGS_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	236;"	macro
IS_FLASH_LOW_POWER_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	212;"	macro
IS_FLASH_PROGRAM_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	197;"	macro
IS_FLASH_PROGRAM_TIME_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	204;"	macro
IS_FLASH_PROG_ADDRESS_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	160;"	macro
IS_FLASH_PROG_BLOCK_NUMBER_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	179;"	macro
IS_FUNCTIONALSTATE_OK	stm8s_stdperiph_driver\inc\stm8s.h	224;"	macro
IS_GPIO_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_gpio.h	104;"	macro
IS_GPIO_PIN_OK	stm8s_stdperiph_driver\inc\stm8s_gpio.h	122;"	macro
IS_I2C_ACK_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	362;"	macro
IS_I2C_ADDMODE_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	370;"	macro
IS_I2C_ADDRESS_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	474;"	macro
IS_I2C_CLEAR_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	416;"	macro
IS_I2C_CLEAR_ITPENDINGBIT_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	440;"	macro
IS_I2C_DIRECTION_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	388;"	macro
IS_I2C_DUTYCYCLE_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	355;"	macro
IS_I2C_EVENT_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	450;"	macro
IS_I2C_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	395;"	macro
IS_I2C_INPUT_CLOCK_FREQ_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	480;"	macro
IS_I2C_INTERRUPT_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	377;"	macro
IS_I2C_ITPENDINGBIT_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	422;"	macro
IS_I2C_OUTPUT_CLOCK_FREQ_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	487;"	macro
IS_I2C_OWN_ADDRESS_OK	stm8s_stdperiph_driver\inc\stm8s_i2c.h	470;"	macro
IS_ITC_INTERRUPTS_DISABLED	stm8s_stdperiph_driver\inc\stm8s_itc.h	147;"	macro
IS_ITC_IRQ_OK	stm8s_stdperiph_driver\inc\stm8s_itc.h	137;"	macro
IS_ITC_PRIORITY_OK	stm8s_stdperiph_driver\inc\stm8s_itc.h	140;"	macro
IS_IWDG_PRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	59;"	macro
IS_IWDG_WRITEACCESS_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	71;"	macro
IS_LSI_FREQUENCY_OK	stm8s_stdperiph_driver\inc\stm8s_awu.h	114;"	macro
IS_LSI_FREQUENCY_OK	stm8s_stdperiph_driver\inc\stm8s_beep.h	86;"	macro
IS_MEMORY_TYPE_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	190;"	macro
IS_OPTION_BYTE_ADDRESS_OK	stm8s_stdperiph_driver\inc\stm8s_flash.h	221;"	macro
IS_RST_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_rst.h	60;"	macro
IS_SPI_BAUDRATE_PRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	206;"	macro
IS_SPI_CLEAR_FLAGS_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	258;"	macro
IS_SPI_CLEAR_IT_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	286;"	macro
IS_SPI_CONFIG_IT_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	265;"	macro
IS_SPI_CRC_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	238;"	macro
IS_SPI_CRC_POLYNOMIAL_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	195;"	macro
IS_SPI_DATA_DIRECTION_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	171;"	macro
IS_SPI_DIRECTION_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	180;"	macro
IS_SPI_FIRSTBIT_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	231;"	macro
IS_SPI_FLAGS_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	245;"	macro
IS_SPI_GET_IT_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	274;"	macro
IS_SPI_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	200;"	macro
IS_SPI_PHASE_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	224;"	macro
IS_SPI_POLARITY_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	218;"	macro
IS_SPI_SLAVEMANAGEMENT_OK	stm8s_stdperiph_driver\inc\stm8s_spi.h	187;"	macro
IS_STATE_VALUE_OK	stm8s_stdperiph_driver\inc\stm8s.h	2691;"	macro
IS_TIM1_AUTOMATIC_OUTPUT_STATE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	180;"	macro
IS_TIM1_BREAK_POLARITY_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	170;"	macro
IS_TIM1_BREAK_STATE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	161;"	macro
IS_TIM1_CHANNEL_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	86;"	macro
IS_TIM1_CLEAR_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	465;"	macro
IS_TIM1_COMPLEMENTARY_CHANNEL_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	94;"	macro
IS_TIM1_COUNTER_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	109;"	macro
IS_TIM1_ENCODER_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	372;"	macro
IS_TIM1_EVENT_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	389;"	macro
IS_TIM1_EXT_POLARITY_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	351;"	macro
IS_TIM1_EXT_PRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	304;"	macro
IS_TIM1_EXT_TRG_FILTER_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	268;"	macro
IS_TIM1_FORCED_ACTION_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	474;"	macro
IS_TIM1_GET_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	452;"	macro
IS_TIM1_GET_IT_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	285;"	macro
IS_TIM1_IC_FILTER_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	265;"	macro
IS_TIM1_IC_POLARITY_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	234;"	macro
IS_TIM1_IC_PRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	258;"	macro
IS_TIM1_IC_SELECTION_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	245;"	macro
IS_TIM1_IT_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	283;"	macro
IS_TIM1_LOCK_LEVEL_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	192;"	macro
IS_TIM1_OCIDLE_STATE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	214;"	macro
IS_TIM1_OCM_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	56;"	macro
IS_TIM1_OCNIDLE_STATE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	224;"	macro
IS_TIM1_OCN_POLARITY_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	132;"	macro
IS_TIM1_OC_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	49;"	macro
IS_TIM1_OC_POLARITY_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	122;"	macro
IS_TIM1_OPM_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	72;"	macro
IS_TIM1_OSSI_STATE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	204;"	macro
IS_TIM1_OUTPUTN_STATE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	152;"	macro
IS_TIM1_OUTPUT_STATE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	142;"	macro
IS_TIM1_PRESCALER_RELOAD_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	361;"	macro
IS_TIM1_PWMI_CHANNEL_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	91;"	macro
IS_TIM1_SLAVE_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	430;"	macro
IS_TIM1_TIXCLK_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	340;"	macro
IS_TIM1_TIX_TRIGGER_SELECTION_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	328;"	macro
IS_TIM1_TRGO_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	413;"	macro
IS_TIM1_TRIGGER_SELECTION_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	320;"	macro
IS_TIM1_UPDATE_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	398;"	macro
IS_TIM2_CHANNEL_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	129;"	macro
IS_TIM2_CLEAR_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	265;"	macro
IS_TIM2_EVENT_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	233;"	macro
IS_TIM2_FORCED_ACTION_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	43;"	macro
IS_TIM2_GET_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	257;"	macro
IS_TIM2_GET_IT_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	209;"	macro
IS_TIM2_IC_FILTER_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	196;"	macro
IS_TIM2_IC_POLARITY_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	163;"	macro
IS_TIM2_IC_PRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	190;"	macro
IS_TIM2_IC_SELECTION1_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	178;"	macro
IS_TIM2_IC_SELECTION_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	174;"	macro
IS_TIM2_IT_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	207;"	macro
IS_TIM2_OCM_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	102;"	macro
IS_TIM2_OC_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	95;"	macro
IS_TIM2_OC_POLARITY_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	143;"	macro
IS_TIM2_OPM_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	118;"	macro
IS_TIM2_OUTPUT_STATE_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	153;"	macro
IS_TIM2_PRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	67;"	macro
IS_TIM2_PRESCALER_RELOAD_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	221;"	macro
IS_TIM2_PWMI_CHANNEL_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	133;"	macro
IS_TIM2_UPDATE_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_tim2.h	242;"	macro
IS_TIM4_EVENT_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_tim4.h	99;"	macro
IS_TIM4_GET_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_tim4.h	107;"	macro
IS_TIM4_IT_OK	stm8s_stdperiph_driver\inc\stm8s_tim4.h	117;"	macro
IS_TIM4_OPM_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_tim4.h	70;"	macro
IS_TIM4_PRESCALER_OK	stm8s_stdperiph_driver\inc\stm8s_tim4.h	54;"	macro
IS_TIM4_PRESCALER_RELOAD_OK	stm8s_stdperiph_driver\inc\stm8s_tim4.h	80;"	macro
IS_TIM4_UPDATE_SOURCE_OK	stm8s_stdperiph_driver\inc\stm8s_tim4.h	90;"	macro
IS_UART1_ADDRESS_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	327;"	macro
IS_UART1_BAUDRATE_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	319;"	macro
IS_UART1_CLEAR_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	233;"	macro
IS_UART1_CLEAR_IT_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	269;"	macro
IS_UART1_CONFIG_IT_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	244;"	macro
IS_UART1_FLAG_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	218;"	macro
IS_UART1_GET_IT_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	256;"	macro
IS_UART1_IRDAMODE_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	278;"	macro
IS_UART1_LINBREAKDETECTIONLENGTH_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	294;"	macro
IS_UART1_MODE_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	184;"	macro
IS_UART1_PARITY_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	311;"	macro
IS_UART1_STOPBITS_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	302;"	macro
IS_UART1_SYNCMODE_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	208;"	macro
IS_UART1_WAKEUP_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	286;"	macro
IS_UART1_WORDLENGTH_OK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	199;"	macro
IS_WWDG_COUNTERVALUE_OK	stm8s_stdperiph_driver\inc\stm8s_wwdg.h	49;"	macro
IS_WWDG_WINDOWLIMITVALUE_OK	stm8s_stdperiph_driver\inc\stm8s_wwdg.h	43;"	macro
ITC	stm8s_stdperiph_driver\inc\stm8s.h	2585;"	macro
ITC_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2479;"	macro
ITC_DeInit	stm8s_stdperiph_driver\inc\stm8s_itc.h	160;"	prototype	signature:(void)
ITC_GetCPUCC	stm8s_stdperiph_driver\inc\stm8s_itc.h	159;"	prototype	signature:(void)
ITC_GetSoftIntStatus	stm8s_stdperiph_driver\inc\stm8s_itc.h	161;"	prototype	signature:(void)
ITC_GetSoftwarePriority	stm8s_stdperiph_driver\inc\stm8s_itc.h	163;"	prototype	signature:(ITC_Irq_TypeDef IrqNum)
ITC_IRQ_ADC1	stm8s_stdperiph_driver\inc\stm8s_itc.h	89;"	enumerator	enum:__anon69
ITC_IRQ_ADC2	stm8s_stdperiph_driver\inc\stm8s_itc.h	85;"	enumerator	enum:__anon69
ITC_IRQ_AWU	stm8s_stdperiph_driver\inc\stm8s_itc.h	40;"	enumerator	enum:__anon69
ITC_IRQ_CAN_RX	stm8s_stdperiph_driver\inc\stm8s_itc.h	49;"	enumerator	enum:__anon69
ITC_IRQ_CAN_TX	stm8s_stdperiph_driver\inc\stm8s_itc.h	50;"	enumerator	enum:__anon69
ITC_IRQ_CLK	stm8s_stdperiph_driver\inc\stm8s_itc.h	41;"	enumerator	enum:__anon69
ITC_IRQ_EEPROM_EEC	stm8s_stdperiph_driver\inc\stm8s_itc.h	99;"	enumerator	enum:__anon69
ITC_IRQ_I2C	stm8s_stdperiph_driver\inc\stm8s_itc.h	75;"	enumerator	enum:__anon69
ITC_IRQ_PORTA	stm8s_stdperiph_driver\inc\stm8s_itc.h	42;"	enumerator	enum:__anon69
ITC_IRQ_PORTB	stm8s_stdperiph_driver\inc\stm8s_itc.h	43;"	enumerator	enum:__anon69
ITC_IRQ_PORTC	stm8s_stdperiph_driver\inc\stm8s_itc.h	44;"	enumerator	enum:__anon69
ITC_IRQ_PORTD	stm8s_stdperiph_driver\inc\stm8s_itc.h	45;"	enumerator	enum:__anon69
ITC_IRQ_PORTE	stm8s_stdperiph_driver\inc\stm8s_itc.h	46;"	enumerator	enum:__anon69
ITC_IRQ_PORTF	stm8s_stdperiph_driver\inc\stm8s_itc.h	54;"	enumerator	enum:__anon69
ITC_IRQ_SPI	stm8s_stdperiph_driver\inc\stm8s_itc.h	57;"	enumerator	enum:__anon69
ITC_IRQ_TIM1_CAPCOM	stm8s_stdperiph_driver\inc\stm8s_itc.h	60;"	enumerator	enum:__anon69
ITC_IRQ_TIM1_OVF	stm8s_stdperiph_driver\inc\stm8s_itc.h	58;"	enumerator	enum:__anon69
ITC_IRQ_TIM3_CAPCOM	stm8s_stdperiph_driver\inc\stm8s_itc.h	72;"	enumerator	enum:__anon69
ITC_IRQ_TIM3_OVF	stm8s_stdperiph_driver\inc\stm8s_itc.h	71;"	enumerator	enum:__anon69
ITC_IRQ_TIM5_CAPCOM	stm8s_stdperiph_driver\inc\stm8s_itc.h	65;"	enumerator	enum:__anon69
ITC_IRQ_TIM5_OVFTRI	stm8s_stdperiph_driver\inc\stm8s_itc.h	63;"	enumerator	enum:__anon69
ITC_IRQ_TIM6_OVFTRI	stm8s_stdperiph_driver\inc\stm8s_itc.h	93;"	enumerator	enum:__anon69
ITC_IRQ_TLI	stm8s_stdperiph_driver\inc\stm8s_itc.h	39;"	enumerator	enum:__anon69
ITC_IRQ_UART1_RX	stm8s_stdperiph_driver\inc\stm8s_itc.h	74;"	enumerator	enum:__anon69
ITC_IRQ_UART1_TX	stm8s_stdperiph_driver\inc\stm8s_itc.h	73;"	enumerator	enum:__anon69
ITC_IRQ_UART2_RX	stm8s_stdperiph_driver\inc\stm8s_itc.h	79;"	enumerator	enum:__anon69
ITC_IRQ_UART2_TX	stm8s_stdperiph_driver\inc\stm8s_itc.h	78;"	enumerator	enum:__anon69
ITC_IRQ_UART3_RX	stm8s_stdperiph_driver\inc\stm8s_itc.h	84;"	enumerator	enum:__anon69
ITC_IRQ_UART3_TX	stm8s_stdperiph_driver\inc\stm8s_itc.h	83;"	enumerator	enum:__anon69
ITC_Irq_TypeDef	stm8s_stdperiph_driver\inc\stm8s_itc.h	100;"	typedef	typeref:enum:__anon69
ITC_PRIORITYLEVEL_0	stm8s_stdperiph_driver\inc\stm8s_itc.h	106;"	enumerator	enum:__anon70
ITC_PRIORITYLEVEL_1	stm8s_stdperiph_driver\inc\stm8s_itc.h	107;"	enumerator	enum:__anon70
ITC_PRIORITYLEVEL_2	stm8s_stdperiph_driver\inc\stm8s_itc.h	108;"	enumerator	enum:__anon70
ITC_PRIORITYLEVEL_3	stm8s_stdperiph_driver\inc\stm8s_itc.h	109;"	enumerator	enum:__anon70
ITC_PriorityLevel_TypeDef	stm8s_stdperiph_driver\inc\stm8s_itc.h	110;"	typedef	typeref:enum:__anon70
ITC_SPRX_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1436;"	macro
ITC_SetSoftwarePriority	stm8s_stdperiph_driver\inc\stm8s_itc.h	162;"	prototype	signature:(ITC_Irq_TypeDef IrqNum, ITC_PriorityLevel_TypeDef PriorityValue)
ITC_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1430;"	typedef	typeref:struct:ITC_struct
ITC_struct	stm8s_stdperiph_driver\inc\stm8s.h	1419;"	struct
ITR	stm8s_stdperiph_driver\inc\stm8s.h	1324;"	member	struct:I2C_struct
ITStatus	stm8s_stdperiph_driver\inc\stm8s.h	221;"	typedef	typeref:enum:__anon2
IWDG	stm8s_stdperiph_driver\inc\stm8s.h	2542;"	macro
IWDG_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2461;"	macro
IWDG_Enable	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	112;"	prototype	signature:(void)
IWDG_KEY_ENABLE	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	45;"	macro
IWDG_KEY_REFRESH	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	40;"	macro
IWDG_PR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1605;"	macro
IWDG_Prescaler_128	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	96;"	enumerator	enum:__anon72
IWDG_Prescaler_16	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	93;"	enumerator	enum:__anon72
IWDG_Prescaler_256	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	97;"	enumerator	enum:__anon72
IWDG_Prescaler_32	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	94;"	enumerator	enum:__anon72
IWDG_Prescaler_4	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	91;"	enumerator	enum:__anon72
IWDG_Prescaler_64	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	95;"	enumerator	enum:__anon72
IWDG_Prescaler_8	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	92;"	enumerator	enum:__anon72
IWDG_Prescaler_TypeDef	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	98;"	typedef	typeref:enum:__anon72
IWDG_RLR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1606;"	macro
IWDG_ReloadCounter	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	111;"	prototype	signature:(void)
IWDG_SetPrescaler	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	109;"	prototype	signature:(IWDG_Prescaler_TypeDef IWDG_Prescaler)
IWDG_SetReload	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	110;"	prototype	signature:(uint8_t IWDG_Reload)
IWDG_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1599;"	typedef	typeref:struct:IWDG_struct
IWDG_WriteAccessCmd	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	108;"	prototype	signature:(IWDG_WriteAccess_TypeDef IWDG_WriteAccess)
IWDG_WriteAccess_Disable	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	85;"	enumerator	enum:__anon71
IWDG_WriteAccess_Enable	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	84;"	enumerator	enum:__anon71
IWDG_WriteAccess_TypeDef	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	86;"	typedef	typeref:enum:__anon71
IWDG_struct	stm8s_stdperiph_driver\inc\stm8s.h	1593;"	struct
KR	stm8s_stdperiph_driver\inc\stm8s.h	1595;"	member	struct:IWDG_struct
LED_Blink	user\led.c	3;"	function	signature:(uint8_t times, uint16_t delay)
LED_Blink	user\main.h	133;"	prototype	signature:(uint8_t times, uint16_t delay)
LED_Indication	user\led.c	13;"	function	signature:(uint8_t type)
LED_Indication	user\main.h	134;"	prototype	signature:(uint8_t type)
LSI_FREQUENCY_MAX	stm8s_stdperiph_driver\inc\stm8s_awu.h	71;"	macro
LSI_FREQUENCY_MAX	stm8s_stdperiph_driver\inc\stm8s_beep.h	58;"	macro
LSI_FREQUENCY_MIN	stm8s_stdperiph_driver\inc\stm8s_awu.h	70;"	macro
LSI_FREQUENCY_MIN	stm8s_stdperiph_driver\inc\stm8s_beep.h	57;"	macro
LSI_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	109;"	macro
LTRH	stm8s_stdperiph_driver\inc\stm8s.h	315;"	member	struct:ADC1_struct
LTRL	stm8s_stdperiph_driver\inc\stm8s.h	316;"	member	struct:ADC1_struct
LUSB_CUR_LIMIT_H	user\main.h	78;"	macro
LUSB_CUR_LIMIT_L	user\main.h	77;"	macro
LUSB_Close	user\main.h	91;"	macro
LUSB_Current	user\main.c	3;"	variable
LUSB_ENABLE	user\main.h	72;"	macro
LUSB_GOING	user\main.h	73;"	macro
LUSB_INSERT	user\main.h	71;"	macro
LUSB_Open	user\main.h	90;"	macro
LUSB_Status	user\main.c	4;"	variable
LUSB_VOL_LEVEL_H	user\main.h	82;"	macro
LUSB_VOL_LEVEL_L	user\main.h	80;"	macro
LUSB_VOL_LEVEL_M	user\main.h	81;"	macro
LUSB_VOL_LIMIT_H	user\main.h	76;"	macro
LUSB_VOL_LIMIT_L	user\main.h	75;"	macro
LUSB_Voltage	user\main.c	3;"	variable
MCR	stm8s_stdperiph_driver\inc\stm8s.h	2052;"	member	struct:__anon5
MCSR	stm8s_stdperiph_driver\inc\stm8s.h	2065;"	member	struct:__anon5::__anon6::__anon7
MDAR1	stm8s_stdperiph_driver\inc\stm8s.h	2071;"	member	struct:__anon5::__anon6::__anon7
MDAR1	stm8s_stdperiph_driver\inc\stm8s.h	2199;"	member	struct:__anon5::__anon6::__anon13
MDAR2	stm8s_stdperiph_driver\inc\stm8s.h	2072;"	member	struct:__anon5::__anon6::__anon7
MDAR2	stm8s_stdperiph_driver\inc\stm8s.h	2200;"	member	struct:__anon5::__anon6::__anon13
MDAR3	stm8s_stdperiph_driver\inc\stm8s.h	2073;"	member	struct:__anon5::__anon6::__anon7
MDAR3	stm8s_stdperiph_driver\inc\stm8s.h	2201;"	member	struct:__anon5::__anon6::__anon13
MDAR4	stm8s_stdperiph_driver\inc\stm8s.h	2074;"	member	struct:__anon5::__anon6::__anon7
MDAR4	stm8s_stdperiph_driver\inc\stm8s.h	2202;"	member	struct:__anon5::__anon6::__anon13
MDAR5	stm8s_stdperiph_driver\inc\stm8s.h	2075;"	member	struct:__anon5::__anon6::__anon7
MDAR5	stm8s_stdperiph_driver\inc\stm8s.h	2203;"	member	struct:__anon5::__anon6::__anon13
MDAR6	stm8s_stdperiph_driver\inc\stm8s.h	2076;"	member	struct:__anon5::__anon6::__anon7
MDAR6	stm8s_stdperiph_driver\inc\stm8s.h	2204;"	member	struct:__anon5::__anon6::__anon13
MDAR7	stm8s_stdperiph_driver\inc\stm8s.h	2077;"	member	struct:__anon5::__anon6::__anon7
MDAR7	stm8s_stdperiph_driver\inc\stm8s.h	2205;"	member	struct:__anon5::__anon6::__anon13
MDAR8	stm8s_stdperiph_driver\inc\stm8s.h	2078;"	member	struct:__anon5::__anon6::__anon7
MDAR8	stm8s_stdperiph_driver\inc\stm8s.h	2206;"	member	struct:__anon5::__anon6::__anon13
MDLCR	stm8s_stdperiph_driver\inc\stm8s.h	2066;"	member	struct:__anon5::__anon6::__anon7
MDLCR	stm8s_stdperiph_driver\inc\stm8s.h	2194;"	member	struct:__anon5::__anon6::__anon13
MEMCPY	stm8s_stdperiph_driver\inc\stm8s.h	126;"	macro
MEMCPY	stm8s_stdperiph_driver\inc\stm8s.h	129;"	macro
MFMI	stm8s_stdperiph_driver\inc\stm8s.h	2193;"	member	struct:__anon5::__anon6::__anon13
MIDR1	stm8s_stdperiph_driver\inc\stm8s.h	2067;"	member	struct:__anon5::__anon6::__anon7
MIDR1	stm8s_stdperiph_driver\inc\stm8s.h	2195;"	member	struct:__anon5::__anon6::__anon13
MIDR2	stm8s_stdperiph_driver\inc\stm8s.h	2068;"	member	struct:__anon5::__anon6::__anon7
MIDR2	stm8s_stdperiph_driver\inc\stm8s.h	2196;"	member	struct:__anon5::__anon6::__anon13
MIDR3	stm8s_stdperiph_driver\inc\stm8s.h	2069;"	member	struct:__anon5::__anon6::__anon7
MIDR3	stm8s_stdperiph_driver\inc\stm8s.h	2197;"	member	struct:__anon5::__anon6::__anon13
MIDR4	stm8s_stdperiph_driver\inc\stm8s.h	2070;"	member	struct:__anon5::__anon6::__anon7
MIDR4	stm8s_stdperiph_driver\inc\stm8s.h	2198;"	member	struct:__anon5::__anon6::__anon13
MSR	stm8s_stdperiph_driver\inc\stm8s.h	2053;"	member	struct:__anon5
MTSRH	stm8s_stdperiph_driver\inc\stm8s.h	2080;"	member	struct:__anon5::__anon6::__anon7
MTSRH	stm8s_stdperiph_driver\inc\stm8s.h	2208;"	member	struct:__anon5::__anon6::__anon13
MTSRL	stm8s_stdperiph_driver\inc\stm8s.h	2079;"	member	struct:__anon5::__anon6::__anon7
MTSRL	stm8s_stdperiph_driver\inc\stm8s.h	2207;"	member	struct:__anon5::__anon6::__anon13
MainLoop	user\main.c	24;"	function	signature:(void)
MainLoop	user\main.c	9;"	prototype	file:	signature:(void)
MskBit	stm8s_stdperiph_driver\inc\stm8s.h	2681;"	macro
NCR2	stm8s_stdperiph_driver\inc\stm8s.h	1502;"	member	struct:FLASH_struct
NEAR	stm8s_stdperiph_driver\inc\stm8s.h	113;"	macro
NEAR	stm8s_stdperiph_driver\inc\stm8s.h	119;"	macro
NEAR	stm8s_stdperiph_driver\inc\stm8s.h	133;"	macro
NFPR	stm8s_stdperiph_driver\inc\stm8s.h	1504;"	member	struct:FLASH_struct
NOPT1	stm8s_stdperiph_driver\inc\stm8s.h	1572;"	member	struct:OPT_struct
NOPT2	stm8s_stdperiph_driver\inc\stm8s.h	1574;"	member	struct:OPT_struct
NOPT3	stm8s_stdperiph_driver\inc\stm8s.h	1576;"	member	struct:OPT_struct
NOPT4	stm8s_stdperiph_driver\inc\stm8s.h	1578;"	member	struct:OPT_struct
NOPT5	stm8s_stdperiph_driver\inc\stm8s.h	1580;"	member	struct:OPT_struct
NOPT7	stm8s_stdperiph_driver\inc\stm8s.h	1584;"	member	struct:OPT_struct
NO_TMNAT_DELAY	user\main.h	110;"	macro
NonHandledInterrupt	stm8_interrupt_vector.c	14;"	function	signature:(void)
OARH	stm8s_stdperiph_driver\inc\stm8s.h	1318;"	member	struct:I2C_struct
OARL	stm8s_stdperiph_driver\inc\stm8s.h	1317;"	member	struct:I2C_struct
ODR	stm8s_stdperiph_driver\inc\stm8s.h	255;"	member	struct:GPIO_struct
OISR	stm8s_stdperiph_driver\inc\stm8s.h	629;"	member	struct:TIM1_struct
OPT	stm8s_stdperiph_driver\inc\stm8s.h	2514;"	macro
OPT0	stm8s_stdperiph_driver\inc\stm8s.h	1570;"	member	struct:OPT_struct
OPT1	stm8s_stdperiph_driver\inc\stm8s.h	1571;"	member	struct:OPT_struct
OPT2	stm8s_stdperiph_driver\inc\stm8s.h	1573;"	member	struct:OPT_struct
OPT3	stm8s_stdperiph_driver\inc\stm8s.h	1575;"	member	struct:OPT_struct
OPT4	stm8s_stdperiph_driver\inc\stm8s.h	1577;"	member	struct:OPT_struct
OPT5	stm8s_stdperiph_driver\inc\stm8s.h	1579;"	member	struct:OPT_struct
OPT7	stm8s_stdperiph_driver\inc\stm8s.h	1583;"	member	struct:OPT_struct
OPTION_BYTE_END_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	68;"	macro
OPTION_BYTE_START_PHYSICAL_ADDRESS	stm8s_stdperiph_driver\inc\stm8s_flash.h	67;"	macro
OPT_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2446;"	macro
OPT_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1586;"	typedef	typeref:struct:OPT_struct
OPT_struct	stm8s_stdperiph_driver\inc\stm8s.h	1568;"	struct
PCKENR1	stm8s_stdperiph_driver\inc\stm8s.h	501;"	member	struct:CLK_struct
PCKENR2	stm8s_stdperiph_driver\inc\stm8s.h	504;"	member	struct:CLK_struct
PIN_BUTON	user\main.h	26;"	macro
PIN_CHG_FULL	user\main.h	18;"	macro
PIN_CHG_WAKE	user\main.h	19;"	macro
PIN_I2C_SCL	user\main.h	28;"	macro
PIN_I2C_SDA	user\main.h	29;"	macro
PIN_LED_1	user\main.h	31;"	macro
PIN_LED_2	user\main.h	32;"	macro
PIN_LED_3	user\main.h	33;"	macro
PIN_LED_4	user\main.h	34;"	macro
PIN_LED_5	user\main.h	35;"	macro
PIN_USB_DPDN	user\main.h	24;"	macro
PIN_USB_EN	user\main.h	25;"	macro
PIN_USB_I	user\main.h	21;"	macro
PIN_USB_U	user\main.h	22;"	macro
PIN_USB_WAKE	user\main.h	20;"	macro
PR	stm8s_stdperiph_driver\inc\stm8s.h	1596;"	member	struct:IWDG_struct
PSCR	stm8s_stdperiph_driver\inc\stm8s.h	1053;"	member	struct:TIM4_struct
PSCR	stm8s_stdperiph_driver\inc\stm8s.h	1121;"	member	struct:TIM5_struct
PSCR	stm8s_stdperiph_driver\inc\stm8s.h	1253;"	member	struct:TIM6_struct
PSCR	stm8s_stdperiph_driver\inc\stm8s.h	1763;"	member	struct:UART1_struct
PSCR	stm8s_stdperiph_driver\inc\stm8s.h	1862;"	member	struct:UART2_struct
PSCR	stm8s_stdperiph_driver\inc\stm8s.h	826;"	member	struct:TIM2_struct
PSCR	stm8s_stdperiph_driver\inc\stm8s.h	948;"	member	struct:TIM3_struct
PSCRH	stm8s_stdperiph_driver\inc\stm8s.h	614;"	member	struct:TIM1_struct
PSCRL	stm8s_stdperiph_driver\inc\stm8s.h	615;"	member	struct:TIM1_struct
PSR	stm8s_stdperiph_driver\inc\stm8s.h	2059;"	member	struct:__anon5
PUKR	stm8s_stdperiph_driver\inc\stm8s.h	1508;"	member	struct:FLASH_struct
Page	stm8s_stdperiph_driver\inc\stm8s.h	2211;"	member	struct:__anon5	typeref:union:__anon5::__anon6
PointerAttr	stm8s_stdperiph_driver\inc\stm8s.h	146;"	macro
PointerAttr	stm8s_stdperiph_driver\inc\stm8s.h	149;"	macro
RCR	stm8s_stdperiph_driver\inc\stm8s.h	618;"	member	struct:TIM1_struct
RECR	stm8s_stdperiph_driver\inc\stm8s.h	2178;"	member	struct:__anon5::__anon6::__anon12
RESERVED	stm8s_stdperiph_driver\inc\stm8s.h	1967;"	member	struct:UART3_struct
RESERVED	stm8s_stdperiph_driver\inc\stm8s.h	304;"	member	struct:ADC1_struct
RESERVED	stm8s_stdperiph_driver\inc\stm8s.h	379;"	member	struct:ADC2_struct
RESERVED	stm8s_stdperiph_driver\inc\stm8s.h	496;"	member	struct:CLK_struct
RESERVED1	stm8s_stdperiph_driver\inc\stm8s.h	1046;"	member	struct:TIM4_struct
RESERVED1	stm8s_stdperiph_driver\inc\stm8s.h	1319;"	member	struct:I2C_struct
RESERVED1	stm8s_stdperiph_driver\inc\stm8s.h	1506;"	member	struct:FLASH_struct
RESERVED1	stm8s_stdperiph_driver\inc\stm8s.h	1581;"	member	struct:OPT_struct
RESERVED1	stm8s_stdperiph_driver\inc\stm8s.h	505;"	member	struct:CLK_struct
RESERVED1	stm8s_stdperiph_driver\inc\stm8s.h	812;"	member	struct:TIM2_struct
RESERVED2	stm8s_stdperiph_driver\inc\stm8s.h	1047;"	member	struct:TIM4_struct
RESERVED2	stm8s_stdperiph_driver\inc\stm8s.h	1328;"	member	struct:I2C_struct
RESERVED2	stm8s_stdperiph_driver\inc\stm8s.h	1507;"	member	struct:FLASH_struct
RESERVED2	stm8s_stdperiph_driver\inc\stm8s.h	1582;"	member	struct:OPT_struct
RESERVED2	stm8s_stdperiph_driver\inc\stm8s.h	813;"	member	struct:TIM2_struct
RESERVED3	stm8s_stdperiph_driver\inc\stm8s.h	1509;"	member	struct:FLASH_struct
RESET	stm8s_stdperiph_driver\inc\stm8s.h	221;"	enumerator	enum:__anon2
RFR	stm8s_stdperiph_driver\inc\stm8s.h	2056;"	member	struct:__anon5
RLR	stm8s_stdperiph_driver\inc\stm8s.h	1597;"	member	struct:IWDG_struct
RST	stm8s_stdperiph_driver\inc\stm8s.h	2539;"	macro
RST_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2458;"	macro
RST_ClearFlag	stm8s_stdperiph_driver\inc\stm8s_rst.h	74;"	prototype	signature:(RST_Flag_TypeDef RST_Flag)
RST_FLAG_EMCF	stm8s_stdperiph_driver\inc\stm8s_rst.h	36;"	enumerator	enum:__anon73
RST_FLAG_ILLOPF	stm8s_stdperiph_driver\inc\stm8s_rst.h	38;"	enumerator	enum:__anon73
RST_FLAG_IWDGF	stm8s_stdperiph_driver\inc\stm8s_rst.h	39;"	enumerator	enum:__anon73
RST_FLAG_SWIMF	stm8s_stdperiph_driver\inc\stm8s_rst.h	37;"	enumerator	enum:__anon73
RST_FLAG_WWDGF	stm8s_stdperiph_driver\inc\stm8s_rst.h	40;"	enumerator	enum:__anon73
RST_Flag_TypeDef	stm8s_stdperiph_driver\inc\stm8s_rst.h	41;"	typedef	typeref:enum:__anon73
RST_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_rst.h	73;"	prototype	signature:(RST_Flag_TypeDef RST_Flag)
RST_SR_EMCF	stm8s_stdperiph_driver\inc\stm8s.h	1665;"	macro
RST_SR_ILLOPF	stm8s_stdperiph_driver\inc\stm8s.h	1667;"	macro
RST_SR_IWDGF	stm8s_stdperiph_driver\inc\stm8s.h	1668;"	macro
RST_SR_SWIMF	stm8s_stdperiph_driver\inc\stm8s.h	1666;"	macro
RST_SR_WWDGF	stm8s_stdperiph_driver\inc\stm8s.h	1669;"	macro
RST_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1659;"	typedef	typeref:struct:RST_struct
RST_struct	stm8s_stdperiph_driver\inc\stm8s.h	1655;"	struct
RXCRCR	stm8s_stdperiph_driver\inc\stm8s.h	1688;"	member	struct:SPI_struct
Reserved1	stm8s_stdperiph_driver\inc\stm8s.h	2181;"	member	struct:__anon5::__anon6::__anon12
Reserved2	stm8s_stdperiph_driver\inc\stm8s.h	2187;"	member	struct:__anon5::__anon6::__anon12
RxFIFO	stm8s_stdperiph_driver\inc\stm8s.h	2210;"	member	union:__anon5::__anon6	typeref:struct:__anon5::__anon6::__anon13
S16_MAX	stm8s_stdperiph_driver\inc\stm8s.h	232;"	macro
S16_MIN	stm8s_stdperiph_driver\inc\stm8s.h	233;"	macro
S32_MAX	stm8s_stdperiph_driver\inc\stm8s.h	235;"	macro
S32_MIN	stm8s_stdperiph_driver\inc\stm8s.h	236;"	macro
S8_MAX	stm8s_stdperiph_driver\inc\stm8s.h	229;"	macro
S8_MIN	stm8s_stdperiph_driver\inc\stm8s.h	230;"	macro
SET	stm8s_stdperiph_driver\inc\stm8s.h	221;"	enumerator	enum:__anon2
SMCR	stm8s_stdperiph_driver\inc\stm8s.h	1109;"	member	struct:TIM5_struct
SMCR	stm8s_stdperiph_driver\inc\stm8s.h	1248;"	member	struct:TIM6_struct
SMCR	stm8s_stdperiph_driver\inc\stm8s.h	600;"	member	struct:TIM1_struct
SPI	stm8s_stdperiph_driver\inc\stm8s.h	2544;"	macro
SPI_BAUDRATEPRESCALER_128	stm8s_stdperiph_driver\inc\stm8s_spi.h	88;"	enumerator	enum:__anon78
SPI_BAUDRATEPRESCALER_16	stm8s_stdperiph_driver\inc\stm8s_spi.h	85;"	enumerator	enum:__anon78
SPI_BAUDRATEPRESCALER_2	stm8s_stdperiph_driver\inc\stm8s_spi.h	82;"	enumerator	enum:__anon78
SPI_BAUDRATEPRESCALER_256	stm8s_stdperiph_driver\inc\stm8s_spi.h	89;"	enumerator	enum:__anon78
SPI_BAUDRATEPRESCALER_32	stm8s_stdperiph_driver\inc\stm8s_spi.h	86;"	enumerator	enum:__anon78
SPI_BAUDRATEPRESCALER_4	stm8s_stdperiph_driver\inc\stm8s_spi.h	83;"	enumerator	enum:__anon78
SPI_BAUDRATEPRESCALER_64	stm8s_stdperiph_driver\inc\stm8s_spi.h	87;"	enumerator	enum:__anon78
SPI_BAUDRATEPRESCALER_8	stm8s_stdperiph_driver\inc\stm8s_spi.h	84;"	enumerator	enum:__anon78
SPI_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2464;"	macro
SPI_BaudRatePrescaler_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	90;"	typedef	typeref:enum:__anon78
SPI_BiDirectionalLineConfig	stm8s_stdperiph_driver\inc\stm8s_spi.h	313;"	prototype	signature:(SPI_Direction_TypeDef SPI_Direction)
SPI_CLOCKPHASE_1EDGE	stm8s_stdperiph_driver\inc\stm8s_spi.h	106;"	enumerator	enum:__anon80
SPI_CLOCKPHASE_2EDGE	stm8s_stdperiph_driver\inc\stm8s_spi.h	107;"	enumerator	enum:__anon80
SPI_CLOCKPOLARITY_HIGH	stm8s_stdperiph_driver\inc\stm8s_spi.h	98;"	enumerator	enum:__anon79
SPI_CLOCKPOLARITY_LOW	stm8s_stdperiph_driver\inc\stm8s_spi.h	97;"	enumerator	enum:__anon79
SPI_CR1_BR	stm8s_stdperiph_driver\inc\stm8s.h	1716;"	macro
SPI_CR1_CPHA	stm8s_stdperiph_driver\inc\stm8s.h	1719;"	macro
SPI_CR1_CPOL	stm8s_stdperiph_driver\inc\stm8s.h	1718;"	macro
SPI_CR1_LSBFIRST	stm8s_stdperiph_driver\inc\stm8s.h	1714;"	macro
SPI_CR1_MSTR	stm8s_stdperiph_driver\inc\stm8s.h	1717;"	macro
SPI_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1697;"	macro
SPI_CR1_SPE	stm8s_stdperiph_driver\inc\stm8s.h	1715;"	macro
SPI_CR2_BDM	stm8s_stdperiph_driver\inc\stm8s.h	1721;"	macro
SPI_CR2_BDOE	stm8s_stdperiph_driver\inc\stm8s.h	1722;"	macro
SPI_CR2_CRCEN	stm8s_stdperiph_driver\inc\stm8s.h	1723;"	macro
SPI_CR2_CRCNEXT	stm8s_stdperiph_driver\inc\stm8s.h	1724;"	macro
SPI_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1698;"	macro
SPI_CR2_RXONLY	stm8s_stdperiph_driver\inc\stm8s.h	1725;"	macro
SPI_CR2_SSI	stm8s_stdperiph_driver\inc\stm8s.h	1727;"	macro
SPI_CR2_SSM	stm8s_stdperiph_driver\inc\stm8s.h	1726;"	macro
SPI_CRCPR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1702;"	macro
SPI_CRC_RX	stm8s_stdperiph_driver\inc\stm8s_spi.h	123;"	enumerator	enum:__anon82
SPI_CRC_TX	stm8s_stdperiph_driver\inc\stm8s_spi.h	124;"	enumerator	enum:__anon82
SPI_CRC_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	125;"	typedef	typeref:enum:__anon82
SPI_CalculateCRCCmd	stm8s_stdperiph_driver\inc\stm8s_spi.h	309;"	prototype	signature:(FunctionalState NewState)
SPI_ClearFlag	stm8s_stdperiph_driver\inc\stm8s_spi.h	315;"	prototype	signature:(SPI_Flag_TypeDef SPI_FLAG)
SPI_ClearITPendingBit	stm8s_stdperiph_driver\inc\stm8s_spi.h	317;"	prototype	signature:(SPI_IT_TypeDef SPI_IT)
SPI_ClockPhase_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	108;"	typedef	typeref:enum:__anon80
SPI_ClockPolarity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	99;"	typedef	typeref:enum:__anon79
SPI_Cmd	stm8s_stdperiph_driver\inc\stm8s_spi.h	303;"	prototype	signature:(FunctionalState NewState)
SPI_DATADIRECTION_1LINE_RX	stm8s_stdperiph_driver\inc\stm8s_spi.h	44;"	enumerator	enum:__anon74
SPI_DATADIRECTION_1LINE_TX	stm8s_stdperiph_driver\inc\stm8s_spi.h	45;"	enumerator	enum:__anon74
SPI_DATADIRECTION_2LINES_FULLDUPLEX	stm8s_stdperiph_driver\inc\stm8s_spi.h	42;"	enumerator	enum:__anon74
SPI_DATADIRECTION_2LINES_RXONLY	stm8s_stdperiph_driver\inc\stm8s_spi.h	43;"	enumerator	enum:__anon74
SPI_DIRECTION_RX	stm8s_stdperiph_driver\inc\stm8s_spi.h	64;"	enumerator	enum:__anon76
SPI_DIRECTION_TX	stm8s_stdperiph_driver\inc\stm8s_spi.h	65;"	enumerator	enum:__anon76
SPI_DR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1701;"	macro
SPI_DataDirection_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	46;"	typedef	typeref:enum:__anon74
SPI_DeInit	stm8s_stdperiph_driver\inc\stm8s_spi.h	296;"	prototype	signature:(void)
SPI_Direction_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	66;"	typedef	typeref:enum:__anon76
SPI_FIRSTBIT_LSB	stm8s_stdperiph_driver\inc\stm8s_spi.h	116;"	enumerator	enum:__anon81
SPI_FIRSTBIT_MSB	stm8s_stdperiph_driver\inc\stm8s_spi.h	115;"	enumerator	enum:__anon81
SPI_FLAG_BSY	stm8s_stdperiph_driver\inc\stm8s_spi.h	131;"	enumerator	enum:__anon83
SPI_FLAG_CRCERR	stm8s_stdperiph_driver\inc\stm8s_spi.h	134;"	enumerator	enum:__anon83
SPI_FLAG_MODF	stm8s_stdperiph_driver\inc\stm8s_spi.h	133;"	enumerator	enum:__anon83
SPI_FLAG_OVR	stm8s_stdperiph_driver\inc\stm8s_spi.h	132;"	enumerator	enum:__anon83
SPI_FLAG_RXNE	stm8s_stdperiph_driver\inc\stm8s_spi.h	137;"	enumerator	enum:__anon83
SPI_FLAG_TXE	stm8s_stdperiph_driver\inc\stm8s_spi.h	136;"	enumerator	enum:__anon83
SPI_FLAG_WKUP	stm8s_stdperiph_driver\inc\stm8s_spi.h	135;"	enumerator	enum:__anon83
SPI_FirstBit_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	117;"	typedef	typeref:enum:__anon81
SPI_Flag_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	138;"	typedef	typeref:enum:__anon83
SPI_GetCRC	stm8s_stdperiph_driver\inc\stm8s_spi.h	310;"	prototype	signature:(SPI_CRC_TypeDef SPI_CRC)
SPI_GetCRCPolynomial	stm8s_stdperiph_driver\inc\stm8s_spi.h	312;"	prototype	signature:(void)
SPI_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_spi.h	314;"	prototype	signature:(SPI_Flag_TypeDef SPI_FLAG)
SPI_GetITStatus	stm8s_stdperiph_driver\inc\stm8s_spi.h	316;"	prototype	signature:(SPI_IT_TypeDef SPI_IT)
SPI_ICR_ERRIE	stm8s_stdperiph_driver\inc\stm8s.h	1731;"	macro
SPI_ICR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1699;"	macro
SPI_ICR_RXEI	stm8s_stdperiph_driver\inc\stm8s.h	1730;"	macro
SPI_ICR_TXEI	stm8s_stdperiph_driver\inc\stm8s.h	1729;"	macro
SPI_ICR_WKIE	stm8s_stdperiph_driver\inc\stm8s.h	1732;"	macro
SPI_ITConfig	stm8s_stdperiph_driver\inc\stm8s_spi.h	304;"	prototype	signature:(SPI_IT_TypeDef SPI_IT, FunctionalState NewState)
SPI_IT_CRCERR	stm8s_stdperiph_driver\inc\stm8s_spi.h	151;"	enumerator	enum:__anon84
SPI_IT_ERR	stm8s_stdperiph_driver\inc\stm8s_spi.h	154;"	enumerator	enum:__anon84
SPI_IT_MODF	stm8s_stdperiph_driver\inc\stm8s_spi.h	150;"	enumerator	enum:__anon84
SPI_IT_OVR	stm8s_stdperiph_driver\inc\stm8s_spi.h	149;"	enumerator	enum:__anon84
SPI_IT_RXNE	stm8s_stdperiph_driver\inc\stm8s_spi.h	153;"	enumerator	enum:__anon84
SPI_IT_TXE	stm8s_stdperiph_driver\inc\stm8s_spi.h	152;"	enumerator	enum:__anon84
SPI_IT_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	155;"	typedef	typeref:enum:__anon84
SPI_IT_WKUP	stm8s_stdperiph_driver\inc\stm8s_spi.h	148;"	enumerator	enum:__anon84
SPI_Init	stm8s_stdperiph_driver\inc\stm8s_spi.h	297;"	prototype	signature:(SPI_FirstBit_TypeDef FirstBit, SPI_BaudRatePrescaler_TypeDef BaudRatePrescaler, SPI_Mode_TypeDef Mode, SPI_ClockPolarity_TypeDef ClockPolarity, SPI_ClockPhase_TypeDef ClockPhase, SPI_DataDirection_TypeDef Data_Direction, SPI_NSS_TypeDef Slave_Management, uint8_t CRCPolynomial)
SPI_MODE_MASTER	stm8s_stdperiph_driver\inc\stm8s_spi.h	73;"	enumerator	enum:__anon77
SPI_MODE_SLAVE	stm8s_stdperiph_driver\inc\stm8s_spi.h	74;"	enumerator	enum:__anon77
SPI_Mode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	75;"	typedef	typeref:enum:__anon77
SPI_NSSInternalSoftwareCmd	stm8s_stdperiph_driver\inc\stm8s_spi.h	307;"	prototype	signature:(FunctionalState NewState)
SPI_NSS_HARD	stm8s_stdperiph_driver\inc\stm8s_spi.h	55;"	enumerator	enum:__anon75
SPI_NSS_SOFT	stm8s_stdperiph_driver\inc\stm8s_spi.h	54;"	enumerator	enum:__anon75
SPI_NSS_TypeDef	stm8s_stdperiph_driver\inc\stm8s_spi.h	56;"	typedef	typeref:enum:__anon75
SPI_RXCRCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1703;"	macro
SPI_ReceiveData	stm8s_stdperiph_driver\inc\stm8s_spi.h	306;"	prototype	signature:(void)
SPI_ResetCRC	stm8s_stdperiph_driver\inc\stm8s_spi.h	311;"	prototype	signature:(void)
SPI_SR_BSY	stm8s_stdperiph_driver\inc\stm8s.h	1734;"	macro
SPI_SR_CRCERR	stm8s_stdperiph_driver\inc\stm8s.h	1737;"	macro
SPI_SR_MODF	stm8s_stdperiph_driver\inc\stm8s.h	1736;"	macro
SPI_SR_OVR	stm8s_stdperiph_driver\inc\stm8s.h	1735;"	macro
SPI_SR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1700;"	macro
SPI_SR_RXNE	stm8s_stdperiph_driver\inc\stm8s.h	1740;"	macro
SPI_SR_TXE	stm8s_stdperiph_driver\inc\stm8s.h	1739;"	macro
SPI_SR_WKUP	stm8s_stdperiph_driver\inc\stm8s.h	1738;"	macro
SPI_SendData	stm8s_stdperiph_driver\inc\stm8s_spi.h	305;"	prototype	signature:(uint8_t Data)
SPI_TXCRCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1704;"	macro
SPI_TransmitCRC	stm8s_stdperiph_driver\inc\stm8s_spi.h	308;"	prototype	signature:(void)
SPI_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1691;"	typedef	typeref:struct:SPI_struct
SPI_struct	stm8s_stdperiph_driver\inc\stm8s.h	1680;"	struct
SR	stm8s_stdperiph_driver\inc\stm8s.h	1657;"	member	struct:RST_struct
SR	stm8s_stdperiph_driver\inc\stm8s.h	1685;"	member	struct:SPI_struct
SR	stm8s_stdperiph_driver\inc\stm8s.h	1753;"	member	struct:UART1_struct
SR	stm8s_stdperiph_driver\inc\stm8s.h	1851;"	member	struct:UART2_struct
SR	stm8s_stdperiph_driver\inc\stm8s.h	1959;"	member	struct:UART3_struct
SR1	stm8s_stdperiph_driver\inc\stm8s.h	1050;"	member	struct:TIM4_struct
SR1	stm8s_stdperiph_driver\inc\stm8s.h	1111;"	member	struct:TIM5_struct
SR1	stm8s_stdperiph_driver\inc\stm8s.h	1250;"	member	struct:TIM6_struct
SR1	stm8s_stdperiph_driver\inc\stm8s.h	1321;"	member	struct:I2C_struct
SR1	stm8s_stdperiph_driver\inc\stm8s.h	603;"	member	struct:TIM1_struct
SR1	stm8s_stdperiph_driver\inc\stm8s.h	816;"	member	struct:TIM2_struct
SR1	stm8s_stdperiph_driver\inc\stm8s.h	940;"	member	struct:TIM3_struct
SR2	stm8s_stdperiph_driver\inc\stm8s.h	1112;"	member	struct:TIM5_struct
SR2	stm8s_stdperiph_driver\inc\stm8s.h	1322;"	member	struct:I2C_struct
SR2	stm8s_stdperiph_driver\inc\stm8s.h	604;"	member	struct:TIM1_struct
SR2	stm8s_stdperiph_driver\inc\stm8s.h	817;"	member	struct:TIM2_struct
SR2	stm8s_stdperiph_driver\inc\stm8s.h	941;"	member	struct:TIM3_struct
SR3	stm8s_stdperiph_driver\inc\stm8s.h	1323;"	member	struct:I2C_struct
STRINGVECTOR	stm8s_stdperiph_driver\inc\stm8s.h	2643;"	macro
SUCCESS	stm8s_stdperiph_driver\inc\stm8s.h	226;"	enumerator	enum:__anon4
SWCR	stm8s_stdperiph_driver\inc\stm8s.h	499;"	member	struct:CLK_struct
SWIMCCR	stm8s_stdperiph_driver\inc\stm8s.h	507;"	member	struct:CLK_struct
SWR	stm8s_stdperiph_driver\inc\stm8s.h	498;"	member	struct:CLK_struct
SetBit	stm8s_stdperiph_driver\inc\stm8s.h	2674;"	macro
TBR	stm8s_stdperiph_driver\inc\stm8s.h	428;"	member	struct:AWU_struct
TBR_Array	stm8s_stdperiph_driver\src\stm8s_awu.c	49;"	variable
TDRH	stm8s_stdperiph_driver\inc\stm8s.h	311;"	member	struct:ADC1_struct
TDRH	stm8s_stdperiph_driver\inc\stm8s.h	382;"	member	struct:ADC2_struct
TDRL	stm8s_stdperiph_driver\inc\stm8s.h	312;"	member	struct:ADC1_struct
TDRL	stm8s_stdperiph_driver\inc\stm8s.h	383;"	member	struct:ADC2_struct
TECR	stm8s_stdperiph_driver\inc\stm8s.h	2177;"	member	struct:__anon5::__anon6::__anon12
TI1_Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	1214;"	function	file:	signature:(uint8_t TIM2_ICPolarity, uint8_t TIM2_ICSelection, uint8_t TIM2_ICFilter)
TI1_Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	33;"	prototype	file:	signature:(uint8_t TIM2_ICPolarity, uint8_t TIM2_ICSelection, uint8_t TIM2_ICFilter)
TI2_Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	1255;"	function	file:	signature:(uint8_t TIM2_ICPolarity, uint8_t TIM2_ICSelection, uint8_t TIM2_ICFilter)
TI2_Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	34;"	prototype	file:	signature:(uint8_t TIM2_ICPolarity, uint8_t TIM2_ICSelection, uint8_t TIM2_ICFilter)
TI3_Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	1296;"	function	file:	signature:(uint8_t TIM2_ICPolarity, uint8_t TIM2_ICSelection, uint8_t TIM2_ICFilter)
TI3_Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	35;"	prototype	file:	signature:(uint8_t TIM2_ICPolarity, uint8_t TIM2_ICSelection, uint8_t TIM2_ICFilter)
TIM1	stm8s_stdperiph_driver\inc\stm8s.h	2561;"	macro
TIM1_ARRH_ARR	stm8s_stdperiph_driver\inc\stm8s.h	765;"	macro
TIM1_ARRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	655;"	macro
TIM1_ARRL_ARR	stm8s_stdperiph_driver\inc\stm8s.h	766;"	macro
TIM1_ARRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	656;"	macro
TIM1_ARRPreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	563;"	prototype	signature:(FunctionalState NewState)
TIM1_AUTOMATICOUTPUT_DISABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	177;"	enumerator	enum:__anon95
TIM1_AUTOMATICOUTPUT_ENABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	176;"	enumerator	enum:__anon95
TIM1_AutomaticOutput_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	178;"	typedef	typeref:enum:__anon95
TIM1_BDTRConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	517;"	prototype	signature:(TIM1_OSSIState_TypeDef TIM1_OSSIState, TIM1_LockLevel_TypeDef TIM1_LockLevel, uint8_t TIM1_DeadTime, TIM1_BreakState_TypeDef TIM1_Break, TIM1_BreakPolarity_TypeDef TIM1_BreakPolarity, TIM1_AutomaticOutput_TypeDef TIM1_AutomaticOutput)
TIM1_BKR_AOE	stm8s_stdperiph_driver\inc\stm8s.h	783;"	macro
TIM1_BKR_BKE	stm8s_stdperiph_driver\inc\stm8s.h	785;"	macro
TIM1_BKR_BKP	stm8s_stdperiph_driver\inc\stm8s.h	784;"	macro
TIM1_BKR_LOCK	stm8s_stdperiph_driver\inc\stm8s.h	788;"	macro
TIM1_BKR_MOE	stm8s_stdperiph_driver\inc\stm8s.h	782;"	macro
TIM1_BKR_OSSI	stm8s_stdperiph_driver\inc\stm8s.h	787;"	macro
TIM1_BKR_OSSR	stm8s_stdperiph_driver\inc\stm8s.h	786;"	macro
TIM1_BKR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	666;"	macro
TIM1_BREAKPOLARITY_HIGH	stm8s_stdperiph_driver\inc\stm8s_tim1.h	168;"	enumerator	enum:__anon94
TIM1_BREAKPOLARITY_LOW	stm8s_stdperiph_driver\inc\stm8s_tim1.h	167;"	enumerator	enum:__anon94
TIM1_BREAK_DISABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	159;"	enumerator	enum:__anon93
TIM1_BREAK_ENABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	158;"	enumerator	enum:__anon93
TIM1_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2469;"	macro
TIM1_BreakPolarity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	169;"	typedef	typeref:enum:__anon94
TIM1_BreakState_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	160;"	typedef	typeref:enum:__anon93
TIM1_CCER1_CC1E	stm8s_stdperiph_driver\inc\stm8s.h	748;"	macro
TIM1_CCER1_CC1NE	stm8s_stdperiph_driver\inc\stm8s.h	746;"	macro
TIM1_CCER1_CC1NP	stm8s_stdperiph_driver\inc\stm8s.h	745;"	macro
TIM1_CCER1_CC1P	stm8s_stdperiph_driver\inc\stm8s.h	747;"	macro
TIM1_CCER1_CC2E	stm8s_stdperiph_driver\inc\stm8s.h	744;"	macro
TIM1_CCER1_CC2NE	stm8s_stdperiph_driver\inc\stm8s.h	742;"	macro
TIM1_CCER1_CC2NP	stm8s_stdperiph_driver\inc\stm8s.h	741;"	macro
TIM1_CCER1_CC2P	stm8s_stdperiph_driver\inc\stm8s.h	743;"	macro
TIM1_CCER1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	649;"	macro
TIM1_CCER2_CC3E	stm8s_stdperiph_driver\inc\stm8s.h	755;"	macro
TIM1_CCER2_CC3NE	stm8s_stdperiph_driver\inc\stm8s.h	753;"	macro
TIM1_CCER2_CC3NP	stm8s_stdperiph_driver\inc\stm8s.h	752;"	macro
TIM1_CCER2_CC3P	stm8s_stdperiph_driver\inc\stm8s.h	754;"	macro
TIM1_CCER2_CC4E	stm8s_stdperiph_driver\inc\stm8s.h	751;"	macro
TIM1_CCER2_CC4P	stm8s_stdperiph_driver\inc\stm8s.h	750;"	macro
TIM1_CCER2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	650;"	macro
TIM1_CCMR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	645;"	macro
TIM1_CCMR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	646;"	macro
TIM1_CCMR3_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	647;"	macro
TIM1_CCMR4_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	648;"	macro
TIM1_CCMR_CCxS	stm8s_stdperiph_driver\inc\stm8s.h	737;"	macro
TIM1_CCMR_ICxF	stm8s_stdperiph_driver\inc\stm8s.h	733;"	macro
TIM1_CCMR_ICxPSC	stm8s_stdperiph_driver\inc\stm8s.h	732;"	macro
TIM1_CCMR_OCM	stm8s_stdperiph_driver\inc\stm8s.h	734;"	macro
TIM1_CCMR_OCxFE	stm8s_stdperiph_driver\inc\stm8s.h	736;"	macro
TIM1_CCMR_OCxPE	stm8s_stdperiph_driver\inc\stm8s.h	735;"	macro
TIM1_CCPreloadControl	stm8s_stdperiph_driver\inc\stm8s_tim1.h	565;"	prototype	signature:(FunctionalState NewState)
TIM1_CCR1H_CCR1	stm8s_stdperiph_driver\inc\stm8s.h	770;"	macro
TIM1_CCR1H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	658;"	macro
TIM1_CCR1L_CCR1	stm8s_stdperiph_driver\inc\stm8s.h	771;"	macro
TIM1_CCR1L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	659;"	macro
TIM1_CCR2H_CCR2	stm8s_stdperiph_driver\inc\stm8s.h	773;"	macro
TIM1_CCR2H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	660;"	macro
TIM1_CCR2L_CCR2	stm8s_stdperiph_driver\inc\stm8s.h	774;"	macro
TIM1_CCR2L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	661;"	macro
TIM1_CCR3H_CCR3	stm8s_stdperiph_driver\inc\stm8s.h	776;"	macro
TIM1_CCR3H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	662;"	macro
TIM1_CCR3L_CCR3	stm8s_stdperiph_driver\inc\stm8s.h	777;"	macro
TIM1_CCR3L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	663;"	macro
TIM1_CCR4H_CCR4	stm8s_stdperiph_driver\inc\stm8s.h	779;"	macro
TIM1_CCR4H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	664;"	macro
TIM1_CCR4L_CCR4	stm8s_stdperiph_driver\inc\stm8s.h	780;"	macro
TIM1_CCR4L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	665;"	macro
TIM1_CCxCmd	stm8s_stdperiph_driver\inc\stm8s_tim1.h	582;"	prototype	signature:(TIM1_Channel_TypeDef TIM1_Channel, FunctionalState NewState)
TIM1_CCxNCmd	stm8s_stdperiph_driver\inc\stm8s_tim1.h	583;"	prototype	signature:(TIM1_Channel_TypeDef TIM1_Channel, FunctionalState NewState)
TIM1_CHANNEL_1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	79;"	enumerator	enum:__anon87
TIM1_CHANNEL_2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	80;"	enumerator	enum:__anon87
TIM1_CHANNEL_3	stm8s_stdperiph_driver\inc\stm8s_tim1.h	81;"	enumerator	enum:__anon87
TIM1_CHANNEL_4	stm8s_stdperiph_driver\inc\stm8s_tim1.h	82;"	enumerator	enum:__anon87
TIM1_CNTRH_CNT	stm8s_stdperiph_driver\inc\stm8s.h	757;"	macro
TIM1_CNTRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	651;"	macro
TIM1_CNTRL_CNT	stm8s_stdperiph_driver\inc\stm8s.h	759;"	macro
TIM1_CNTRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	652;"	macro
TIM1_COUNTERMODE_CENTERALIGNED1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	104;"	enumerator	enum:__anon88
TIM1_COUNTERMODE_CENTERALIGNED2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	105;"	enumerator	enum:__anon88
TIM1_COUNTERMODE_CENTERALIGNED3	stm8s_stdperiph_driver\inc\stm8s_tim1.h	106;"	enumerator	enum:__anon88
TIM1_COUNTERMODE_DOWN	stm8s_stdperiph_driver\inc\stm8s_tim1.h	103;"	enumerator	enum:__anon88
TIM1_COUNTERMODE_UP	stm8s_stdperiph_driver\inc\stm8s_tim1.h	102;"	enumerator	enum:__anon88
TIM1_CR1_ARPE	stm8s_stdperiph_driver\inc\stm8s.h	678;"	macro
TIM1_CR1_CEN	stm8s_stdperiph_driver\inc\stm8s.h	684;"	macro
TIM1_CR1_CMS	stm8s_stdperiph_driver\inc\stm8s.h	679;"	macro
TIM1_CR1_DIR	stm8s_stdperiph_driver\inc\stm8s.h	680;"	macro
TIM1_CR1_OPM	stm8s_stdperiph_driver\inc\stm8s.h	681;"	macro
TIM1_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	637;"	macro
TIM1_CR1_UDIS	stm8s_stdperiph_driver\inc\stm8s.h	683;"	macro
TIM1_CR1_URS	stm8s_stdperiph_driver\inc\stm8s.h	682;"	macro
TIM1_CR2_CCPC	stm8s_stdperiph_driver\inc\stm8s.h	689;"	macro
TIM1_CR2_COMS	stm8s_stdperiph_driver\inc\stm8s.h	688;"	macro
TIM1_CR2_MMS	stm8s_stdperiph_driver\inc\stm8s.h	687;"	macro
TIM1_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	638;"	macro
TIM1_CR2_TI1S	stm8s_stdperiph_driver\inc\stm8s.h	686;"	macro
TIM1_Channel_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	83;"	typedef	typeref:enum:__anon87
TIM1_ClearFlag	stm8s_stdperiph_driver\inc\stm8s_tim1.h	602;"	prototype	signature:(TIM1_FLAG_TypeDef TIM1_FLAG)
TIM1_ClearITPendingBit	stm8s_stdperiph_driver\inc\stm8s_tim1.h	604;"	prototype	signature:(TIM1_IT_TypeDef TIM1_IT)
TIM1_Cmd	stm8s_stdperiph_driver\inc\stm8s_tim1.h	530;"	prototype	signature:(FunctionalState NewState)
TIM1_CounterModeConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	558;"	prototype	signature:(TIM1_CounterMode_TypeDef TIM1_CounterMode)
TIM1_CounterMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	107;"	typedef	typeref:enum:__anon88
TIM1_CtrlPWMOutputs	stm8s_stdperiph_driver\inc\stm8s_tim1.h	531;"	prototype	signature:(FunctionalState NewState)
TIM1_DTR_DTG	stm8s_stdperiph_driver\inc\stm8s.h	790;"	macro
TIM1_DTR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	667;"	macro
TIM1_DeInit	stm8s_stdperiph_driver\inc\stm8s_tim1.h	488;"	prototype	signature:(void)
TIM1_EGR_BG	stm8s_stdperiph_driver\inc\stm8s.h	723;"	macro
TIM1_EGR_CC1G	stm8s_stdperiph_driver\inc\stm8s.h	729;"	macro
TIM1_EGR_CC2G	stm8s_stdperiph_driver\inc\stm8s.h	728;"	macro
TIM1_EGR_CC3G	stm8s_stdperiph_driver\inc\stm8s.h	727;"	macro
TIM1_EGR_CC4G	stm8s_stdperiph_driver\inc\stm8s.h	726;"	macro
TIM1_EGR_COMG	stm8s_stdperiph_driver\inc\stm8s.h	725;"	macro
TIM1_EGR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	644;"	macro
TIM1_EGR_TG	stm8s_stdperiph_driver\inc\stm8s.h	724;"	macro
TIM1_EGR_UG	stm8s_stdperiph_driver\inc\stm8s.h	730;"	macro
TIM1_ENCODERMODE_TI1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	367;"	enumerator	enum:__anon109
TIM1_ENCODERMODE_TI12	stm8s_stdperiph_driver\inc\stm8s_tim1.h	369;"	enumerator	enum:__anon109
TIM1_ENCODERMODE_TI2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	368;"	enumerator	enum:__anon109
TIM1_ETRClockMode1Config	stm8s_stdperiph_driver\inc\stm8s_tim1.h	534;"	prototype	signature:(TIM1_ExtTRGPSC_TypeDef TIM1_ExtTRGPrescaler, TIM1_ExtTRGPolarity_TypeDef TIM1_ExtTRGPolarity, uint8_t ExtTRGFilter)
TIM1_ETRClockMode2Config	stm8s_stdperiph_driver\inc\stm8s_tim1.h	537;"	prototype	signature:(TIM1_ExtTRGPSC_TypeDef TIM1_ExtTRGPrescaler, TIM1_ExtTRGPolarity_TypeDef TIM1_ExtTRGPolarity, uint8_t ExtTRGFilter)
TIM1_ETRConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	540;"	prototype	signature:(TIM1_ExtTRGPSC_TypeDef TIM1_ExtTRGPrescaler, TIM1_ExtTRGPolarity_TypeDef TIM1_ExtTRGPolarity, uint8_t ExtTRGFilter)
TIM1_ETR_ECE	stm8s_stdperiph_driver\inc\stm8s.h	696;"	macro
TIM1_ETR_ETF	stm8s_stdperiph_driver\inc\stm8s.h	698;"	macro
TIM1_ETR_ETP	stm8s_stdperiph_driver\inc\stm8s.h	695;"	macro
TIM1_ETR_ETPS	stm8s_stdperiph_driver\inc\stm8s.h	697;"	macro
TIM1_ETR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	640;"	macro
TIM1_EVENTSOURCE_BREAK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	386;"	enumerator	enum:__anon110
TIM1_EVENTSOURCE_CC1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	380;"	enumerator	enum:__anon110
TIM1_EVENTSOURCE_CC2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	381;"	enumerator	enum:__anon110
TIM1_EVENTSOURCE_CC3	stm8s_stdperiph_driver\inc\stm8s_tim1.h	382;"	enumerator	enum:__anon110
TIM1_EVENTSOURCE_CC4	stm8s_stdperiph_driver\inc\stm8s_tim1.h	383;"	enumerator	enum:__anon110
TIM1_EVENTSOURCE_COM	stm8s_stdperiph_driver\inc\stm8s_tim1.h	384;"	enumerator	enum:__anon110
TIM1_EVENTSOURCE_TRIGGER	stm8s_stdperiph_driver\inc\stm8s_tim1.h	385;"	enumerator	enum:__anon110
TIM1_EVENTSOURCE_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	379;"	enumerator	enum:__anon110
TIM1_EXTTRGPOLARITY_INVERTED	stm8s_stdperiph_driver\inc\stm8s_tim1.h	347;"	enumerator	enum:__anon107
TIM1_EXTTRGPOLARITY_NONINVERTED	stm8s_stdperiph_driver\inc\stm8s_tim1.h	348;"	enumerator	enum:__anon107
TIM1_EXTTRGPSC_DIV2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	299;"	enumerator	enum:__anon104
TIM1_EXTTRGPSC_DIV4	stm8s_stdperiph_driver\inc\stm8s_tim1.h	300;"	enumerator	enum:__anon104
TIM1_EXTTRGPSC_DIV8	stm8s_stdperiph_driver\inc\stm8s_tim1.h	301;"	enumerator	enum:__anon104
TIM1_EXTTRGPSC_OFF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	298;"	enumerator	enum:__anon104
TIM1_EncoderInterfaceConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	554;"	prototype	signature:(TIM1_EncoderMode_TypeDef TIM1_EncoderMode, TIM1_ICPolarity_TypeDef TIM1_IC1Polarity, TIM1_ICPolarity_TypeDef TIM1_IC2Polarity)
TIM1_EncoderMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	370;"	typedef	typeref:enum:__anon109
TIM1_EventSource_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	387;"	typedef	typeref:enum:__anon110
TIM1_ExtTRGPSC_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	302;"	typedef	typeref:enum:__anon104
TIM1_ExtTRGPolarity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	349;"	typedef	typeref:enum:__anon107
TIM1_FLAG_BREAK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	445;"	enumerator	enum:__anon114
TIM1_FLAG_CC1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	439;"	enumerator	enum:__anon114
TIM1_FLAG_CC1OF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	446;"	enumerator	enum:__anon114
TIM1_FLAG_CC2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	440;"	enumerator	enum:__anon114
TIM1_FLAG_CC2OF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	447;"	enumerator	enum:__anon114
TIM1_FLAG_CC3	stm8s_stdperiph_driver\inc\stm8s_tim1.h	441;"	enumerator	enum:__anon114
TIM1_FLAG_CC3OF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	448;"	enumerator	enum:__anon114
TIM1_FLAG_CC4	stm8s_stdperiph_driver\inc\stm8s_tim1.h	442;"	enumerator	enum:__anon114
TIM1_FLAG_CC4OF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	449;"	enumerator	enum:__anon114
TIM1_FLAG_COM	stm8s_stdperiph_driver\inc\stm8s_tim1.h	443;"	enumerator	enum:__anon114
TIM1_FLAG_TRIGGER	stm8s_stdperiph_driver\inc\stm8s_tim1.h	444;"	enumerator	enum:__anon114
TIM1_FLAG_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	450;"	typedef	typeref:enum:__anon114
TIM1_FLAG_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	438;"	enumerator	enum:__anon114
TIM1_FORCEDACTION_ACTIVE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	470;"	enumerator	enum:__anon115
TIM1_FORCEDACTION_INACTIVE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	471;"	enumerator	enum:__anon115
TIM1_ForcedAction_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	472;"	typedef	typeref:enum:__anon115
TIM1_ForcedOC1Config	stm8s_stdperiph_driver\inc\stm8s_tim1.h	559;"	prototype	signature:(TIM1_ForcedAction_TypeDef TIM1_ForcedAction)
TIM1_ForcedOC2Config	stm8s_stdperiph_driver\inc\stm8s_tim1.h	560;"	prototype	signature:(TIM1_ForcedAction_TypeDef TIM1_ForcedAction)
TIM1_ForcedOC3Config	stm8s_stdperiph_driver\inc\stm8s_tim1.h	561;"	prototype	signature:(TIM1_ForcedAction_TypeDef TIM1_ForcedAction)
TIM1_ForcedOC4Config	stm8s_stdperiph_driver\inc\stm8s_tim1.h	562;"	prototype	signature:(TIM1_ForcedAction_TypeDef TIM1_ForcedAction)
TIM1_GenerateEvent	stm8s_stdperiph_driver\inc\stm8s_tim1.h	574;"	prototype	signature:(TIM1_EventSource_TypeDef TIM1_EventSource)
TIM1_GetCapture1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	595;"	prototype	signature:(void)
TIM1_GetCapture2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	596;"	prototype	signature:(void)
TIM1_GetCapture3	stm8s_stdperiph_driver\inc\stm8s_tim1.h	597;"	prototype	signature:(void)
TIM1_GetCapture4	stm8s_stdperiph_driver\inc\stm8s_tim1.h	598;"	prototype	signature:(void)
TIM1_GetCounter	stm8s_stdperiph_driver\inc\stm8s_tim1.h	599;"	prototype	signature:(void)
TIM1_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_tim1.h	601;"	prototype	signature:(TIM1_FLAG_TypeDef TIM1_FLAG)
TIM1_GetITStatus	stm8s_stdperiph_driver\inc\stm8s_tim1.h	603;"	prototype	signature:(TIM1_IT_TypeDef TIM1_IT)
TIM1_GetPrescaler	stm8s_stdperiph_driver\inc\stm8s_tim1.h	600;"	prototype	signature:(void)
TIM1_ICInit	stm8s_stdperiph_driver\inc\stm8s_tim1.h	522;"	prototype	signature:(TIM1_Channel_TypeDef TIM1_Channel, TIM1_ICPolarity_TypeDef TIM1_ICPolarity, TIM1_ICSelection_TypeDef TIM1_ICSelection, TIM1_ICPSC_TypeDef TIM1_ICPrescaler, uint8_t TIM1_ICFilter)
TIM1_ICPOLARITY_FALLING	stm8s_stdperiph_driver\inc\stm8s_tim1.h	231;"	enumerator	enum:__anon100
TIM1_ICPOLARITY_RISING	stm8s_stdperiph_driver\inc\stm8s_tim1.h	230;"	enumerator	enum:__anon100
TIM1_ICPSC_DIV1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	252;"	enumerator	enum:__anon102
TIM1_ICPSC_DIV2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	253;"	enumerator	enum:__anon102
TIM1_ICPSC_DIV4	stm8s_stdperiph_driver\inc\stm8s_tim1.h	254;"	enumerator	enum:__anon102
TIM1_ICPSC_DIV8	stm8s_stdperiph_driver\inc\stm8s_tim1.h	255;"	enumerator	enum:__anon102
TIM1_ICPSC_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	256;"	typedef	typeref:enum:__anon102
TIM1_ICPolarity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	232;"	typedef	typeref:enum:__anon100
TIM1_ICSELECTION_DIRECTTI	stm8s_stdperiph_driver\inc\stm8s_tim1.h	240;"	enumerator	enum:__anon101
TIM1_ICSELECTION_INDIRECTTI	stm8s_stdperiph_driver\inc\stm8s_tim1.h	241;"	enumerator	enum:__anon101
TIM1_ICSELECTION_TRGI	stm8s_stdperiph_driver\inc\stm8s_tim1.h	242;"	enumerator	enum:__anon101
TIM1_ICSelection_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	243;"	typedef	typeref:enum:__anon101
TIM1_IER_BIE	stm8s_stdperiph_driver\inc\stm8s.h	700;"	macro
TIM1_IER_CC1IE	stm8s_stdperiph_driver\inc\stm8s.h	706;"	macro
TIM1_IER_CC2IE	stm8s_stdperiph_driver\inc\stm8s.h	705;"	macro
TIM1_IER_CC3IE	stm8s_stdperiph_driver\inc\stm8s.h	704;"	macro
TIM1_IER_CC4IE	stm8s_stdperiph_driver\inc\stm8s.h	703;"	macro
TIM1_IER_COMIE	stm8s_stdperiph_driver\inc\stm8s.h	702;"	macro
TIM1_IER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	641;"	macro
TIM1_IER_TIE	stm8s_stdperiph_driver\inc\stm8s.h	701;"	macro
TIM1_IER_UIE	stm8s_stdperiph_driver\inc\stm8s.h	707;"	macro
TIM1_ITConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	532;"	prototype	signature:(TIM1_IT_TypeDef TIM1_IT, FunctionalState NewState)
TIM1_IT_BREAK	stm8s_stdperiph_driver\inc\stm8s_tim1.h	280;"	enumerator	enum:__anon103
TIM1_IT_CC1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	274;"	enumerator	enum:__anon103
TIM1_IT_CC2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	275;"	enumerator	enum:__anon103
TIM1_IT_CC3	stm8s_stdperiph_driver\inc\stm8s_tim1.h	276;"	enumerator	enum:__anon103
TIM1_IT_CC4	stm8s_stdperiph_driver\inc\stm8s_tim1.h	277;"	enumerator	enum:__anon103
TIM1_IT_COM	stm8s_stdperiph_driver\inc\stm8s_tim1.h	278;"	enumerator	enum:__anon103
TIM1_IT_TRIGGER	stm8s_stdperiph_driver\inc\stm8s_tim1.h	279;"	enumerator	enum:__anon103
TIM1_IT_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	281;"	typedef	typeref:enum:__anon103
TIM1_IT_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	273;"	enumerator	enum:__anon103
TIM1_InternalClockConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	533;"	prototype	signature:(void)
TIM1_LOCKLEVEL_1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	187;"	enumerator	enum:__anon96
TIM1_LOCKLEVEL_2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	188;"	enumerator	enum:__anon96
TIM1_LOCKLEVEL_3	stm8s_stdperiph_driver\inc\stm8s_tim1.h	189;"	enumerator	enum:__anon96
TIM1_LOCKLEVEL_OFF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	186;"	enumerator	enum:__anon96
TIM1_LockLevel_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	190;"	typedef	typeref:enum:__anon96
TIM1_OC1FastConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	570;"	prototype	signature:(FunctionalState NewState)
TIM1_OC1Init	stm8s_stdperiph_driver\inc\stm8s_tim1.h	492;"	prototype	signature:(TIM1_OCMode_TypeDef TIM1_OCMode, TIM1_OutputState_TypeDef TIM1_OutputState, TIM1_OutputNState_TypeDef TIM1_OutputNState, uint16_t TIM1_Pulse, TIM1_OCPolarity_TypeDef TIM1_OCPolarity, TIM1_OCNPolarity_TypeDef TIM1_OCNPolarity, TIM1_OCIdleState_TypeDef TIM1_OCIdleState, TIM1_OCNIdleState_TypeDef TIM1_OCNIdleState)
TIM1_OC1NPolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	576;"	prototype	signature:(TIM1_OCNPolarity_TypeDef TIM1_OCNPolarity)
TIM1_OC1PolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	575;"	prototype	signature:(TIM1_OCPolarity_TypeDef TIM1_OCPolarity)
TIM1_OC1PreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	566;"	prototype	signature:(FunctionalState NewState)
TIM1_OC2FastConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	571;"	prototype	signature:(FunctionalState NewState)
TIM1_OC2Init	stm8s_stdperiph_driver\inc\stm8s_tim1.h	499;"	prototype	signature:(TIM1_OCMode_TypeDef TIM1_OCMode, TIM1_OutputState_TypeDef TIM1_OutputState, TIM1_OutputNState_TypeDef TIM1_OutputNState, uint16_t TIM1_Pulse, TIM1_OCPolarity_TypeDef TIM1_OCPolarity, TIM1_OCNPolarity_TypeDef TIM1_OCNPolarity, TIM1_OCIdleState_TypeDef TIM1_OCIdleState, TIM1_OCNIdleState_TypeDef TIM1_OCNIdleState)
TIM1_OC2NPolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	578;"	prototype	signature:(TIM1_OCNPolarity_TypeDef TIM1_OCNPolarity)
TIM1_OC2PolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	577;"	prototype	signature:(TIM1_OCPolarity_TypeDef TIM1_OCPolarity)
TIM1_OC2PreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	567;"	prototype	signature:(FunctionalState NewState)
TIM1_OC3FastConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	572;"	prototype	signature:(FunctionalState NewState)
TIM1_OC3Init	stm8s_stdperiph_driver\inc\stm8s_tim1.h	506;"	prototype	signature:(TIM1_OCMode_TypeDef TIM1_OCMode, TIM1_OutputState_TypeDef TIM1_OutputState, TIM1_OutputNState_TypeDef TIM1_OutputNState, uint16_t TIM1_Pulse, TIM1_OCPolarity_TypeDef TIM1_OCPolarity, TIM1_OCNPolarity_TypeDef TIM1_OCNPolarity, TIM1_OCIdleState_TypeDef TIM1_OCIdleState, TIM1_OCNIdleState_TypeDef TIM1_OCNIdleState)
TIM1_OC3NPolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	580;"	prototype	signature:(TIM1_OCNPolarity_TypeDef TIM1_OCNPolarity)
TIM1_OC3PolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	579;"	prototype	signature:(TIM1_OCPolarity_TypeDef TIM1_OCPolarity)
TIM1_OC3PreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	568;"	prototype	signature:(FunctionalState NewState)
TIM1_OC4FastConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	573;"	prototype	signature:(FunctionalState NewState)
TIM1_OC4Init	stm8s_stdperiph_driver\inc\stm8s_tim1.h	513;"	prototype	signature:(TIM1_OCMode_TypeDef TIM1_OCMode, TIM1_OutputState_TypeDef TIM1_OutputState, uint16_t TIM1_Pulse, TIM1_OCPolarity_TypeDef TIM1_OCPolarity, TIM1_OCIdleState_TypeDef TIM1_OCIdleState)
TIM1_OC4PolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	581;"	prototype	signature:(TIM1_OCPolarity_TypeDef TIM1_OCPolarity)
TIM1_OC4PreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	569;"	prototype	signature:(FunctionalState NewState)
TIM1_OCIDLESTATE_RESET	stm8s_stdperiph_driver\inc\stm8s_tim1.h	211;"	enumerator	enum:__anon98
TIM1_OCIDLESTATE_SET	stm8s_stdperiph_driver\inc\stm8s_tim1.h	210;"	enumerator	enum:__anon98
TIM1_OCIdleState_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	212;"	typedef	typeref:enum:__anon98
TIM1_OCMODE_ACTIVE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	42;"	enumerator	enum:__anon85
TIM1_OCMODE_INACTIVE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	43;"	enumerator	enum:__anon85
TIM1_OCMODE_PWM1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	45;"	enumerator	enum:__anon85
TIM1_OCMODE_PWM2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	46;"	enumerator	enum:__anon85
TIM1_OCMODE_TIMING	stm8s_stdperiph_driver\inc\stm8s_tim1.h	41;"	enumerator	enum:__anon85
TIM1_OCMODE_TOGGLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	44;"	enumerator	enum:__anon85
TIM1_OCMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	47;"	typedef	typeref:enum:__anon85
TIM1_OCNIDLESTATE_RESET	stm8s_stdperiph_driver\inc\stm8s_tim1.h	221;"	enumerator	enum:__anon99
TIM1_OCNIDLESTATE_SET	stm8s_stdperiph_driver\inc\stm8s_tim1.h	220;"	enumerator	enum:__anon99
TIM1_OCNIdleState_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	222;"	typedef	typeref:enum:__anon99
TIM1_OCNPOLARITY_HIGH	stm8s_stdperiph_driver\inc\stm8s_tim1.h	128;"	enumerator	enum:__anon90
TIM1_OCNPOLARITY_LOW	stm8s_stdperiph_driver\inc\stm8s_tim1.h	129;"	enumerator	enum:__anon90
TIM1_OCNPolarity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	130;"	typedef	typeref:enum:__anon90
TIM1_OCPOLARITY_HIGH	stm8s_stdperiph_driver\inc\stm8s_tim1.h	118;"	enumerator	enum:__anon89
TIM1_OCPOLARITY_LOW	stm8s_stdperiph_driver\inc\stm8s_tim1.h	119;"	enumerator	enum:__anon89
TIM1_OCPolarity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	120;"	typedef	typeref:enum:__anon89
TIM1_OISR_OIS1	stm8s_stdperiph_driver\inc\stm8s.h	798;"	macro
TIM1_OISR_OIS1N	stm8s_stdperiph_driver\inc\stm8s.h	797;"	macro
TIM1_OISR_OIS2	stm8s_stdperiph_driver\inc\stm8s.h	796;"	macro
TIM1_OISR_OIS2N	stm8s_stdperiph_driver\inc\stm8s.h	795;"	macro
TIM1_OISR_OIS3	stm8s_stdperiph_driver\inc\stm8s.h	794;"	macro
TIM1_OISR_OIS3N	stm8s_stdperiph_driver\inc\stm8s.h	793;"	macro
TIM1_OISR_OIS4	stm8s_stdperiph_driver\inc\stm8s.h	792;"	macro
TIM1_OISR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	668;"	macro
TIM1_OPMODE_REPETITIVE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	69;"	enumerator	enum:__anon86
TIM1_OPMODE_SINGLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	68;"	enumerator	enum:__anon86
TIM1_OPMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	70;"	typedef	typeref:enum:__anon86
TIM1_OSSISTATE_DISABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	201;"	enumerator	enum:__anon97
TIM1_OSSISTATE_ENABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	200;"	enumerator	enum:__anon97
TIM1_OSSIState_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	202;"	typedef	typeref:enum:__anon97
TIM1_OUTPUTNSTATE_DISABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	148;"	enumerator	enum:__anon92
TIM1_OUTPUTNSTATE_ENABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	149;"	enumerator	enum:__anon92
TIM1_OUTPUTSTATE_DISABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	138;"	enumerator	enum:__anon91
TIM1_OUTPUTSTATE_ENABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	139;"	enumerator	enum:__anon91
TIM1_OutputNState_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	150;"	typedef	typeref:enum:__anon92
TIM1_OutputState_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	140;"	typedef	typeref:enum:__anon91
TIM1_PSCH_PSC	stm8s_stdperiph_driver\inc\stm8s.h	761;"	macro
TIM1_PSCL_PSC	stm8s_stdperiph_driver\inc\stm8s.h	763;"	macro
TIM1_PSCRELOADMODE_IMMEDIATE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	358;"	enumerator	enum:__anon108
TIM1_PSCRELOADMODE_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	357;"	enumerator	enum:__anon108
TIM1_PSCRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	653;"	macro
TIM1_PSCRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	654;"	macro
TIM1_PSCReloadMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	359;"	typedef	typeref:enum:__anon108
TIM1_PWMIConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	526;"	prototype	signature:(TIM1_Channel_TypeDef TIM1_Channel, TIM1_ICPolarity_TypeDef TIM1_ICPolarity, TIM1_ICSelection_TypeDef TIM1_ICSelection, TIM1_ICPSC_TypeDef TIM1_ICPrescaler, uint8_t TIM1_ICFilter)
TIM1_PrescalerConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	557;"	prototype	signature:(uint16_t Prescaler, TIM1_PSCReloadMode_TypeDef TIM1_PSCReloadMode)
TIM1_RCR_REP	stm8s_stdperiph_driver\inc\stm8s.h	768;"	macro
TIM1_RCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	657;"	macro
TIM1_SLAVEMODE_EXTERNAL1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	427;"	enumerator	enum:__anon113
TIM1_SLAVEMODE_GATED	stm8s_stdperiph_driver\inc\stm8s_tim1.h	425;"	enumerator	enum:__anon113
TIM1_SLAVEMODE_RESET	stm8s_stdperiph_driver\inc\stm8s_tim1.h	424;"	enumerator	enum:__anon113
TIM1_SLAVEMODE_TRIGGER	stm8s_stdperiph_driver\inc\stm8s_tim1.h	426;"	enumerator	enum:__anon113
TIM1_SMCR_MSM	stm8s_stdperiph_driver\inc\stm8s.h	691;"	macro
TIM1_SMCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	639;"	macro
TIM1_SMCR_SMS	stm8s_stdperiph_driver\inc\stm8s.h	693;"	macro
TIM1_SMCR_TS	stm8s_stdperiph_driver\inc\stm8s.h	692;"	macro
TIM1_SR1_BIF	stm8s_stdperiph_driver\inc\stm8s.h	709;"	macro
TIM1_SR1_CC1IF	stm8s_stdperiph_driver\inc\stm8s.h	715;"	macro
TIM1_SR1_CC2IF	stm8s_stdperiph_driver\inc\stm8s.h	714;"	macro
TIM1_SR1_CC3IF	stm8s_stdperiph_driver\inc\stm8s.h	713;"	macro
TIM1_SR1_CC4IF	stm8s_stdperiph_driver\inc\stm8s.h	712;"	macro
TIM1_SR1_COMIF	stm8s_stdperiph_driver\inc\stm8s.h	711;"	macro
TIM1_SR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	642;"	macro
TIM1_SR1_TIF	stm8s_stdperiph_driver\inc\stm8s.h	710;"	macro
TIM1_SR1_UIF	stm8s_stdperiph_driver\inc\stm8s.h	716;"	macro
TIM1_SR2_CC1OF	stm8s_stdperiph_driver\inc\stm8s.h	721;"	macro
TIM1_SR2_CC2OF	stm8s_stdperiph_driver\inc\stm8s.h	720;"	macro
TIM1_SR2_CC3OF	stm8s_stdperiph_driver\inc\stm8s.h	719;"	macro
TIM1_SR2_CC4OF	stm8s_stdperiph_driver\inc\stm8s.h	718;"	macro
TIM1_SR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	643;"	macro
TIM1_SelectCOM	stm8s_stdperiph_driver\inc\stm8s_tim1.h	564;"	prototype	signature:(FunctionalState NewState)
TIM1_SelectHallSensor	stm8s_stdperiph_driver\inc\stm8s_tim1.h	549;"	prototype	signature:(FunctionalState NewState)
TIM1_SelectInputTrigger	stm8s_stdperiph_driver\inc\stm8s_tim1.h	546;"	prototype	signature:(TIM1_TS_TypeDef TIM1_InputTriggerSource)
TIM1_SelectMasterSlaveMode	stm8s_stdperiph_driver\inc\stm8s_tim1.h	553;"	prototype	signature:(FunctionalState NewState)
TIM1_SelectOCxM	stm8s_stdperiph_driver\inc\stm8s_tim1.h	584;"	prototype	signature:(TIM1_Channel_TypeDef TIM1_Channel, TIM1_OCMode_TypeDef TIM1_OCMode)
TIM1_SelectOnePulseMode	stm8s_stdperiph_driver\inc\stm8s_tim1.h	550;"	prototype	signature:(TIM1_OPMode_TypeDef TIM1_OPMode)
TIM1_SelectOutputTrigger	stm8s_stdperiph_driver\inc\stm8s_tim1.h	551;"	prototype	signature:(TIM1_TRGOSource_TypeDef TIM1_TRGOSource)
TIM1_SelectSlaveMode	stm8s_stdperiph_driver\inc\stm8s_tim1.h	552;"	prototype	signature:(TIM1_SlaveMode_TypeDef TIM1_SlaveMode)
TIM1_SetAutoreload	stm8s_stdperiph_driver\inc\stm8s_tim1.h	586;"	prototype	signature:(uint16_t Autoreload)
TIM1_SetCompare1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	587;"	prototype	signature:(uint16_t Compare1)
TIM1_SetCompare2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	588;"	prototype	signature:(uint16_t Compare2)
TIM1_SetCompare3	stm8s_stdperiph_driver\inc\stm8s_tim1.h	589;"	prototype	signature:(uint16_t Compare3)
TIM1_SetCompare4	stm8s_stdperiph_driver\inc\stm8s_tim1.h	590;"	prototype	signature:(uint16_t Compare4)
TIM1_SetCounter	stm8s_stdperiph_driver\inc\stm8s_tim1.h	585;"	prototype	signature:(uint16_t Counter)
TIM1_SetIC1Prescaler	stm8s_stdperiph_driver\inc\stm8s_tim1.h	591;"	prototype	signature:(TIM1_ICPSC_TypeDef TIM1_IC1Prescaler)
TIM1_SetIC2Prescaler	stm8s_stdperiph_driver\inc\stm8s_tim1.h	592;"	prototype	signature:(TIM1_ICPSC_TypeDef TIM1_IC2Prescaler)
TIM1_SetIC3Prescaler	stm8s_stdperiph_driver\inc\stm8s_tim1.h	593;"	prototype	signature:(TIM1_ICPSC_TypeDef TIM1_IC3Prescaler)
TIM1_SetIC4Prescaler	stm8s_stdperiph_driver\inc\stm8s_tim1.h	594;"	prototype	signature:(TIM1_ICPSC_TypeDef TIM1_IC4Prescaler)
TIM1_SlaveMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	428;"	typedef	typeref:enum:__anon113
TIM1_TIXEXTERNALCLK1SOURCE_TI1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	336;"	enumerator	enum:__anon106
TIM1_TIXEXTERNALCLK1SOURCE_TI1ED	stm8s_stdperiph_driver\inc\stm8s_tim1.h	335;"	enumerator	enum:__anon106
TIM1_TIXEXTERNALCLK1SOURCE_TI2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	337;"	enumerator	enum:__anon106
TIM1_TIxExternalCLK1Source_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	338;"	typedef	typeref:enum:__anon106
TIM1_TIxExternalClockConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	543;"	prototype	signature:(TIM1_TIxExternalCLK1Source_TypeDef TIM1_TIxExternalCLKSource, TIM1_ICPolarity_TypeDef TIM1_ICPolarity, uint8_t ICFilter)
TIM1_TRGOSOURCE_ENABLE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	405;"	enumerator	enum:__anon112
TIM1_TRGOSOURCE_OC1REF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	408;"	enumerator	enum:__anon112
TIM1_TRGOSOURCE_OC2REF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	409;"	enumerator	enum:__anon112
TIM1_TRGOSOURCE_OC3REF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	410;"	enumerator	enum:__anon112
TIM1_TRGOSOURCE_RESET	stm8s_stdperiph_driver\inc\stm8s_tim1.h	404;"	enumerator	enum:__anon112
TIM1_TRGOSOURCE_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim1.h	406;"	enumerator	enum:__anon112
TIM1_TRGOSource_OC1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	407;"	enumerator	enum:__anon112
TIM1_TRGOSource_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	411;"	typedef	typeref:enum:__anon112
TIM1_TS_ETRF	stm8s_stdperiph_driver\inc\stm8s_tim1.h	317;"	enumerator	enum:__anon105
TIM1_TS_TI1FP1	stm8s_stdperiph_driver\inc\stm8s_tim1.h	315;"	enumerator	enum:__anon105
TIM1_TS_TI1F_ED	stm8s_stdperiph_driver\inc\stm8s_tim1.h	314;"	enumerator	enum:__anon105
TIM1_TS_TI2FP2	stm8s_stdperiph_driver\inc\stm8s_tim1.h	316;"	enumerator	enum:__anon105
TIM1_TS_TIM5	stm8s_stdperiph_driver\inc\stm8s_tim1.h	313;"	enumerator	enum:__anon105
TIM1_TS_TIM6	stm8s_stdperiph_driver\inc\stm8s_tim1.h	312;"	enumerator	enum:__anon105
TIM1_TS_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	318;"	typedef	typeref:enum:__anon105
TIM1_TimeBaseInit	stm8s_stdperiph_driver\inc\stm8s_tim1.h	489;"	prototype	signature:(uint16_t TIM1_Prescaler, TIM1_CounterMode_TypeDef TIM1_CounterMode, uint16_t TIM1_Period, uint8_t TIM1_RepetitionCounter)
TIM1_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	631;"	typedef	typeref:struct:TIM1_struct
TIM1_UPDATESOURCE_GLOBAL	stm8s_stdperiph_driver\inc\stm8s_tim1.h	394;"	enumerator	enum:__anon111
TIM1_UPDATESOURCE_REGULAR	stm8s_stdperiph_driver\inc\stm8s_tim1.h	395;"	enumerator	enum:__anon111
TIM1_UpdateDisableConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	547;"	prototype	signature:(FunctionalState NewState)
TIM1_UpdateRequestConfig	stm8s_stdperiph_driver\inc\stm8s_tim1.h	548;"	prototype	signature:(TIM1_UpdateSource_TypeDef TIM1_UpdateSource)
TIM1_UpdateSource_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim1.h	396;"	typedef	typeref:enum:__anon111
TIM1_struct	stm8s_stdperiph_driver\inc\stm8s.h	596;"	struct
TIM2	stm8s_stdperiph_driver\inc\stm8s.h	2566;"	macro
TIM2_ARRH_ARR	stm8s_stdperiph_driver\inc\stm8s.h	916;"	macro
TIM2_ARRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	855;"	macro
TIM2_ARRL_ARR	stm8s_stdperiph_driver\inc\stm8s.h	917;"	macro
TIM2_ARRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	856;"	macro
TIM2_ARRPreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	296;"	prototype	signature:(FunctionalState NewState)
TIM2_ARRPreloadConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	567;"	function	signature:(FunctionalState NewState)
TIM2_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2470;"	macro
TIM2_CCER1_CC1E	stm8s_stdperiph_driver\inc\stm8s.h	906;"	macro
TIM2_CCER1_CC1P	stm8s_stdperiph_driver\inc\stm8s.h	905;"	macro
TIM2_CCER1_CC2E	stm8s_stdperiph_driver\inc\stm8s.h	904;"	macro
TIM2_CCER1_CC2P	stm8s_stdperiph_driver\inc\stm8s.h	903;"	macro
TIM2_CCER1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	850;"	macro
TIM2_CCER2_CC3E	stm8s_stdperiph_driver\inc\stm8s.h	909;"	macro
TIM2_CCER2_CC3P	stm8s_stdperiph_driver\inc\stm8s.h	908;"	macro
TIM2_CCER2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	851;"	macro
TIM2_CCMR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	847;"	macro
TIM2_CCMR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	848;"	macro
TIM2_CCMR3_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	849;"	macro
TIM2_CCMR_CCxS	stm8s_stdperiph_driver\inc\stm8s.h	901;"	macro
TIM2_CCMR_ICxF	stm8s_stdperiph_driver\inc\stm8s.h	898;"	macro
TIM2_CCMR_ICxPSC	stm8s_stdperiph_driver\inc\stm8s.h	897;"	macro
TIM2_CCMR_OCM	stm8s_stdperiph_driver\inc\stm8s.h	899;"	macro
TIM2_CCMR_OCxPE	stm8s_stdperiph_driver\inc\stm8s.h	900;"	macro
TIM2_CCPreloadControl	stm8s_stdperiph_driver\inc\stm8s_tim2.h	297;"	prototype	signature:(FunctionalState NewState)
TIM2_CCR1H_CCR1	stm8s_stdperiph_driver\inc\stm8s.h	919;"	macro
TIM2_CCR1H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	857;"	macro
TIM2_CCR1L_CCR1	stm8s_stdperiph_driver\inc\stm8s.h	920;"	macro
TIM2_CCR1L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	858;"	macro
TIM2_CCR2H_CCR2	stm8s_stdperiph_driver\inc\stm8s.h	922;"	macro
TIM2_CCR2H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	859;"	macro
TIM2_CCR2L_CCR2	stm8s_stdperiph_driver\inc\stm8s.h	923;"	macro
TIM2_CCR2L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	860;"	macro
TIM2_CCR3H_CCR3	stm8s_stdperiph_driver\inc\stm8s.h	925;"	macro
TIM2_CCR3H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	861;"	macro
TIM2_CCR3L_CCR3	stm8s_stdperiph_driver\inc\stm8s.h	926;"	macro
TIM2_CCR3L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	862;"	macro
TIM2_CCxCmd	stm8s_stdperiph_driver\inc\stm8s_tim2.h	305;"	prototype	signature:(TIM2_Channel_TypeDef TIM2_Channel, FunctionalState NewState)
TIM2_CCxCmd	stm8s_stdperiph_driver\src\stm8s_tim2.c	759;"	function	signature:(TIM2_Channel_TypeDef TIM2_Channel, FunctionalState NewState)
TIM2_CHANNEL_1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	124;"	enumerator	enum:__anon32
TIM2_CHANNEL_2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	125;"	enumerator	enum:__anon32
TIM2_CHANNEL_3	stm8s_stdperiph_driver\inc\stm8s_tim2.h	126;"	enumerator	enum:__anon32
TIM2_CNTRH_CNT	stm8s_stdperiph_driver\inc\stm8s.h	911;"	macro
TIM2_CNTRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	852;"	macro
TIM2_CNTRL_CNT	stm8s_stdperiph_driver\inc\stm8s.h	912;"	macro
TIM2_CNTRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	853;"	macro
TIM2_CR1_ARPE	stm8s_stdperiph_driver\inc\stm8s.h	872;"	macro
TIM2_CR1_CEN	stm8s_stdperiph_driver\inc\stm8s.h	876;"	macro
TIM2_CR1_OPM	stm8s_stdperiph_driver\inc\stm8s.h	873;"	macro
TIM2_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	842;"	macro
TIM2_CR1_UDIS	stm8s_stdperiph_driver\inc\stm8s.h	875;"	macro
TIM2_CR1_URS	stm8s_stdperiph_driver\inc\stm8s.h	874;"	macro
TIM2_Channel_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	127;"	typedef	typeref:enum:__anon32
TIM2_ClearFlag	stm8s_stdperiph_driver\inc\stm8s_tim2.h	321;"	prototype	signature:(TIM2_FLAG_TypeDef TIM2_FLAG)
TIM2_ClearFlag	stm8s_stdperiph_driver\src\stm8s_tim2.c	1132;"	function	signature:(TIM2_FLAG_TypeDef TIM2_FLAG)
TIM2_ClearITPendingBit	stm8s_stdperiph_driver\inc\stm8s_tim2.h	323;"	prototype	signature:(TIM2_IT_TypeDef TIM2_IT)
TIM2_ClearITPendingBit	stm8s_stdperiph_driver\src\stm8s_tim2.c	1188;"	function	signature:(TIM2_IT_TypeDef TIM2_IT)
TIM2_Cmd	stm8s_stdperiph_driver\inc\stm8s_tim2.h	286;"	prototype	signature:(FunctionalState NewState)
TIM2_Cmd	stm8s_stdperiph_driver\src\stm8s_tim2.c	339;"	function	signature:(FunctionalState NewState)
TIM2_DeInit	stm8s_stdperiph_driver\inc\stm8s_tim2.h	279;"	prototype	signature:(void)
TIM2_DeInit	stm8s_stdperiph_driver\src\stm8s_tim2.c	46;"	function	signature:(void)
TIM2_EGR_CC1G	stm8s_stdperiph_driver\inc\stm8s.h	894;"	macro
TIM2_EGR_CC2G	stm8s_stdperiph_driver\inc\stm8s.h	893;"	macro
TIM2_EGR_CC3G	stm8s_stdperiph_driver\inc\stm8s.h	892;"	macro
TIM2_EGR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	846;"	macro
TIM2_EGR_UG	stm8s_stdperiph_driver\inc\stm8s.h	895;"	macro
TIM2_EVENTSOURCE_CC1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	228;"	enumerator	enum:__anon40
TIM2_EVENTSOURCE_CC2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	229;"	enumerator	enum:__anon40
TIM2_EVENTSOURCE_CC3	stm8s_stdperiph_driver\inc\stm8s_tim2.h	230;"	enumerator	enum:__anon40
TIM2_EVENTSOURCE_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	227;"	enumerator	enum:__anon40
TIM2_EventSource_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	231;"	typedef	typeref:enum:__anon40
TIM2_FLAG_CC1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	249;"	enumerator	enum:__anon42
TIM2_FLAG_CC1OF	stm8s_stdperiph_driver\inc\stm8s_tim2.h	252;"	enumerator	enum:__anon42
TIM2_FLAG_CC2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	250;"	enumerator	enum:__anon42
TIM2_FLAG_CC2OF	stm8s_stdperiph_driver\inc\stm8s_tim2.h	253;"	enumerator	enum:__anon42
TIM2_FLAG_CC3	stm8s_stdperiph_driver\inc\stm8s_tim2.h	251;"	enumerator	enum:__anon42
TIM2_FLAG_CC3OF	stm8s_stdperiph_driver\inc\stm8s_tim2.h	254;"	enumerator	enum:__anon42
TIM2_FLAG_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	255;"	typedef	typeref:enum:__anon42
TIM2_FLAG_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	248;"	enumerator	enum:__anon42
TIM2_FORCEDACTION_ACTIVE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	39;"	enumerator	enum:__anon28
TIM2_FORCEDACTION_INACTIVE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	40;"	enumerator	enum:__anon28
TIM2_ForcedAction_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	41;"	typedef	typeref:enum:__anon28
TIM2_ForcedOC1Config	stm8s_stdperiph_driver\inc\stm8s_tim2.h	293;"	prototype	signature:(TIM2_ForcedAction_TypeDef TIM2_ForcedAction)
TIM2_ForcedOC1Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	512;"	function	signature:(TIM2_ForcedAction_TypeDef TIM2_ForcedAction)
TIM2_ForcedOC2Config	stm8s_stdperiph_driver\inc\stm8s_tim2.h	294;"	prototype	signature:(TIM2_ForcedAction_TypeDef TIM2_ForcedAction)
TIM2_ForcedOC2Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	531;"	function	signature:(TIM2_ForcedAction_TypeDef TIM2_ForcedAction)
TIM2_ForcedOC3Config	stm8s_stdperiph_driver\inc\stm8s_tim2.h	295;"	prototype	signature:(TIM2_ForcedAction_TypeDef TIM2_ForcedAction)
TIM2_ForcedOC3Config	stm8s_stdperiph_driver\src\stm8s_tim2.c	550;"	function	signature:(TIM2_ForcedAction_TypeDef TIM2_ForcedAction)
TIM2_GenerateEvent	stm8s_stdperiph_driver\inc\stm8s_tim2.h	301;"	prototype	signature:(TIM2_EventSource_TypeDef TIM2_EventSource)
TIM2_GenerateEvent	stm8s_stdperiph_driver\src\stm8s_tim2.c	663;"	function	signature:(TIM2_EventSource_TypeDef TIM2_EventSource)
TIM2_GetCapture1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	315;"	prototype	signature:(void)
TIM2_GetCapture1	stm8s_stdperiph_driver\src\stm8s_tim2.c	1001;"	function	signature:(void)
TIM2_GetCapture2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	316;"	prototype	signature:(void)
TIM2_GetCapture2	stm8s_stdperiph_driver\src\stm8s_tim2.c	1021;"	function	signature:(void)
TIM2_GetCapture3	stm8s_stdperiph_driver\inc\stm8s_tim2.h	317;"	prototype	signature:(void)
TIM2_GetCapture3	stm8s_stdperiph_driver\src\stm8s_tim2.c	1041;"	function	signature:(void)
TIM2_GetCounter	stm8s_stdperiph_driver\inc\stm8s_tim2.h	318;"	prototype	signature:(void)
TIM2_GetCounter	stm8s_stdperiph_driver\src\stm8s_tim2.c	1061;"	function	signature:(void)
TIM2_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_tim2.h	320;"	prototype	signature:(TIM2_FLAG_TypeDef TIM2_FLAG)
TIM2_GetFlagStatus	stm8s_stdperiph_driver\src\stm8s_tim2.c	1096;"	function	signature:(TIM2_FLAG_TypeDef TIM2_FLAG)
TIM2_GetITStatus	stm8s_stdperiph_driver\inc\stm8s_tim2.h	322;"	prototype	signature:(TIM2_IT_TypeDef TIM2_IT)
TIM2_GetITStatus	stm8s_stdperiph_driver\src\stm8s_tim2.c	1154;"	function	signature:(TIM2_IT_TypeDef TIM2_IT)
TIM2_GetPrescaler	stm8s_stdperiph_driver\inc\stm8s_tim2.h	319;"	prototype	signature:(void)
TIM2_GetPrescaler	stm8s_stdperiph_driver\src\stm8s_tim2.c	1076;"	function	signature:(void)
TIM2_ICInit	stm8s_stdperiph_driver\inc\stm8s_tim2.h	284;"	prototype	signature:(TIM2_Channel_TypeDef TIM2_Channel, TIM2_ICPolarity_TypeDef TIM2_ICPolarity, TIM2_ICSelection_TypeDef TIM2_ICSelection, TIM2_ICPSC_TypeDef TIM2_ICPrescaler, uint8_t TIM2_ICFilter)
TIM2_ICInit	stm8s_stdperiph_driver\src\stm8s_tim2.c	210;"	function	signature:(TIM2_Channel_TypeDef TIM2_Channel, TIM2_ICPolarity_TypeDef TIM2_ICPolarity, TIM2_ICSelection_TypeDef TIM2_ICSelection, TIM2_ICPSC_TypeDef TIM2_ICPrescaler, uint8_t TIM2_ICFilter)
TIM2_ICPOLARITY_FALLING	stm8s_stdperiph_driver\inc\stm8s_tim2.h	160;"	enumerator	enum:__anon35
TIM2_ICPOLARITY_RISING	stm8s_stdperiph_driver\inc\stm8s_tim2.h	159;"	enumerator	enum:__anon35
TIM2_ICPSC_DIV1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	184;"	enumerator	enum:__anon37
TIM2_ICPSC_DIV2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	185;"	enumerator	enum:__anon37
TIM2_ICPSC_DIV4	stm8s_stdperiph_driver\inc\stm8s_tim2.h	186;"	enumerator	enum:__anon37
TIM2_ICPSC_DIV8	stm8s_stdperiph_driver\inc\stm8s_tim2.h	187;"	enumerator	enum:__anon37
TIM2_ICPSC_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	188;"	typedef	typeref:enum:__anon37
TIM2_ICPolarity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	161;"	typedef	typeref:enum:__anon35
TIM2_ICSELECTION_DIRECTTI	stm8s_stdperiph_driver\inc\stm8s_tim2.h	169;"	enumerator	enum:__anon36
TIM2_ICSELECTION_INDIRECTTI	stm8s_stdperiph_driver\inc\stm8s_tim2.h	170;"	enumerator	enum:__anon36
TIM2_ICSELECTION_TRGI	stm8s_stdperiph_driver\inc\stm8s_tim2.h	171;"	enumerator	enum:__anon36
TIM2_ICSelection_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	172;"	typedef	typeref:enum:__anon36
TIM2_IER_CC1IE	stm8s_stdperiph_driver\inc\stm8s.h	880;"	macro
TIM2_IER_CC2IE	stm8s_stdperiph_driver\inc\stm8s.h	879;"	macro
TIM2_IER_CC3IE	stm8s_stdperiph_driver\inc\stm8s.h	878;"	macro
TIM2_IER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	843;"	macro
TIM2_IER_UIE	stm8s_stdperiph_driver\inc\stm8s.h	881;"	macro
TIM2_ITConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	287;"	prototype	signature:(TIM2_IT_TypeDef TIM2_IT, FunctionalState NewState)
TIM2_ITConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	369;"	function	signature:(TIM2_IT_TypeDef TIM2_IT, FunctionalState NewState)
TIM2_IT_CC1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	202;"	enumerator	enum:__anon38
TIM2_IT_CC2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	203;"	enumerator	enum:__anon38
TIM2_IT_CC3	stm8s_stdperiph_driver\inc\stm8s_tim2.h	204;"	enumerator	enum:__anon38
TIM2_IT_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	205;"	typedef	typeref:enum:__anon38
TIM2_IT_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	201;"	enumerator	enum:__anon38
TIM2_InternalClockConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	288;"	prototype	signature:(void)
TIM2_OC1Init	stm8s_stdperiph_driver\inc\stm8s_tim2.h	281;"	prototype	signature:(TIM2_OCMode_TypeDef TIM2_OCMode, TIM2_OutputState_TypeDef TIM2_OutputState, uint16_t TIM2_Pulse, TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC1Init	stm8s_stdperiph_driver\src\stm8s_tim2.c	104;"	function	signature:(TIM2_OCMode_TypeDef TIM2_OCMode, TIM2_OutputState_TypeDef TIM2_OutputState, uint16_t TIM2_Pulse, TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC1PolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	302;"	prototype	signature:(TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC1PolarityConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	681;"	function	signature:(TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC1PreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	298;"	prototype	signature:(FunctionalState NewState)
TIM2_OC1PreloadConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	590;"	function	signature:(FunctionalState NewState)
TIM2_OC2Init	stm8s_stdperiph_driver\inc\stm8s_tim2.h	282;"	prototype	signature:(TIM2_OCMode_TypeDef TIM2_OCMode, TIM2_OutputState_TypeDef TIM2_OutputState, uint16_t TIM2_Pulse, TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC2Init	stm8s_stdperiph_driver\src\stm8s_tim2.c	138;"	function	signature:(TIM2_OCMode_TypeDef TIM2_OCMode, TIM2_OutputState_TypeDef TIM2_OutputState, uint16_t TIM2_Pulse, TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC2PolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	303;"	prototype	signature:(TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC2PolarityConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	706;"	function	signature:(TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC2PreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	299;"	prototype	signature:(FunctionalState NewState)
TIM2_OC2PreloadConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	613;"	function	signature:(FunctionalState NewState)
TIM2_OC3Init	stm8s_stdperiph_driver\inc\stm8s_tim2.h	283;"	prototype	signature:(TIM2_OCMode_TypeDef TIM2_OCMode, TIM2_OutputState_TypeDef TIM2_OutputState, uint16_t TIM2_Pulse, TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC3Init	stm8s_stdperiph_driver\src\stm8s_tim2.c	175;"	function	signature:(TIM2_OCMode_TypeDef TIM2_OCMode, TIM2_OutputState_TypeDef TIM2_OutputState, uint16_t TIM2_Pulse, TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC3PolarityConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	304;"	prototype	signature:(TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC3PolarityConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	731;"	function	signature:(TIM2_OCPolarity_TypeDef TIM2_OCPolarity)
TIM2_OC3PreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	300;"	prototype	signature:(FunctionalState NewState)
TIM2_OC3PreloadConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	636;"	function	signature:(FunctionalState NewState)
TIM2_OCMODE_ACTIVE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	88;"	enumerator	enum:__anon30
TIM2_OCMODE_INACTIVE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	89;"	enumerator	enum:__anon30
TIM2_OCMODE_PWM1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	91;"	enumerator	enum:__anon30
TIM2_OCMODE_PWM2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	92;"	enumerator	enum:__anon30
TIM2_OCMODE_TIMING	stm8s_stdperiph_driver\inc\stm8s_tim2.h	87;"	enumerator	enum:__anon30
TIM2_OCMODE_TOGGLE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	90;"	enumerator	enum:__anon30
TIM2_OCMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	93;"	typedef	typeref:enum:__anon30
TIM2_OCPOLARITY_HIGH	stm8s_stdperiph_driver\inc\stm8s_tim2.h	139;"	enumerator	enum:__anon33
TIM2_OCPOLARITY_LOW	stm8s_stdperiph_driver\inc\stm8s_tim2.h	140;"	enumerator	enum:__anon33
TIM2_OCPolarity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	141;"	typedef	typeref:enum:__anon33
TIM2_OPMODE_REPETITIVE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	115;"	enumerator	enum:__anon31
TIM2_OPMODE_SINGLE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	114;"	enumerator	enum:__anon31
TIM2_OPMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	116;"	typedef	typeref:enum:__anon31
TIM2_OUTPUTSTATE_DISABLE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	149;"	enumerator	enum:__anon34
TIM2_OUTPUTSTATE_ENABLE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	150;"	enumerator	enum:__anon34
TIM2_OutputState_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	151;"	typedef	typeref:enum:__anon34
TIM2_PRESCALER_1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	49;"	enumerator	enum:__anon29
TIM2_PRESCALER_1024	stm8s_stdperiph_driver\inc\stm8s_tim2.h	59;"	enumerator	enum:__anon29
TIM2_PRESCALER_128	stm8s_stdperiph_driver\inc\stm8s_tim2.h	56;"	enumerator	enum:__anon29
TIM2_PRESCALER_16	stm8s_stdperiph_driver\inc\stm8s_tim2.h	53;"	enumerator	enum:__anon29
TIM2_PRESCALER_16384	stm8s_stdperiph_driver\inc\stm8s_tim2.h	63;"	enumerator	enum:__anon29
TIM2_PRESCALER_2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	50;"	enumerator	enum:__anon29
TIM2_PRESCALER_2048	stm8s_stdperiph_driver\inc\stm8s_tim2.h	60;"	enumerator	enum:__anon29
TIM2_PRESCALER_256	stm8s_stdperiph_driver\inc\stm8s_tim2.h	57;"	enumerator	enum:__anon29
TIM2_PRESCALER_32	stm8s_stdperiph_driver\inc\stm8s_tim2.h	54;"	enumerator	enum:__anon29
TIM2_PRESCALER_32768	stm8s_stdperiph_driver\inc\stm8s_tim2.h	64;"	enumerator	enum:__anon29
TIM2_PRESCALER_4	stm8s_stdperiph_driver\inc\stm8s_tim2.h	51;"	enumerator	enum:__anon29
TIM2_PRESCALER_4096	stm8s_stdperiph_driver\inc\stm8s_tim2.h	61;"	enumerator	enum:__anon29
TIM2_PRESCALER_512	stm8s_stdperiph_driver\inc\stm8s_tim2.h	58;"	enumerator	enum:__anon29
TIM2_PRESCALER_64	stm8s_stdperiph_driver\inc\stm8s_tim2.h	55;"	enumerator	enum:__anon29
TIM2_PRESCALER_8	stm8s_stdperiph_driver\inc\stm8s_tim2.h	52;"	enumerator	enum:__anon29
TIM2_PRESCALER_8192	stm8s_stdperiph_driver\inc\stm8s_tim2.h	62;"	enumerator	enum:__anon29
TIM2_PSCRELOADMODE_IMMEDIATE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	218;"	enumerator	enum:__anon39
TIM2_PSCRELOADMODE_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim2.h	217;"	enumerator	enum:__anon39
TIM2_PSCR_PSC	stm8s_stdperiph_driver\inc\stm8s.h	914;"	macro
TIM2_PSCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	854;"	macro
TIM2_PSCReloadMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	219;"	typedef	typeref:enum:__anon39
TIM2_PWMIConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	285;"	prototype	signature:(TIM2_Channel_TypeDef TIM2_Channel, TIM2_ICPolarity_TypeDef TIM2_ICPolarity, TIM2_ICSelection_TypeDef TIM2_ICSelection, TIM2_ICPSC_TypeDef TIM2_ICPrescaler, uint8_t TIM2_ICFilter)
TIM2_PWMIConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	265;"	function	signature:(TIM2_Channel_TypeDef TIM2_Channel, TIM2_ICPolarity_TypeDef TIM2_ICPolarity, TIM2_ICSelection_TypeDef TIM2_ICSelection, TIM2_ICPSC_TypeDef TIM2_ICPrescaler, uint8_t TIM2_ICFilter)
TIM2_PrescalerConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	292;"	prototype	signature:(TIM2_Prescaler_TypeDef Prescaler, TIM2_PSCReloadMode_TypeDef TIM2_PSCReloadMode)
TIM2_PrescalerConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	489;"	function	signature:(TIM2_Prescaler_TypeDef Prescaler, TIM2_PSCReloadMode_TypeDef TIM2_PSCReloadMode)
TIM2_Prescaler_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	65;"	typedef	typeref:enum:__anon29
TIM2_SR1_CC1IF	stm8s_stdperiph_driver\inc\stm8s.h	885;"	macro
TIM2_SR1_CC2IF	stm8s_stdperiph_driver\inc\stm8s.h	884;"	macro
TIM2_SR1_CC3IF	stm8s_stdperiph_driver\inc\stm8s.h	883;"	macro
TIM2_SR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	844;"	macro
TIM2_SR1_UIF	stm8s_stdperiph_driver\inc\stm8s.h	886;"	macro
TIM2_SR2_CC1OF	stm8s_stdperiph_driver\inc\stm8s.h	890;"	macro
TIM2_SR2_CC2OF	stm8s_stdperiph_driver\inc\stm8s.h	889;"	macro
TIM2_SR2_CC3OF	stm8s_stdperiph_driver\inc\stm8s.h	888;"	macro
TIM2_SR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	845;"	macro
TIM2_SelectOCxM	stm8s_stdperiph_driver\inc\stm8s_tim2.h	306;"	prototype	signature:(TIM2_Channel_TypeDef TIM2_Channel, TIM2_OCMode_TypeDef TIM2_OCMode)
TIM2_SelectOCxM	stm8s_stdperiph_driver\src\stm8s_tim2.c	824;"	function	signature:(TIM2_Channel_TypeDef TIM2_Channel, TIM2_OCMode_TypeDef TIM2_OCMode)
TIM2_SelectOnePulseMode	stm8s_stdperiph_driver\inc\stm8s_tim2.h	291;"	prototype	signature:(TIM2_OPMode_TypeDef TIM2_OPMode)
TIM2_SelectOnePulseMode	stm8s_stdperiph_driver\src\stm8s_tim2.c	443;"	function	signature:(TIM2_OPMode_TypeDef TIM2_OPMode)
TIM2_SetAutoreload	stm8s_stdperiph_driver\inc\stm8s_tim2.h	308;"	prototype	signature:(uint16_t Autoreload)
TIM2_SetAutoreload	stm8s_stdperiph_driver\src\stm8s_tim2.c	881;"	function	signature:(uint16_t Autoreload)
TIM2_SetCompare1	stm8s_stdperiph_driver\inc\stm8s_tim2.h	309;"	prototype	signature:(uint16_t Compare1)
TIM2_SetCompare1	stm8s_stdperiph_driver\src\stm8s_tim2.c	897;"	function	signature:(uint16_t Compare1)
TIM2_SetCompare2	stm8s_stdperiph_driver\inc\stm8s_tim2.h	310;"	prototype	signature:(uint16_t Compare2)
TIM2_SetCompare2	stm8s_stdperiph_driver\src\stm8s_tim2.c	912;"	function	signature:(uint16_t Compare2)
TIM2_SetCompare3	stm8s_stdperiph_driver\inc\stm8s_tim2.h	311;"	prototype	signature:(uint16_t Compare3)
TIM2_SetCompare3	stm8s_stdperiph_driver\src\stm8s_tim2.c	927;"	function	signature:(uint16_t Compare3)
TIM2_SetCounter	stm8s_stdperiph_driver\inc\stm8s_tim2.h	307;"	prototype	signature:(uint16_t Counter)
TIM2_SetCounter	stm8s_stdperiph_driver\src\stm8s_tim2.c	866;"	function	signature:(uint16_t Counter)
TIM2_SetIC1Prescaler	stm8s_stdperiph_driver\inc\stm8s_tim2.h	312;"	prototype	signature:(TIM2_ICPSC_TypeDef TIM2_IC1Prescaler)
TIM2_SetIC1Prescaler	stm8s_stdperiph_driver\src\stm8s_tim2.c	946;"	function	signature:(TIM2_ICPSC_TypeDef TIM2_IC1Prescaler)
TIM2_SetIC2Prescaler	stm8s_stdperiph_driver\inc\stm8s_tim2.h	313;"	prototype	signature:(TIM2_ICPSC_TypeDef TIM2_IC2Prescaler)
TIM2_SetIC2Prescaler	stm8s_stdperiph_driver\src\stm8s_tim2.c	966;"	function	signature:(TIM2_ICPSC_TypeDef TIM2_IC2Prescaler)
TIM2_SetIC3Prescaler	stm8s_stdperiph_driver\inc\stm8s_tim2.h	314;"	prototype	signature:(TIM2_ICPSC_TypeDef TIM2_IC3Prescaler)
TIM2_SetIC3Prescaler	stm8s_stdperiph_driver\src\stm8s_tim2.c	986;"	function	signature:(TIM2_ICPSC_TypeDef TIM2_IC3Prescaler)
TIM2_TimeBaseInit	stm8s_stdperiph_driver\inc\stm8s_tim2.h	280;"	prototype	signature:(TIM2_Prescaler_TypeDef TIM2_Prescaler, uint16_t TIM2_Period)
TIM2_TimeBaseInit	stm8s_stdperiph_driver\src\stm8s_tim2.c	85;"	function	signature:( TIM2_Prescaler_TypeDef TIM2_Prescaler, uint16_t TIM2_Period)
TIM2_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	836;"	typedef	typeref:struct:TIM2_struct
TIM2_UPDATESOURCE_GLOBAL	stm8s_stdperiph_driver\inc\stm8s_tim2.h	238;"	enumerator	enum:__anon41
TIM2_UPDATESOURCE_REGULAR	stm8s_stdperiph_driver\inc\stm8s_tim2.h	239;"	enumerator	enum:__anon41
TIM2_UpdateDisableConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	289;"	prototype	signature:(FunctionalState NewState)
TIM2_UpdateDisableConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	394;"	function	signature:(FunctionalState NewState)
TIM2_UpdateRequestConfig	stm8s_stdperiph_driver\inc\stm8s_tim2.h	290;"	prototype	signature:(TIM2_UpdateSource_TypeDef TIM2_UpdateSource)
TIM2_UpdateRequestConfig	stm8s_stdperiph_driver\src\stm8s_tim2.c	418;"	function	signature:(TIM2_UpdateSource_TypeDef TIM2_UpdateSource)
TIM2_UpdateSource_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim2.h	240;"	typedef	typeref:enum:__anon41
TIM2_Update_IRQHandler	stm8_interrupt_vector.c	63;"	function	signature:(void)
TIM2_struct	stm8s_stdperiph_driver\inc\stm8s.h	808;"	struct
TIM3	stm8s_stdperiph_driver\inc\stm8s.h	2571;"	macro
TIM3_ARRH_ARR	stm8s_stdperiph_driver\inc\stm8s.h	1025;"	macro
TIM3_ARRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	973;"	macro
TIM3_ARRL_ARR	stm8s_stdperiph_driver\inc\stm8s.h	1026;"	macro
TIM3_ARRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	974;"	macro
TIM3_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2471;"	macro
TIM3_CCER1_CC1E	stm8s_stdperiph_driver\inc\stm8s.h	1018;"	macro
TIM3_CCER1_CC1P	stm8s_stdperiph_driver\inc\stm8s.h	1017;"	macro
TIM3_CCER1_CC2E	stm8s_stdperiph_driver\inc\stm8s.h	1016;"	macro
TIM3_CCER1_CC2P	stm8s_stdperiph_driver\inc\stm8s.h	1015;"	macro
TIM3_CCER1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	969;"	macro
TIM3_CCMR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	967;"	macro
TIM3_CCMR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	968;"	macro
TIM3_CCMR_CCxS	stm8s_stdperiph_driver\inc\stm8s.h	1013;"	macro
TIM3_CCMR_ICxF	stm8s_stdperiph_driver\inc\stm8s.h	1010;"	macro
TIM3_CCMR_ICxPSC	stm8s_stdperiph_driver\inc\stm8s.h	1009;"	macro
TIM3_CCMR_OCM	stm8s_stdperiph_driver\inc\stm8s.h	1011;"	macro
TIM3_CCMR_OCxPE	stm8s_stdperiph_driver\inc\stm8s.h	1012;"	macro
TIM3_CCR1H_CCR1	stm8s_stdperiph_driver\inc\stm8s.h	1028;"	macro
TIM3_CCR1H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	975;"	macro
TIM3_CCR1L_CCR1	stm8s_stdperiph_driver\inc\stm8s.h	1029;"	macro
TIM3_CCR1L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	976;"	macro
TIM3_CCR2H_CCR2	stm8s_stdperiph_driver\inc\stm8s.h	1031;"	macro
TIM3_CCR2H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	977;"	macro
TIM3_CCR2L_CCR2	stm8s_stdperiph_driver\inc\stm8s.h	1032;"	macro
TIM3_CCR2L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	978;"	macro
TIM3_CNTRH_CNT	stm8s_stdperiph_driver\inc\stm8s.h	1020;"	macro
TIM3_CNTRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	970;"	macro
TIM3_CNTRL_CNT	stm8s_stdperiph_driver\inc\stm8s.h	1021;"	macro
TIM3_CNTRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	971;"	macro
TIM3_CR1_ARPE	stm8s_stdperiph_driver\inc\stm8s.h	988;"	macro
TIM3_CR1_CEN	stm8s_stdperiph_driver\inc\stm8s.h	992;"	macro
TIM3_CR1_OPM	stm8s_stdperiph_driver\inc\stm8s.h	989;"	macro
TIM3_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	962;"	macro
TIM3_CR1_UDIS	stm8s_stdperiph_driver\inc\stm8s.h	991;"	macro
TIM3_CR1_URS	stm8s_stdperiph_driver\inc\stm8s.h	990;"	macro
TIM3_EGR_CC1G	stm8s_stdperiph_driver\inc\stm8s.h	1006;"	macro
TIM3_EGR_CC2G	stm8s_stdperiph_driver\inc\stm8s.h	1005;"	macro
TIM3_EGR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	966;"	macro
TIM3_EGR_UG	stm8s_stdperiph_driver\inc\stm8s.h	1007;"	macro
TIM3_IER_CC1IE	stm8s_stdperiph_driver\inc\stm8s.h	995;"	macro
TIM3_IER_CC2IE	stm8s_stdperiph_driver\inc\stm8s.h	994;"	macro
TIM3_IER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	963;"	macro
TIM3_IER_UIE	stm8s_stdperiph_driver\inc\stm8s.h	996;"	macro
TIM3_PSCR_PSC	stm8s_stdperiph_driver\inc\stm8s.h	1023;"	macro
TIM3_PSCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	972;"	macro
TIM3_SR1_CC1IF	stm8s_stdperiph_driver\inc\stm8s.h	999;"	macro
TIM3_SR1_CC2IF	stm8s_stdperiph_driver\inc\stm8s.h	998;"	macro
TIM3_SR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	964;"	macro
TIM3_SR1_UIF	stm8s_stdperiph_driver\inc\stm8s.h	1000;"	macro
TIM3_SR2_CC1OF	stm8s_stdperiph_driver\inc\stm8s.h	1003;"	macro
TIM3_SR2_CC2OF	stm8s_stdperiph_driver\inc\stm8s.h	1002;"	macro
TIM3_SR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	965;"	macro
TIM3_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	956;"	typedef	typeref:struct:TIM3_struct
TIM3_struct	stm8s_stdperiph_driver\inc\stm8s.h	936;"	struct
TIM4	stm8s_stdperiph_driver\inc\stm8s.h	2577;"	macro
TIM4_ARRPreloadConfig	stm8s_stdperiph_driver\inc\stm8s_tim4.h	140;"	prototype	signature:(FunctionalState NewState)
TIM4_ARR_ARR	stm8s_stdperiph_driver\inc\stm8s.h	1094;"	macro
TIM4_ARR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1068;"	macro
TIM4_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2472;"	macro
TIM4_CNTR_CNT	stm8s_stdperiph_driver\inc\stm8s.h	1090;"	macro
TIM4_CNTR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1066;"	macro
TIM4_CR1_ARPE	stm8s_stdperiph_driver\inc\stm8s.h	1078;"	macro
TIM4_CR1_CEN	stm8s_stdperiph_driver\inc\stm8s.h	1082;"	macro
TIM4_CR1_OPM	stm8s_stdperiph_driver\inc\stm8s.h	1079;"	macro
TIM4_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1062;"	macro
TIM4_CR1_UDIS	stm8s_stdperiph_driver\inc\stm8s.h	1081;"	macro
TIM4_CR1_URS	stm8s_stdperiph_driver\inc\stm8s.h	1080;"	macro
TIM4_ClearFlag	stm8s_stdperiph_driver\inc\stm8s_tim4.h	147;"	prototype	signature:(TIM4_FLAG_TypeDef TIM4_FLAG)
TIM4_ClearITPendingBit	stm8s_stdperiph_driver\inc\stm8s_tim4.h	149;"	prototype	signature:(TIM4_IT_TypeDef TIM4_IT)
TIM4_Cmd	stm8s_stdperiph_driver\inc\stm8s_tim4.h	134;"	prototype	signature:(FunctionalState NewState)
TIM4_DeInit	stm8s_stdperiph_driver\inc\stm8s_tim4.h	132;"	prototype	signature:(void)
TIM4_EGR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1065;"	macro
TIM4_EGR_UG	stm8s_stdperiph_driver\inc\stm8s.h	1088;"	macro
TIM4_EVENTSOURCE_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim4.h	96;"	enumerator	enum:__anon120
TIM4_EventSource_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim4.h	97;"	typedef	typeref:enum:__anon120
TIM4_FLAG_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim4.h	105;"	typedef	typeref:enum:__anon121
TIM4_FLAG_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim4.h	104;"	enumerator	enum:__anon121
TIM4_GenerateEvent	stm8s_stdperiph_driver\inc\stm8s_tim4.h	141;"	prototype	signature:(TIM4_EventSource_TypeDef TIM4_EventSource)
TIM4_GetCounter	stm8s_stdperiph_driver\inc\stm8s_tim4.h	144;"	prototype	signature:(void)
TIM4_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_tim4.h	146;"	prototype	signature:(TIM4_FLAG_TypeDef TIM4_FLAG)
TIM4_GetITStatus	stm8s_stdperiph_driver\inc\stm8s_tim4.h	148;"	prototype	signature:(TIM4_IT_TypeDef TIM4_IT)
TIM4_GetPrescaler	stm8s_stdperiph_driver\inc\stm8s_tim4.h	145;"	prototype	signature:(void)
TIM4_IER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1063;"	macro
TIM4_IER_UIE	stm8s_stdperiph_driver\inc\stm8s.h	1084;"	macro
TIM4_ITConfig	stm8s_stdperiph_driver\inc\stm8s_tim4.h	135;"	prototype	signature:(TIM4_IT_TypeDef TIM4_IT, FunctionalState NewState)
TIM4_IT_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim4.h	115;"	typedef	typeref:enum:__anon122
TIM4_IT_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim4.h	114;"	enumerator	enum:__anon122
TIM4_OPMODE_REPETITIVE	stm8s_stdperiph_driver\inc\stm8s_tim4.h	67;"	enumerator	enum:__anon117
TIM4_OPMODE_SINGLE	stm8s_stdperiph_driver\inc\stm8s_tim4.h	66;"	enumerator	enum:__anon117
TIM4_OPMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim4.h	68;"	typedef	typeref:enum:__anon117
TIM4_PRESCALER_1	stm8s_stdperiph_driver\inc\stm8s_tim4.h	44;"	enumerator	enum:__anon116
TIM4_PRESCALER_128	stm8s_stdperiph_driver\inc\stm8s_tim4.h	51;"	enumerator	enum:__anon116
TIM4_PRESCALER_16	stm8s_stdperiph_driver\inc\stm8s_tim4.h	48;"	enumerator	enum:__anon116
TIM4_PRESCALER_2	stm8s_stdperiph_driver\inc\stm8s_tim4.h	45;"	enumerator	enum:__anon116
TIM4_PRESCALER_32	stm8s_stdperiph_driver\inc\stm8s_tim4.h	49;"	enumerator	enum:__anon116
TIM4_PRESCALER_4	stm8s_stdperiph_driver\inc\stm8s_tim4.h	46;"	enumerator	enum:__anon116
TIM4_PRESCALER_64	stm8s_stdperiph_driver\inc\stm8s_tim4.h	50;"	enumerator	enum:__anon116
TIM4_PRESCALER_8	stm8s_stdperiph_driver\inc\stm8s_tim4.h	47;"	enumerator	enum:__anon116
TIM4_PSCRELOADMODE_IMMEDIATE	stm8s_stdperiph_driver\inc\stm8s_tim4.h	77;"	enumerator	enum:__anon118
TIM4_PSCRELOADMODE_UPDATE	stm8s_stdperiph_driver\inc\stm8s_tim4.h	76;"	enumerator	enum:__anon118
TIM4_PSCR_PSC	stm8s_stdperiph_driver\inc\stm8s.h	1092;"	macro
TIM4_PSCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1067;"	macro
TIM4_PSCReloadMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim4.h	78;"	typedef	typeref:enum:__anon118
TIM4_PrescalerConfig	stm8s_stdperiph_driver\inc\stm8s_tim4.h	139;"	prototype	signature:(TIM4_Prescaler_TypeDef Prescaler, TIM4_PSCReloadMode_TypeDef TIM4_PSCReloadMode)
TIM4_Prescaler_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim4.h	52;"	typedef	typeref:enum:__anon116
TIM4_SR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1064;"	macro
TIM4_SR1_UIF	stm8s_stdperiph_driver\inc\stm8s.h	1086;"	macro
TIM4_SelectOnePulseMode	stm8s_stdperiph_driver\inc\stm8s_tim4.h	138;"	prototype	signature:(TIM4_OPMode_TypeDef TIM4_OPMode)
TIM4_SetAutoreload	stm8s_stdperiph_driver\inc\stm8s_tim4.h	143;"	prototype	signature:(uint8_t Autoreload)
TIM4_SetCounter	stm8s_stdperiph_driver\inc\stm8s_tim4.h	142;"	prototype	signature:(uint8_t Counter)
TIM4_TimeBaseInit	stm8s_stdperiph_driver\inc\stm8s_tim4.h	133;"	prototype	signature:(TIM4_Prescaler_TypeDef TIM4_Prescaler, uint8_t TIM4_Period)
TIM4_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1056;"	typedef	typeref:struct:TIM4_struct
TIM4_UPDATESOURCE_GLOBAL	stm8s_stdperiph_driver\inc\stm8s_tim4.h	86;"	enumerator	enum:__anon119
TIM4_UPDATESOURCE_REGULAR	stm8s_stdperiph_driver\inc\stm8s_tim4.h	87;"	enumerator	enum:__anon119
TIM4_UpdateDisableConfig	stm8s_stdperiph_driver\inc\stm8s_tim4.h	136;"	prototype	signature:(FunctionalState NewState)
TIM4_UpdateRequestConfig	stm8s_stdperiph_driver\inc\stm8s_tim4.h	137;"	prototype	signature:(TIM4_UpdateSource_TypeDef TIM4_UpdateSource)
TIM4_UpdateSource_TypeDef	stm8s_stdperiph_driver\inc\stm8s_tim4.h	88;"	typedef	typeref:enum:__anon119
TIM4_struct	stm8s_stdperiph_driver\inc\stm8s.h	1042;"	struct
TIM5	stm8s_stdperiph_driver\inc\stm8s.h	2581;"	macro
TIM5_ARRH_ARR	stm8s_stdperiph_driver\inc\stm8s.h	1222;"	macro
TIM5_ARRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1151;"	macro
TIM5_ARRL_ARR	stm8s_stdperiph_driver\inc\stm8s.h	1223;"	macro
TIM5_ARRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1152;"	macro
TIM5_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2473;"	macro
TIM5_CCER1_CC1E	stm8s_stdperiph_driver\inc\stm8s.h	1212;"	macro
TIM5_CCER1_CC1P	stm8s_stdperiph_driver\inc\stm8s.h	1211;"	macro
TIM5_CCER1_CC2E	stm8s_stdperiph_driver\inc\stm8s.h	1210;"	macro
TIM5_CCER1_CC2P	stm8s_stdperiph_driver\inc\stm8s.h	1209;"	macro
TIM5_CCER1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1146;"	macro
TIM5_CCER2_CC3E	stm8s_stdperiph_driver\inc\stm8s.h	1215;"	macro
TIM5_CCER2_CC3P	stm8s_stdperiph_driver\inc\stm8s.h	1214;"	macro
TIM5_CCER2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1147;"	macro
TIM5_CCMR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1143;"	macro
TIM5_CCMR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1144;"	macro
TIM5_CCMR3_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1145;"	macro
TIM5_CCMR_CCxS	stm8s_stdperiph_driver\inc\stm8s.h	1207;"	macro
TIM5_CCMR_ICxF	stm8s_stdperiph_driver\inc\stm8s.h	1204;"	macro
TIM5_CCMR_ICxPSC	stm8s_stdperiph_driver\inc\stm8s.h	1203;"	macro
TIM5_CCMR_OCM	stm8s_stdperiph_driver\inc\stm8s.h	1205;"	macro
TIM5_CCMR_OCxPE	stm8s_stdperiph_driver\inc\stm8s.h	1206;"	macro
TIM5_CCMR_TIxDirect_Set	stm8s_stdperiph_driver\inc\stm8s.h	1234;"	macro
TIM5_CCR1H_CCR1	stm8s_stdperiph_driver\inc\stm8s.h	1225;"	macro
TIM5_CCR1H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1153;"	macro
TIM5_CCR1L_CCR1	stm8s_stdperiph_driver\inc\stm8s.h	1226;"	macro
TIM5_CCR1L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1154;"	macro
TIM5_CCR2H_CCR2	stm8s_stdperiph_driver\inc\stm8s.h	1228;"	macro
TIM5_CCR2H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1155;"	macro
TIM5_CCR2L_CCR2	stm8s_stdperiph_driver\inc\stm8s.h	1229;"	macro
TIM5_CCR2L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1156;"	macro
TIM5_CCR3H_CCR3	stm8s_stdperiph_driver\inc\stm8s.h	1231;"	macro
TIM5_CCR3H_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1157;"	macro
TIM5_CCR3L_CCR3	stm8s_stdperiph_driver\inc\stm8s.h	1232;"	macro
TIM5_CCR3L_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1158;"	macro
TIM5_CNTRH_CNT	stm8s_stdperiph_driver\inc\stm8s.h	1217;"	macro
TIM5_CNTRH_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1148;"	macro
TIM5_CNTRL_CNT	stm8s_stdperiph_driver\inc\stm8s.h	1218;"	macro
TIM5_CNTRL_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1149;"	macro
TIM5_CR1_ARPE	stm8s_stdperiph_driver\inc\stm8s.h	1168;"	macro
TIM5_CR1_CEN	stm8s_stdperiph_driver\inc\stm8s.h	1172;"	macro
TIM5_CR1_OPM	stm8s_stdperiph_driver\inc\stm8s.h	1169;"	macro
TIM5_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1136;"	macro
TIM5_CR1_UDIS	stm8s_stdperiph_driver\inc\stm8s.h	1171;"	macro
TIM5_CR1_URS	stm8s_stdperiph_driver\inc\stm8s.h	1170;"	macro
TIM5_CR2_MMS	stm8s_stdperiph_driver\inc\stm8s.h	1175;"	macro
TIM5_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1137;"	macro
TIM5_CR2_TI1S	stm8s_stdperiph_driver\inc\stm8s.h	1174;"	macro
TIM5_EGR_CC1G	stm8s_stdperiph_driver\inc\stm8s.h	1200;"	macro
TIM5_EGR_CC2G	stm8s_stdperiph_driver\inc\stm8s.h	1199;"	macro
TIM5_EGR_CC3G	stm8s_stdperiph_driver\inc\stm8s.h	1198;"	macro
TIM5_EGR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1142;"	macro
TIM5_EGR_TG	stm8s_stdperiph_driver\inc\stm8s.h	1197;"	macro
TIM5_EGR_UG	stm8s_stdperiph_driver\inc\stm8s.h	1201;"	macro
TIM5_IER_CC1IE	stm8s_stdperiph_driver\inc\stm8s.h	1184;"	macro
TIM5_IER_CC2IE	stm8s_stdperiph_driver\inc\stm8s.h	1183;"	macro
TIM5_IER_CC3IE	stm8s_stdperiph_driver\inc\stm8s.h	1182;"	macro
TIM5_IER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1139;"	macro
TIM5_IER_TIE	stm8s_stdperiph_driver\inc\stm8s.h	1181;"	macro
TIM5_IER_UIE	stm8s_stdperiph_driver\inc\stm8s.h	1185;"	macro
TIM5_PSCR_PSC	stm8s_stdperiph_driver\inc\stm8s.h	1220;"	macro
TIM5_PSCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1150;"	macro
TIM5_SMCR_MSM	stm8s_stdperiph_driver\inc\stm8s.h	1177;"	macro
TIM5_SMCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1138;"	macro
TIM5_SMCR_SMS	stm8s_stdperiph_driver\inc\stm8s.h	1179;"	macro
TIM5_SMCR_TS	stm8s_stdperiph_driver\inc\stm8s.h	1178;"	macro
TIM5_SR1_CC1IF	stm8s_stdperiph_driver\inc\stm8s.h	1190;"	macro
TIM5_SR1_CC2IF	stm8s_stdperiph_driver\inc\stm8s.h	1189;"	macro
TIM5_SR1_CC3IF	stm8s_stdperiph_driver\inc\stm8s.h	1188;"	macro
TIM5_SR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1140;"	macro
TIM5_SR1_TIF	stm8s_stdperiph_driver\inc\stm8s.h	1187;"	macro
TIM5_SR1_UIF	stm8s_stdperiph_driver\inc\stm8s.h	1191;"	macro
TIM5_SR2_CC1OF	stm8s_stdperiph_driver\inc\stm8s.h	1195;"	macro
TIM5_SR2_CC2OF	stm8s_stdperiph_driver\inc\stm8s.h	1194;"	macro
TIM5_SR2_CC3OF	stm8s_stdperiph_driver\inc\stm8s.h	1193;"	macro
TIM5_SR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1141;"	macro
TIM5_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1130;"	typedef	typeref:struct:TIM5_struct
TIM5_struct	stm8s_stdperiph_driver\inc\stm8s.h	1105;"	struct
TIM6	stm8s_stdperiph_driver\inc\stm8s.h	2582;"	macro
TIM6_ARR_ARR	stm8s_stdperiph_driver\inc\stm8s.h	1303;"	macro
TIM6_ARR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1268;"	macro
TIM6_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2474;"	macro
TIM6_CNTR_CNT	stm8s_stdperiph_driver\inc\stm8s.h	1299;"	macro
TIM6_CNTR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1266;"	macro
TIM6_CR1_ARPE	stm8s_stdperiph_driver\inc\stm8s.h	1278;"	macro
TIM6_CR1_CEN	stm8s_stdperiph_driver\inc\stm8s.h	1282;"	macro
TIM6_CR1_OPM	stm8s_stdperiph_driver\inc\stm8s.h	1279;"	macro
TIM6_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1260;"	macro
TIM6_CR1_UDIS	stm8s_stdperiph_driver\inc\stm8s.h	1281;"	macro
TIM6_CR1_URS	stm8s_stdperiph_driver\inc\stm8s.h	1280;"	macro
TIM6_CR2_MMS	stm8s_stdperiph_driver\inc\stm8s.h	1284;"	macro
TIM6_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1261;"	macro
TIM6_EGR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1265;"	macro
TIM6_EGR_TG	stm8s_stdperiph_driver\inc\stm8s.h	1296;"	macro
TIM6_EGR_UG	stm8s_stdperiph_driver\inc\stm8s.h	1297;"	macro
TIM6_IER_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1263;"	macro
TIM6_IER_TIE	stm8s_stdperiph_driver\inc\stm8s.h	1290;"	macro
TIM6_IER_UIE	stm8s_stdperiph_driver\inc\stm8s.h	1291;"	macro
TIM6_PSCR_PSC	stm8s_stdperiph_driver\inc\stm8s.h	1301;"	macro
TIM6_PSCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1267;"	macro
TIM6_SMCR_MSM	stm8s_stdperiph_driver\inc\stm8s.h	1286;"	macro
TIM6_SMCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1262;"	macro
TIM6_SMCR_SMS	stm8s_stdperiph_driver\inc\stm8s.h	1288;"	macro
TIM6_SMCR_TS	stm8s_stdperiph_driver\inc\stm8s.h	1287;"	macro
TIM6_SR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1264;"	macro
TIM6_SR1_TIF	stm8s_stdperiph_driver\inc\stm8s.h	1293;"	macro
TIM6_SR1_UIF	stm8s_stdperiph_driver\inc\stm8s.h	1294;"	macro
TIM6_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1256;"	typedef	typeref:struct:TIM6_struct
TIM6_struct	stm8s_stdperiph_driver\inc\stm8s.h	1244;"	struct
TIM_Configuration	user\config.c	58;"	function	signature:(void)
TIM_Configuration	user\main.h	142;"	prototype	signature:(void)
TINY	stm8s_stdperiph_driver\inc\stm8s.h	114;"	macro
TINY	stm8s_stdperiph_driver\inc\stm8s.h	120;"	macro
TINY	stm8s_stdperiph_driver\inc\stm8s.h	134;"	macro
TMNAT_DELAY	user\main.h	111;"	macro
TPR	stm8s_stdperiph_driver\inc\stm8s.h	2055;"	member	struct:__anon5
TRISER	stm8s_stdperiph_driver\inc\stm8s.h	1327;"	member	struct:I2C_struct
TRUE	stm8s_stdperiph_driver\inc\stm8s.h	219;"	enumerator	enum:__anon1
TSR	stm8s_stdperiph_driver\inc\stm8s.h	2054;"	member	struct:__anon5
TXCRCR	stm8s_stdperiph_driver\inc\stm8s.h	1689;"	member	struct:SPI_struct
TmnatDelay	user\main.c	7;"	variable
TxMailbox	stm8s_stdperiph_driver\inc\stm8s.h	2082;"	member	union:__anon5::__anon6	typeref:struct:__anon5::__anon6::__anon7
U16_MAX	stm8s_stdperiph_driver\inc\stm8s.h	231;"	macro
U32_MAX	stm8s_stdperiph_driver\inc\stm8s.h	234;"	macro
U8_MAX	stm8s_stdperiph_driver\inc\stm8s.h	228;"	macro
UART1	stm8s_stdperiph_driver\inc\stm8s.h	2549;"	macro
UART1_ADDRESS_MAX	stm8s_stdperiph_driver\inc\stm8s_uart1.h	326;"	macro
UART1_BRR1_DIVM	stm8s_stdperiph_driver\inc\stm8s.h	1799;"	macro
UART1_BRR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1772;"	macro
UART1_BRR2_DIVF	stm8s_stdperiph_driver\inc\stm8s.h	1802;"	macro
UART1_BRR2_DIVM	stm8s_stdperiph_driver\inc\stm8s.h	1801;"	macro
UART1_BRR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1773;"	macro
UART1_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2466;"	macro
UART1_CR1_M	stm8s_stdperiph_driver\inc\stm8s.h	1807;"	macro
UART1_CR1_PCEN	stm8s_stdperiph_driver\inc\stm8s.h	1809;"	macro
UART1_CR1_PIEN	stm8s_stdperiph_driver\inc\stm8s.h	1811;"	macro
UART1_CR1_PS	stm8s_stdperiph_driver\inc\stm8s.h	1810;"	macro
UART1_CR1_R8	stm8s_stdperiph_driver\inc\stm8s.h	1804;"	macro
UART1_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1774;"	macro
UART1_CR1_T8	stm8s_stdperiph_driver\inc\stm8s.h	1805;"	macro
UART1_CR1_UARTD	stm8s_stdperiph_driver\inc\stm8s.h	1806;"	macro
UART1_CR1_WAKE	stm8s_stdperiph_driver\inc\stm8s.h	1808;"	macro
UART1_CR2_ILIEN	stm8s_stdperiph_driver\inc\stm8s.h	1816;"	macro
UART1_CR2_REN	stm8s_stdperiph_driver\inc\stm8s.h	1818;"	macro
UART1_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1775;"	macro
UART1_CR2_RIEN	stm8s_stdperiph_driver\inc\stm8s.h	1815;"	macro
UART1_CR2_RWU	stm8s_stdperiph_driver\inc\stm8s.h	1819;"	macro
UART1_CR2_SBK	stm8s_stdperiph_driver\inc\stm8s.h	1820;"	macro
UART1_CR2_TCIEN	stm8s_stdperiph_driver\inc\stm8s.h	1814;"	macro
UART1_CR2_TEN	stm8s_stdperiph_driver\inc\stm8s.h	1817;"	macro
UART1_CR2_TIEN	stm8s_stdperiph_driver\inc\stm8s.h	1813;"	macro
UART1_CR3_CKEN	stm8s_stdperiph_driver\inc\stm8s.h	1824;"	macro
UART1_CR3_CPHA	stm8s_stdperiph_driver\inc\stm8s.h	1826;"	macro
UART1_CR3_CPOL	stm8s_stdperiph_driver\inc\stm8s.h	1825;"	macro
UART1_CR3_LBCL	stm8s_stdperiph_driver\inc\stm8s.h	1827;"	macro
UART1_CR3_LINEN	stm8s_stdperiph_driver\inc\stm8s.h	1822;"	macro
UART1_CR3_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1776;"	macro
UART1_CR3_STOP	stm8s_stdperiph_driver\inc\stm8s.h	1823;"	macro
UART1_CR4_ADD	stm8s_stdperiph_driver\inc\stm8s.h	1832;"	macro
UART1_CR4_LBDF	stm8s_stdperiph_driver\inc\stm8s.h	1831;"	macro
UART1_CR4_LBDIEN	stm8s_stdperiph_driver\inc\stm8s.h	1829;"	macro
UART1_CR4_LBDL	stm8s_stdperiph_driver\inc\stm8s.h	1830;"	macro
UART1_CR4_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1777;"	macro
UART1_CR5_HDSEL	stm8s_stdperiph_driver\inc\stm8s.h	1836;"	macro
UART1_CR5_IREN	stm8s_stdperiph_driver\inc\stm8s.h	1838;"	macro
UART1_CR5_IRLP	stm8s_stdperiph_driver\inc\stm8s.h	1837;"	macro
UART1_CR5_NACK	stm8s_stdperiph_driver\inc\stm8s.h	1835;"	macro
UART1_CR5_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1778;"	macro
UART1_CR5_SCEN	stm8s_stdperiph_driver\inc\stm8s.h	1834;"	macro
UART1_ClearFlag	stm8s_stdperiph_driver\inc\stm8s_uart1.h	363;"	prototype	signature:(UART1_Flag_TypeDef UART1_FLAG)
UART1_ClearITPendingBit	stm8s_stdperiph_driver\inc\stm8s_uart1.h	365;"	prototype	signature:(UART1_IT_TypeDef UART1_IT)
UART1_Cmd	stm8s_stdperiph_driver\inc\stm8s_uart1.h	343;"	prototype	signature:(FunctionalState NewState)
UART1_DeInit	stm8s_stdperiph_driver\inc\stm8s_uart1.h	339;"	prototype	signature:(void)
UART1_FLAG_FE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	119;"	enumerator	enum:__anon131
UART1_FLAG_IDLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	116;"	enumerator	enum:__anon131
UART1_FLAG_LBDF	stm8s_stdperiph_driver\inc\stm8s_uart1.h	121;"	enumerator	enum:__anon131
UART1_FLAG_NF	stm8s_stdperiph_driver\inc\stm8s_uart1.h	118;"	enumerator	enum:__anon131
UART1_FLAG_OR	stm8s_stdperiph_driver\inc\stm8s_uart1.h	117;"	enumerator	enum:__anon131
UART1_FLAG_PE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	120;"	enumerator	enum:__anon131
UART1_FLAG_RXNE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	115;"	enumerator	enum:__anon131
UART1_FLAG_SBK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	122;"	enumerator	enum:__anon131
UART1_FLAG_TC	stm8s_stdperiph_driver\inc\stm8s_uart1.h	114;"	enumerator	enum:__anon131
UART1_FLAG_TXE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	113;"	enumerator	enum:__anon131
UART1_Flag_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	123;"	typedef	typeref:enum:__anon131
UART1_GTR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1779;"	macro
UART1_GetFlagStatus	stm8s_stdperiph_driver\inc\stm8s_uart1.h	362;"	prototype	signature:(UART1_Flag_TypeDef UART1_FLAG)
UART1_GetITStatus	stm8s_stdperiph_driver\inc\stm8s_uart1.h	364;"	prototype	signature:(UART1_IT_TypeDef UART1_IT)
UART1_HalfDuplexCmd	stm8s_stdperiph_driver\inc\stm8s_uart1.h	345;"	prototype	signature:(FunctionalState NewState)
UART1_IRDAMODE_LOWPOWER	stm8s_stdperiph_driver\inc\stm8s_uart1.h	45;"	enumerator	enum:__anon123
UART1_IRDAMODE_NORMAL	stm8s_stdperiph_driver\inc\stm8s_uart1.h	44;"	enumerator	enum:__anon123
UART1_ITConfig	stm8s_stdperiph_driver\inc\stm8s_uart1.h	344;"	prototype	signature:(UART1_IT_TypeDef UART1_IT, FunctionalState NewState)
UART1_IT_IDLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	155;"	enumerator	enum:__anon132
UART1_IT_LBDF	stm8s_stdperiph_driver\inc\stm8s_uart1.h	158;"	enumerator	enum:__anon132
UART1_IT_OR	stm8s_stdperiph_driver\inc\stm8s_uart1.h	156;"	enumerator	enum:__anon132
UART1_IT_PE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	157;"	enumerator	enum:__anon132
UART1_IT_RXNE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	154;"	enumerator	enum:__anon132
UART1_IT_RXNE_OR	stm8s_stdperiph_driver\inc\stm8s_uart1.h	159;"	enumerator	enum:__anon132
UART1_IT_TC	stm8s_stdperiph_driver\inc\stm8s_uart1.h	153;"	enumerator	enum:__anon132
UART1_IT_TXE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	152;"	enumerator	enum:__anon132
UART1_IT_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	160;"	typedef	typeref:enum:__anon132
UART1_Init	stm8s_stdperiph_driver\inc\stm8s_uart1.h	340;"	prototype	signature:(uint32_t BaudRate, UART1_WordLength_TypeDef WordLength, UART1_StopBits_TypeDef StopBits, UART1_Parity_TypeDef Parity, UART1_SyncMode_TypeDef SyncMode, UART1_Mode_TypeDef Mode)
UART1_IrDACmd	stm8s_stdperiph_driver\inc\stm8s_uart1.h	347;"	prototype	signature:(FunctionalState NewState)
UART1_IrDAConfig	stm8s_stdperiph_driver\inc\stm8s_uart1.h	346;"	prototype	signature:(UART1_IrDAMode_TypeDef UART1_IrDAMode)
UART1_IrDAMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	46;"	typedef	typeref:enum:__anon123
UART1_LINBREAKDETECTIONLENGTH_10BITS	stm8s_stdperiph_driver\inc\stm8s_uart1.h	58;"	enumerator	enum:__anon125
UART1_LINBREAKDETECTIONLENGTH_11BITS	stm8s_stdperiph_driver\inc\stm8s_uart1.h	59;"	enumerator	enum:__anon125
UART1_LINBreakDetectionConfig	stm8s_stdperiph_driver\inc\stm8s_uart1.h	348;"	prototype	signature:(UART1_LINBreakDetectionLength_TypeDef UART1_LINBreakDetectionLength)
UART1_LINBreakDetectionLength_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	60;"	typedef	typeref:enum:__anon125
UART1_LINCmd	stm8s_stdperiph_driver\inc\stm8s_uart1.h	349;"	prototype	signature:(FunctionalState NewState)
UART1_MODE_RX_DISABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	106;"	enumerator	enum:__anon130
UART1_MODE_RX_ENABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	103;"	enumerator	enum:__anon130
UART1_MODE_TXRX_ENABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	107;"	enumerator	enum:__anon130
UART1_MODE_TX_DISABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	105;"	enumerator	enum:__anon130
UART1_MODE_TX_ENABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	104;"	enumerator	enum:__anon130
UART1_Mode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	108;"	typedef	typeref:enum:__anon130
UART1_PARITY_EVEN	stm8s_stdperiph_driver\inc\stm8s_uart1.h	76;"	enumerator	enum:__anon127
UART1_PARITY_NO	stm8s_stdperiph_driver\inc\stm8s_uart1.h	75;"	enumerator	enum:__anon127
UART1_PARITY_ODD	stm8s_stdperiph_driver\inc\stm8s_uart1.h	77;"	enumerator	enum:__anon127
UART1_PSCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1780;"	macro
UART1_Parity_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	78;"	typedef	typeref:enum:__anon127
UART1_ReceiveData8	stm8s_stdperiph_driver\inc\stm8s_uart1.h	354;"	prototype	signature:(void)
UART1_ReceiveData9	stm8s_stdperiph_driver\inc\stm8s_uart1.h	355;"	prototype	signature:(void)
UART1_ReceiverWakeUpCmd	stm8s_stdperiph_driver\inc\stm8s_uart1.h	353;"	prototype	signature:(FunctionalState NewState)
UART1_SR_FE	stm8s_stdperiph_driver\inc\stm8s.h	1796;"	macro
UART1_SR_IDLE	stm8s_stdperiph_driver\inc\stm8s.h	1793;"	macro
UART1_SR_NF	stm8s_stdperiph_driver\inc\stm8s.h	1795;"	macro
UART1_SR_OR	stm8s_stdperiph_driver\inc\stm8s.h	1794;"	macro
UART1_SR_PE	stm8s_stdperiph_driver\inc\stm8s.h	1797;"	macro
UART1_SR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1771;"	macro
UART1_SR_RXNE	stm8s_stdperiph_driver\inc\stm8s.h	1792;"	macro
UART1_SR_TC	stm8s_stdperiph_driver\inc\stm8s.h	1791;"	macro
UART1_SR_TXE	stm8s_stdperiph_driver\inc\stm8s.h	1790;"	macro
UART1_STOPBITS_0_5	stm8s_stdperiph_driver\inc\stm8s_uart1.h	67;"	enumerator	enum:__anon126
UART1_STOPBITS_1	stm8s_stdperiph_driver\inc\stm8s_uart1.h	66;"	enumerator	enum:__anon126
UART1_STOPBITS_1_5	stm8s_stdperiph_driver\inc\stm8s_uart1.h	69;"	enumerator	enum:__anon126
UART1_STOPBITS_2	stm8s_stdperiph_driver\inc\stm8s_uart1.h	68;"	enumerator	enum:__anon126
UART1_SYNCMODE_CLOCK_DISABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	83;"	enumerator	enum:__anon128
UART1_SYNCMODE_CLOCK_ENABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	84;"	enumerator	enum:__anon128
UART1_SYNCMODE_CPHA_BEGINING	stm8s_stdperiph_driver\inc\stm8s_uart1.h	88;"	enumerator	enum:__anon128
UART1_SYNCMODE_CPHA_MIDDLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	87;"	enumerator	enum:__anon128
UART1_SYNCMODE_CPOL_HIGH	stm8s_stdperiph_driver\inc\stm8s_uart1.h	86;"	enumerator	enum:__anon128
UART1_SYNCMODE_CPOL_LOW	stm8s_stdperiph_driver\inc\stm8s_uart1.h	85;"	enumerator	enum:__anon128
UART1_SYNCMODE_LASTBIT_DISABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	89;"	enumerator	enum:__anon128
UART1_SYNCMODE_LASTBIT_ENABLE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	90;"	enumerator	enum:__anon128
UART1_SendBreak	stm8s_stdperiph_driver\inc\stm8s_uart1.h	358;"	prototype	signature:(void)
UART1_SendData8	stm8s_stdperiph_driver\inc\stm8s_uart1.h	356;"	prototype	signature:(uint8_t Data)
UART1_SendData9	stm8s_stdperiph_driver\inc\stm8s_uart1.h	357;"	prototype	signature:(uint16_t Data)
UART1_SetAddress	stm8s_stdperiph_driver\inc\stm8s_uart1.h	359;"	prototype	signature:(uint8_t UART1_Address)
UART1_SetGuardTime	stm8s_stdperiph_driver\inc\stm8s_uart1.h	360;"	prototype	signature:(uint8_t UART1_GuardTime)
UART1_SetPrescaler	stm8s_stdperiph_driver\inc\stm8s_uart1.h	361;"	prototype	signature:(uint8_t UART1_Prescaler)
UART1_SmartCardCmd	stm8s_stdperiph_driver\inc\stm8s_uart1.h	350;"	prototype	signature:(FunctionalState NewState)
UART1_SmartCardNACKCmd	stm8s_stdperiph_driver\inc\stm8s_uart1.h	351;"	prototype	signature:(FunctionalState NewState)
UART1_StopBits_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	70;"	typedef	typeref:enum:__anon126
UART1_SyncMode_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	91;"	typedef	typeref:enum:__anon128
UART1_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1765;"	typedef	typeref:struct:UART1_struct
UART1_WAKEUP_ADDRESSMARK	stm8s_stdperiph_driver\inc\stm8s_uart1.h	52;"	enumerator	enum:__anon124
UART1_WAKEUP_IDLELINE	stm8s_stdperiph_driver\inc\stm8s_uart1.h	51;"	enumerator	enum:__anon124
UART1_WORDLENGTH_8D	stm8s_stdperiph_driver\inc\stm8s_uart1.h	96;"	enumerator	enum:__anon129
UART1_WORDLENGTH_9D	stm8s_stdperiph_driver\inc\stm8s_uart1.h	97;"	enumerator	enum:__anon129
UART1_WakeUpConfig	stm8s_stdperiph_driver\inc\stm8s_uart1.h	352;"	prototype	signature:(UART1_WakeUp_TypeDef UART1_WakeUp)
UART1_WakeUp_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	53;"	typedef	typeref:enum:__anon124
UART1_WordLength_TypeDef	stm8s_stdperiph_driver\inc\stm8s_uart1.h	98;"	typedef	typeref:enum:__anon129
UART1_struct	stm8s_stdperiph_driver\inc\stm8s.h	1751;"	struct
UART2	stm8s_stdperiph_driver\inc\stm8s.h	2553;"	macro
UART2_BRR1_DIVM	stm8s_stdperiph_driver\inc\stm8s.h	1899;"	macro
UART2_BRR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1871;"	macro
UART2_BRR2_DIVF	stm8s_stdperiph_driver\inc\stm8s.h	1902;"	macro
UART2_BRR2_DIVM	stm8s_stdperiph_driver\inc\stm8s.h	1901;"	macro
UART2_BRR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1872;"	macro
UART2_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2467;"	macro
UART2_CR1_M	stm8s_stdperiph_driver\inc\stm8s.h	1907;"	macro
UART2_CR1_PCEN	stm8s_stdperiph_driver\inc\stm8s.h	1909;"	macro
UART2_CR1_PIEN	stm8s_stdperiph_driver\inc\stm8s.h	1911;"	macro
UART2_CR1_PS	stm8s_stdperiph_driver\inc\stm8s.h	1910;"	macro
UART2_CR1_R8	stm8s_stdperiph_driver\inc\stm8s.h	1904;"	macro
UART2_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1873;"	macro
UART2_CR1_T8	stm8s_stdperiph_driver\inc\stm8s.h	1905;"	macro
UART2_CR1_UARTD	stm8s_stdperiph_driver\inc\stm8s.h	1906;"	macro
UART2_CR1_WAKE	stm8s_stdperiph_driver\inc\stm8s.h	1908;"	macro
UART2_CR2_ILIEN	stm8s_stdperiph_driver\inc\stm8s.h	1916;"	macro
UART2_CR2_REN	stm8s_stdperiph_driver\inc\stm8s.h	1918;"	macro
UART2_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1874;"	macro
UART2_CR2_RIEN	stm8s_stdperiph_driver\inc\stm8s.h	1915;"	macro
UART2_CR2_RWU	stm8s_stdperiph_driver\inc\stm8s.h	1919;"	macro
UART2_CR2_SBK	stm8s_stdperiph_driver\inc\stm8s.h	1920;"	macro
UART2_CR2_TCIEN	stm8s_stdperiph_driver\inc\stm8s.h	1914;"	macro
UART2_CR2_TEN	stm8s_stdperiph_driver\inc\stm8s.h	1917;"	macro
UART2_CR2_TIEN	stm8s_stdperiph_driver\inc\stm8s.h	1913;"	macro
UART2_CR3_CKEN	stm8s_stdperiph_driver\inc\stm8s.h	1924;"	macro
UART2_CR3_CPHA	stm8s_stdperiph_driver\inc\stm8s.h	1926;"	macro
UART2_CR3_CPOL	stm8s_stdperiph_driver\inc\stm8s.h	1925;"	macro
UART2_CR3_LBCL	stm8s_stdperiph_driver\inc\stm8s.h	1927;"	macro
UART2_CR3_LINEN	stm8s_stdperiph_driver\inc\stm8s.h	1922;"	macro
UART2_CR3_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1875;"	macro
UART2_CR3_STOP	stm8s_stdperiph_driver\inc\stm8s.h	1923;"	macro
UART2_CR4_ADD	stm8s_stdperiph_driver\inc\stm8s.h	1932;"	macro
UART2_CR4_LBDF	stm8s_stdperiph_driver\inc\stm8s.h	1931;"	macro
UART2_CR4_LBDIEN	stm8s_stdperiph_driver\inc\stm8s.h	1929;"	macro
UART2_CR4_LBDL	stm8s_stdperiph_driver\inc\stm8s.h	1930;"	macro
UART2_CR4_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1876;"	macro
UART2_CR5_HDSEL	stm8s_stdperiph_driver\inc\stm8s.h	1936;"	macro
UART2_CR5_IREN	stm8s_stdperiph_driver\inc\stm8s.h	1938;"	macro
UART2_CR5_IRLP	stm8s_stdperiph_driver\inc\stm8s.h	1937;"	macro
UART2_CR5_NACK	stm8s_stdperiph_driver\inc\stm8s.h	1935;"	macro
UART2_CR5_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1877;"	macro
UART2_CR5_SCEN	stm8s_stdperiph_driver\inc\stm8s.h	1934;"	macro
UART2_CR6_LASE	stm8s_stdperiph_driver\inc\stm8s.h	1942;"	macro
UART2_CR6_LDUM	stm8s_stdperiph_driver\inc\stm8s.h	1940;"	macro
UART2_CR6_LHDF	stm8s_stdperiph_driver\inc\stm8s.h	1944;"	macro
UART2_CR6_LHDIEN	stm8s_stdperiph_driver\inc\stm8s.h	1943;"	macro
UART2_CR6_LSF	stm8s_stdperiph_driver\inc\stm8s.h	1945;"	macro
UART2_CR6_LSLV	stm8s_stdperiph_driver\inc\stm8s.h	1941;"	macro
UART2_CR6_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1878;"	macro
UART2_GTR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1879;"	macro
UART2_PSCR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1880;"	macro
UART2_SR_FE	stm8s_stdperiph_driver\inc\stm8s.h	1896;"	macro
UART2_SR_IDLE	stm8s_stdperiph_driver\inc\stm8s.h	1893;"	macro
UART2_SR_NF	stm8s_stdperiph_driver\inc\stm8s.h	1895;"	macro
UART2_SR_OR	stm8s_stdperiph_driver\inc\stm8s.h	1894;"	macro
UART2_SR_PE	stm8s_stdperiph_driver\inc\stm8s.h	1897;"	macro
UART2_SR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1870;"	macro
UART2_SR_RXNE	stm8s_stdperiph_driver\inc\stm8s.h	1892;"	macro
UART2_SR_TC	stm8s_stdperiph_driver\inc\stm8s.h	1891;"	macro
UART2_SR_TXE	stm8s_stdperiph_driver\inc\stm8s.h	1890;"	macro
UART2_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1864;"	typedef	typeref:struct:UART2_struct
UART2_struct	stm8s_stdperiph_driver\inc\stm8s.h	1849;"	struct
UART3	stm8s_stdperiph_driver\inc\stm8s.h	2558;"	macro
UART3_BRR1_DIVM	stm8s_stdperiph_driver\inc\stm8s.h	2002;"	macro
UART3_BRR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1977;"	macro
UART3_BRR2_DIVF	stm8s_stdperiph_driver\inc\stm8s.h	2005;"	macro
UART3_BRR2_DIVM	stm8s_stdperiph_driver\inc\stm8s.h	2004;"	macro
UART3_BRR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1978;"	macro
UART3_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2468;"	macro
UART3_CR1_M	stm8s_stdperiph_driver\inc\stm8s.h	2010;"	macro
UART3_CR1_PCEN	stm8s_stdperiph_driver\inc\stm8s.h	2012;"	macro
UART3_CR1_PIEN	stm8s_stdperiph_driver\inc\stm8s.h	2014;"	macro
UART3_CR1_PS	stm8s_stdperiph_driver\inc\stm8s.h	2013;"	macro
UART3_CR1_R8	stm8s_stdperiph_driver\inc\stm8s.h	2007;"	macro
UART3_CR1_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1979;"	macro
UART3_CR1_T8	stm8s_stdperiph_driver\inc\stm8s.h	2008;"	macro
UART3_CR1_UARTD	stm8s_stdperiph_driver\inc\stm8s.h	2009;"	macro
UART3_CR1_WAKE	stm8s_stdperiph_driver\inc\stm8s.h	2011;"	macro
UART3_CR2_ILIEN	stm8s_stdperiph_driver\inc\stm8s.h	2019;"	macro
UART3_CR2_REN	stm8s_stdperiph_driver\inc\stm8s.h	2021;"	macro
UART3_CR2_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1980;"	macro
UART3_CR2_RIEN	stm8s_stdperiph_driver\inc\stm8s.h	2018;"	macro
UART3_CR2_RWU	stm8s_stdperiph_driver\inc\stm8s.h	2022;"	macro
UART3_CR2_SBK	stm8s_stdperiph_driver\inc\stm8s.h	2023;"	macro
UART3_CR2_TCIEN	stm8s_stdperiph_driver\inc\stm8s.h	2017;"	macro
UART3_CR2_TEN	stm8s_stdperiph_driver\inc\stm8s.h	2020;"	macro
UART3_CR2_TIEN	stm8s_stdperiph_driver\inc\stm8s.h	2016;"	macro
UART3_CR3_LINEN	stm8s_stdperiph_driver\inc\stm8s.h	2025;"	macro
UART3_CR3_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1981;"	macro
UART3_CR3_STOP	stm8s_stdperiph_driver\inc\stm8s.h	2026;"	macro
UART3_CR4_ADD	stm8s_stdperiph_driver\inc\stm8s.h	2031;"	macro
UART3_CR4_LBDF	stm8s_stdperiph_driver\inc\stm8s.h	2030;"	macro
UART3_CR4_LBDIEN	stm8s_stdperiph_driver\inc\stm8s.h	2028;"	macro
UART3_CR4_LBDL	stm8s_stdperiph_driver\inc\stm8s.h	2029;"	macro
UART3_CR4_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1982;"	macro
UART3_CR6_LASE	stm8s_stdperiph_driver\inc\stm8s.h	2035;"	macro
UART3_CR6_LDUM	stm8s_stdperiph_driver\inc\stm8s.h	2033;"	macro
UART3_CR6_LHDF	stm8s_stdperiph_driver\inc\stm8s.h	2037;"	macro
UART3_CR6_LHDIEN	stm8s_stdperiph_driver\inc\stm8s.h	2036;"	macro
UART3_CR6_LSF	stm8s_stdperiph_driver\inc\stm8s.h	2038;"	macro
UART3_CR6_LSLV	stm8s_stdperiph_driver\inc\stm8s.h	2034;"	macro
UART3_CR6_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1983;"	macro
UART3_SR_FE	stm8s_stdperiph_driver\inc\stm8s.h	1999;"	macro
UART3_SR_IDLE	stm8s_stdperiph_driver\inc\stm8s.h	1996;"	macro
UART3_SR_NF	stm8s_stdperiph_driver\inc\stm8s.h	1998;"	macro
UART3_SR_OR	stm8s_stdperiph_driver\inc\stm8s.h	1997;"	macro
UART3_SR_PE	stm8s_stdperiph_driver\inc\stm8s.h	2000;"	macro
UART3_SR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1976;"	macro
UART3_SR_RXNE	stm8s_stdperiph_driver\inc\stm8s.h	1995;"	macro
UART3_SR_TC	stm8s_stdperiph_driver\inc\stm8s.h	1994;"	macro
UART3_SR_TXE	stm8s_stdperiph_driver\inc\stm8s.h	1993;"	macro
UART3_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1970;"	typedef	typeref:struct:UART3_struct
UART3_struct	stm8s_stdperiph_driver\inc\stm8s.h	1957;"	struct
UART_ByteSend	user\main.h	63;"	macro
UART_Configuration	user\config.c	119;"	function	signature:(void)
UART_Configuration	user\main.h	145;"	prototype	signature:(void)
USE_FULL_ASSERT	user\stm8s_conf.h	84;"	macro
USE_STDPERIPH_DRIVER	stm8s_stdperiph_driver\inc\stm8s.h	86;"	macro
VECTOR_ID	stm8s_stdperiph_driver\inc\stm8s.h	2644;"	macro
ValBit	stm8s_stdperiph_driver\inc\stm8s.h	2683;"	macro
WR	stm8s_stdperiph_driver\inc\stm8s.h	1620;"	member	struct:WWDG_struct
WWDG	stm8s_stdperiph_driver\inc\stm8s.h	2541;"	macro
WWDG_BaseAddress	stm8s_stdperiph_driver\inc\stm8s.h	2460;"	macro
WWDG_CR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1628;"	macro
WWDG_CR_T	stm8s_stdperiph_driver\inc\stm8s.h	1641;"	macro
WWDG_CR_T6	stm8s_stdperiph_driver\inc\stm8s.h	1640;"	macro
WWDG_CR_WDGA	stm8s_stdperiph_driver\inc\stm8s.h	1639;"	macro
WWDG_GetCounter	stm8s_stdperiph_driver\inc\stm8s_wwdg.h	65;"	prototype	signature:(void)
WWDG_Init	stm8s_stdperiph_driver\inc\stm8s_wwdg.h	63;"	prototype	signature:(uint8_t Counter, uint8_t WindowValue)
WWDG_SWReset	stm8s_stdperiph_driver\inc\stm8s_wwdg.h	66;"	prototype	signature:(void)
WWDG_SetCounter	stm8s_stdperiph_driver\inc\stm8s_wwdg.h	64;"	prototype	signature:(uint8_t Counter)
WWDG_SetWindowValue	stm8s_stdperiph_driver\inc\stm8s_wwdg.h	67;"	prototype	signature:(uint8_t WindowValue)
WWDG_TypeDef	stm8s_stdperiph_driver\inc\stm8s.h	1622;"	typedef	typeref:struct:WWDG_struct
WWDG_WR_MSB	stm8s_stdperiph_driver\inc\stm8s.h	1643;"	macro
WWDG_WR_RESET_VALUE	stm8s_stdperiph_driver\inc\stm8s.h	1629;"	macro
WWDG_WR_W	stm8s_stdperiph_driver\inc\stm8s.h	1644;"	macro
WWDG_struct	stm8s_stdperiph_driver\inc\stm8s.h	1617;"	struct
_COSMIC_	stm8s_stdperiph_driver\inc\stm8s.h	73;"	macro
_IAR_	stm8s_stdperiph_driver\inc\stm8s.h	77;"	macro
_RAISONANCE_	stm8s_stdperiph_driver\inc\stm8s.h	75;"	macro
__CONFIG_H	user\main.h	2;"	macro
__I	stm8s_stdperiph_driver\inc\stm8s.h	194;"	macro
__IO	stm8s_stdperiph_driver\inc\stm8s.h	196;"	macro
__MODS0__	d:\program files\cosmic\cxstm8_eval\hstm8\mods0.h	11;"	macro
__O	stm8s_stdperiph_driver\inc\stm8s.h	195;"	macro
__STM8S_ADC1_H	stm8s_stdperiph_driver\inc\stm8s_adc1.h	23;"	macro
__STM8S_AWU_H	stm8s_stdperiph_driver\inc\stm8s_awu.h	24;"	macro
__STM8S_BEEP_H	stm8s_stdperiph_driver\inc\stm8s_beep.h	25;"	macro
__STM8S_CLK_H	stm8s_stdperiph_driver\inc\stm8s_clk.h	25;"	macro
__STM8S_CONF_H	user\stm8s_conf.h	24;"	macro
__STM8S_EXTI_H__	stm8s_stdperiph_driver\inc\stm8s_exti.h	24;"	macro
__STM8S_FLASH_H	stm8s_stdperiph_driver\inc\stm8s_flash.h	24;"	macro
__STM8S_GPIO_H	stm8s_stdperiph_driver\inc\stm8s_gpio.h	24;"	macro
__STM8S_H	stm8s_stdperiph_driver\inc\stm8s.h	24;"	macro
__STM8S_I2C_H	stm8s_stdperiph_driver\inc\stm8s_i2c.h	24;"	macro
__STM8S_ITC_H__	stm8s_stdperiph_driver\inc\stm8s_itc.h	24;"	macro
__STM8S_IWDG_H	stm8s_stdperiph_driver\inc\stm8s_iwdg.h	24;"	macro
__STM8S_RST_H	stm8s_stdperiph_driver\inc\stm8s_rst.h	23;"	macro
__STM8S_SPI_H	stm8s_stdperiph_driver\inc\stm8s_spi.h	24;"	macro
__STM8S_STDPERIPH_VERSION	stm8s_stdperiph_driver\inc\stm8s.h	174;"	macro
__STM8S_STDPERIPH_VERSION_MAIN	stm8s_stdperiph_driver\inc\stm8s.h	170;"	macro
__STM8S_STDPERIPH_VERSION_RC	stm8s_stdperiph_driver\inc\stm8s.h	173;"	macro
__STM8S_STDPERIPH_VERSION_SUB1	stm8s_stdperiph_driver\inc\stm8s.h	171;"	macro
__STM8S_STDPERIPH_VERSION_SUB2	stm8s_stdperiph_driver\inc\stm8s.h	172;"	macro
__STM8S_TIM1_H	stm8s_stdperiph_driver\inc\stm8s_tim1.h	24;"	macro
__STM8S_TIM2_H	stm8s_stdperiph_driver\inc\stm8s_tim2.h	24;"	macro
__STM8S_TIM4_H	stm8s_stdperiph_driver\inc\stm8s_tim4.h	24;"	macro
__STM8S_UART1_H	stm8s_stdperiph_driver\inc\stm8s_uart1.h	24;"	macro
__STM8S_WWDG_H	stm8s_stdperiph_driver\inc\stm8s_wwdg.h	24;"	macro
_stext	stm8_interrupt_vector.c	78;"	prototype	file:
_vectab	stm8_interrupt_vector.c	81;"	variable
assert_failed	user\main.c	71;"	function	signature:(u8* file, u32 line)
assert_failed	user\stm8s_conf.h	99;"	prototype	signature:(uint8_t* file, uint32_t line)
assert_param	user\stm8s_conf.h	101;"	macro
assert_param	user\stm8s_conf.h	97;"	macro
bool	stm8s_stdperiph_driver\inc\stm8s.h	219;"	typedef	typeref:enum:__anon1
disableInterrupts	stm8s_stdperiph_driver\inc\stm8s.h	2602;"	macro
disableInterrupts	stm8s_stdperiph_driver\inc\stm8s.h	2611;"	macro
disableInterrupts	stm8s_stdperiph_driver\inc\stm8s.h	2621;"	macro
enableInterrupts	stm8s_stdperiph_driver\inc\stm8s.h	2601;"	macro
enableInterrupts	stm8s_stdperiph_driver\inc\stm8s.h	2610;"	macro
enableInterrupts	stm8s_stdperiph_driver\inc\stm8s.h	2620;"	macro
halt	stm8s_stdperiph_driver\inc\stm8s.h	2608;"	macro
halt	stm8s_stdperiph_driver\inc\stm8s.h	2617;"	macro
halt	stm8s_stdperiph_driver\inc\stm8s.h	2627;"	macro
int16_t	stm8s_stdperiph_driver\inc\stm8s.h	200;"	typedef
int32_t	stm8s_stdperiph_driver\inc\stm8s.h	201;"	typedef
int8_t	stm8s_stdperiph_driver\inc\stm8s.h	199;"	typedef
interrupt_handler	stm8_interrupt_vector.c	11;"	member	struct:interrupt_vector	file:
interrupt_handler_t	stm8_interrupt_vector.c	7;"	typedef	file:
interrupt_instruction	stm8_interrupt_vector.c	10;"	member	struct:interrupt_vector	file:
interrupt_vector	stm8_interrupt_vector.c	9;"	struct	file:
main	user\main.c	11;"	function	signature:(void)
nop	stm8s_stdperiph_driver\inc\stm8s.h	2605;"	macro
nop	stm8s_stdperiph_driver\inc\stm8s.h	2614;"	macro
nop	stm8s_stdperiph_driver\inc\stm8s.h	2624;"	macro
rim	stm8s_stdperiph_driver\inc\stm8s.h	2603;"	macro
rim	stm8s_stdperiph_driver\inc\stm8s.h	2612;"	macro
rim	stm8s_stdperiph_driver\inc\stm8s.h	2622;"	macro
s16	stm8s_stdperiph_driver\inc\stm8s.h	211;"	typedef
s32	stm8s_stdperiph_driver\inc\stm8s.h	210;"	typedef
s8	stm8s_stdperiph_driver\inc\stm8s.h	212;"	typedef
sim	stm8s_stdperiph_driver\inc\stm8s.h	2604;"	macro
sim	stm8s_stdperiph_driver\inc\stm8s.h	2613;"	macro
sim	stm8s_stdperiph_driver\inc\stm8s.h	2623;"	macro
trap	stm8s_stdperiph_driver\inc\stm8s.h	2606;"	macro
trap	stm8s_stdperiph_driver\inc\stm8s.h	2615;"	macro
trap	stm8s_stdperiph_driver\inc\stm8s.h	2625;"	macro
u16	stm8s_stdperiph_driver\inc\stm8s.h	215;"	typedef
u32	stm8s_stdperiph_driver\inc\stm8s.h	214;"	typedef
u8	stm8s_stdperiph_driver\inc\stm8s.h	216;"	typedef
uint16_t	stm8s_stdperiph_driver\inc\stm8s.h	205;"	typedef
uint32_t	stm8s_stdperiph_driver\inc\stm8s.h	206;"	typedef
uint8_t	stm8s_stdperiph_driver\inc\stm8s.h	204;"	typedef
wfi	stm8s_stdperiph_driver\inc\stm8s.h	2607;"	macro
wfi	stm8s_stdperiph_driver\inc\stm8s.h	2616;"	macro
wfi	stm8s_stdperiph_driver\inc\stm8s.h	2626;"	macro
