<!DOCTYPE devcfg SYSTEM "devcfg.dtd"[]>
<devcfg>
<name>analog_base_station_M</name>
<type>Master/Stereo output base station</type>
<hardware_platform>CC85XX Headset</hardware_platform>
<operation>Autonomous</operation>
<usb_descriptor>Standard output</usb_descriptor>
<mini_prod_test_en>0</mini_prod_test_en>
<pwc_rev>1.4.0</pwc_rev>
<desc></desc>
<task>
<name>Advanced Options</name>
<attr>
<name>Acquire timeslot period</name>
<value>5750 us</value>
</attr>
<attr>
<name>Fade out when muting</name>
<value>1</value>
</attr>
<attr>
<name>Protocol version</name>
<value>1</value>
</attr>
<attr>
<name>RF data rate</name>
<value>5 Mbps</value>
</attr>
<attr>
<name>Timeslot alignment</name>
<value>Disabled</value>
</attr>
<attr>
<name>Timeslot period</name>
<value>Automatic selection</value>
</attr>
</task>
<task>
<name>Audio Device Customization</name>
<attr>
<name>ACTIVE to LOW-POWER</name>
<value></value>
</attr>
<attr>
<name>Enable digital audio input valid pin</name>
<value>0</value>
</attr>
<attr>
<name>INACTIVE to LOW-POWER</name>
<value></value>
</attr>
<attr>
<name>INACTIVE to SR-SWITCH</name>
<value></value>
</attr>
<attr>
<name>LOW-POWER to ACTIVE</name>
<value></value>
</attr>
<attr>
<name>LOW-POWER to INACTIVE</name>
<value></value>
</attr>
<attr>
<name>OFF to SR-SWITCH</name>
<value></value>
</attr>
<attr>
<name>SR-SWITCH 32000 to INACTIVE</name>
<value></value>
</attr>
<attr>
<name>SR-SWITCH 40275 to INACTIVE</name>
<value></value>
</attr>
<attr>
<name>SR-SWITCH 44100 to INACTIVE</name>
<value></value>
</attr>
<attr>
<name>SR-SWITCH 48000 to INACTIVE</name>
<value></value>
</attr>
<attr>
<name>SR-SWITCH to OFF</name>
<value></value>
</attr>
</task>
<task>
<name>Audio Interface</name>
<attr>
<name>Audio device</name>
<value>AIC3204</value>
</attr>
<attr>
<name>BCLK multiplier</name>
<value>64</value>
</attr>
<attr>
<name>Clock source</name>
<value>Internal with MCLK</value>
</attr>
<attr>
<name>Custom setup</name>
<value>Disabled</value>
</attr>
<attr>
<name>Interface format</name>
<value>I2S</value>
</attr>
<attr>
<name>MCLK multiplier</name>
<value>256</value>
</attr>
<attr>
<name>Resolution</name>
<value>16</value>
</attr>
</task>
<task>
<name>Audio Streaming Master Static</name>
<attr>
<name>Default sample rate</name>
<value>48000</value>
</attr>
<attr>
<name>M2S0 DSP IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 logical channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S1 DSP IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S1 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S1 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S1 logical channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S1 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S2 DSP IO channel</name>
<value>2</value>
</attr>
<attr>
<name>M2S2 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S2 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S2 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>M2S2 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S3 DSP IO channel</name>
<value>3</value>
</attr>
<attr>
<name>M2S3 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S3 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S3 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>M2S3 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S4 DSP IO channel</name>
<value>4</value>
</attr>
<attr>
<name>M2S4 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S4 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S4 logical channel</name>
<value>4</value>
</attr>
<attr>
<name>M2S4 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S5 DSP IO channel</name>
<value>5</value>
</attr>
<attr>
<name>M2S5 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S5 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S5 logical channel</name>
<value>5</value>
</attr>
<attr>
<name>M2S5 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M0 DSP IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 IO pin</name>
<value>1</value>
</attr>
<attr>
<name>S2M0 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>S2M0 streaming format</name>
<value>SLAC</value>
</attr>
<attr>
<name>S2M1 DSP IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M1 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M1 IO pin</name>
<value>1</value>
</attr>
<attr>
<name>S2M1 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>S2M1 streaming format</name>
<value>SLAC</value>
</attr>
<attr>
<name>S2M2 DSP IO channel</name>
<value>2</value>
</attr>
<attr>
<name>S2M2 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M2 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M2 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>S2M2 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M3 DSP IO channel</name>
<value>3</value>
</attr>
<attr>
<name>S2M3 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M3 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M3 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>S2M3 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M4 DSP IO channel</name>
<value>4</value>
</attr>
<attr>
<name>S2M4 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M4 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M4 logical channel</name>
<value>4</value>
</attr>
<attr>
<name>S2M4 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M5 DSP IO channel</name>
<value>5</value>
</attr>
<attr>
<name>S2M5 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M5 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M5 logical channel</name>
<value>5</value>
</attr>
<attr>
<name>S2M5 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>SR32000 enabled</name>
<value>1</value>
</attr>
<attr>
<name>SR32000 latency</name>
<value>1024</value>
</attr>
<attr>
<name>SR40275 enabled</name>
<value>1</value>
</attr>
<attr>
<name>SR40275 latency</name>
<value>1024</value>
</attr>
<attr>
<name>SR44100 enabled</name>
<value>1</value>
</attr>
<attr>
<name>SR44100 latency</name>
<value>1024</value>
</attr>
<attr>
<name>SR48000 enabled</name>
<value>1</value>
</attr>
<attr>
<name>SR48000 latency</name>
<value>2048</value>
</attr>
</task>
<task>
<name>Audio Streaming Slave Dynamic</name>
<attr>
<name>Dynamic selection count</name>
<value>2</value>
</attr>
<attr>
<name>Dynamic selection mechanism</name>
<value>None</value>
</attr>
<attr>
<name>IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 logical channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S1 logical channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S2 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>M2S3 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>M2S4 logical channel</name>
<value>4</value>
</attr>
<attr>
<name>M2S5 logical channel</name>
<value>5</value>
</attr>
<attr>
<name>M2S6 logical channel</name>
<value>6</value>
</attr>
<attr>
<name>M2S7 logical channel</name>
<value>7</value>
</attr>
<attr>
<name>S2M0 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>S2M1 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>S2M2 logical channel</name>
<value>4</value>
</attr>
<attr>
<name>S2M3 logical channel</name>
<value>5</value>
</attr>
</task>
<task>
<name>Audio Streaming Slave EHIF</name>
<attr>
<name>M2S0 DSP IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S1 DSP IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S1 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S1 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S2 DSP IO channel</name>
<value>2</value>
</attr>
<attr>
<name>M2S2 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S2 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S3 DSP IO channel</name>
<value>3</value>
</attr>
<attr>
<name>M2S3 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S3 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S4 DSP IO channel</name>
<value>4</value>
</attr>
<attr>
<name>M2S4 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S4 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S5 DSP IO channel</name>
<value>5</value>
</attr>
<attr>
<name>M2S5 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S5 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 DSP IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M1 DSP IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M1 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M1 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M2 DSP IO channel</name>
<value>2</value>
</attr>
<attr>
<name>S2M2 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M2 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M3 DSP IO channel</name>
<value>3</value>
</attr>
<attr>
<name>S2M3 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M3 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M4 DSP IO channel</name>
<value>4</value>
</attr>
<attr>
<name>S2M4 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M4 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M5 DSP IO channel</name>
<value>5</value>
</attr>
<attr>
<name>S2M5 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M5 IO pin</name>
<value>0</value>
</attr>
</task>
<task>
<name>Audio Streaming Slave Static</name>
<attr>
<name>M2S0 DSP IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 logical channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S1 DSP IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S1 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S1 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S1 logical channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S2 DSP IO channel</name>
<value>2</value>
</attr>
<attr>
<name>M2S2 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S2 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S2 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>M2S3 DSP IO channel</name>
<value>3</value>
</attr>
<attr>
<name>M2S3 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S3 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S3 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>M2S4 DSP IO channel</name>
<value>4</value>
</attr>
<attr>
<name>M2S4 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S4 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S4 logical channel</name>
<value>4</value>
</attr>
<attr>
<name>M2S5 DSP IO channel</name>
<value>5</value>
</attr>
<attr>
<name>M2S5 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S5 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>M2S5 logical channel</name>
<value>5</value>
</attr>
<attr>
<name>S2M0 DSP IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 logical channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M1 DSP IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M1 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M1 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M1 logical channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M2 DSP IO channel</name>
<value>2</value>
</attr>
<attr>
<name>S2M2 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M2 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M2 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>S2M3 DSP IO channel</name>
<value>3</value>
</attr>
<attr>
<name>S2M3 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M3 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M3 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>S2M4 DSP IO channel</name>
<value>4</value>
</attr>
<attr>
<name>S2M4 I2S IO channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M4 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M4 logical channel</name>
<value>4</value>
</attr>
<attr>
<name>S2M5 DSP IO channel</name>
<value>5</value>
</attr>
<attr>
<name>S2M5 I2S IO channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M5 IO pin</name>
<value>0</value>
</attr>
<attr>
<name>S2M5 logical channel</name>
<value>5</value>
</attr>
</task>
<task>
<name>Audio Streaming USB Static</name>
<attr>
<name>M2S0 logical channel</name>
<value>0</value>
</attr>
<attr>
<name>M2S0 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S1 logical channel</name>
<value>1</value>
</attr>
<attr>
<name>M2S1 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S2 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>M2S2 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S3 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>M2S3 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S4 logical channel</name>
<value>4</value>
</attr>
<attr>
<name>M2S4 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>M2S5 logical channel</name>
<value>5</value>
</attr>
<attr>
<name>M2S5 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M0 logical channel</name>
<value>0</value>
</attr>
<attr>
<name>S2M0 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M1 logical channel</name>
<value>1</value>
</attr>
<attr>
<name>S2M1 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M2 logical channel</name>
<value>2</value>
</attr>
<attr>
<name>S2M2 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M3 logical channel</name>
<value>3</value>
</attr>
<attr>
<name>S2M3 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M4 logical channel</name>
<value>4</value>
</attr>
<attr>
<name>S2M4 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>S2M5 logical channel</name>
<value>5</value>
</attr>
<attr>
<name>S2M5 streaming format</name>
<value>PCM16</value>
</attr>
<attr>
<name>SR32000 enabled</name>
<value>0</value>
</attr>
<attr>
<name>SR32000 latency</name>
<value>1024</value>
</attr>
<attr>
<name>SR44100 enabled</name>
<value>0</value>
</attr>
<attr>
<name>SR44100 latency</name>
<value>1024</value>
</attr>
<attr>
<name>SR48000 enabled</name>
<value>1</value>
</attr>
<attr>
<name>SR48000 latency</name>
<value>1024</value>
</attr>
</task>
<task>
<name>Device Identification</name>
<attr>
<name>Manufacturer ID</name>
<value>00000001</value>
</attr>
<attr>
<name>Product ID</name>
<value>00000001</value>
</attr>
<attr>
<name>Product name</name>
<value>Dual_mic</value>
</attr>
<attr>
<name>USB device release</name>
<value></value>
</attr>
<attr>
<name>USB product ID</name>
<value></value>
</attr>
<attr>
<name>USB vendor ID</name>
<value></value>
</attr>
</task>
<task>
<name>Human Interface Device</name>
<attr>
<name>HID feature set</name>
<value>Play control</value>
</attr>
</task>
<task>
<name>IO Mapping</name>
<attr>
<name>Active IO level</name>
<value>00000</value>
</attr>
<attr>
<name>Alternate network status LED</name>
<value></value>
</attr>
<attr>
<name>Audio channel selection bit 0</name>
<value></value>
</attr>
<attr>
<name>Audio channel selection bit 1</name>
<value></value>
</attr>
<attr>
<name>Audio channel selection bit 2</name>
<value></value>
</attr>
<attr>
<name>Audio channel selection button</name>
<value></value>
</attr>
<attr>
<name>Audio device PVDD control</name>
<value></value>
</attr>
<attr>
<name>Audio device reset control</name>
<value>GIO2</value>
</attr>
<attr>
<name>Digital audio input valid</name>
<value></value>
</attr>
<attr>
<name>External host interface interrupt</name>
<value></value>
</attr>
<attr>
<name>Fast forward RC button</name>
<value></value>
</attr>
<attr>
<name>Fast forward RC output</name>
<value></value>
</attr>
<attr>
<name>Input volume mute RC button</name>
<value></value>
</attr>
<attr>
<name>Input volume mute RC output</name>
<value></value>
</attr>
<attr>
<name>Input volume mute button</name>
<value></value>
</attr>
<attr>
<name>Mini production test control</name>
<value></value>
</attr>
<attr>
<name>Network pairing button</name>
<value>CSN(C)</value>
</attr>
<attr>
<name>Network standby control button</name>
<value></value>
</attr>
<attr>
<name>Network standby disable RC button</name>
<value></value>
</attr>
<attr>
<name>Network standby disable RC output</name>
<value></value>
</attr>
<attr>
<name>Network standby enable RC button</name>
<value></value>
</attr>
<attr>
<name>Network standby enable RC output</name>
<value></value>
</attr>
<attr>
<name>Network standby toggle RC button</name>
<value></value>
</attr>
<attr>
<name>Network standby toggle RC output</name>
<value></value>
</attr>
<attr>
<name>Network status LED</name>
<value>GIO12</value>
</attr>
<attr>
<name>Output balance left button</name>
<value></value>
</attr>
<attr>
<name>Output balance right button</name>
<value></value>
</attr>
<attr>
<name>Output volume decrement RC button</name>
<value></value>
</attr>
<attr>
<name>Output volume decrement RC output</name>
<value></value>
</attr>
<attr>
<name>Output volume decrement button</name>
<value></value>
</attr>
<attr>
<name>Output volume increment RC button</name>
<value></value>
</attr>
<attr>
<name>Output volume increment RC output</name>
<value></value>
</attr>
<attr>
<name>Output volume increment button</name>
<value></value>
</attr>
<attr>
<name>Output volume mute RC button</name>
<value></value>
</attr>
<attr>
<name>Output volume mute RC output</name>
<value></value>
</attr>
<attr>
<name>Output volume mute button</name>
<value></value>
</attr>
<attr>
<name>Peripheral IO force pull in power-down</name>
<value>00000</value>
</attr>
<attr>
<name>Play-Pause RC button</name>
<value></value>
</attr>
<attr>
<name>Play-Pause RC output</name>
<value></value>
</attr>
<attr>
<name>Power control button</name>
<value></value>
</attr>
<attr>
<name>Power-down indication</name>
<value></value>
</attr>
<attr>
<name>Rewind RC button</name>
<value></value>
</attr>
<attr>
<name>Rewind RC output</name>
<value></value>
</attr>
<attr>
<name>Scan next track RC button</name>
<value></value>
</attr>
<attr>
<name>Scan next track RC output</name>
<value></value>
</attr>
<attr>
<name>Scan previous track RC button</name>
<value></value>
</attr>
<attr>
<name>Scan previous track RC output</name>
<value></value>
</attr>
<attr>
<name>Timeslot alignment control input</name>
<value></value>
</attr>
<attr>
<name>Timeslot alignment control output</name>
<value></value>
</attr>
</task>
<task>
<name>Power Management</name>
<attr>
<name>Input silence detection average threshold</name>
<value>0</value>
</attr>
<attr>
<name>Input silence detection peak threshold</name>
<value>0</value>
</attr>
<attr>
<name>Maximum current consumption</name>
<value>100</value>
</attr>
<attr>
<name>Power control</name>
<value>None</value>
</attr>
<attr>
<name>Power-down on audio input silence</name>
<value>0</value>
</attr>
<attr>
<name>Power-down on audio input silence timeout</name>
<value>1800</value>
</attr>
<attr>
<name>Power-down on audio output silence</name>
<value>0</value>
</attr>
<attr>
<name>Power-down on audio output silence timeout</name>
<value>1800</value>
</attr>
<attr>
<name>Power-down on network inactivity</name>
<value>0</value>
</attr>
<attr>
<name>Power-down on network inactivity timeout</name>
<value>300</value>
</attr>
<attr>
<name>Power-reduction on audio input silence</name>
<value>0</value>
</attr>
<attr>
<name>Power-reduction on audio input silence timeout</name>
<value>5</value>
</attr>
<attr>
<name>Power-reduction on audio output silence</name>
<value>0</value>
</attr>
<attr>
<name>Power-reduction on audio output silence timeout</name>
<value>300</value>
</attr>
<attr>
<name>Power-reduction on network inactivity</name>
<value>0</value>
</attr>
<attr>
<name>Power-reduction on network inactivity timeout</name>
<value>30</value>
</attr>
<attr>
<name>Power-reduction on network standby ADD state</name>
<value>OFF</value>
</attr>
<attr>
<name>VBAT monitoring</name>
<value>0</value>
</attr>
<attr>
<name>VBAT operation threshold</name>
<value>3.100</value>
</attr>
<attr>
<name>VBAT power-up threshold</name>
<value>3.200</value>
</attr>
<attr>
<name>VBAT resistor</name>
<value>100000</value>
</attr>
<attr>
<name>VBAT warning disable threshold</name>
<value>3.500</value>
</attr>
<attr>
<name>VBAT warning enable threshold</name>
<value>3.350</value>
</attr>
</task>
<task>
<name>Radio</name>
<attr>
<name>Antenna diversity enable</name>
<value>0</value>
</attr>
<attr>
<name>Default network ID</name>
<value>FFFFFFFE</value>
</attr>
<attr>
<name>Maximum slave count</name>
<value>2</value>
</attr>
<attr>
<name>Normal LBT threshold</name>
<value>-65</value>
</attr>
<attr>
<name>Pairing button enable</name>
<value>1</value>
</attr>
<attr>
<name>Pairing button timeout</name>
<value>10.0</value>
</attr>
<attr>
<name>Pairing filter level</name>
<value>0</value>
</attr>
<attr>
<name>Pairing mechanism</name>
<value>Protocol master pairing signal</value>
</attr>
<attr>
<name>Pairing minimum RSSI</name>
<value>-20</value>
</attr>
<attr>
<name>Product ID filter mask</name>
<value>00000000</value>
</attr>
<attr>
<name>Product ID filter ref</name>
<value>00000000</value>
</attr>
<attr>
<name>RF channel mask</name>
<value>7FFFE</value>
</attr>
<attr>
<name>Range extender</name>
<value>CC2590 (HGM)</value>
</attr>
<attr>
<name>Target TX power</name>
<value>5</value>
</attr>
<attr>
<name>Timeslot alignment LBT threshold</name>
<value>-40</value>
</attr>
</task>
<task>
<name>Status Indication</name>
<attr>
<name>ACTIVE LED pattern</name>
<value>100,0</value>
</attr>
<attr>
<name>ALONE LED pattern</name>
<value>2,98</value>
</attr>
<attr>
<name>Alternate status LED usage</name>
<value>None</value>
</attr>
<attr>
<name>LOW BATTERY LED pattern</name>
<value>2,23</value>
</attr>
<attr>
<name>LOW BATTERY pattern enable</name>
<value>0</value>
</attr>
<attr>
<name>PAIRING LED pattern</name>
<value>2,16,2,80</value>
</attr>
<attr>
<name>Power-down indication enable</name>
<value>0</value>
</attr>
<attr>
<name>STANDBY LED pattern</name>
<value>50,50</value>
</attr>
<attr>
<name>Status LED enable</name>
<value>1</value>
</attr>
</task>
<task>
<name>User Interface</name>
<attr>
<name>Button custom timing setup</name>
<value>0</value>
</attr>
<attr>
<name>Click + repeat delay</name>
<value>40</value>
</attr>
<attr>
<name>Click + repeat minimum idle time</name>
<value>10</value>
</attr>
<attr>
<name>Click + repeat period</name>
<value>10</value>
</attr>
<attr>
<name>Click maximum hold time</name>
<value>100</value>
</attr>
<attr>
<name>Click minimum idle time</name>
<value>20</value>
</attr>
<attr>
<name>Fast forward</name>
<value>0</value>
</attr>
<attr>
<name>Hold delay</name>
<value>160</value>
</attr>
<attr>
<name>Hold minimum idle time</name>
<value>20</value>
</attr>
<attr>
<name>Input volume mute</name>
<value>0</value>
</attr>
<attr>
<name>Network standby disable</name>
<value>0</value>
</attr>
<attr>
<name>Network standby enable</name>
<value>0</value>
</attr>
<attr>
<name>Network standby toggle</name>
<value>0</value>
</attr>
<attr>
<name>Output volume decrement</name>
<value>0</value>
</attr>
<attr>
<name>Output volume increment</name>
<value>0</value>
</attr>
<attr>
<name>Output volume mute</name>
<value>0</value>
</attr>
<attr>
<name>Play-Pause</name>
<value>0</value>
</attr>
<attr>
<name>Repeat delay</name>
<value>160</value>
</attr>
<attr>
<name>Repeat minimum idle time</name>
<value>10</value>
</attr>
<attr>
<name>Repeat period</name>
<value>10</value>
</attr>
<attr>
<name>Rewind</name>
<value>0</value>
</attr>
<attr>
<name>Scan next track</name>
<value>0</value>
</attr>
<attr>
<name>Scan previous track</name>
<value>0</value>
</attr>
<attr>
<name>State minimum idle time</name>
<value>10</value>
</attr>
</task>
<task>
<name>Volume Control Master</name>
<attr>
<name>Input button control type</name>
<value>Remote</value>
</attr>
<attr>
<name>Input buttons</name>
<value>None</value>
</attr>
<attr>
<name>Input local fixed offset</name>
<value>0.0</value>
</attr>
<attr>
<name>Input local minimum</name>
<value>0.0</value>
</attr>
<attr>
<name>Input remote minimum</name>
<value>0.0</value>
</attr>
<attr>
<name>Input step amount</name>
<value>1</value>
</attr>
<attr>
<name>Input step duration</name>
<value>10</value>
</attr>
<attr>
<name>Output button control type</name>
<value>Local</value>
</attr>
<attr>
<name>Output buttons</name>
<value>None</value>
</attr>
<attr>
<name>Output local default</name>
<value>0.0</value>
</attr>
<attr>
<name>Output local fixed offset</name>
<value>0.0</value>
</attr>
<attr>
<name>Output local minimum</name>
<value>-50.0</value>
</attr>
<attr>
<name>Output remote default</name>
<value>0.0</value>
</attr>
<attr>
<name>Output remote minimum</name>
<value>-50.0</value>
</attr>
<attr>
<name>Output step amount</name>
<value>1</value>
</attr>
<attr>
<name>Output step duration</name>
<value>10</value>
</attr>
</task>
<task>
<name>Volume Control Slave</name>
<attr>
<name>Input buttons</name>
<value>None</value>
</attr>
<attr>
<name>Input local fixed offset</name>
<value>0.0</value>
</attr>
<attr>
<name>Input local minimum</name>
<value>0.0</value>
</attr>
<attr>
<name>Input multi-channel offset enable</name>
<value>1</value>
</attr>
<attr>
<name>Input step amount</name>
<value>1</value>
</attr>
<attr>
<name>Input step duration</name>
<value>10</value>
</attr>
<attr>
<name>Input volume control type</name>
<value>Local</value>
</attr>
<attr>
<name>Output buttons</name>
<value>None</value>
</attr>
<attr>
<name>Output local default</name>
<value>0.0</value>
</attr>
<attr>
<name>Output local fixed offset</name>
<value>0.0</value>
</attr>
<attr>
<name>Output local minimum</name>
<value>-50.0</value>
</attr>
<attr>
<name>Output multi-channel offset enable</name>
<value>1</value>
</attr>
<attr>
<name>Output step amount</name>
<value>1</value>
</attr>
<attr>
<name>Output step duration</name>
<value>10</value>
</attr>
<attr>
<name>Output volume control type</name>
<value>Local</value>
</attr>
</task>
</devcfg>
