
<li>fet430_1.s43 - Software Toggle P5.1</li>
<li>fet430_adc12_01.s43 - ADC12, Sample A0, Set P5.1 if A0 > 0.5*AVcc</li>
<li>fet430_adc12_02.s43 - ADC12, Using the Internal Reference</li>
<li>fet430_adc12_03.s43 - ADC12, Sample A10 Temp, Set P5.1 if temp ++ ~2c</li>
<li>fet430_adc12_04.s43 - ADC12, Extend Sampling Period With SHT Bits</li>
<li>fet430_adc12_05.s43 - ADC12, Using an External Reference</li>
<li>fet430_adc12_06.s43 - ADC12, Repeated Sequence of Conversions</li>
<li>fet430_adc12_07.s43 - ADC12, Repeated Single Channel Conversions</li>
<li>fet430_adc12_08.s43 - ADC12, Using 10 External Channels of Conversion</li>
<li>fet430_adc12_09.s43 - ADC12, Sequence of Conversions (non-repeated)</li>
<li>fet430_adc12_10.s43 - ADC12, Sample A10 Temp and Convert to oC and oF</li>
<li>fet430_adc12_11.s43 - ADC12, Using the Internal Reference, Channel A12</li>
<li>fet430_adc12_12.s43 - ADC12, Using the Internal Reference, Channel A13</li>
<li>fet430_adc12_13.s43 - ADC12, Using the Internal Reference, Channel A14</li>
<li>fet430_adc12_14.s43 - ADC12, Using the Internal Reference, Channel A15</li>
<li>fet430_bt_01.s43 - Basic Timer, Toggle P5.1 Inside ISR, DCO SMCLK</li>
<li>fet430_bt_02.s43 - Basic Timer, Toggle P5.1 Inside ISR, 32kHz ACLK</li>
<li>fet430_clks_01.s43 - FLL+, Output MCLK, SMCLK, ACLK Using 32kHz XTAL</li>
<li>fet430_clks_02.s43 - FLL+, Output 32kHz Xtal + HF Xtal + Internal DCO</li>
<li>fet430_dac12_01.s43 - DAC12_0, Output 1.0V on DAC0</li>
<li>fet430_dac12_02.s43 - DAC12_1, Output 2.0V on DAC1</li>
<li>fet430_dac12_03.s43 - DAC12_0, Output Voltage Ramp on DAC0</li>
<li>fet430_dac12_04.s43 - DAC12_0, Output Voltage Ramp on VeREF+</li>
<li>fet430_dma_01.s43 - DMA0, Repeated Burst to-from RAM, Software Trigger</li>
<li>fet430_dma_02.s43 - DMA0, Repeated Block To P5OUT, CCR2IFG Trigger</li>
<li>fet430_dma_03.s43 - DMA0, Repeated Block UART0 9600, CCR2IFG, ACLK</li>
<li>fet430_dma_04.s43 - DMA0, Block Mode UART1 9600, ACLK</li>
<li>fet430_dma_05.s43 - DMA0, Repeated Block to DAC0 Sine Output, CCR2, DCO</li>
<li>fet430_dma_06.s43 - DMA0, ADC12 A10 Block Xfer to RAM, Timer_B, SMCLK</li>
<li>fet430_dma_07.s43 - DMA0, ADC12 A10 Block Xfer to Flash, Timer_B, SMCLK</li>
<li>fet430_fll_01.s43 - FLL+, Runs Internal DCO at 2.45MHz</li>
<li>fet430_fll_02.s43 - FLL+, Runs Internal DCO at 8MHz</li>
<li>fet430_hfxt2.s43 - FLL+, MCLK Configured to Operate from XT2 HF XTAL</li>
<li>fet430_isp.s43 - Flash In-System Program Memory</li>
<li>fet430_lcd_01.s43 - LCD, Display "0123456" on SBLCDA4 LCD</li>
<li>fet430_lcd_02.s43 - LCD, Display "430" on Varitronix VI-322 LCD</li>
<li>fet430_lpm3.s43 - FLL+, LPM3 Using Basic Timer ISR, 32kHz ACLK</li>
<li>fet430_oa_01.s43 - OA0, Comparator Mode</li>
<li>fet430_oa_02.s43 - OA0, Comparator in General-Purpose Mode</li>
<li>fet430_oa_03.s43 - OA0, General-Purpose Mode</li>
<li>fet430_oa_04.s43 - OA0, Inverting PGA Mode</li>
<li>fet430_oa_05.s43 - OA0, Non-Inverting PGA Mode</li>
<li>fet430_oa_06.s43 - OA0, Unity-Gain Buffer Mode</li>
<li>fet430_oa_07.s43 - OA1, Comparator Mode</li>
<li>fet430_oa_08.s43 - OA1, Comparator in General-Purpose Mode</li>
<li>fet430_oa_09.s43 - OA1, Inverting PGA Mode</li>
<li>fet430_oa_10.s43 - OA1, Non-Inverting PGA Mode</li>
<li>fet430_oa_11.s43 - OA1, Unity-Gain Buffer Mode</li>
<li>fet430_oa_12.s43 - 3-Amp Differential Amplifier with OA0, OA1, and OA2</li>
<li>fet430_oa_13.s43 - 3-Amp Differential Amplifier with OA1, OA2, and OA0</li>
<li>fet430_oa_14.s43 - 3-Amp Differential Amplifier with OA2, OA0, and OA1</li>
<li>fet430_spi0_016x.s43 - USART0, SPI Interface to HC165/164 Shift Registers</li>
<li>fet430_svs_01.s43 - SVS, POR @ 2.5V Vcc</li>
<li>fet430_ta_01.s43 - Timer_A, Toggle P5.1, CCR0 Cont. Mode ISR, DCO SMCLK</li>
<li>fet430_ta_02.s43 - Timer_A, Toggle P5.1, CCR0 Up Mode ISR, DCO SMCLK</li>
<li>fet430_ta_03.s43 - Timer_A, Toggle P5.1, Overflow ISR, DCO SMCLK</li>
<li>fet430_ta_04.s43 - Timer_A, Toggle P5.1, Overflow ISR, 32kHz ACLK</li>
<li>fet430_ta_05.s43 - Timer_A, Toggle P5.1, CCR0 Up Mode ISR, 32kHz ACLK</li>
<li>fet430_ta_16.s43 - Timer_A, PWM TA1-2 Up Mode, DCO SMCLK</li>
<li>fet430_ta_17.s43 - Timer_A, PWM TA1-2 Up Mode, 32kHz ACLK</li>
<li>fet430_tb_01.s43 - Timer_B, Toggle P5.1, CCR0 Cont. Mode ISR, DCO SMCLK</li>
<li>fet430_tb_02.s43 - Timer_B, Toggle P5.1, CCR0 Up Mode ISR, DCO SMCLK</li>
<li>fet430_tb_03.s43 - Timer_B, Toggle P5.1, Overflow ISR, DCO SMCLK</li>
<li>fet430_tb_04.s43 - Timer_B, Toggle P5.1, Overflow ISR, 32kHz ACLK</li>
<li>fet430_tb_05.s43 - Timer_B, Toggle P5.1, CCR0 Up Mode ISR, 32kHz ACLK</li>
<li>fet430_tb_10.s43 - Timer_B, PWM TB1-2 Up Mode, DCO SMCLK</li>
<li>fet430_tb_11.s43 - Timer_B, PWM TB1-2 Up Mode, 32kHz ACLK</li>
<li>fet430_uart01_0115k.s43 - USART0, 115200 UART Echo ISR, DCO SMCLK</li>
<li>fet430_uart01_02400.s43 - USART0, 2400 UART Ultra-low Pwr Echo ISR, 32kHz ACLK</li>
<li>fet430_uart01_09600.s43 - USART0, 9600 UART Echo ISR, DCO SMCLK</li>
<li>fet430_uart01_19200.s43 - USART0, 19200 UART Echo ISR, DCO SMCLK</li>
<li>fet430_uart02_19200.s43 - USART0, 19200 UART Ultra-low Pwr Echo ISR, DCO SMCLK</li>
<li>fet430_wdt_01.s43 - WDT, Toggle P5.1, Interval Overflow ISR, DCO SMCLK</li>
<li>fet430_wdt_02.s43 - WDT, Toggle P5.1, Interval Overflow ISR, 32kHz ACLK</li>
