
<li>msp430x42x0_1 - Software Toggle P1.0</li>
<li>msp430x42x0_bt_01 - Basic Timer, Toggle P1.0 Inside ISR, DCO SMCLK</li>
<li>msp430x42x0_bt_02 - Basic Timer, Toggle P1.0 Inside ISR, 32kHz ACLK</li>
<li>msp430x42x0_clks_01 - FLL+, Output MCLK, ACLK Using 32kHz XTAL and DCO</li>
<li>msp430x42x0_dac_01 - DAC0 1V output</li>
<li>msp430x42x0_dac_02 - DAC0 1V output with 3x reference</li>
<li>msp430x42x0_dac_03 - DAC0 1V output with AVcc (3v) ref</li>
<li>msp430x42x0_fll_01 - FLL+, Runs Internal DCO at 2.45MHz</li>
<li>msp430x42x0_fll_02 - FLL+, Runs Internal DCO at 8MHz</li>
<li>msp430x42x0_isp - Flash In-System Program Memory</li>
<li>msp430x42x0_lcda_04 - LCD_A Put "0123456" on SBLCDA4 LCD</li>
<li>msp430x42x0_lcda_05 - LCD_A Put "0123456" on SBLCDA4 LCD</li>
<li>msp430x42x0_lcda_06 - LCD_A run a 0-9 counter on TI LCD</li>
<li>msp430x42x0_LFxtal_nmi.s - LFXT1 Oscillator Fault Detection</li>
<li>msp430x42x0_lpm3 - FLL+, LPM3 Using Basic Timer ISR, 32kHz ACLK</li>
<li>msp430x42x0_sd16a_03 - SD16_A, Continuous Conversion on a Single Channel</li>
<li>msp430x42x0_sd16a_04 - SD16_A, Single Conversion on Single Channel Polling IFG</li>
<li>msp430x42x0_sd16a_05 - SD16_A, Single Conversion on Single Channel Using ISR</li>
<li>msp430x42x0_sd16a_07 - SD16_A, Using the Integrated Battery Sensor</li>
<li>msp430x42x0_sd16a_08 - SD16_A, Single Conversion on a Channel using buffered input</li>
<li>msp430x42x0_sd16a_09 - SD16_A, Single Conversion on a Single Channel Using ISR</li>
<li>msp430x42x0_sd16a_10 - SD16_A, Single Conversion on Single Channel Using ISR 1024 Extended Oversampling Rate</li>
<li>msp430x42x0_sd16a_11 - SD16_A, Single Conversion on Single Channel Using ISR ACLK input to SD16_A</li>
<li>msp430x42x0_sd16a_12 - SD16_A, Single Conversion on Single Channel Using ISR SMCLK input is divided by 32</li>
<li>msp430x42x0_ta_01 - Timer_A, Toggle P1.0, CCR0 Cont. Mode ISR, DCO SMCLK</li>
<li>msp430x42x0_ta_02 - Timer_A, Toggle P1.0, CCR0 Up Mode ISR, DCO SMCLK</li>
<li>msp430x42x0_ta_03 - Timer_A, Toggle P1.0, Overflow ISR, DCO SMCLK</li>
<li>msp430x42x0_ta_04 - Timer_A, Toggle P1.0, Overflow ISR, 32kHz ACLK</li>
<li>msp430x42x0_ta_05 - Timer_A, Toggle P1.0, CCR0 Up Mode ISR, 32kHz ACLK</li>
<li>msp430x42x0_ta_16 - Timer_A, PWM TA1-2 Up Mode, DCO SMCLK</li>
<li>msp430x42x0_ta_17 - Timer_A, PWM TA1-2 Up Mode, 32kHz ACLK</li>
<li>msp430x42x0_ta_22 - Timer_A, Output 40kHz Square Wave, Up Mode, SMCLK DCO</li>
<li>msp430x42x0_ta_25 - Timer_A, Output DTMF, Cont. Mode, DCO SMCLK</li>
<li>msp430x42x0_ta_uart115k - Timer_A, UART 115200 Echo, DCO SMCLK</li>
<li>msp430x42x0_ta_uart2400 - Timer_A, UART 2400 Ultra-low Power Echo, 32kHz ACLK</li>
<li>msp430x42x0_ta_uart9600 - Timer_A, UART 9600 Echo, DCO SMCLK</li>
<li>msp430x42x0_wdt_01 - WDT, Toggle P1.0, Interval Overflow ISR, DCO SMCLK</li>
<li>msp430x42x0_wdt_02 - WDT, Toggle P1.0, Interval Overflow ISR, 32kHz ACLK</li>