
<li>fet120_1.c - Software Toggle P1.0</li>
<li>fet120_adc10_01.c - ADC10, Sample A0, AVcc Ref, Set P1.0 if > 0.5*AVcc</li>
<li>fet120_adc10_02.c - ADC10, Sample A0, 1.5V Ref, Set P1.0 if > 0.2V</li>
<li>fet120_adc10_03.c - ADC10, Sample A10 Temp, Set P1.0 if Temp ++ ~2C</li>
<li>fet120_adc10_04.c - ADC10, Sample A0, Signed, Set P1.0 if > 0.5*AVcc</li>
<li>fet120_adc10_05.c - ADC10, Sample A11, Lo_Batt, Set P1.0 if < 2.3V</li>
<li>fet120_adc10_06.c - ADC10, Output Internal Vref on P2.4 & ADCCLK on P1.0</li>
<li>fet120_adc10_07.c - ADC10, DTC Sample A0 64x, AVcc, Repeat Single, DCO</li>
<li>fet120_adc10_08.c - ADC10, DTC Sample A0 64x, 1.5V, Repeat Single, DCO</li>
<li>fet120_adc10_09.c - ADC10, DTC Sample A10 64x, 1.5V, Repeat Single, DCO</li>
<li>fet120_adc10_10.c - ADC10, DTC Sample A2-0, AVcc, Single Sequence, DCO</li>
<li>fet120_adc10_11.c - ADC10, Sample A0, 1.5V, TA1 Trig, Set P1.0 if > 0.5V</li>
<li>fet120_adc10_12.c - ADC10, Sample A7, 1.5V, TA1 Trig, Ultra-Low Pwr</li>
<li>fet120_adc10_13.c - ADC10, DTC Sample A1 32x, AVcc, TA0 Trig, DCO</li>
<li>fet120_adc10_14.c - ADC10, DTC Sample A1-0 32x, AVcc, Repeat Seq, DCO</li>
<li>fet120_adc10_15.c - ADC10, DTC Sample A10 32x to Flash, Int Ref, DCO</li>
<li>fet120_adc10_temp.c - ADC10, Sample A10 Temp and Convert to oC and oF</li>
<li>fet120_clks.c - Basic Clock, Output Buffered SMCLK, ACLK and MCLK/10</li>
<li>fet120_flash_write.c - Flash In-System Programming, Copy SegA to SegB</li>
<li>fet120_fll_01.c - Basic Clock, Implement Auto RSEL SW FLL</li>
<li>fet120_fll_02.c - Basic Clock, Implement Cont. SW FLL with Auto RSEL</li>
<li>fet120_hfxtal.c - Basic Clock, MCLK Sourced from HF XTAL</li>
<li>fet120_lpm3.c - Basic Clock, LPM3 Using WDT ISR, 32kHz ACLK</li>
<li>fet120_nmi.c - Basic Clock, Configure RST/NMI as NMI</li>
<li>fet120_rosc.c - DCOCLK Biased with External Resistor Rosc</li>
<li>fet120_spi0_016x.c - USART0, SPI Interface with HC165/164 Shift Registers</li>
<li>fet120_spi0_mstr.c - USART0, SPI 3-Wire Master</li>
<li>fet120_spi0_slav.c - USART0, SPI 3-Wire Slave</li>
<li>fet120_ta_01.c - Timer_A, Toggle P1.0, CCR0 Cont. Mode ISR, DCO SMCLK</li>
<li>fet120_ta_02.c - Timer_A, Toggle P1.0, CCR0 Up Mode ISR, DCO SMCLK</li>
<li>fet120_ta_03.c - Timer_A, Toggle P1.0, Overflow ISR, DCO SMCLK</li>
<li>fet120_ta_04.c - Timer_A, Toggle P1.0, Overflow ISR, 32kHz ACLK</li>
<li>fet120_ta_05.c - Timer_A, Toggle P1.0, CCR0 Up Mode ISR, 32kHz ACLK</li>
<li>fet120_ta_06.c - Timer_A, Toggle P1.0, CCR1 Cont. Mode ISR, DCO SMCLK</li>
<li>fet120_ta_07.c - Timer_A, Toggle P1.0-3, Cont. Mode ISR, DCO SMCLK</li>
<li>fet120_ta_08.c - Timer_A, Toggle P1.0-3, Cont. Mode ISR, 32kHz ACLK</li>
<li>fet120_ta_09.c - Timer_A, Toggle P1.0-3, Cont. Mode ISR, HF XTAL ACLK</li>
<li>fet120_ta_10.c - Timer_A, Toggle P1.1/TA0, Up Mode, DCO SMCLK</li>
<li>fet120_ta_11.c - Timer_A, Toggle P1.1/TA0, Up Mode, 32kHz ACLK</li>
<li>fet120_ta_12.c - Timer_A, Toggle P1.1/TA0, Up Mode, HF XTAL ACLK</li>
<li>fet120_ta_13.c - Timer_A, Toggle P1.1/TA0, Up/Down Mode, DCO SMCLK</li>
<li>fet120_ta_14.c - Timer_A, Toggle P1.1/TA0, Up/Down Mode, 32kHz ACLK</li>
<li>fet120_ta_15.c - Timer_A, Toggle P1.1/TA0, Up/Down Mode, HF XTAL ACLK</li>
<li>fet120_ta_16.c - Timer_A, PWM TA1-2, Up Mode, DCO SMCLK</li>
<li>fet120_ta_17.c - Timer_A, PWM TA1-2, Up Mode, 32kHz ACLK</li>
<li>fet120_ta_18.c - Timer_A, PWM TA1-2, Up Mode, HF XTAL ACLK</li>
<li>fet120_ta_19.c - Timer_A, PWM TA1-2, Up/Down Mode, DCO SMCLK</li>
<li>fet120_ta_20.c - Timer_A, PWM TA1-2, Up/Down Mode, 32kHz ACLK</li>
<li>fet120_ta_21.c - Timer_A, PWM TA1-2, Up/Down Mode, HF XTAL ACLK</li>
<li>fet120_uart01_0115k.c - USART0, UART 115200 Echo ISR, HF XTAL ACLK</li>
<li>fet120_uart01_02400.c - USART0, Ultra-Low Pwr UART 2400 Echo ISR, 32kHz ACLK</li>
<li>fet120_uart01_09600.c - USART0, UART 9600 Echo ISR, HF XTAL ACLK</li>
<li>fet120_uart01_19200.c - USART0, UART 19200 Echo ISR, HF XTAL ACLK</li>
<li>fet120_uart02_09600.c - USART0, Ultra-Low Pwr UART 9600 Echo ISR, 32kHz ACLK</li>
<li>fet120_uart02_19200.c - USART0, Ultra-Low Pwr UART 19200 Echo ISR, 32kHz ACLK</li>
<li>fet120_uart03_09600.c - USART0, UART 9600 Echo ISR, 32kHz ACLK + DCO</li>
<li>fet120_uart03_19200.c - USART0, UART 19200 Echo ISR, 32kHz ACLK + DCO</li>
<li>fet120_uart04_09600.c - USART0, UART 9600 Echo ISR, No XTAL, Rosc DCO Only</li>
<li>fet120_uart04_19200.c - USART0, UART 19200 Echo ISR, No XTAL, Rosc DCO Only</li>
<li>fet120_uart05_09600.c - USART0, Ultra-Low Pwr 9600 Echo ISR, 32kHz ACLK</li>
<li>fet120_uart06_09600.c - USART0, Ultra-Low Pwr UART 9600 String, 32kHz ACLK</li>
<li>fet120_wdt_01.c - WDT, Toggle P1.0, Interval Overflow ISR, DCO SMCLK</li>
<li>fet120_wdt_02.c - WDT, Toggle P1.0, Interval Overflow ISR, 32kHz ACLK</li>
<li>fet120_wdt_03.c - WDT, Toggle P1.0, Interval Overflow ISR, HF XTAL ACLK</li>
