File Name                         Description
--------------------------------------------------------------------------------
msp430x20x1_ca_01.s43             Comp_A, Output Reference Voltages on P1.1
msp430x20x1_ca_02.s43             Comp_A, Detect Threshold, Set P1.0 if P1.1 > 0.25*Vcc
msp430x20x1_ca_03.s43             Comp_A, Simple 2.2V Low Battery Detect
msp430x20x3_1.s43                 Software Toggle P1.0
msp430x20x3_1_vlo.s43             Software Toggle P1.0, MCLK = VLO/8
msp430x20x3_clks.s43              Basic Clock, Output Buffered SMCLK, ACLK and MCLK/10
msp430x20x3_flashwrite_01.s43     Flash In-System Programming, Copy SegC to SegD
msp430x20x3_flashwrite_03.s43     Flash In-System Programming w/ EEI, Copy SegC to SegD
msp430x20x3_LFxtal_nmi.s43        LFXT1 Oscillator Fault Detection
msp430x20x3_lpm3.s43              Basic Clock, LPM3 Using WDT ISR, 32kHz ACLK
msp430x20x3_lpm3_vlo.s43          Basic Clock, LPM3 Using WDT ISR, VLO ACLK
msp430x20x3_nmi.s43               Basic Clock, Configure RST/NMI as NMI
msp430x20x3_P1_01.s43             Software Poll P1.4, Set P1.0 if P1.4 = 1
msp430x20x3_P1_02.s43             Software Port Interrupt on P1.4 from LPM4
msp430x20x3_P1_03.s43             Poll P1 With Software with Internal Pull-up
msp430x20x3_P1_04.s43             P1 Interrupt from LPM4 with Internal Pull-up
msp430x20x3_sd16A_01.s43          SD16A, Sample A1+ Continuously, Set P1.0 if > 0.3V
msp430x20x3_sd16A_02.s43          SD16, Using the Integrated Temperature Sensor
msp430x20x3_ta_01.s43             Timer_A, Toggle P1.0, CCR0 Cont. Mode ISR, DCO SMCLK
msp430x20x3_ta_02.s43             Timer_A, Toggle P1.0, CCR0 Up Mode ISR, DCO SMCLK
msp430x20x3_ta_03.s43             Timer_A, Toggle P1.0, Overflow ISR, DCO SMCLK
msp430x20x3_ta_04.s43             Timer_A, Toggle P1.0, Overflow ISR, 32kHz ACLK
msp430x20x3_ta_05.s43             Timer_A, Toggle P1.0, CCR0 Up Mode ISR, 32kHz ACLK
msp430x20x3_ta_06.s43             Timer_A, Toggle P1.0, CCR1 Cont. Mode ISR, DCO SMCLK
msp430x20x3_ta_07.s43             Timer_A, Toggle P1.0-3, Cont. Mode ISR, DCO SMCLK
msp430x20x3_ta_08.s43             Timer_A, Toggle P1.0-2, Cont. Mode ISR, 32kHz ACLK
msp430x20x3_ta_10.s43             Timer_A, Toggle P1.1/TA0, Up Mode, DCO SMCLK
msp430x20x3_ta_11.s43             Timer_A, Toggle P1.1/TA0, Up Mode, 32kHz ACLK
msp430x20x3_ta_13.s43             Timer_A, Toggle P1.1/TA0, Up/Down Mode, DCO SMCLK
msp430x20x3_ta_14.s43             Timer_A, Toggle P1.1/TA0, Up/Down Mode, 32kHz ACLK
msp430x20x3_ta_16.s43             Timer_A, PWM TA1, Up Mode, DCO SMCLK
msp430x20x3_ta_17.s43             Timer_A, PWM TA1, Up Mode, 32kHz ACLK
msp430x20x3_ta_19.s43             Timer_A, PWM TA1, Up/Down Mode, DCO SMCLK
msp430x20x3_ta_20.s43             Timer_A, PWM TA1-2, Up/Down Mode, 32kHz ACLK
msp430x20x3_ta_uart2400.s43       Timer_A, Ultra-Low Pwr UART 2400 Echo, 32kHz ACLK
msp430x20x3_usi_01.s43            USICNT Used as a One-Shot Timer Function, DCO SMCLK
msp430x20x3_usi_02.s43            SPI full-Duplex 3-wire Master
msp430x20x3_usi_03.s43            SPI full-Duplex 3-wire Slave
msp430x20x3_usi_04.s43            USI SPI Interface to HC165/164 Shift Registers
msp430x20x3_usi_05.s43            USI SPI Interface to TLC549 8-bit ADC
msp430x20x3_wdt_01.s43            WDT, Toggle P1.0, Interval Overflow ISR, DCO SMCLK
msp430x20x3_wdt_02.s43            WDT, Toggle P1.0, Interval Overflow ISR, 32kHz ACLK
msp430x20x3_wdt_04.s43            WDT+ Failsafe Clock, DCO SMCLK
msp430x20x3_wdt_05.s43            Reset on Invalid Address fetch, Toggle P1.0
msp430x20x3_wdt_06.s43            WDT+ Failsafe Clock, 32kHz ACLK