File Name                         Description
--------------------------------------------------------------------------------
msp430x20x1_ca_01.c               Comp_A, Output Reference Voltages on P1.1
msp430x20x1_ca_02.c               Comp_A, Detect Threshold, Set P1.0 if P1.1 > 0.25*Vcc
msp430x20x1_ca_03.c               Comp_A, Simple 2.2V Low Battery Detect
msp430x20x3_1.c                   Software Toggle P1.0
msp430x20x3_1_vlo.c               Software Toggle P1.0, MCLK = VLO/8
msp430x20x3_clks.c                Basic Clock, Output Buffered SMCLK, ACLK and MCLK/10
msp430x20x3_flashwrite_01.c       Flash In-System Programming, Copy SegC to SegD
msp430x20x3_flashwrite_03.c       Flash In-System Programming w/ EEI, Copy SegC to SegD
msp430x20x3_flashwrite_04.c       Flash In-System Programming w/ EEI, Copy SegD to A,B,C
msp430x20x3_LFxtal_nmi.c          LFXT1 Oscillator Fault Detection
msp430x20x3_lpm3.c                Basic Clock, LPM3 Using WDT ISR, 32kHz ACLK
msp430x20x3_lpm3_vlo.c            Basic Clock, LPM3 Using WDT ISR, VLO ACLK
msp430x20x3_nmi.c                 Basic Clock, Configure RST/NMI as NMI
msp430x20x3_P1_01.c               Software Poll P1.4, Set P1.0 if P1.4 = 1
msp430x20x3_P1_02.c               Software Port Interrupt Service on P1.4 from LPM4
msp430x20x3_P1_03.c               Poll P1 With Software with Internal Pull-up
msp430x20x3_P1_04.c               P1 Interrupt from LPM4 with Internal Pull-up
msp430x20x3_sd16A_01.c            SD16A, Sample A1+ Continuously, Set P1.0 if > 0.3V
msp430x20x3_sd16A_02.c            SD16, Using the Integrated Temperature Sensor
msp430x20x3_ta_01.c               Timer_A, Toggle P1.0, CCR0 Cont. Mode ISR, DCO SMCLK
msp430x20x3_ta_02.c               Timer_A, Toggle P1.0, CCR0 Up Mode ISR, DCO SMCLK
msp430x20x3_ta_03.c               Timer_A, Toggle P1.0, Overflow ISR, DCO SMCLK
msp430x20x3_ta_04.c               Timer_A, Toggle P1.0, Overflow ISR, 32kHz ACLK
msp430x20x3_ta_05.c               Timer_A, Toggle P1.0, CCR0 Up Mode ISR, 32kHz ACLK
msp430x20x3_ta_06.c               Timer_A, Toggle P1.0, CCR1 Cont. Mode ISR, DCO SMCLK
msp430x20x3_ta_07.c               Timer_A, Toggle P1.0-2, Cont. Mode ISR, DCO SMCLK
msp430x20x3_ta_08.c               Timer_A, Toggle P1.0-2, Cont. Mode ISR, 32kHz ACLK
msp430x20x3_ta_10.c               Timer_A, Toggle P1.1/TA0, Up Mode, DCO SMCLK
msp430x20x3_ta_11.c               Timer_A, Toggle P1.1/TA0, Up Mode, 32kHz ACLK
msp430x20x3_ta_13.c               Timer_A, Toggle P1.1/TA0, Up/Down Mode, DCO SMCLK
msp430x20x3_ta_14.c               Timer_A, Toggle P1.1/TA0, Up/Down Mode, 32kHz ACLK
msp430x20x3_ta_16.c               Timer_A, PWM TA1-2, Up Mode, DCO SMCLK
msp430x20x3_ta_17.c               Timer_A, PWM TA1, Up Mode, 32kHz ACLK
msp430x20x3_ta_19.c               Timer_A, PWM TA1, Up/Down Mode, DCO SMCLK
msp430x20x3_ta_20.c               Timer_A, PWM TA1, Up/Down Mode, 32kHz ACLK
msp430x20x3_ta_uart2400.c         Timer_A, Ultra-Low Pwr UART 2400 Echo, 32kHz ACLK
msp430x20x3_usi_01.c              USICNT Used as a One-Shot Timer Function, DCO SMCLK
msp430x20x3_usi_02.c              SPI full-Duplex 3-wire Master
msp430x20x3_usi_03.c              SPI full-Duplex 3-wire Slave
msp430x20x3_usi_04.c              USI SPI Interface with HC165/164 Shift Registers
msp430x20x3_usi_05.c              USI SPI Interface to TLC549 8-bit ADC
msp430x20x3_usi_06.c              I2C Master Receiver, single byte
msp430x20x3_usi_07.c              I2C Master Transmitter, single byte
msp430x20x3_usi_08.c              I2C Slave Receiver, single byte
msp430x20x3_usi_09.c              I2C Slave Transmitter, single byte
msp430x20x3_wdt_01.c              WDT, Toggle P1.0, Interval Overflow ISR, DCO SMCLK
msp430x20x3_wdt_02.c              WDT, Toggle P1.0, Interval Overflow ISR, 32kHz ACLK
msp430x20x3_wdt_04.c              WDT+ Failsafe Clock, DCO SMCLK
msp430x20x3_wdt_05.c              Reset on Invalid Address fetch, Toggle P1.0
msp430x20x3_wdt_06.c              WDT+ Failsafe Clock, 32kHz ACLK