;******************************************************************************
;   MSP-FET430P120 Demo - ADC10, DTC Sample A1-0 32x, AVcc, Repeat Seq, DCO
;
;   Description: Use DTC to sample A1/A0 repeat sequence 32x(64 total samples)
;   with reference to AVcc.  Software writes to ADC10SC to trigger sample burst.
;   In Mainloop MSP430 waits in LPM0 to save power until ADC10 conversion
;   complete, ADC10_ISR will force exit from any LPMx in Mainloop on reti.
;   ADC10 internal oscillator times sample period (16x) and conversion (13x).
;   DTC transfers conversion code to RAM 200h - 280h.  ADC10(DTC) interrupt
;   will return system active. P1.0 set at start of conversion burst, reset
;   on completion.
;   //* MSP430F1232 or MSP430F1132 Device Required *//
;
;                MSP430F1232
;             -----------------
;         /|\|              XIN|-
;          | |                 |
;          --|RST          XOUT|-
;            |                 |
;        >---|A1           P1.0|-->LED
;        >---|A0
;
;   M. Buccini
;   Texas Instruments Inc.
;   Feb 2005
;   Built with IAR Embedded Workbench Version: 3.21A
;******************************************************************************
#include  <msp430x12x2.h>
;------------------------------------------------------------------------------
            ORG     0E000h                  ; Program Start
;------------------------------------------------------------------------------
RESET       mov.w   #0300h,SP               ; Initialize stackpointer
StopWDT     mov.w   #WDTPW+WDTHOLD,&WDTCTL  ; Stop WDT
SetupADC10  mov.w   #INCH_1+CONSEQ_3,&ADC10CTL1 ; A1/A0, repeat multi channel
            mov.w   #ADC10SHT_2+MSC+ADC10ON+ADC10IE,&ADC10CTL0 ;
            bis.b   #03h,&ADC10AE           ; P2.0,1 ADC option select
            mov.b   #040h,&ADC10DTC1        ; 64 conversions
SetupP1     bis.b   #001h,&P1DIR            ; P1.0 output
                                            ;
Mainloop    bis.b   #001h,&P1OUT            ; P1.0 = 1
busy_test   bit     #BUSY,&ADC10CTL1        ; ADC10 core inactive?
            jnz     busy_test               ;
            mov.w   #0200h,&ADC10SA         ; Data buffer start
            bis.w   #ENC+ADC10SC,&ADC10CTL0 ; Start sampling
            bis.w   #CPUOFF+GIE,SR          ; CPU off, Enable interrupts
            bic.b   #001h,&P1OUT            ; P1.0 = 0
            jmp     Mainloop                ; Again
                                            ;
;------------------------------------------------------------------------------
ADC10_ISR;
;------------------------------------------------------------------------------
            bic.w   #ENC,&ADC10CTL0         ; ADC10 disabled
            mov.w   #GIE,0(SP)              ; Exit any LPMx on reti
            reti                            ;		
                                            ;
;------------------------------------------------------------------------------
;           Interrupt Vectors
;------------------------------------------------------------------------------
            ORG     0FFFEh                  ; MSP430 RESET Vector
            DW      RESET                   ;
            ORG     0FFEAh                  ; ADC10 Vector
            DW      ADC10_ISR               ;
            END
