
<li>fet410_1.c - Software Toggle P5.1</li>
<li>fet410_LFxtal_nmi.c - LFXT1 Oscillator Fault Detection</li>
<li>fet410_bt_01.c - Basic Timer, Toggle P5.1 Inside ISR, DCO SMCLK</li>
<li>fet410_bt_02.c - Basic Timer, Toggle P5.1 Inside ISR, 32kHz ACLK</li>
<li>fet410_clks_01.c - FLL+, Output MCLK, ACLK Using 32kHz XTAL and DCO</li>
<li>fet410_fll_01.c - FLL+, Runs Internal DCO at 2.45MHz</li>
<li>fet410_fll_02.c - FLL+, Runs Internal DCO at 8MHz</li>
<li>fet410_lcd_01.c - LCD, Display "6543210" on STK/EVK LCD</li>
<li>fet410_lcd_02.c - LCD, Display Numbers on a Static LCD</li>
<li>fet410_lcd_03.c - LCD, Display Numbers on a 4-Mux LCD</li>
<li>fet410_lpm3.c - FLL+, LPM3 Using Basic Timer ISR, 32kHz ACLK</li>
<li>fet410_sd16_01.c - SD16, Continuous Conversion on a Group of Channels</li>
<li>fet410_sd16_02.c - SD16, Single Conversion on a Group of Channels</li>
<li>fet410_sd16_03.c - SD16, Continuous Conversion on a Single Channel</li>
<li>fet410_sd16_04.c - SD16, Single Conversion on Single Channel Polling IFG</li>
<li>fet410_sd16_05.c - SD16, Single Conversion on a Single Channel Using ISR</li>
<li>fet410_sd16_06.c - SD16, Using the Integrated Temperature Sensor</li>
<li>fet410_ta_01.c - Timer_A, Toggle P5.1, CCR0 Cont. Mode ISR, DCO SMCLK</li>
<li>fet410_ta_02.c - Timer_A, Toggle P5.1, CCR0 Up Mode ISR, DCO SMCLK</li>
<li>fet410_ta_03.c - Timer_A, Toggle P5.1, Overflow ISR, DCO SMCLK</li>
<li>fet410_ta_04.c - Timer_A, Toggle P5.1, Overflow ISR, 32kHz ACLK</li>
<li>fet410_ta_05.c - Timer_A, Toggle P5.1, CCR0 Up Mode ISR, 32kHz ACLK</li>
<li>fet410_ta_16.c - Timer_A, PWM TA1-2 Up Mode, DCO SMCLK</li>
<li>fet410_ta_17.c - Timer_A, PWM TA1-2 Up Mode, 32kHz ACLK</li>
<li>fet410_ta_uart115k.c - Timer_A, UART 115200 Echo, DCO SMCLK</li>
<li>fet410_ta_uart2400.c - Timer_A, UART 2400 Ultra-low Power Echo, 32kHz ACLK</li>
<li>fet410_ta_uart9600.c - Timer_A, UART 9600 Echo, DCO SMCLK</li>
<li>fet410_wdt_01.c - WDT, Toggle P5.1, Interval Overflow ISR, DCO SMCLK</li>
<li>fet410_wdt_02.c - WDT, Toggle P5.1, Interval Overflow ISR, 32kHz ACLK</li>
