msp430x22x4_1.c                 Software Toggle P1.0
msp430x22x4_1_vlo.c             Software Toggle P1.0, MCLK = VLO/8
msp430x22x4_lpm3.c              Basic Clock, LPM3 Using WDT ISR, 32kHz ACLK
msp430x22x4_lpm3_vlo.c          Basic Clock, LPM3 Using WDT ISR, VLO ACLK
msp430x22x4_nmi.c               Configure RST/NMI as NMI
msp430x22x4_p1_01.c             Software Poll P1.3, Set P1.0 if P1.3 = 1
msp430x22x4_p1_02.c             Software Port Interrupt Service on P1.3 from LPM4
msp430x22x4_p1_03.c             Poll P1 With Software with Internal Pull-up
msp430x22x4_p1_04.c             P1 Interrupt from LPM4 with Internal Pull-up
msp430x22x4_oa_01.c             OA0, Comparator Mode
msp430x22x4_oa_02.c             OA0, General-Purpose Mode
msp430x22x4_oa_03.c             OA0, Inverting PGA Mode
msp430x22x4_oa_04.c             OA0, Non-Inverting PGA Mode
msp430x22x4_oa_05.c             OA0, Unity-Gain Buffer Mode
msp430x22x4_oa_06.c             OA1, Comparator Mode
msp430x22x4_oa_07.c             OA1, General-Purpose Mode
msp430x22x4_oa_08.c             OA1, Inverting PGA Mode
msp430x22x4_oa_09.c             OA1, Non-Inverting PGA Mode
msp430x22x4_oa_10.c             OA1, Unity-Gain Buffer Mode
msp430x22x4_adc10_01.c          ADC10, Sample A0, AVcc Ref, Set P1.0 if A0 > 0.5*AVcc
msp430x22x4_adc10_02.c          ADC10, Sample A0, 1.5V Ref, Set P1.0 if A0 > 0.2V
msp430x22x4_adc10_03.c          ADC10, Sample A10 Temp, Set P1.0 if Temp ++ ~2C
msp430x22x4_adc10_04.c          ADC10, Sample A0, Signed, Set P1.0 if A0 > 0.5*AVcc
msp430x22x4_adc10_05.c          ADC10, Sample A11, Lo_Batt, Set P1.0 if AVcc < 2.3V
msp430x22x4_adc10_06.c          ADC10, Output Internal Vref on P2.4 & ADCCLK on P1.0
msp430x22x4_adc10_07.c          ADC10, DTC Sample A0 64x, AVcc, Repeat Single, DCO
msp430x22x4_adc10_08.c          ADC10, DTC Sample A0 64x, 1.5V, Repeat Single, DCO
msp430x22x4_adc10_09.c          ADC10, DTC Sample A10 64x, 1.5V, Repeat Single, DCO
msp430x22x4_adc10_10.c          ADC10, DTC Sample A2-0, AVcc, Single Sequence, DCO
msp430x22x4_adc10_11.c          ADC10, Sample A0, 1.5V, TA1 Trig, Set P1.0 if > 0.5V
msp430x22x4_adc10_12.c          ADC10, Sample A7, 1.5V, TA1 Trig, Ultra-Low Pwr
msp430x22x4_adc10_13.c          ADC10, DTC Sample A1 32x, AVcc, TA0 Trig, DCO
msp430x22x4_adc10_14.c          ADC10, DTC Sample A1-0 32x, AVcc, Repeat Seq, DCO
msp430x22x4_adc10_15.c          ADC10, DTC Sample A10 32x to Flash, Int Ref, DCO
msp430x22x4_adc10_16.c          ADC10, DTC Sample A0 -> TA1, AVcc, DCO
msp430x22x4_adc10_17.c          ADC10, DTC Sample A0 -> TA1, AVcc, HF XTAL
msp430x22x4_adc10_18.c          ADC10, DTC Sample A1/0 -> TA1/2, 2.5V, HF XTAL
msp430x22x4_adc10_19.c          ADC10, DTC Sample A0 64x, AVcc, HF XTAL
msp430x22x4_adc10_20.c          ADC10, DTC Sample A0 2-Blk Cont. Mode, AVcc, HF XTAL
msp430x22x4_adc10_temp.c        ADC10, Sample A10 Temp and Convert to oC and oF
msp430x22x4_flashwrite_01.c     Flash In-System Programming, Copy SegC to SegD
msp430x22x4_flashwrite_03.c     Flash In-System Programming w/ EEI, Copy SegC to SegD
msp430x22x4_flashwrite_04.c     Flash In-System Programming w/ EEI, Copy SegD to A/B/C
msp430x22x4_clks.c              Basic Clock, Output Buffered SMCLK, ACLK and MCLK/10
msp430x22x4_fll_01.c            Basic Clock, Implement Auto RSEL SW FLL
msp430x22x4_fll_02.c            Basic Clock, Implement Cont. SW FLL with Auto RSEL
msp430x22x4_hfxtal.c            Basic Clock, MCLK Sourced from HF XTAL
msp430x22x4_hfxtal_nmi.c        Basic Clock, LFXT1/MCLK Sourced from HF XTAL, NMI
msp430x22x4_rosc.c              DCOCLK Biased with External Resistor Rosc
msp430x22x4_dco_flashcal.c      DCO Calibration Constants Programmer
msp430x22x4_ta_01.c             Timer_A, Toggle P1.0, TACCR0 Cont. Mode ISR, DCO SMCLK
msp430x22x4_ta_02.c             Timer_A, Toggle P1.0, TACCR0 Up Mode ISR, DCO SMCLK
msp430x22x4_ta_03.c             Timer_A, Toggle P1.0, Overflow ISR, DCO SMCLK
msp430x22x4_ta_04.c             Timer_A, Toggle P1.0, Overflow ISR, 32kHz ACLK
msp430x22x4_ta_05.c             Timer_A, Toggle P1.0, TACCR0 Up Mode ISR, 32kHz ACLK
msp430x22x4_ta_06.c             Timer_A, Toggle P1.0, TACCR1 Cont. Mode ISR, DCO SMCLK
msp430x22x4_ta_07.c             Timer_A, Toggle P1.0-3, Cont. Mode ISR, DCO SMCLK
msp430x22x4_ta_08.c             Timer_A, Toggle P1.0-3, Cont. Mode ISR, 32kHz ACLK
msp430x22x4_ta_09.c             Timer_A, Toggle P1.0-3, Cont. Mode ISR, HF XTAL ACLK
msp430x22x4_ta_10.c             Timer_A, Toggle P1.1/TA0, Up Mode, DCO SMCLK
msp430x22x4_ta_11.c             Timer_A, Toggle P1.1/TA0, Up Mode, 32kHz ACLK
msp430x22x4_ta_12.c             Timer_A, Toggle P1.1/TA0, Up Mode, HF XTAL ACLK
msp430x22x4_ta_13.c             Timer_A, Toggle P1.1/TA0, Up/Down Mode, DCO SMCLK
msp430x22x4_ta_14.c             Timer_A, Toggle P1.1/TA0, Up/Down Mode, 32kHz ACLK
msp430x22x4_ta_15.c             Timer_A, Toggle P1.1/TA0, Up/Down Mode, HF XTAL ACLK
msp430x22x4_ta_16.c             Timer_A, PWM TA1-2, Up Mode, DCO SMCLK
msp430x22x4_ta_17.c             Timer_A, PWM TA1-2, Up Mode, 32kHz ACLK
msp430x22x4_ta_18.c             Timer_A, PWM TA1-2, Up Mode, HF XTAL ACLK
msp430x22x4_ta_19.c             Timer_A, PWM TA1-2, Up/Down Mode, DCO SMCLK
msp430x22x4_ta_20.c             Timer_A, PWM TA1-2, Up/Down Mode, 32kHz ACLK
msp430x22x4_ta_21.c             Timer_A, PWM TA1-2, Up/Down Mode, HF XTAL ACLK
msp430x22x4_ta_22.c             Timer_A, Ultra-Low Pwr Pulse Accumulator
msp430x22x4_tb_01.c             Timer_B, Toggle P1.0, TBCCR0 Cont. Mode ISR, DCO SMCLK
msp430x22x4_tb_02.c             Timer_B, Toggle P1.0, TBCCR0 Up Mode ISR, DCO SMCLK
msp430x22x4_tb_03.c             Timer_B, Toggle P1.0, Overflow ISR, DCO SMCLK
msp430x22x4_tb_04.c             Timer_B, Toggle P1.0, Overflow ISR, 32kHz ACLK
msp430x22x4_tb_05.c             Timer_B, Toggle P1.0, TBCCR0 Up Mode ISR, 32kHz ACLK
msp430x22x4_tb_06.c             Timer_B, Toggle P1.0, TBCCR1 Cont. Mode ISR, DCO SMCLK
msp430x22x4_tb_07.c             Timer_B, Toggle P4.0-2, Cont. Mode ISR, DCO SMCLK
msp430x22x4_tb_08.c             Timer_B, Toggle P4.0-2, Cont. Mode ISR, 32kHz ACLK
msp430x22x4_tb_09.c             Timer_B, Toggle P4.0-2, Cont. Mode ISR, HF XTAL ACLK
msp430x22x4_tb_10.c             Timer_B, PWM TB1-2, Up Mode, DCO SMCLK
msp430x22x4_tb_11.c             Timer_B, PWM TB1-2, Up Mode, 32kHz ACLK
msp430x22x4_tb_12.c             Timer_B, PWM TB1-2, Up Mode, HF XTAL ACLK
msp430x22x4_tb_13.c             Timer_B, PWM TB1-2, Up/Down Mode, DCO SMCLK
msp430x22x4_tb_14.c             Timer_B, PWM TB1-2, Up/Down Mode, 32kHz ACLK
msp430x22x4_tb_15.c             Timer_B, PWM TB1-2, Up/Down Mode, HF XTAL ACLK
msp430x22x4_wdt_01.c            WDT, Toggle P1.0, Interval Overflow ISR, DCO SMCLK
msp430x22x4_wdt_02.c            WDT, Toggle P1.0, Interval Overflow ISR, 32kHz ACLK
msp430x22x4_wdt_04.c            WDT+ Failsafe Clock, DCO SMCLK
msp430x22x4_wdt_05.c            Reset on Invalid Address fetch, Toggle P1.0
msp430x22x4_wdt_06.c            WDT+ Failsafe Clock, 32kHz ACLK
msp430x22x4_uscia0_uart_01_115k.c               USCI_A0, 115200 UART Echo ISR, DCO SMCLK
msp430x22x4_uscia0_uart_01_115k_lpm.c           USCI_A0, 115200 UART Echo ISR, DCO SMCLK, LPM4
msp430x22x4_uscia0_uart_01_19200.c              USCI_A0, 19200 UART Echo ISR, DCO SMCLK
msp430x22x4_uscia0_uart_01_19200_2.c            USCI_A0, UART 19200 Echo ISR, HF XTAL SMCLK
msp430x22x4_uscia0_uart_01_9600.c               USCI_A0, 9600 UART Echo ISR, DCO SMCLK
msp430x22x4_uscia0_uart_05_9600.c               USCI_A0, Ultra-Low Pwr UART 9600 Echo ISR, 32kHz ACLK
msp430x22x4_uscia0_uart_06_9600.c               USCI_A0, Ultra-Low Pwr UART 9600 String, 32kHz ACLK
msp430x22x4_uscia0_uart_07_9600.c               USCI_A0, Ultra-Low Pwr UART 9600 RX/TX, 32kHz ACLK
msp430x22x4_uscia0_uart_08_9600.c               USCI_A0, UART 9600 Full-Duplex Transceiver, 32kHz ACLK
msp430x22x4_uscia0_spi_01.c     USCI_A0, SPI Interface to HC164 Shift Register
msp430x22x4_uscia0_spi_02.c     USCI_A0, SPI Interface to HC165 Shift Register
msp430x22x4_uscia0_spi_03.c     USCI_A0, SPI Interface to HC165/164 Shift Registers
msp430x22x4_uscia0_spi_09.c     USCI_A0, SPI 3-Wire Master Incremented Data
msp430x22x4_uscia0_spi_10.c     USCI_A0, SPI 3-Wire Slave Data Echo
msp430x22x4_uscib0_spi_01.c     USCI_B0, SPI Interface to TLC549 8-Bit ADC
msp430x22x4_uscib0_spi_02.c     USCI_B0, SPI Interface to TLV1549 10-Bit ADC
msp430x22x4_uscia0_irda_01.c    USCI_A0 IrDA External Loopback Test, 8MHz SMCLK
msp430x22x4_uscia0_irda_02.c    USCI_A0 IrDA Monitor, 8MHz SMCLK
msp430x22x4_uscia0_irda_03.c    USCI_A0 IrDA Physical Layer Comm, 8MHz SMCLK
msp430x22x4_uscib0_i2c_01.c     USCI_B0 I2C Master to TMP100, Set P5.1 if Temp > 28C
msp430x22x4_uscib0_i2c_02.c     USCI_B0 I2C Master Interface to PCF8574, Read/Write
msp430x22x4_uscib0_i2c_03.c     USCI_B0 I2C Master Interface to DAC8571, Write
msp430x22x4_uscib0_i2c_04.c     USCI_B0 I2C Master RX single bytes from MSP430 Slave
msp430x22x4_uscib0_i2c_05.c     USCI_B0 I2C Slave TX single bytes to MSP430 Master
msp430x22x4_uscib0_i2c_06.c     USCI_B0 I2C Master TX single bytes to MSP430 Slave
msp430x22x4_uscib0_i2c_07.c     USCI_B0 I2C Slave RX single bytes from MSP430 Master
msp430x22x4_uscib0_i2c_08.c     USCI_B0 I2C Master TX multiple bytes to MSP430 Slave
msp430x22x4_uscib0_i2c_09.c     USCI_B0 I2C Slave RX multiple bytes from MSP430 Master
msp430x22x4_uscib0_i2c_10.c     USCI_B0 I2C Master RX multiple bytes from MSP430 Slave
msp430x22x4_uscib0_i2c_11.c     USCI_B0 I2C Slave TX multiple bytes to MSP430 Master
