
<li>fet440_1.c - Software Toggle P5.1</li>
<li>fet440_LFxtal_nmi.c - LFXT1 Oscillator Fault Detection</li>
<li>fet440_adc12_01.c - ADC12, Sample A0, Set P5.1 if A0 > 0.5*AVcc</li>
<li>fet440_adc12_02.c - ADC12, Single Conversion on Single Channel</li>
<li>fet440_adc12_03.c - ADC12, Using an External Reference</li>
<li>fet440_adc12_04.c - ADC12, Extend Sampling Period with SHT Bits</li>
<li>fet440_adc12_05.c - ADC12, Using the Internal Reference</li>
<li>fet440_adc12_06.c - ADC12, Repeated Sequence of Conversions</li>
<li>fet440_adc12_07.c - ADC12, Repeated Single Channel Conversions</li>
<li>fet440_adc12_08.c - ADC12, Using 10 External Channels for Conversion</li>
<li>fet440_adc12_09.c - ADC12, Sequence of Conversions (non-repeated)</li>
<li>fet440_adc12_10.c - ADC12, Using the Temperature Sensor</li>
<li>fet440_adc12_11.c - ADC12, Sample A10 Temp and Convert to oC, TA1 Trigger</li>
<li>fet440_bt_01.c - Basic Timer, Toggle P5.1 Inside ISR, DCO SMCLK</li>
<li>fet440_bt_02.c - Basic Timer, Toggle P5.1 Inside ISR, 32kHz ACLK</li>
<li>fet440_clks_02.c - FLL+, Output 32kHz Xtal + HF Xtal + Internal DCO</li>
<li>fet440_fll_01.c - FLL+, Runs Internal DCO at 2.45MHz</li>
<li>fet440_fll_02.c - FLL+, Runs Internal DCO at 8MHz</li>
<li>fet440_lcd_01.c - LCD, Display "6543210" on STK/EVK LCD</li>
<li>fet440_lcd_02.c - LCD, Displays Numbers on a Static LCD</li>
<li>fet440_lcd_03.c - LCD, Displays Numbers on a 4-Mux LCD</li>
<li>fet440_lpm3.c - FLL+, LPM3 Using Basic Timer ISR, 32kHz ACLK</li>
<li>fet440_spi0_016x.c - USART0, SPI Interface with HC165/164 Shift Registers</li>
<li>fet440_svs_01.c - SVS, POR @ 2.5V Vcc</li>
<li>fet440_ta_01.c - Timer_A, Toggle P5.1, CCR0 Cont. Mode ISR, DCO SMCLK</li>
<li>fet440_ta_02.c - Timer_A, Toggle P5.1, CCR0 Up Mode ISR, DCO SMCLK</li>
<li>fet440_ta_03.c - Timer_A, Toggle P5.1, Overflow ISR, DCO SMCLK</li>
<li>fet440_ta_04.c - Timer_A, Toggle P5.1, Overflow ISR, 32kHz ACLK</li>
<li>fet440_ta_05.c - Timer_A, Toggle P5.1, CCR0 Up Mode ISR, 32kHz ACLK</li>
<li>fet440_ta_16.c - Timer_A, PWM TA1-2 Up Mode, DCO SMCLK</li>
<li>fet440_ta_17.c - Timer_A, PWM TA1-2 Up Mode, 32kHz ACLK</li>
<li>fet440_tb_01.c - Timer_B, Toggle P5.1, CCR0 Cont. Mode ISR, DCO SMCLK</li>
<li>fet440_tb_02.c - Timer_B, Toggle P5.1, CCR0 Up Mode ISR, DCO SMCLK</li>
<li>fet440_tb_03.c - Timer_B, Toggle P5.1, Overflow ISR, DCO SMCLK</li>
<li>fet440_tb_04.c - Timer_B, Toggle P5.1, Overflow ISR, 32kHz ACLK</li>
<li>fet440_tb_05.c - Timer_B, Toggle P5.1, CCR0 Up Mode ISR, 32kHz ACLK</li>
<li>fet440_tb_10.c - Timer_B, PWM TB1-6 Up Mode, DCO SMCLK</li>
<li>fet440_tb_11.c - Timer_B, PWM TB1-6 Up Mode, 32kHz ACLK</li>
<li>fet440_uart01_0115k.c - USART0, 115200 UART Echo ISR, DCO SMCLK</li>
<li>fet440_uart01_02400.c - USART0, 2400 UART Ultra-low Pwr Echo ISR, 32kHz ACLK</li>
<li>fet440_uart01_09600.c - USART0, 9600 UART Echo ISR, DCO SMCLK</li>
<li>fet440_uart01_19200.c - USART0, 19200 UART Echo ISR, DCO SMCLK</li>
<li>fet440_uart02_19200.c - USART0, 19200 UART Ultra-low Pwr Echo ISR, 32kHz ACLK</li>
<li>fet440_uart11_19200.c - USART1, 19200 UART Echo ISR, DCO SMCLK</li>
<li>fet440_uart11_38400.c - USART1, 38400 UART Echo ISR, DCO SMCLK</li>
<li>fet440_wdt_01.c - WDT, Toggle P5.1, Interval Overflow ISR, DCO SMCLK</li>
<li>fet440_wdt_02.c - WDT, Toggle P5.1, Interval Overflow ISR, 32kHz ACLK</li>
