
<li>fet410_1.s43 - Software Toggle P5.1</li>
<li>fet410_LFxtal_nmi.s43 - LFXT1 Oscillator Fault Detection</li>
<li>fet410_bt_01.s43 - Basic Timer, Toggle P5.1 Inside ISR, DCO SMCLK</li>
<li>fet410_bt_02.s43 - Basic Timer, Toggle P5.1 Inside ISR, 32kHz ACLK</li>
<li>fet410_clks_01.s43 - FLL+, Output MCLK, ACLK Using 32kHz XTAL and DCO</li>
<li>fet410_fll_01.s43 - FLL+, Runs Internal DCO at 2.45MHz</li>
<li>fet410_fll_02.s43 - FLL+, Runs Internal DCO at 8MHz</li>
<li>fet410_isp.s43 - Flash In-System Program Memory</li>
<li>fet410_lcd_01.s43 - LCD, Display "6543210" on STK/EVK LCD</li>
<li>fet410_lcd_02.s43 - LCD, Display Numbers on a Static LCD</li>
<li>fet410_lcd_03.s43 - LCD, Display Numbers on a 4-Mux LCD</li>
<li>fet410_lpm3.s43 - FLL+, LPM3 Using Basic Timer ISR, 32kHz ACLK</li>
<li>fet410_sd16_01.s43 - SD16, Continuous Conversion on a Group of Channels</li>
<li>fet410_sd16_02.s43 - SD16, Single Conversion on a Group of Channels</li>
<li>fet410_sd16_03.s43 - SD16, Continuous Conversion on a Single Channel</li>
<li>fet410_sd16_04.s43 - SD16, Single Conversion on Single Channel Polling IFG</li>
<li>fet410_sd16_05.s43 - SD16, Single Conversion on Single Channel Using ISR</li>
<li>fet410_sd16_06.s43 - SD16, Using the Integrated Temperature Sensor</li>
<li>fet410_ta_01.s43 - Timer_A, Toggle P5.1, CCR0 Cont. Mode ISR, DCO SMCLK</li>
<li>fet410_ta_02.s43 - Timer_A, Toggle P5.1, CCR0 Up Mode ISR, DCO SMCLK</li>
<li>fet410_ta_03.s43 - Timer_A, Toggle P5.1, Overflow ISR, DCO SMCLK</li>
<li>fet410_ta_04.s43 - Timer_A, Toggle P5.1, Overflow ISR, 32kHz ACLK</li>
<li>fet410_ta_05.s43 - Timer_A, Toggle P5.1, CCR0 Up Mode ISR, 32kHz ACLK</li>
<li>fet410_ta_16.s43 - Timer_A, PWM TA1-2 Up Mode, DCO SMCLK</li>
<li>fet410_ta_17.s43 - Timer_A, PWM TA1-2 Up Mode, 32kHz ACLK</li>
<li>fet410_ta_22.s43 - Timer_A, Output 40kHz Square Wave, Up Mode, SMCLK DCO</li>
<li>fet410_ta_25.s43 - Timer_A, Output DTMF, Cont. Mode, DCO SMCLK</li>
<li>fet410_ta_uart115k.s43 - Timer_A, UART 115200 Echo, DCO SMCLK</li>
<li>fet410_ta_uart2400.s43 - Timer_A, UART 2400 Ultra-low Power Echo, 32kHz ACLK</li>
<li>fet410_ta_uart9600.s43 - Timer_A, UART 9600 Echo, DCO SMCLK</li>
<li>fet410_wdt_01.s43 - WDT, Toggle P5.1, Interval Overflow ISR, DCO SMCLK</li>
<li>fet410_wdt_02.s43 - WDT, Toggle P5.1, Interval Overflow ISR, 32kHz ACLK</li>
