/*
 * Do not modify this file; it is automatically generated from the template
 * linkcmd.xdt in the ti.platforms.stellaris package and will be overwritten.
 */

/*
 * put '"'s around paths because, without this, the linker
 * considers '-' as minus operator, not a file name character.
 */


-l"D:\workspace_teco\modbus_cpld_20160527\Debug\configPkg\package\cfg\modbus_comm_pem3.oem3"
-l"D:\ti\mcusdk_1_00_00_68\products\uia_1_01_01_14\packages\ti\uia\services\lib\release\ti.uia.services.aem3"
-l"D:\ti\mcusdk_1_00_00_68\products\uia_1_01_01_14\packages\ti\uia\sysbios\lib\release\ti.uia.sysbios.aem3"
-l"D:\ti\mcusdk_1_00_00_68\products\uia_1_01_01_14\packages\ti\uia\runtime\lib\release\ti.uia.runtime.aem3"
-l"D:\ti\mcusdk_1_00_00_68\products\xdctools_3_23_04_60\packages\ti\catalog\arm\cortexm3\concertoInit\lib\Boot.aem3"
-l"D:\ti\mcusdk_1_00_00_68\packages\ti\drivers\lib\instrumented\emac_mware.aem3"
-l"D:\ti\mcusdk_1_00_00_68\packages\ti\drivers\lib\instrumented\gpio_mware.aem3"
-l"D:\ti\mcusdk_1_00_00_68\packages\ti\drivers\lib\instrumented\i2c_mware.aem3"
-l"D:\ti\mcusdk_1_00_00_68\packages\ti\drivers\lib\instrumented\sdspi_mware.aem3"
-l"D:\ti\mcusdk_1_00_00_68\packages\ti\drivers\lib\instrumented\uart_mware.aem3"
-l"D:\ti\mcusdk_1_00_00_68\packages\ti\drivers\lib\instrumented\usbmschfatfs_mware.aem3"
-l"D:\ti\mcusdk_1_00_00_68\products\uia_1_01_01_14\packages\ti\uia\events\lib\release\ti.uia.events.aem3"
-l"D:\ti\mcusdk_1_00_00_68\products\bios_6_33_04_39\packages\ti\sysbios\fatfs\lib\release\ti.sysbios.fatfs.aem3"
-l"D:\ti\mcusdk_1_00_00_68\products\bios_6_33_04_39\packages\ti\sysbios\lib\instrumented_em3\sysbios\sysbios.lib"
-l"D:\ti\mcusdk_1_00_00_68\products\xdctools_3_23_04_60\packages\ti\targets\arm\rtsarm\lib\ti.targets.arm.rtsarm.aem3"
-l"D:\ti\mcusdk_1_00_00_68\products\xdctools_3_23_04_60\packages\ti\targets\arm\rtsarm\lib\boot.aem3"
-l"D:\ti\mcusdk_1_00_00_68\products\xdctools_3_23_04_60\packages\ti\targets\arm\rtsarm\lib\auto_init.aem3"

--retain="*(xdc.meta)"

/* C6x Elf symbols */
--symbol_map __TI_STACK_SIZE=__STACK_SIZE
--symbol_map __TI_STACK_BASE=__stack
--symbol_map _stack=__stack


--args 0x0
-heap  0x0
-stack 0x1000

/*
 * Linker command file contributions from all loaded packages:
 */

/* Content from xdc.services.global (null): */

/* Content from xdc (null): */

/* Content from xdc.corevers (null): */

/* Content from xdc.shelf (null): */

/* Content from xdc.services.spec (null): */

/* Content from xdc.services.intern.xsr (null): */

/* Content from xdc.services.intern.gen (null): */

/* Content from xdc.services.intern.cmd (null): */

/* Content from xdc.bld (null): */

/* Content from ti.targets (null): */

/* Content from ti.targets.arm (null): */

/* Content from ti.targets.arm.elf (null): */

/* Content from xdc.rov (null): */

/* Content from xdc.runtime (null): */

/* Content from xdc.services.getset (null): */

/* Content from ti.targets.arm.rtsarm (null): */

/* Content from ti.sysbios.interfaces (null): */

/* Content from ti.sysbios.family (null): */

/* Content from ti.sysbios (null): */

/* Content from ti.sysbios.family.arm (ti/sysbios/family/arm/linkcmd.xdt): */
--retain "*(.vecs)"

/* Content from ti.sysbios.hal (null): */

/* Content from ti.sysbios.knl (null): */

/* Content from ti.sysbios.family.arm.f28m35x (null): */

/* Content from ti.sysbios.fatfs (null): */

/* Content from xdc.rta (null): */

/* Content from ti.uia.events (null): */

/* Content from xdc.runtime.knl (null): */

/* Content from ti.sysbios.syncs (null): */

/* Content from ti.mcusdk (null): */

/* Content from ti.drivers (null): */

/* Content from ti.sysbios.gates (null): */

/* Content from ti.sysbios.heaps (null): */

/* Content from ti.sysbios.utils (null): */

/* Content from ti.sysbios.xdcruntime (null): */

/* Content from ti.sysbios.family.arm.m3 (ti/sysbios/family/arm/m3/linkcmd.xdt): */
--retain "*(.resetVecs)"

/* Content from ti.sysbios.family.arm.lm3 (null): */

/* Content from ti.catalog.arm.cortexm3 (null): */

/* Content from ti.catalog.peripherals.hdvicp2 (null): */

/* Content from ti.catalog (null): */

/* Content from ti.catalog.arm.peripherals.timers (null): */

/* Content from xdc.platform (null): */

/* Content from xdc.cfg (null): */

/* Content from ti.catalog.arm.cortexm3.concertoInit (ti/catalog/arm/cortexm3/concertoInit/linkcmd.xdt): */
-u _ti_catalog_arm_cortexm3_concertoInit_Boot_entry

SECTIONS {
    .flashfuncs  : LOAD = FLASH, RUN = C03SRAM, table(BINIT)
}


/* Content from ti.platforms.concertoM3 (null): */

/* Content from ti.uia.runtime (null): */

/* Content from ti.uia.sysbios (null): */

/* Content from ti.uia.services (null): */

/* Content from configPkg (null): */



/*
 * symbolic aliases for static instance objects
 */
xdc_runtime_Startup__EXECFXN__C = 1;
xdc_runtime_Startup__RESETFXN__C = 1;
TSK_idle = ti_sysbios_knl_Task_Object__table__V + 0;


SECTIONS
{
    .bootVecs:  type = DSECT
    .vecs: load > 0x20000000
    .resetVecs: load > 0x200040
    .ti_catalog_arm_cortexm3_concertoInit_begin: load >> FLASH_BOOT



    xdc.meta: type = COPY
}

