#

##

##

    礦ision Build Log
    Project:
    G:\公司程序\公司自己程序\atmega128单片机程序\LM3SXX\led.uvproj
    Project File Date:  07/29/2016

    Output:
    Rebuild target 'LM3S8962'
    assembling Startup.s...
    compiling pbdata.c...
    compiling main.c...
    compiling gpio.c...
    linking...
    Program Size: Code=3408 RO-data=260 RW-data=284 ZI-data=356
    FromELF: creating hex file...
    ".\output\led.axf" - 0 Error(s), 0 Warning(s).

己程序\\atmega128单片机程序\\LM3SXX\\output\\led.axf" Set JLink Project File to "G:\公司程序\公司自己程序\atmega128单片机程序\LM3SXX\JLinkSettings.ini" * JLink Info: Device "LM3S8962" selected (256 KB flash, 64 KB RAM). JLink info: ------------ DLL: V4.80g, compiled Feb 13 2014 20:50:02 Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08 Hardware: V8.00 Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL * JLink Info: TotalIRLen = 4, IRPrint = 0x01 * JLink Info: Found Cortex-M3 r1p1, Little endian. * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots * JLink Info: TPIU fitted. ROMTableAddr = 0xE00FF003 Target info: ------------ Device: LM3S8962 VTarget = 3.371V State of Pins: TCK: 1, TDI: 0, TDO: 0, TMS: 0, TRES: 1, TRST: 1 Hardware-Breakpoints: 6 Software-Breakpoints: 8192 Watchpoints: 4 JTAG speed: 2000 kHz Erase Done. Programming Done. Verify OK.