#

##

##

    礦ision Build Log
    Project:
    E:\TM4C培训\工程模板\TM4C\ex8-UART_IRda\test.uvproj
    Project File Date:  06/25/2014

    Output:
    Build target 'TM4C'
    compiling main.c...
    linking...
    Program Size: Code=1136 RO-data=16 RW-data=0 ZI-data=352
    ".\Output\test.axf" - 0 Error(s), 0 Warning(s).
    Load "E:\\TM4C培训\\工程模板\\TM4C\\ex8-UART_IRda\\Output\\test.axf"
    Set JLink Project File to "E:\TM4C培训\工程模板\TM4C\ex8-UART_IRda\JLinkSettings.ini"
    * JLink Info: Device "TM4C123BH6PM" selected (256 KB flash, 32 KB RAM).

    JLink info:
    ------------
    DLL: V4.80g, compiled Feb 13 2014 20:50:02
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found Cortex-M4 r0p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: TM4C123BH6PM
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 0, TRES: 1, TRST: 0
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...

peed: 4000 kHz Erase Done. Programming Done. Verify OK. Application running ...