- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_LcdcLiddTiming Struct Reference
LCDC Data Structures

Timing parameters for LCDC in LIDD mode. More...

`#include <csl_lcdc.h>`

## Data Fields
Uint16 | wSu
Uint16 | wStrobe
Uint16 | wHold
Uint16 | rSu
Uint16 | rStrobe
Uint16 | rHold
Uint16 | ta

## Detailed Description

Timing parameters for LCDC in LIDD mode.

Used to configure timing parameters in LIDD mode

## Field Documentation

Uint16 CSL_LcdcLiddTiming::rHold

Read Strobe Hold cycles (0-15)

Uint16 CSL_LcdcLiddTiming::rStrobe

Read Strobe Duration cycles (0-63)

Uint16 CSL_LcdcLiddTiming::rSu

Read Strobe Set-Up cycles (0-31)

Uint16 CSL_LcdcLiddTiming::ta

Turn Around cycles (0-3)

Uint16 CSL_LcdcLiddTiming::wHold

Write Strobe Hold cycles (0-15)

Uint16 CSL_LcdcLiddTiming::wStrobe

Write Strobe Duration cycles (0-63)

Uint16 CSL_LcdcLiddTiming::wSu

Write Strobe Set-Up cycles (0-31)

The documentation for this struct was generated from the following file:

- csl_lcdc.h