- Main Page
- Modules
- Data Structures
- Files

Enumerations
USB CDC Enumerated Data Types
CDC

## Enumerations
enum | CSL_CdcRequestRet { CSL_CDC_REQUEST_DONE = 0, CSL_CDC_REQUEST_STALL, CSL_CDC_REQUEST_SEND_ACK, CSL_CDC_REQUEST_GET_ACK, CSL_CDC_REQUEST_DATA_IN, CSL_CDC_REQUEST_DATA_OUT }
| This Enum defines the Cdc request return values.
enum | CSL_CdcMediaStatus { CSL_CDC_MEDIACCESS_OVERFLOW, CSL_CDC_MEDIACCESS_SUCCESS, CSL_CDC_MEDIACCESS_NOTPRESENT, CSL_CDC_MEDIACCESS_WRITEPROTECT, CSL_CDC_MEDIACCESS_BADMEDIA }
| This Enum defines the Cdc media access status. More...

## Enumeration Type Documentation

enum CSL_CdcMediaStatus

This Enum defines the Cdc media access status.

Enumerator:

  CSL_CDC_MEDIACCESS_OVERFLOW | Media over flow error
  CSL_CDC_MEDIACCESS_SUCCESS | Media Access success
  CSL_CDC_MEDIACCESS_NOTPRESENT | Media not present on the system
  CSL_CDC_MEDIACCESS_WRITEPROTECT | Media is write protected
  CSL_CDC_MEDIACCESS_BADMEDIA | Media is found as bad