- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_I2cIsrAddr Struct Reference
I2C Data Structures

I2C callback pointer structure. More...

`#include <csl_i2c.h>`

## Data Fields
CSL_I2C_EVENT_ISR | alAddr
| ISR for arbitration loss event.
CSL_I2C_EVENT_ISR | nackAddr
| ISR for no acknowledgement event.
CSL_I2C_EVENT_ISR | ardyAddr
| ISR for access ready event.
CSL_I2C_EVENT_ISR | rrdyAddr
| ISR for receive ready event.
CSL_I2C_EVENT_ISR | xrdyAddr
| ISR for transmit ready event.
CSL_I2C_EVENT_ISR | scdAddr
| ISR for stop condition detected event.
CSL_I2C_EVENT_ISR | aasAddr
| ISR for address as slave event.

## Detailed Description

I2C callback pointer structure.

This structure contains pointers to I2C interrupt callback functions

The documentation for this struct was generated from the following file:

- csl_i2c.h