- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_SdioResponse Struct Reference
SDIO Data Structures

Response array received from the controller. More...

`#include <csl_sdio.h>`

## Data Fields
Uint16 | respBuf [8]

## Detailed Description

Response array received from the controller.

This object holds the information the response that is received for a command sent to the card.

## Field Documentation

Uint16 CSL_SdioResponse::respBuf[8]

The response will interpreted as: respBuf[0] - R2[15:0] respBuf[1] - R2[31:16] respBuf[2] - R2[47:32] respBuf[3] - R2[63:48] respBuf[4] - R2[79:64] respBuf[5] - R2[95:80] respBuf[6] - R2[111:96] or R1/R1B/R3/R4/R5/R6[23:8] respBuf[7] - R2[127:112] or R1/R1B/R3/R4/R5/R6[39:24]

Referenced by SDIO_getResponse().

The documentation for this struct was generated from the following file:

- csl_sdio.h