- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_MmcsdResponse Struct Reference
MMC/SD Data Structures

Response array received from the controller. More...

`#include <csl_mmcsd.h>`

## Data Fields
Uint16 | response [CSL_MMCSD_RESP_COUNT]

## Detailed Description

Response array received from the controller.

This object holds the information of the response received for a command sent to the card.

## Field Documentation

Uint16 CSL_MmcsdResponse::response[CSL_MMCSD_RESP_COUNT]

The response will interpreted as: response[0] - R2[15:0] response[1] - R2[31:16] response[2] - R2[47:32] response[3] - R2[63:48] response[4] - R2[79:64] response[5] - R2[95:80] response[6] - R2[111:96] or R1/R1B/R3/R4/R5/R6[23:8] response[7] - R2[127:112] or R1/R1B/R3/R4/R5/R6[39:24]

The documentation for this struct was generated from the following file:

- csl_mmcsd.h